  Configuring PPP on OpenVMS? (RAS) 
 The Question is:
 
Hi..
     I hv a 1000a with openvms 7.1h1. I want to connect a remote pc with
win95 to this server through dialup adapter(tcp/ip-ppp).For this I
configured serial port at 1000a by following commands.
ucx&gt;set interface ucx&gt;pp0/host=192.1.1.9/destination=192.1.1.8
ucx&gt;serial device=tta0
 
After that when I given 'show interface' it is showing 'pp0' but no tcp/ip
address.Even self ping is also not working.Please let me know what other
steps I need to take for configuring PPP at 1000a.
   With many many thanks in advance....Pradeep
 
 The Answer is:
 
  Please see the existing discussions of PPP, configuring PPP,
  and (the current lack of) RAS support on OpenVMS here in the
  OpenVMS Ask The Wizard area.
 
 
