  FTAM and remote command execution? 
 The Question is:
 
while using FTAM, is it possible to execute a command at the remote host ?
 
 
 The Answer is:
 
  The usual approaches involve DECnet task-to-task (DECnet Phase IV,
  DECnet-Plus, or DECnet-Plus over IP), or various IP tools such as rsh
  and rexec.
 
