  configuring TCP/IP (UCX) lpr print queues? 
 The Question is:
 
I know how to make a reverse telnet lisener port and queue using a 90M.
 
Do you know the settings to make it an LPD Queue to a 90M.
 
Thanks,
 
Jeff
 
 The Answer is:
 
  Please see Chapter 16, "Setting Up and Managing the LPR/LPD Print Service"
  in the TCP/IP Services for OpenVMS (UCX) Management manual.  The use of
  the provided ucx$lprsetup tool is the easiest, but you may need to use
  some of the features available only via manual configuration of the
  printcap file or via the various associated logical names.
 
  You will, in particular, want to have the current TCP/IP Services for
  OpenVMS (UCX) version and the associated ECO kit installed.  You will
  also want to have the DNAS V2.2 or later software installed on the
  DECserver 90M.
 
