  Permanent telnet device? 
 The Question is:
 
With TCPIP v5.0a, is there a permanent TNA or BG device similar to the
 permanent NTY device offered by Process Software's MultiNet?
 
(With MultiNet, you can specify that a NTY device persist after the telnet
 connection is closed). So far I have been able to find only
one reference to the term "TNA permanent or temporary".  This is on page 4-71
 of the Digital TCP/IP User's guide (it's a footnote).
 
Regards
 Marie
 
 
 
 The Answer is:
 
  Please see the documentation around the TCP/IP Services for OpenVMS
  TELNET command CREATE_SESSION.
 
  Alternatively -- depending on what you are up to -- bump the channel
  count in the device UCB.
 
