  Problems with MOP and network switch? 
 The Question is:
 
We try to boot an Alpha-Server via MOP-Protocol. This works fine if we do
not use a switch instead of a hub.
We installed an analyzer and the last "good" thing we see is a response from
the mop-server. After this initial response only the client tries to
reconnect to the boot-server.
 
Is this a major problem?
Is there something to configure to the switch?
 
 
 The Answer is:
 
  Please contact your network support organization or the switch vendor,
  as it would appear there is a problem with the configuration.  (And
  without further details of the switch, it is impossible to provide any
  particular suggestions -- based on the correct operation of the MOP
  download, it would appear OpenVMS is correctly configured and that
  the switch is not.)
