  TCP/IP WAN Transport Requirements? 
 The Question is:
 
Does UCX have limitations when utilizing a WAN transport such as Frame Relay
to contact a terminal server which in turn is connected to a modem?
 
 
 The Answer is:
 
  Your question is sufficiently terse as to be extremely difficult
  to answer.
 
  TCP/IP Services for OpenVMS provides an IP transport.
 
  What might be configured in the intervening IP network is generally
  expected to be entirely transparent.
 
  If there are problems, please contact the support organization for
  the network link and (if applicable) intervening network hardware.
 
  If there are problems with the TCP/IP Services product, please contact
  the Compaq Customer Support Center.
 
