  Changing the IP Address? 
 The Question is:
 
how do you change the ip address on an ethernet interface?
 
 The Answer is :
 
  Information on changing the IP host addresses is mentioned in various
  existing topics, including:
 
    (430), (1069), (3991), (5777), (5906), (7710), (8004), etc.
 
  There are other discussions related to IP addressing, including IP
  subnetting and IP supernetting, as well.
 
  On TCP/IP Services package versions prior to V5.0, you will want to
  use the UCX$CONFIG tool when you wish to change your IP host address.
  With the TCP/IP Services V5.0 and later versions, you will want to
  use the TCPIP$CONFIG tool.
 
  Please consider reviewing the available product documentation for
  TCP/IP Services, as well.  The documentation will provide insight
  into the operations of TCP/IP Services and the configuration tool.
 
  The OpenVMS FAQ contains pointers to the documentation website; to
  to the website with the OpenVMS operating system and the TCP/IP
  Services HTML-format product documentation.
 
 Answer written or last revised on  24-JUL-2003 
