;*****************************************************************;
;*****************************************************************;
;**                                                             **;
;**      (C)Copyright 1985-2002, American Megatrends, Inc.      **;
;**                                                             **;
;**                     All Rights Reserved.                    **;
;**                                                             **;
;**           6145-F Northbelt Pkwy, Norcross, GA 30071         **;
;**                                                             **;
;**                     Phone (770)-246-8600                    **;
;**                                                             **;
;*****************************************************************;
;*****************************************************************;

AMIBIOS Setup Script Processor
Version 2.49 (AMISSP Language Version 2)
Copyright (c)1995-1997 American Megatrends, Inc.

Input files:
  BUILD\SSPLIST.SSP (Custom CMOS Page Implementation)

                                 CMOS  CMOS CMOS  Default Failsafe            
Question                         Token Reg. Mask  Value   Value    CkSum Fixed
------------------------------------------------------------------------------
Q_BOOT_FIRST_DEVICE              4088h 11h  000Fh 0000h   0000h    Yes   No 
	(Input file: CORE\SETUP\TEMPLATE.SSP)

Q_COLOR                          41B8h 37h  000Fh 0000h   0000h    Yes   Yes
	(Input file: CORE\SETUP\TEMPLATE.SSP)

Q_DISPLAY_TYPE                   30A3h 14h  0038h 0001h   0001h    Yes   Yes
             00h = _STR$_Absent                    
             01h = _STR$_VGAEGA                    
             02h = RESERVED                        
             03h = _STR$_CGA40x25                  
             04h = RESERVED                        
             05h = _STR$_CGA80x25                  
             06h = RESERVED                        
             07h = _STR$_Mono                      
	(Input file: CORE\CORE.SSP)

Q_DISPLAY_MODE                   108Ch 11h  0010h 0000h   0000h    Yes   No 
             00h = _STR$_Graphics                  
             01h = _STR$_text                      
	(Input file: INTEL\COREMOD\BOOT.SSP)

Q_DATE                           0008h 00h  0000h 0000h   0000h    Yes   No 
             (Control Function = DateControlFunc_FAR)
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_TIME                           0008h 00h  0000h 0000h   0000h    Yes   No 
             (Control Function = TimeControlFunc_FAR)
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_SECONDS                    8000h 00h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_SECONDS_ALARM              8008h 01h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_MINUTES                    8010h 02h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_MINUTES_ALARM              8018h 03h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_HOURS                      8020h 04h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_HOURS_ALARM                8028h 05h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_DAY_OF_WEEK                8030h 06h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_DAY                        8038h 07h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_MONTH                      8040h 08h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_YEAR                       8048h 09h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_STATUS_A                   8050h 0Ah  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_STATUS_B                   8058h 0Bh  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_STATUS_C                   8060h 0Ch  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_STATUS_D                   8068h 0Dh  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_DIAG_STATUS                8070h 0Eh  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_RTC_SHUTDOWN_STATUS            8078h 0Fh  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_FLOPPY_COUNT                   20A6h 14h  00C0h 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_MATHCO_PRESENT                 10A1h 14h  0002h 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_FLOPPY_PRESENT                 10A0h 14h  0001h 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_BASE_MEMORY_LSB                80A8h 15h  00FFh 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_BASE_MEMORY_MSB                80B0h 16h  00FFh 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_EXT_MEMORY_LSB                 80B8h 17h  00FFh 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_EXT_MEMORY_MSB                 80C0h 18h  00FFh 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_PM_TYPE                        4094h 12h  00F0h 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_PS_TYPE                        4090h 12h  000Fh 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_PM_WPCOM                       00F0h 1Eh  FFFFh 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_PS_WPCOM                       0120h 24h  FFFFh 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_PM_E_TYPE                      208Dh 11h  0060h 0001h   0001h    Yes   No 
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_PS_E_TYPE                      2098h 13h  0003h 0001h   0001h    Yes   No 
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_SM_E_TYPE                      209Ah 13h  000Ch 0001h   0001h    Yes   No 
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_SS_E_TYPE                      209Ch 13h  0030h 0001h   0001h    Yes   No 
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_3M_E_TYPE                      209Eh 13h  00C0h 0001h   0001h    Yes   No 
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_3S_E_TYPE                      2148h 29h  0003h 0001h   0001h    Yes   No 
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_4M_E_TYPE                      214Ah 29h  000Ch 0001h   0001h    Yes   No 
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_4S_E_TYPE                      214Ch 29h  0030h 0001h   0001h    Yes   No 
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_CHECKSUM_MSB                   8170h 2Eh  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_CHECKSUM_LSB                   8178h 2Fh  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_POST_EXT_MEMORY_LSB            8180h 30h  00FFh 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_POST_EXT_MEMORY_MSB            8188h 31h  00FFh 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_CENTURY                        8190h 32h  00FFh 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_SCRATCH_33                     8198h 33h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_SCRATCH_34                     81A0h 34h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_SCRATCH_35                     81A8h 35h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_SCRATCH_36                     81B0h 36h  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_EXT_CMOS_CHECKSUM_MSB          81F0h 3Eh  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_EXT_CMOS_CHECKSUM_LSB          81F8h 3Fh  00FFh 0000h   0000h    No    Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_SM_WPCOM                       0218h 43h  FFFFh 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_SS_WPCOM                       0248h 49h  FFFFh 0000h   0000h    Yes   Yes
	(Input file: INTEL\COREMOD\MAIN.SSP)

Q_FLOPPY_A                       4084h 10h  00F0h 0004h   0004h    Yes   Yes
             (External Function = oem_floppyA_type_extfunc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_FLOPPY_B                       4080h 10h  000Fh 0000h   0000h    Yes   Yes
             00h = _STR$_Disabled                  
             01h = _STR$_KB_360                    
             02h = _STR$_MB_12                     
             03h = _STR$_KB_720                    
             04h = _STR$_MB_144                    
             05h = _STR$_MB_288                    
             06h = STR_RESERVED                    
             07h = STR_RESERVED                    
             08h = STR_RESERVED                    
             09h = STR_RESERVED                    
             0Ah = STR_RESERVED                    
             0Bh = STR_RESERVED                    
             0Ch = STR_RESERVED                    
             0Dh = STR_RESERVED                    
             0Eh = STR_RESERVED                    
             0Fh = STR_RESERVED                    
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PCI_IDE_CONTROLLER             31BCh 37h  0070h 0004h   0004h    Yes   No 
             00h = RESERVED                        
             01h = _str$_Disabled                  
             02h = _str$_Primary                   
             03h = _str$_Secondary                 
             04h = _str$_Both                      
             05h = RESERVED                        
             06h = RESERVED                        
             07h = RESERVED                        
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PM_EXT_TYPE                    80C8h 19h  00FFh 0030h   0030h    Yes   Yes
             (External Function = pm_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PM_CYL                         00D8h 1Bh  FFFFh 0000h   0000h    Yes   Yes
             (Control Function = PMCylControlFunc_FAR)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PM_HD                          80E8h 1Dh  00FFh 0000h   0000h    Yes   Yes
             (Control Function = PMHeadControlFunc_FAR)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PM_SPT                         8100h 20h  00FFh 0000h   0000h    Yes   Yes
             (Control Function = PMSptControlFunc_FAR)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PM_LBA_MODE                    1150h 2Ah  0001h 0001h   0001h    Yes   Yes
             (External Function = pm_lba_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PM_BLOCK_MODE                  1151h 2Ah  0002h 0001h   0001h    Yes   Yes
             (External Function = pm_block_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PM_PIO_MODE                    3153h 2Ah  0038h 0000h   0000h    Yes   Yes
             (External Function = pm_pio_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PM_32BIT_XFER                  1152h 2Ah  0004h 0000h   0000h    Yes   Yes
             (External Function = pm_32bit_xfer_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PM_SMART                       214Eh 29h  00C0h 0000h   0000h    Yes   No 
             (External Function = pm_smart_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PM_DMA_MODE                    41C3h 38h  0078h 0000h   0000h    Yes   No 
             (External Function = pm_dma_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PM_EMULATION_TYPE              2156h 2Ah  00C0h 0000h   0000h    Yes   No 
             (External Function = pm_emulation_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PS_EXT_TYPE                    80D0h 1Ah  00FFh 0030h   0030h    Yes   Yes
             (External Function = ps_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PS_CYL                         0108h 21h  FFFFh 0000h   0000h    Yes   Yes
             (Control Function = PSCylControlFunc_FAR)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PS_HD                          8118h 23h  00FFh 0000h   0000h    Yes   Yes
             (Control Function = PSHeadControlFunc_FAR)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PS_SPT                         8130h 26h  00FFh 0000h   0000h    Yes   Yes
             (Control Function = PSSptControlFunc_FAR)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PS_LBA_MODE                    1158h 2Bh  0001h 0001h   0001h    Yes   Yes
             (External Function = ps_lba_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PS_BLOCK_MODE                  1159h 2Bh  0002h 0001h   0001h    Yes   Yes
             (External Function = ps_block_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PS_32BIT_XFER                  115Ah 2Bh  0004h 0000h   0000h    Yes   Yes
             (External Function = ps_32bit_xfer_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PS_PIO_MODE                    315Bh 2Bh  0038h 0000h   0000h    Yes   Yes
             (External Function = ps_pio_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PS_DMA_MODE                    41C8h 39h  000Fh 0000h   0000h    Yes   No 
             (External Function = ps_dma_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PS_SMART                       215Eh 2Bh  00C0h 0000h   0000h    Yes   No 
             (External Function = ps_smart_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PS_EMULATION_TYPE              2166h 2Ch  00C0h 0000h   0000h    Yes   No 
             (External Function = ps_emulation_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SM_TYPE                        8138h 27h  00FFh 0030h   0030h    Yes   Yes
             (External Function = sm_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SM_CYL                         0200h 40h  FFFFh 0000h   0000h    Yes   Yes
             (Control Function = SMCylControlFunc_FAR)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SM_HD                          8210h 42h  00FFh 0000h   0000h    Yes   Yes
             (Control Function = SMHeadControlFunc_FAR)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SM_SPT                         8228h 45h  00FFh 0000h   0000h    Yes   Yes
             (Control Function = SMSptControlFunc_FAR)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SM_LBA_MODE                    1160h 2Ch  0001h 0001h   0001h    Yes   Yes
             (External Function = sm_lba_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SM_BLOCK_MODE                  1161h 2Ch  0002h 0001h   0001h    Yes   Yes
             (External Function = sm_block_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SM_PIO_MODE                    3163h 2Ch  0038h 0000h   0000h    Yes   Yes
             (External Function = sm_pio_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SM_32BIT_XFER                  1162h 2Ch  0004h 0000h   0000h    Yes   Yes
             (External Function = sm_32bit_xfer_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SM_DMA_MODE                    41CCh 39h  00F0h 0000h   0000h    Yes   No 
             (External Function = sm_dma_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SM_SMART                       216Eh 2Dh  00C0h 0000h   0000h    Yes   No 
             (External Function = sm_smart_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SM_EMULATION_TYPE              21C0h 38h  0003h 0000h   0000h    Yes   No 
             (External Function = sm_emulation_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SS_TYPE                        8140h 28h  00FFh 0030h   0030h    Yes   Yes
             (External Function = ss_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SS_CYL                         0230h 46h  FFFFh 0000h   0000h    Yes   Yes
             (Control Function = SSCylControlFunc_FAR)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SS_HD                          8240h 48h  00FFh 0000h   0000h    Yes   Yes
             (Control Function = SSHeadControlFunc_FAR)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SS_SPT                         8258h 4Bh  00FFh 0000h   0000h    Yes   Yes
             (Control Function = SSSptControlFunc_FAR)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SS_LBA_MODE                    1168h 2Dh  0001h 0001h   0001h    Yes   Yes
             (External Function = ss_lba_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SS_BLOCK_MODE                  1169h 2Dh  0002h 0001h   0001h    Yes   Yes
             (External Function = ss_block_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SS_PIO_MODE                    316Bh 2Dh  0038h 0000h   0000h    Yes   Yes
             (External Function = ss_pio_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SS_DMA_MODE                    41D8h 3Bh  000Fh 0000h   0000h    Yes   No 
             (External Function = ss_dma_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SS_32BIT_XFER                  116Ah 2Dh  0004h 0000h   0000h    Yes   Yes
             (External Function = ss_32bit_xfer_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SS_SMART                       21DCh 3Bh  0030h 0000h   0000h    Yes   No 
             (External Function = ss_smart_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_SS_EMULATION_TYPE              21DEh 3Bh  00C0h 0000h   0000h    Yes   No 
             (External Function = ss_emulation_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3M_TYPE                        81E0h 3Ch  00FFh 0030h   0030h    Yes   No 
             (External Function = m3_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3M_LBA_MODE                    108Fh 11h  0080h 0001h   0001h    Yes   No 
             (External Function = m3_lba_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3M_PIO_MODE                    31E8h 3Dh  0007h 0000h   0000h    Yes   No 
             (External Function = m3_pio_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3M_BLOCK_MODE                  11BFh 37h  0080h 0001h   0001h    Yes   No 
             (External Function = m3_block_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3M_DMA_MODE                    41EBh 3Dh  0078h 0000h   0000h    Yes   No 
             (External Function = m3_dma_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3M_32BIT_XFER                  11C7h 38h  0080h 0000h   0000h    Yes   No 
             (External Function = m3_32bit_xfer_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3M_SMART                       2261h 4Ch  0006h 0000h   0000h    Yes   No 
             (External Function = m3_smart_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3M_EMULATION_TYPE              2263h 4Ch  0018h 0000h   0000h    Yes   No 
             (External Function = m3_emulation_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3S_TYPE                        83B0h 76h  00FFh 0030h   0030h    Yes   No 
             (External Function = s3_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3S_LBA_MODE                    11EFh 3Dh  0080h 0001h   0001h    Yes   No 
             (External Function = s3_lba_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3S_BLOCK_MODE                  1265h 4Ch  0020h 0001h   0001h    Yes   No 
             (External Function = s3_block_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3S_PIO_MODE                    32ACh 55h  0070h 0000h   0000h    Yes   No 
             (External Function = s3_pio_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3S_DMA_MODE                    42B4h 56h  00F0h 0000h   0000h    Yes   No 
             (External Function = s3_dma_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3S_SMART                       2266h 4Ch  00C0h 0000h   0000h    Yes   No 
             (External Function = s3_smart_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3S_32BIT_XFER                  1291h 52h  0002h 0000h   0000h    Yes   No 
             (External Function = s3_32bit_xfer_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_3S_EMULATION_TYPE              23A9h 75h  0006h 0000h   0000h    Yes   No 
             (External Function = s3_emulation_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4M_TYPE                        83B8h 77h  00FFh 0030h   0030h    Yes   No 
             (External Function = m4_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4M_LBA_MODE                    12AFh 55h  0080h 0001h   0001h    Yes   No 
             (External Function = m4_lba_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4M_BLOCK_MODE                  12B1h 56h  0002h 0001h   0001h    Yes   No 
             (External Function = m4_block_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4M_PIO_MODE                    33ABh 75h  0038h 0000h   0000h    Yes   No 
             (External Function = m4_pio_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4M_DMA_MODE                    43C0h 78h  000Fh 0000h   0000h    Yes   No 
             (External Function = m4_dma_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4M_SMART                       23AEh 75h  00C0h 0000h   0000h    Yes   No 
             (External Function = m4_smart_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4M_32BIT_XFER                  13C4h 78h  0010h 0000h   0000h    Yes   No 
             (External Function = m4_32bit_xfer_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4M_EMULATION_TYPE              23C5h 78h  0060h 0000h   0000h    Yes   No 
             (External Function = m4_emulation_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4S_TYPE                        83C8h 79h  00FFh 0030h   0030h    Yes   No 
             (External Function = s4_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4S_LBA_MODE                    13C7h 78h  0080h 0001h   0001h    Yes   No 
             (External Function = s4_lba_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4S_BLOCK_MODE                  13D0h 7Ah  0001h 0001h   0001h    Yes   No 
             (External Function = s4_block_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4S_PIO_MODE                    33D1h 7Ah  000Eh 0000h   0000h    Yes   No 
             (External Function = s4_pio_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4S_DMA_MODE                    43D4h 7Ah  00F0h 0000h   0000h    Yes   No 
             (External Function = s4_dma_mode_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4S_SMART                       23D8h 7Bh  0003h 0000h   0000h    Yes   No 
             (External Function = s4_smart_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4S_32BIT_XFER                  13DAh 7Bh  0004h 0000h   0000h    Yes   No 
             (External Function = s4_32bit_xfer_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_4S_EMULATION_TYPE              23DBh 7Bh  0018h 0000h   0000h    Yes   No 
             (External Function = s4_emulation_type_func)
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_HDD_ACCESS_CONTROL             13DDh 7Bh  0020h 0000h   0000h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_ATA_DETECT_TIME_OUT            33E0h 7Ch  0007h 0007h   0007h    Yes   No 
             00h = _str$_0                         
             01h = _str$_5                         
             02h = _str$_10                        
             03h = _str$_15                        
             04h = _str$_20                        
             05h = _str$_25                        
             06h = _str$_30                        
             07h = _str$_35                        
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_ATA_80PIN_CABLE_DETECT         23DEh 7Bh  00C0h 0000h   0000h    Yes   No 
             00h = _str$_host80_device80           
             01h = _str$_host80                    
             02h = _str$_device80                  
	(Input file: INTEL\COREMOD\ADVANCED.SSP)

Q_PNP_AWARE_OS                   13E3h 7Ch  0008h 0001h   0001h    Yes   No 
             00h = _str$_No                        
             01h = _str$_Yes                       
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_PCI_LATENCY_TIMER              33E4h 7Ch  0070h 0001h   0001h    Yes   No 
             00h = _str$_32                        
             01h = _str$_64                        
             02h = _str$_96                        
             03h = _str$_128                       
             04h = _str$_160                       
             05h = _str$_192                       
             06h = _str$_224                       
             07h = _str$_248                       
	(Input file: OEMBOARD\oemboard.ssp)

Q_PCI_VGA_IRQ                    13E7h 7Ch  0080h 0000h   0000h    Yes   No 
             00h = _str$_Yes                       
             01h = _str$_No                        
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_PCI_PALETTE_SNOOP              13E8h 7Dh  0001h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_PCI_IDE_BUS_MASTER             13E9h 7Dh  0002h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_PCI_OFFBOARD_IDE               33EAh 7Dh  001Ch 0000h   0000h    Yes   No 
             00h = _str$_Auto                      
             01h = _str$_Slot1                     
             02h = _str$_Slot2                     
             03h = _str$_Slot3                     
             04h = _str$_Slot4                     
             05h = _str$_Slot5                     
             06h = _str$_Slot6                     
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_PCI_OFFBOARD_IDE_PRI_IRQ       33EDh 7Dh  00E0h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_INTA                      
             02h = _str$_INTB                      
             03h = _str$_INTC                      
             04h = _str$_INTD                      
             05h = RESERVED                        
             06h = RESERVED                        
             07h = _str$_Hardwired                 
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_PCI_OFFBOARD_IDE_SEC_IRQ       33F8h 7Fh  0007h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_INTA                      
             02h = _str$_INTB                      
             03h = _str$_INTC                      
             04h = _str$_INTD                      
             05h = RESERVED                        
             06h = RESERVED                        
             07h = _str$_Hardwired                 
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_IRQ3_USED_BY_ISA               13FBh 7Fh  0008h 0000h   0000h    Yes   No 
             00h = _str$_Available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_IRQ4_USED_BY_ISA               13FCh 7Fh  0010h 0000h   0000h    Yes   No 
             00h = _str$_Available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_IRQ5_USED_BY_ISA               13FDh 7Fh  0020h 0000h   0000h    Yes   No 
             00h = _str$_Available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_IRQ7_USED_BY_ISA               13FEh 7Fh  0040h 0000h   0000h    Yes   No 
             00h = _str$_Available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_IRQ9_USED_BY_ISA               13FFh 7Fh  0080h 0000h   0000h    Yes   No 
             00h = _str$_Available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_IRQ10_USED_BY_ISA              1400h 80h  0001h 0000h   0000h    Yes   No 
             00h = _str$_Available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_IRQ11_USED_BY_ISA              1401h 80h  0002h 0000h   0000h    Yes   No 
             00h = _str$_Available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_IRQ14_USED_BY_ISA              1402h 80h  0004h 0000h   0000h    Yes   No 
             00h = _str$_Available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_IRQ15_USED_BY_ISA              1403h 80h  0008h 0000h   0000h    Yes   No 
             00h = _str$_Available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_DMA0_USED_BY_ISA               1404h 80h  0010h 0000h   0000h    Yes   No 
             00h = _str$_available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_DMA1_USED_BY_ISA               1405h 80h  0020h 0000h   0000h    Yes   No 
             00h = _str$_available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_DMA3_USED_BY_ISA               1406h 80h  0040h 0000h   0000h    Yes   No 
             00h = _str$_available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_DMA5_USED_BY_ISA               1407h 80h  0080h 0000h   0000h    Yes   No 
             00h = _str$_available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_DMA6_USED_BY_ISA               1408h 81h  0001h 0000h   0000h    Yes   No 
             00h = _str$_available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_DMA7_USED_BY_ISA               1409h 81h  0002h 0000h   0000h    Yes   No 
             00h = _str$_available                 
             01h = _str$_reserved                  
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_MEM_SIZE_USED_BY_ISA           240Ah 81h  000Ch 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_16k                       
             02h = _str$_32k                       
             03h = _str$_64k                       
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_MEM_BASE_USED_BY_ISA           340Ch 81h  0070h 0002h   0002h    Yes   No 
             00h = _str$_C0000                     
             01h = _str$_C4000                     
             02h = _str$_C8000                     
             03h = _str$_CC000                     
             04h = _str$_D0000                     
             05h = _str$_D4000                     
             06h = _str$_D8000                     
             07h = _str$_DC000                     
	(Input file: INTEL\COREMOD\PCIPNP.SSP)

Q_QUICK_BOOT                     140Fh 81h  0080h 0001h   0001h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: INTEL\COREMOD\BOOT.SSP)

Q_INITIAL_DISPLAY                1410h 82h  0001h 0001h   0001h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_ADDON_ROM_DISPLAY              1411h 82h  0002h 0001h   0001h    Yes   No 
             00h = _STR$_Force_BIOS                
             01h = _STR$_Keep_Current              
	(Input file: OEMBOARD\oemboard.ssp)

Q_NUM_LOCK                       1412h 82h  0004h 0000h   0000h    Yes   No 
             00h = _STR$_Off                       
             01h = _STR$_On                        
	(Input file: INTEL\COREMOD\BOOT.SSP)

Q_MOUSE_SUPPORT                  2413h 82h  0018h 0002h   0002h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
             02h = _STR$_Auto                      
	(Input file: INTEL\COREMOD\BOOT.SSP)

Q_TYPEMATIC_RATE                 1760h ECh  0001h 0001h   0001h    Yes   No 
             00h = _STR$_Slow                      
             01h = _STR$_Fast                      
	(Input file: INTEL\COREMOD\BOOT.SSP)

Q_KEYBOARD_PRESENT               10A2h 14h  0004h 0001h   0001h    Yes   Yes
             00h = _STR$_Absent                    
             01h = _STR$_Present                   
	(Input file: INTEL\COREMOD\BOOT.SSP)

Q_PARITY_ERROR                   1761h ECh  0002h 0001h   0001h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: INTEL\COREMOD\BOOT.SSP)

Q_OS2_COMP_MODE                  1762h ECh  0004h 0000h   0000h    Yes   No 
             00h = _STR$_No                        
             01h = _STR$_Yes                       
	(Input file: INTEL\COREMOD\BOOT.SSP)

Q_WAIT_FOR_F1                    1415h 82h  0020h 0001h   0001h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: INTEL\COREMOD\BOOT.SSP)

Q_DISPLAY_HIT_DEL                1416h 82h  0040h 0001h   0001h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: INTEL\COREMOD\BOOT.SSP)

Q_SUPERVISOR_PASSWORD            7418h 83h  00FFh 0000h   0000h    Yes   No 
             (Control Function = ChangeSuperPwdControlFunc_FAR)
	(Input file: BSP\EM\INTELSECURITY\SECURITY.SSP)

Q_DENY_SETUP                     2450h 8Ah  0003h 0003h   0003h    Yes   No 
             (External Function = user_access_level_func)
	(Input file: BSP\EM\INTELSECURITY\SECURITY.SSP)

Q_USER_PASSWORD                  7458h 8Bh  00FFh 0000h   0000h    Yes   No 
             (Control Function = ChangeUserPwdControlFunc_FAR)
	(Input file: BSP\EM\INTELSECURITY\SECURITY.SSP)

Q_PASSWORD_CHECK                 1417h 82h  0080h 0000h   0000h    Yes   No 
             (External Function = password_check_func)
	(Input file: BSP\EM\INTELSECURITY\SECURITY.SSP)

Q_VIRUS_PROTECTION               1452h 8Ah  0004h 0000h   0000h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: BSP\EM\INTELSECURITY\SECURITY.SSP)

Q_I19_TRAP_ALLOW                 1453h 8Ah  0008h 0001h   0001h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_FIRST_BOOT_DRIVE               4454h 8Ah  00F0h 0000h   0000h    Yes   No 
             (External Function = boot_device_proc_1)
	(Input file: CORE\\BBS.SSP)

Q_SECOND_BOOT_DRIVE              4490h 92h  000Fh 0001h   0001h    Yes   No 
             (External Function = boot_device_proc_2)
	(Input file: CORE\\BBS.SSP)

Q_THIRD_BOOT_DRIVE               4494h 92h  00F0h 0002h   0002h    Yes   No 
             (External Function = boot_device_proc_3)
	(Input file: CORE\\BBS.SSP)

Q_FOURTH_BOOT_DRIVE              4498h 93h  000Fh 0003h   0003h    Yes   No 
             (External Function = boot_device_proc_4)
	(Input file: CORE\\BBS.SSP)

Q_FIFTH_BOOT_DRIVE               449Ch 93h  00F0h 0004h   0004h    Yes   No 
             (External Function = boot_device_proc_5)
	(Input file: CORE\\BBS.SSP)

Q_SIXTH_BOOT_DRIVE               44A0h 94h  000Fh 0005h   0005h    Yes   No 
             (External Function = boot_device_proc_6)
	(Input file: CORE\\BBS.SSP)

Q_SEVENTH_BOOT_DRIVE             44A4h 94h  00F0h 0006h   0006h    Yes   No 
             (External Function = boot_device_proc_7)
	(Input file: CORE\\BBS.SSP)

Q_EIGHTH_BOOT_DRIVE              44A8h 95h  000Fh 0007h   0007h    Yes   No 
             (External Function = boot_device_proc_8)
	(Input file: CORE\\BBS.SSP)

Q_NINETH_BOOT_DRIVE              44ACh 95h  00F0h 0008h   0008h    Yes   No 
             (External Function = boot_device_proc_9)
	(Input file: CORE\\BBS.SSP)

Q_TENTH_BOOT_DRIVE               44B0h 96h  000Fh 0009h   0009h    Yes   No 
             (External Function = boot_device_proc_10)
	(Input file: CORE\\BBS.SSP)

Q_ELEVENTH_BOOT_DRIVE            44B4h 96h  00F0h 000Ah   000Ah    Yes   No 
             (External Function = boot_device_proc_11)
	(Input file: CORE\\BBS.SSP)

Q_TWELVETH_BOOT_DRIVE            44B8h 97h  000Fh 000Bh   000Bh    Yes   No 
             (External Function = boot_device_proc_12)
	(Input file: CORE\\BBS.SSP)

Q_HD_FIRST_BOOT_DRIVE            44BCh 97h  00F0h 0000h   0000h    Yes   No 
             (External Function = hd_device_proc_1)
	(Input file: CORE\\BBS.SSP)

Q_HD_SECOND_BOOT_DRIVE           44C0h 98h  000Fh 0001h   0001h    Yes   No 
             (External Function = hd_device_proc_2)
	(Input file: CORE\\BBS.SSP)

Q_HD_THIRD_BOOT_DRIVE            44C4h 98h  00F0h 0002h   0002h    Yes   No 
             (External Function = hd_device_proc_3)
	(Input file: CORE\\BBS.SSP)

Q_HD_FOURTH_BOOT_DRIVE           44C8h 99h  000Fh 0003h   0003h    Yes   No 
             (External Function = hd_device_proc_4)
	(Input file: CORE\\BBS.SSP)

Q_HD_FIFTH_BOOT_DRIVE            44CCh 99h  00F0h 0004h   0004h    Yes   No 
             (External Function = hd_device_proc_5)
	(Input file: CORE\\BBS.SSP)

Q_HD_SIXTH_BOOT_DRIVE            44D0h 9Ah  000Fh 0005h   0005h    Yes   No 
             (External Function = hd_device_proc_6)
	(Input file: CORE\\BBS.SSP)

Q_HD_SEVENTH_BOOT_DRIVE          44D4h 9Ah  00F0h 0006h   0006h    Yes   No 
             (External Function = hd_device_proc_7)
	(Input file: CORE\\BBS.SSP)

Q_HD_EIGHTH_BOOT_DRIVE           44D8h 9Bh  000Fh 0007h   0007h    Yes   No 
             (External Function = hd_device_proc_8)
	(Input file: CORE\\BBS.SSP)

Q_HD_NINETH_BOOT_DRIVE           44DCh 9Bh  00F0h 0008h   0008h    Yes   No 
             (External Function = hd_device_proc_9)
	(Input file: CORE\\BBS.SSP)

Q_HD_TENTH_BOOT_DRIVE            44E0h 9Ch  000Fh 0009h   0009h    Yes   No 
             (External Function = hd_device_proc_10)
	(Input file: CORE\\BBS.SSP)

Q_HD_ELEVENTH_BOOT_DRIVE         44E4h 9Ch  00F0h 000Ah   000Ah    Yes   No 
             (External Function = hd_device_proc_11)
	(Input file: CORE\\BBS.SSP)

Q_HD_TWELVETH_BOOT_DRIVE         44E8h 9Dh  000Fh 000Bh   000Bh    Yes   No 
             (External Function = hd_device_proc_12)
	(Input file: CORE\\BBS.SSP)

Q_RD_FIRST_BOOT_DRIVE            34ECh 9Dh  0070h 0000h   0000h    Yes   No 
             (External Function = rd_device_proc_1)
	(Input file: CORE\\BBS.SSP)

Q_RD_SECOND_BOOT_DRIVE           34F0h 9Eh  0007h 0001h   0001h    Yes   No 
             (External Function = rd_device_proc_2)
	(Input file: CORE\\BBS.SSP)

Q_RD_THIRD_BOOT_DRIVE            34F3h 9Eh  0038h 0002h   0002h    Yes   No 
             (External Function = rd_device_proc_3)
	(Input file: CORE\\BBS.SSP)

Q_RD_FOURTH_BOOT_DRIVE           34F8h 9Fh  0007h 0003h   0003h    Yes   No 
             (External Function = rd_device_proc_4)
	(Input file: CORE\\BBS.SSP)

Q_CD_FIRST_BOOT_DRIVE            34FBh 9Fh  0038h 0000h   0000h    Yes   No 
             (External Function = cd_device_proc_1)
	(Input file: CORE\\BBS.SSP)

Q_CD_SECOND_BOOT_DRIVE           3500h A0h  0007h 0001h   0001h    Yes   No 
             (External Function = cd_device_proc_2)
	(Input file: CORE\\BBS.SSP)

Q_CD_THIRD_BOOT_DRIVE            3503h A0h  0038h 0002h   0002h    Yes   No 
             (External Function = cd_device_proc_3)
	(Input file: CORE\\BBS.SSP)

Q_CD_FOURTH_BOOT_DRIVE           3508h A1h  0007h 0003h   0003h    Yes   No 
             (External Function = cd_device_proc_4)
	(Input file: CORE\\BBS.SSP)

Q_FLOPPY_CONTROLLER              24F6h 9Eh  00C0h 0002h   0002h    Yes   No 
             00h = RESERVED                        
             01h = _str$_Disabled                  
             02h = _str$_Enabled                   
	(Input file: BSP\SETUP\IO.SSP)

Q_COMA_PORT                      350Bh A1h  0038h 0002h   0002h    Yes   No 
             (External Function = com_a_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_COMB_PORT                      3510h A2h  0007h 0003h   0003h    Yes   No 
             (External Function = com_b_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_COMB_MODE                      24FEh 9Fh  00C0h 0000h   0000h    Yes   No 
	(Input file: BSP\SETUP\IO.SSP)

Q_COMB_DUPLEX_MODE               14EFh 9Dh  0080h 0001h   0001h    Yes   No 
	(Input file: BSP\SETUP\IO.SSP)

Q_COMB_IRRX_PIN                  1506h A0h  0040h 0001h   0001h    Yes   No 
	(Input file: BSP\SETUP\IO.SSP)

Q_BU_UPDATE                      1507h A0h  0080h 0001h   0001h    Yes   No 
             00h = _STR$_DISABLED                  
             01h = _STR$_ENABLED                   
	(Input file: BSP\CPU\CPU.SSP)

Q_CPUID_LIMIT                    150Eh A1h  0040h 0000h   0000h    Yes   No 
             00h = _STR$_DISABLED                  
             01h = _STR$_ENABLED                   
	(Input file: BSP\CPU\CPU.SSP)

Q_INTERNAL_CACHE                 2513h A2h  0018h 0002h   0002h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_WriteThru                 
             02h = _STR$_WriteBack                 
	(Input file: BSP\CPU\CPU.SSP)

Q_L3_CACHE                       1260h 4Ch  0001h 0000h   0000h    Yes   Yes
	(Input file: BSP\CPU\CPU.SSP)

I_CPU_FREQ_RATIO                 8298h 53h  00FFh 00FEh   00FEh    Yes   Yes
             (Control Function = ProcRatioControlFunc_FAR)
	(Input file: OEMBOARD\oemboard.ssp)

I_CPU_VID                        82A0h 54h  00FFh 003Eh   003Eh    Yes   Yes
	(Input file: BSP\CPU\CPU.SSP)

Q_NX_Support                     12B0h 56h  0001h 0001h   0001h    Yes   Yes
             (External Function = NXSupportControlFunc_FAR)
	(Input file: BSP\CPU\CPU.SSP)

Q_HW_Prefetcher                  12B2h 56h  0004h 0000h   0000h    Yes   Yes
             (External Function = HWPrefetcherControlFunc_FAR)
	(Input file: BSP\CPU\CPU.SSP)

Q_ACL_Prefetch                   12B3h 56h  0008h 0000h   0000h    Yes   Yes
             (External Function = ACLPrefetchControlFunc_FAR)
	(Input file: BSP\CPU\CPU.SSP)

Q_REMAP                          150Fh A1h  0080h 0001h   0001h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: BSP\SETUP\nb.ssp)

Q_C0000_SHADOW                   3515h A2h  00E0h 0000h   0000h    Yes   No 
             00h = _str$_DISABLED                  
             01h = _str$_UNCACHED                  
             02h = _str$_CACHEDsWP                 
             03h = _str$_CACHEDsWT                 
             04h = _str$_CACHEDsWB                 
             05h = RESERVED                        
             06h = RESERVED                        
             07h = RESERVED                        
	(Input file: BSP\SETUP\nb.ssp)

Q_C4000_SHADOW                   3518h A3h  0007h 0000h   0000h    Yes   No 
             00h = _str$_DISABLED                  
             01h = _str$_UNCACHED                  
             02h = _str$_CACHEDsWP                 
             03h = _str$_CACHEDsWT                 
             04h = _str$_CACHEDsWB                 
             05h = RESERVED                        
             06h = RESERVED                        
             07h = RESERVED                        
	(Input file: BSP\SETUP\nb.ssp)

Q_C8000_SHADOW                   351Bh A3h  0038h 0000h   0000h    Yes   No 
             00h = _str$_DISABLED                  
             01h = _str$_UNCACHED                  
             02h = _str$_CACHEDsWP                 
             03h = _str$_CACHEDsWT                 
             04h = _str$_CACHEDsWB                 
             05h = RESERVED                        
             06h = RESERVED                        
             07h = RESERVED                        
	(Input file: BSP\SETUP\nb.ssp)

Q_CC000_SHADOW                   3520h A4h  0007h 0000h   0000h    Yes   No 
             00h = _str$_DISABLED                  
             01h = _str$_UNCACHED                  
             02h = _str$_CACHEDsWP                 
             03h = _str$_CACHEDsWT                 
             04h = _str$_CACHEDsWB                 
             05h = RESERVED                        
             06h = RESERVED                        
             07h = RESERVED                        
	(Input file: BSP\SETUP\nb.ssp)

Q_D0000_SHADOW                   3523h A4h  0038h 0000h   0000h    Yes   No 
             00h = _str$_DISABLED                  
             01h = _str$_UNCACHED                  
             02h = _str$_CACHEDsWP                 
             03h = _str$_CACHEDsWT                 
             04h = _str$_CACHEDsWB                 
             05h = RESERVED                        
             06h = RESERVED                        
             07h = RESERVED                        
	(Input file: BSP\SETUP\nb.ssp)

Q_D4000_SHADOW                   3528h A5h  0007h 0000h   0000h    Yes   No 
             00h = _str$_DISABLED                  
             01h = _str$_UNCACHED                  
             02h = _str$_CACHEDsWP                 
             03h = _str$_CACHEDsWT                 
             04h = _str$_CACHEDsWB                 
             05h = RESERVED                        
             06h = RESERVED                        
             07h = RESERVED                        
	(Input file: BSP\SETUP\nb.ssp)

Q_D8000_SHADOW                   352Bh A5h  0038h 0000h   0000h    Yes   No 
             00h = _str$_DISABLED                  
             01h = _str$_UNCACHED                  
             02h = _str$_CACHEDsWP                 
             03h = _str$_CACHEDsWT                 
             04h = _str$_CACHEDsWB                 
             05h = RESERVED                        
             06h = RESERVED                        
             07h = RESERVED                        
	(Input file: BSP\SETUP\nb.ssp)

Q_DC000_SHADOW                   3530h A6h  0007h 0000h   0000h    Yes   No 
             00h = _str$_DISABLED                  
             01h = _str$_UNCACHED                  
             02h = _str$_CACHEDsWP                 
             03h = _str$_CACHEDsWT                 
             04h = _str$_CACHEDsWB                 
             05h = RESERVED                        
             06h = RESERVED                        
             07h = RESERVED                        
	(Input file: BSP\SETUP\nb.ssp)

Q_HT_SUPPORT                     1288h 51h  0001h 0001h   0001h    Yes   Yes
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
             (External Function = HTSupportControlFunc_FAR)
	(Input file: BSP\SETUP\nb.ssp)

Q_MEM_RAS_FEATURE                2289h 51h  0006h 0000h   0000h    Yes   Yes
             (External Function = Memory_ras_feature)
	(Input file: BSP\SETUP\nb.ssp)

Q_RAS_FEATURE_SUPPORTED          8660h CCh  00FFh 0000h   0000h    No    Yes
	(Input file: BSP\SETUP\nb.ssp)

Q_EXT_CMOS_PHY_LAYOUT0           8740h E8h  00FFh 0000h   0000h    No    Yes
	(Input file: BSP\SETUP\nb.ssp)

Q_EXT_CMOS_PHY_LAYOUT1           8748h E9h  00FFh 0000h   0000h    No    Yes
	(Input file: BSP\SETUP\nb.ssp)

Q_EXT_CMOS_PHY_LAYOUT2           8750h EAh  00FFh 0000h   0000h    No    Yes
	(Input file: BSP\SETUP\nb.ssp)

Q_EXT_CMOS_PHY_LAYOUT3           8758h EBh  00FFh 0000h   0000h    No    Yes
	(Input file: BSP\SETUP\nb.ssp)

Q_AC97_AUDIO                     151Eh A3h  0040h 0000h   0000h    Yes   No 
             00h = _str$_Auto                      
             01h = _str$_Disabled                  
	(Input file: BSP\SETUP\sb.ssp)

Q_MC97_MODEM                     151Fh A3h  0080h 0000h   0000h    Yes   No 
             00h = _str$_Auto                      
             01h = _str$_Disabled                  
	(Input file: BSP\SETUP\sb.ssp)

Q_CPU_BIST_ENABLE                1526h A4h  0040h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_ICH_DELAYED_TRANSACTION        1527h A4h  0080h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\SETUP\sb.ssp)

Q_ICH_DCB_ENABLE                 152Eh A5h  0040h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\SETUP\sb.ssp)

Q_PCI_ATA_MODE                   152Fh A5h  0080h 0000h   0000h    Yes   No 
             00h = _str$_Legacy_Mode               
             01h = _str$_Native_Mode               
	(Input file: BSP\SETUP\sb.ssp)

Q_PCI_PATA_CHANNEL               2533h A6h  0018h 0003h   0003h    Yes   No 
             (External Function = pci_pata_channel_ef)
	(Input file: BSP\SETUP\sb.ssp)

Q_PCI_SATA_CHANNEL               1535h A6h  0020h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\SETUP\sb.ssp)

Q_SATA_AS_RAID                   1536h A6h  0040h 0000h   0000h    Yes   No 
             (External Function = sata_as_raid_ef)
	(Input file: BSP\SETUP\sb.ssp)

Q_SATA_MODE                      1537h A6h  0080h 0000h   0000h    Yes   No 
             (External Function = sata_mode_ef)
	(Input file: BSP\SETUP\sb.ssp)

Q_FIRST_CHANNEL                  1538h A7h  0001h 0000h   0000h    Yes   No 
             (External Function = first_channel_ef)
	(Input file: BSP\SETUP\sb.ssp)

Q_SECOND_CHANNEL                 1539h A7h  0002h 0000h   0000h    Yes   No 
             (External Function = second_channel_ef)
	(Input file: BSP\SETUP\sb.ssp)

Q_THIRD_CHANNEL                  153Ah A7h  0004h 0001h   0001h    Yes   No 
             (External Function = third_channel_ef)
	(Input file: BSP\SETUP\sb.ssp)

Q_ACPI_OS                        153Bh A7h  0008h 0001h   0001h    Yes   No 
             00h = _str$_NO                        
             01h = _str$_YES                       
	(Input file: BSP\eM\ACPI\ACPI.SSP)

Q_ACPI_2                         153Ch A7h  0010h 0000h   0000h    Yes   No 
             00h = _str$_NO                        
             01h = _str$_YES                       
	(Input file: BSP\eM\ACPI\ACPI.SSP)

Q_ACPI_APIC_TBL                  153Dh A7h  0020h 0001h   0001h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: BSP\eM\ACPI\ACPI.SSP)

Q_APIC_ACPI_IRQ                  153Eh A7h  0040h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\eM\ACPI\ACPI.SSP)

Q_ACPI_EXCH_BUF                  153Fh A7h  0080h 0001h   0001h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: BSP\eM\ACPI\ACPI.SSP)

Q_ACPI_HEADLESS_MODE             1540h A8h  0001h 0000h   0000h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: BSP\eM\ACPI\ACPI.SSP)

Q_REMOTE_ACCESS                  1541h A8h  0002h 0000h   0000h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
             (External Function = oem_to_change_q_headless)
	(Input file: OEMBOARD\oemboard.ssp)

Q_RA_COM_NO                      2542h A8h  000Ch 0002h   0002h    Yes   No 
             00h = RESERVED                        
             01h = _STR$_ra_COM1                   
             02h = _STR$_ra_COM2                   
             03h = RESERVED                        
             (External Function = SerConnetor_extfunc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_RA_COM_MODE                    3544h A8h  0070h 0002h   0002h    Yes   No 
             00h = _str$_Baud_9600                 
             01h = STR_RESERVED                    
             02h = _str$_Baud_19200                
             03h = STR_RESERVED                    
             04h = STR_RESERVED                    
             05h = _str$_Baud_57600                
             06h = _str$_Baud_115200               
             07h = STR_RESERVED                    
	(Input file: OEMBOARD\oemboard.ssp)

Q_TERMINAL_TYPE                  2548h A9h  0003h 0000h   0000h    Yes   No 
             00h = _str$_TermTypePcansi            
             01h = _STR$_acpi_cr_VT100             
             02h = _str$_TermTypeVt100p            
             03h = _str$_TermTypeVtutf8            
	(Input file: OEMBOARD\oemboard.ssp)

Q_USB_WAKEUP_FROM_S3S4           1547h A8h  0080h 0000h   0000h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: BSP\eM\ACPI\ACPI.SSP)

Q_ACPI_S4                        83F0h 7Eh  00FFh 0000h   0000h    No    Yes
	(Input file: BSP\eM\ACPI\ACPI.SSP)

Q_ECC_EVENT_LOGGING              154Ah A9h  0004h 0001h   0001h    Yes   No 
             (External Function = CheckCriticalEventLogEnable)
	(Input file: OEMBOARD\oemboard.ssp)

Q_Hub_Interface_Event_Logging    154Bh A9h  0008h 0001h   0001h    Yes   No 
             (External Function = CheckCriticalEventLogEnable)
	(Input file: OEMBOARD\oemboard.ssp)

Q_System_Bus_Event_Logging       154Ch A9h  0010h 0001h   0001h    Yes   No 
             (External Function = CheckCriticalEventLogEnable)
	(Input file: OEMBOARD\oemboard.ssp)

Q_Memory_Buffer_Event_Logging    154Dh A9h  0020h 0000h   0000h    Yes   No 
	(Input file: OEMBOARD\oemboard.ssp)

Q_PCI_ERROR_LOGGING              154Eh A9h  0040h 0001h   0001h    Yes   No 
             (External Function = CheckCriticalEventLogEnable)
	(Input file: OEMBOARD\oemboard.ssp)

Q_INTEL_SPEEDSTEP_TECH           3550h AAh  0007h 0003h   0003h    Yes   No 
             (External Function = speedstep_cpu_ef)
	(Input file: OEMBOARD\oemboard.ssp)

Q_geyserville_type               154Fh A9h  0080h 0000h   0000h    Yes   No 
             00h = _STR$_g_III                     
             01h = _STR$_g_Iplus                   
	(Input file: BSP\EM\IST\IST.SSP)

Q_MPS_REVISION                   1553h AAh  0008h 0001h   0000h    Yes   No 
             00h = _str$_Mps_11                    
             01h = _str$_Mps_14                    
	(Input file: BSP\EM\MPS\MPS.SSP)

Q_ASPM_ENABLE                    1554h AAh  0010h 0000h   0000h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: BSP\EM\PCIE\PCIE.SSP)

Q_PCIE_ERROR_REPORTING           1555h AAh  0020h 0000h   0000h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: BSP\EM\PCIE\PCIE.SSP)

Q_PCIE_PORT2                     2556h AAh  00C0h 0000h   0000h    Yes   No 
             00h = _STR$_Auto                      
             01h = _STR$_Enabled                   
             02h = _STR$_Disabled                  
	(Input file: CSP\EM\PCIE\PCIENB.SSP)

Q_PCIE_PORT3                     2558h ABh  0003h 0000h   0000h    Yes   No 
             00h = _STR$_Auto                      
             01h = _STR$_Enabled                   
             02h = _STR$_Disabled                  
	(Input file: CSP\EM\PCIE\PCIENB.SSP)

Q_PCIE_PORT4                     255Ah ABh  000Ch 0000h   0000h    Yes   No 
             00h = _STR$_Auto                      
             01h = _STR$_Enabled                   
             02h = _STR$_Disabled                  
	(Input file: CSP\EM\PCIE\PCIENB.SSP)

Q_PCIE_PORT5                     255Ch ABh  0030h 0000h   0000h    Yes   No 
             00h = _STR$_Auto                      
             01h = _STR$_Enabled                   
             02h = _STR$_Disabled                  
	(Input file: CSP\EM\PCIE\PCIENB.SSP)

Q_PCIE_PORT6                     255Eh ABh  00C0h 0000h   0000h    Yes   No 
             00h = _STR$_Auto                      
             01h = _STR$_Enabled                   
             02h = _STR$_Disabled                  
	(Input file: CSP\EM\PCIE\PCIENB.SSP)

Q_PCIE_PORT7                     2560h ACh  0003h 0000h   0000h    Yes   No 
             00h = _STR$_Auto                      
             01h = _STR$_Enabled                   
             02h = _STR$_Disabled                  
	(Input file: CSP\EM\PCIE\PCIENB.SSP)

Q_PXH_IO_DECODE                  1562h ACh  0004h 0000h   0000h    Yes   No 
             00h = _STR$_4KDecode                  
             01h = _STR$_1KDecode                  
	(Input file: BSP\EM\PXH\PXH.SSP)

Q_PXH_RASERR_HANDLING            1563h ACh  0008h 0000h   0000h    Yes   No 
             00h = _STR$_ClearRASError             
             01h = _STR$_LeaveRASError             
	(Input file: BSP\EM\PXH\PXH.SSP)

Q_PXH_VGA_DECODE                 1564h ACh  0010h 0001h   0001h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: BSP\EM\PXH\PXH.SSP)

Q_PXH_PCIX_CLOCK                 4568h ADh  000Fh 0000h   0000h    Yes   No 
             00h = _STR$_AUTO                      
             01h = _STR$_33Mhz_PCI                 
             02h = _STR$_66Mhz_PCI                 
             03h = _STR$_66Mhz_PCIX                
             04h = _STR$_100Mhz_PCIX               
             05h = _STR$_133Mhz_PCIX               
             06h = _STR$_66Mhz_PCIX_M2             
             07h = _STR$_100Mhz_PCIX_M2            
             08h = _STR$_133Mhz_PCIX_M2            
	(Input file: BSP\EM\PXH\PXH.SSP)

Q_USB_FUNCTION_ENABLE            3565h ACh  00E0h 0003h   0003h    Yes   No 
             00h = _str$_Disabled                  
             01h = RESERVED                        
             02h = RESERVED                        
             03h = _str$_Enabled                   
             04h = RESERVED                        
             05h = RESERVED                        
             06h = RESERVED                        
             07h = RESERVED                        
	(Input file: OEMBOARD\oemboard.ssp)

Q_USB20_ENABLE                   156Ch ADh  0010h 0000h   0000h    Yes   No 
             00h = _str$_Enabled                   
             01h = _str$_Disabled                  
	(Input file: OEMBOARD\oemboard.ssp)

Q_USB_LEGACY_ENABLE              256Dh ADh  0060h 0002h   0002h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
             02h = _str$_Auto                      
	(Input file: OEMBOARD\oemboard.ssp)

Q_USB_LEGACY_KEYBOARD            156Fh ADh  0080h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: CSP\EM\USB\USB.SSP)

Q_USB_LEGACY_MOUSE               1570h AEh  0001h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: CSP\EM\USB\USB.SSP)

Q_USB_6460_EMULATION             1571h AEh  0002h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: CSP\EM\USB\USB.SSP)

Q_USB_LEGACY_STORAGE             1572h AEh  0004h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: CSP\EM\USB\USB.SSP)

Q_USB_STORAGE_DEVICE_DELAY       2573h AEh  0018h 0001h   0001h    Yes   No 
             00h = _str$_USB_10SEC                 
             01h = _str$_USB_20SEC                 
             02h = _str$_USB_30SEC                 
             03h = _str$_USB_40SEC                 
	(Input file: CSP\EM\USB\USB.SSP)

Q_USB_HISPEED_SUPPORT            1575h AEh  0020h 0001h   0001h    Yes   No 
             (External Function = farUSBHiSpeedSupportExtFunc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_USB_BEEP                       1576h AEh  0040h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_USB_MASS_DEV1_EMULATION        3578h AFh  0007h 0000h   0000h    Yes   No 
             (External Function = farUSBMassDev1EmuExtFunc)
	(Input file: CSP\EM\USB\USB.SSP)

Q_USB_MASS_DEV2_EMULATION        357Bh AFh  0038h 0000h   0000h    Yes   No 
             (External Function = farUSBMassDev2EmuExtFunc)
	(Input file: CSP\EM\USB\USB.SSP)

Q_USB_MASS_DEV3_EMULATION        3580h B0h  0007h 0000h   0000h    Yes   No 
             (External Function = farUSBMassDev3EmuExtFunc)
	(Input file: CSP\EM\USB\USB.SSP)

Q_USB_MASS_DEV4_EMULATION        3583h B0h  0038h 0000h   0000h    Yes   No 
             (External Function = farUSBMassDev4EmuExtFunc)
	(Input file: CSP\EM\USB\USB.SSP)

Q_USB_MASS_DEV5_EMULATION        3588h B1h  0007h 0000h   0000h    Yes   No 
             (External Function = farUSBMassDev5EmuExtFunc)
	(Input file: CSP\EM\USB\USB.SSP)

Q_USB_MASS_DEV6_EMULATION        358Bh B1h  0038h 0000h   0000h    Yes   No 
             (External Function = farUSBMassDev6EmuExtFunc)
	(Input file: CSP\EM\USB\USB.SSP)

Q_LANGUAGE                       0590h B2h  FFFFh 0000h   0000h    Yes   No 
	(Input file: BSP\SETUP\OEM.SSP)

Q_FLOPPY_SWAP                    1577h AEh  0080h 0000h   0000h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: BSP\SETUP\OEM.SSP)

Q_PCI_SLOT1_IRQ                  45A0h B4h  000Fh 0000h   0000h    Yes   No 
             00h = _str$_auto                      
             01h = RESERVED                        
             02h = RESERVED                        
             03h = _str$_3                         
             04h = _str$_4                         
             05h = _str$_5                         
             06h = RESERVED                        
             07h = _str$_7                         
             08h = RESERVED                        
             09h = _str$_9                         
             0Ah = _str$_10                        
             0Bh = _str$_11                        
             0Ch = _str$_12                        
             0Dh = RESERVED                        
             0Eh = _str$_14                        
             0Fh = _str$_15                        
	(Input file: BSP\SETUP\OEM.SSP)

Q_PCI_SLOT2_IRQ                  45A4h B4h  00F0h 0000h   0000h    Yes   No 
             00h = _str$_auto                      
             01h = RESERVED                        
             02h = RESERVED                        
             03h = _str$_3                         
             04h = _str$_4                         
             05h = _str$_5                         
             06h = RESERVED                        
             07h = _str$_7                         
             08h = RESERVED                        
             09h = _str$_9                         
             0Ah = _str$_10                        
             0Bh = _str$_11                        
             0Ch = _str$_12                        
             0Dh = RESERVED                        
             0Eh = _str$_14                        
             0Fh = _str$_15                        
	(Input file: BSP\SETUP\OEM.SSP)

Q_PCI_SLOT3_IRQ                  45A8h B5h  000Fh 0000h   0000h    Yes   No 
             00h = _str$_auto                      
             01h = RESERVED                        
             02h = RESERVED                        
             03h = _str$_3                         
             04h = _str$_4                         
             05h = _str$_5                         
             06h = RESERVED                        
             07h = _str$_7                         
             08h = RESERVED                        
             09h = _str$_9                         
             0Ah = _str$_10                        
             0Bh = _str$_11                        
             0Ch = _str$_12                        
             0Dh = RESERVED                        
             0Eh = _str$_14                        
             0Fh = _str$_15                        
	(Input file: BSP\SETUP\OEM.SSP)

Q_PCI_SLOT4_IRQ                  45ACh B5h  00F0h 0000h   0000h    Yes   No 
             00h = _str$_auto                      
             01h = RESERVED                        
             02h = RESERVED                        
             03h = _str$_3                         
             04h = _str$_4                         
             05h = _str$_5                         
             06h = RESERVED                        
             07h = _str$_7                         
             08h = RESERVED                        
             09h = _str$_9                         
             0Ah = _str$_10                        
             0Bh = _str$_11                        
             0Ch = _str$_12                        
             0Dh = RESERVED                        
             0Eh = _str$_14                        
             0Fh = _str$_15                        
	(Input file: BSP\SETUP\OEM.SSP)

Q_Dual_Monitor_Video             157Eh AFh  0040h 0000h   0000h    Yes   No 
             (External Function = oem_Dual_Monitor_Video)
	(Input file: OEMBOARD\oemboard.ssp)

Q_ONBOARD_RIDE_ENABLE            157Fh AFh  0080h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\EM\IntelSetup\IntelSetup.ssp)

Q_ONBOARD_RIDE_ROM_ENABLE        1586h B0h  0040h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\EM\IntelSetup\IntelSetup.ssp)

Q_ONBOARD_SCSI_ENABLE            1587h B0h  0080h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_ONBOARD_SCSI_ROM_ENABLE        158Eh B1h  0040h 0001h   0001h    Yes   No 
             (External Function = oem_Refer_to_OPROM_MODE)
	(Input file: OEMBOARD\oemboard.ssp)

Q_ONBOARD_NIC1_ENABLE            158Fh B1h  0080h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_ONBOARD_NIC1_ROM_ENABLE        15B0h B6h  0001h 0001h   0001h    Yes   No 
             (External Function = oem_Refer_to_NIC1)
	(Input file: OEMBOARD\oemboard.ssp)

Q_ONBOARD_NIC2_ENABLE            15B1h B6h  0002h 0001h   0001h    Yes   No 
             (External Function = OnBoard_NIC2_ext_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_ONBOARD_NIC2_ROM_ENABLE        15B2h B6h  0004h 0001h   0001h    Yes   No 
             (External Function = oem_shadewhen_nic2_disable)
	(Input file: OEMBOARD\oemboard.ssp)

Q_ONBOARD_VIDEO_ENABLE           15B3h B6h  0008h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_SLOT1_ROM                      15B4h B6h  0010h 0001h   0001h    Yes   No 
             (External Function = slot1_rom_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SLOT2_ROM                      15B5h B6h  0020h 0001h   0001h    Yes   No 
             (External Function = slot2_rom_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SLOT3_ROM                      15B6h B6h  0040h 0001h   0001h    Yes   No 
             (External Function = slot3_rom_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SLOT4_ROM                      15B7h B6h  0080h 0001h   0001h    Yes   No 
             (External Function = slot4_rom_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SLOT5_ROM                      15B8h B7h  0001h 0001h   0001h    Yes   No 
             (External Function = slot5_rom_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SLOT6_ROM                      15B9h B7h  0002h 0001h   0001h    Yes   No 
             (External Function = slot6_rom_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SLOT7_ROM                      15BAh B7h  0004h 0001h   0001h    Yes   No 
             (External Function = slot7_rom_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SLOT8_ROM                      15BBh B7h  0008h 0001h   0001h    Yes   No 
             (External Function = slot8_rom_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SLOT9_ROM                      15BCh B7h  0010h 0001h   0001h    Yes   No 
             (External Function = slot9_rom_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SLOT10_ROM                     15BDh B7h  0020h 0001h   0001h    Yes   No 
             (External Function = slot10_rom_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SLOT11_ROM                     15BEh B7h  0040h 0001h   0001h    Yes   No 
	(Input file: BSP\EM\IntelSetup\IntelSetup.ssp)

Q_SLOT12_ROM                     15BFh B7h  0080h 0001h   0001h    Yes   No 
	(Input file: BSP\EM\IntelSetup\IntelSetup.ssp)

Q_BMC_IRQ                        25C0h B8h  0003h 0003h   0003h    Yes   No 
	(Input file: BSP\EM\NEC\ABS.ssp)

Q_POWER_FAILURE_OPTION           25C2h B8h  000Ch 0000h   0000h    Yes   No 
             (External Function = ac_link_proc)
	(Input file: BSP\EM\ServerManagement\Server.ssp)

Q_POST_ERROR_PAUSE               15C4h B8h  0010h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\EM\NEC\ABS.ssp)

Q_TEMP_SENSOR                    15C5h B8h  0020h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\EM\NEC\ABS.ssp)

Q_NEC_SERIAL_BOTH                82B8h 57h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\NEC\ABS.ssp)

Q_NEC_LAN_BOTH                   82C0h 58h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\NEC\ABS.ssp)

Q_CLEAR_ALL_EVENT_LOG_ABS        15C6h B8h  0040h 0000h   0000h    Yes   No 
	(Input file: BSP\EM\NEC\ABS.ssp)

Q_MEMFAIL_CLR_ABS                15C7h B8h  0080h 0000h   0000h    Yes   No 
	(Input file: BSP\EM\IMT\IMT.SSP)

Q_FRB_RETESTCPU_ABS              15C8h B9h  0001h 0000h   0000h    Yes   No 
	(Input file: BSP\EM\NEC\ABS.ssp)

Q_SCAN_USER_FLASH_AREA           15C9h B9h  0002h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
             (External Function = User_Binary_EXTFUNC)
	(Input file: OEMBOARD\oemboard.ssp)

Q_INTEL_INT15_BITS               85D0h BAh  00FFh 0080h   0083h    Yes   No 
	(Input file: BSP\EM\OEMINT15\OEMINT15.SSP)

Q_REMOTE_ESC                     15CAh B9h  0004h 0000h   0000h    Yes   No 
	(Input file: BSP\EM\OEMINT15\OEMINT15.SSP)

Q_REMOTE_F12                     15CBh B9h  0008h 0000h   0000h    Yes   No 
	(Input file: BSP\EM\OEMINT15\OEMINT15.SSP)

Q_INTEL_MEMORY_TEST_ENABLE       15CCh B9h  0010h 0000h   0000h    Yes   No 
             00h = _STR$_Enabled                   
             01h = _STR$_Disabled                  
	(Input file: BSP\EM\IMT\IMT.SSP)

Q_BACKGROUND_TEST                15CDh B9h  0020h 0000h   0000h    Yes   No 
             00h = _STR$_Enabled                   
             01h = _STR$_Disabled                  
	(Input file: BSP\EM\IMT\IMT.SSP)

Q_EXTMEMTEST_BUMP                25CEh B9h  00C0h 0003h   0003h    Yes   No 
             00h = _STR$_1_MB                      
             01h = _STR$_1_KB                      
             02h = _STR$_every_location            
             03h = _STR$_Disabled                  
	(Input file: BSP\EM\IMT\IMT.SSP)

Q_BAD_DIMM_SIGN                  82C8h 59h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\IMT.SSP)

Q_BAD_DIMMS                      82D8h 5Bh  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\IMT.SSP)

Q_BAD_DIMMS_RETEST               82E0h 5Ch  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\IMT.SSP)

Q_BAD_DIMMS_PREVIOUS             82E8h 5Dh  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\IMT.SSP)

Q_FORCE_MEM_ONLINE               1278h 4Fh  0001h 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\IMT.SSP)

Q_VACANT_DIMMS                   82F0h 5Eh  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\IMT.SSP)

Q_SET_PRESENT                    427Ah 4Fh  003Ch 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\IMT.SSP)

Q_INTEL_MEMORY_REMAP_ENABLE      15D8h BBh  0001h 0000h   0000h    Yes   No 
             00h = _STR$_Enabled                   
             01h = _STR$_Disabled                  
	(Input file: BSP\EM\IMT\MEMORYR.SSP)

Q_MEMFAIL_CLR                    15D9h BBh  0002h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\EM\IMT\MEMORYR.SSP)

Q_BAD_DIMM_DRB1                  8300h 60h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\MEMORYR.SSP)

Q_BAD_DIMM_DRB3                  8308h 61h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\MEMORYR.SSP)

Q_BAD_DIMM_DRB5                  8310h 62h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\MEMORYR.SSP)

Q_BAD_DIMM_DRA0                  8318h 63h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\MEMORYR.SSP)

Q_BAD_DIMM_DRA1                  8320h 64h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\MEMORYR.SSP)

Q_BAD_DIMM_DRA2                  8328h 65h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\IMT\MEMORYR.SSP)

Q_DIMM0_Status                   15DAh BBh  0004h 0000h   0000h    Yes   No 
             (External Function = imt_DIMM0_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_DIMM1_Status                   15DBh BBh  0008h 0000h   0000h    Yes   No 
             (External Function = imt_DIMM1_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_DIMM2_Status                   15DCh BBh  0010h 0000h   0000h    Yes   No 
             (External Function = imt_DIMM2_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_DIMM3_Status                   15DDh BBh  0020h 0000h   0000h    Yes   No 
             (External Function = imt_DIMM3_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_PW_UNATTENDED_START            15DEh BBh  0040h 0000h   0000h    Yes   No 
             (External Function = CheckUserPwdInstall)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SECURE_MODE_TIMEOUT            35E0h BCh  0007h 0000h   0000h    Yes   No 
             (External Function = SecureModeTimeout_func)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SECURE_MODE_HOTKEY             15DFh BBh  0080h 0000h   0000h    Yes   No 
             (External Function = SecureModeHotkey_func)
	(Input file: OEMBOARD\oemboard.ssp)

Q_POWER_SWITCH_INHIBIT           15E3h BCh  0008h 0000h   0000h    Yes   No 
             (External Function = SahaleePowerandReset)
	(Input file: OEMBOARD\oemboard.ssp)

Q_RESET_SWITCH_INHIBIT           15E4h BCh  0010h 0000h   0000h    Yes   No 
             (External Function = SahaleePowerandReset)
	(Input file: OEMBOARD\oemboard.ssp)

Q_NMI_SWITCH_INHIBIT             15E5h BCh  0020h 0000h   0000h    Yes   No 
             00h = _STR$_Disabled                  
             01h = _STR$_Enabled                   
	(Input file: BSP\EM\INTELSECURITY\SECURITY.SSP)

Q_PASSWORD_CHECKSUM_LOWBYTE      8268h 4Dh  00FFh 0000h   0000h    No    Yes
	(Input file: BSP\EM\INTELSECURITY\SECURITY.SSP)

Q_PASSWORD_CHECKSUM_HIGHBYTE     8280h 50h  00FFh 0000h   0000h    No    Yes
	(Input file: BSP\EM\INTELSECURITY\SECURITY.SSP)

Q_PASSWORD_FAILURE_TALLY         227Eh 4Fh  00C0h 0000h   0000h    No    No 
	(Input file: BSP\EM\INTELSECURITY\SECURITY.SSP)

Q_PROGMTR_COUNT                  8330h 66h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\INTELSECURITY\SECURITY.SSP)

Q_NMI_PERR                       15E6h BCh  0040h 0001h   0001h    Yes   No 
             (External Function = NMI_PERR_ExtFunc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_NMI_SERR                       15E7h BCh  0080h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\EM\ServerManagement\Server.ssp)

Q_PEF_SETUP                      15E8h BDh  0001h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\EM\ServerManagement\Server.ssp)

Q_SYSMGMT_BMC                    8338h 67h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\Server.ssp)

Q_F4_SERVPART_CFG                8340h 68h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\Server.ssp)

Q_SERVPART_CFG                   8348h 69h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\Server.ssp)

Q_SYSMGMT_LAN_REDIR              15E9h BDh  0002h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_SYSMGMT_LAN_ALERT              15EAh BDh  0004h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\EM\ServerManagement\LAN.ssp)

Q_SYSMGMT_LAN_DEV                25EBh BDh  0018h 0001h   0001h    Yes   No 
             00h = RESERVED                        
             01h = _str$_LanDev1                   
             02h = _str$_LanDev2                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_LAN_CHANNEL                    12F9h 5Fh  0002h 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\LAN.ssp)

Q_INT19_TRAPPED                  12FAh 5Fh  0004h 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\LAN.ssp)

Q_SYSMGMT_SERIAL_REDIR           15EDh BDh  0020h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_SYSMGMT_SERIAL_PORT            25EEh BDh  00C0h 0001h   0001h    Yes   No 
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_ABS_SYSMGMT_SERIAL_REDIR       25F0h BEh  0003h 0000h   0000h    Yes   No 
             (External Function = SerRedir_extfunc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SYSMGMT_SERIAL_RATE            35F2h BEh  001Ch 0002h   0002h    Yes   No 
             00h = _str$_Baud_9600                 
             01h = STR_RESERVED                    
             02h = _str$_Baud_19200                
             03h = STR_RESERVED                    
             04h = _str$_Baud_38400                
             05h = _str$_Baud_57600                
             06h = _str$_Baud_115200               
	(Input file: OEMBOARD\oemboard.ssp)

Q_SYSMGMT_SERIAL_FLOW            25F5h BEh  0060h 0001h   0001h    Yes   No 
             00h = _str$_FlowCtrlNone              
             01h = _str$_FlowCtrlCTS               
             02h = _str$_FlowCtrlXONOFF            
             03h = _str$_FlowCtrlCTSCD             
	(Input file: OEMBOARD\oemboard.ssp)

Q_SYSMGMT_SERIAL_TERM            25F8h BFh  0003h 0002h   0002h    Yes   No 
             00h = _str$_TermTypePcansi            
             01h = STR_RESERVED                    
             02h = _str$_TermTypeVt100p            
             03h = _str$_TermTypeVtutf8            
	(Input file: OEMBOARD\oemboard.ssp)

Q_SYSMGMT_SERIAL_RESET           15F7h BEh  0080h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_SYSMGMT_CONTINUE_SERIAL_REDIR  25FAh BFh  000Ch 0002h   0002h    Yes   No 
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_ACPI_OS_HEADLESS               25FCh BFh  0030h 0000h   0000h    Yes   No 
             00h = _STR$_DISABLED                  
             01h = STR_RESERVED                    
             02h = _STR$_serial1                   
             03h = _STR$_serial2                   
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_SYSMGMT_SERIAL_ACPI_RATE       25FEh BFh  00C0h 0001h   0001h    Yes   No 
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_SYSMGMT_SERIAL_ACPI_FLOW       2600h C0h  0003h 0001h   0001h    Yes   No 
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_SYSMGMT_SERIAL_ACPI_TERM       2602h C0h  000Ch 0002h   0002h    Yes   No 
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_WHICH_REDIR                    8350h 6Ah  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_SERIAL_LOCAL_REMOTE            8358h 6Bh  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_SYSMGMT_SERIAL_REDIR_BACK      8360h 6Ch  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_SYSMGMT_SERIAL_PORT_BACK       8368h 6Dh  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_SYSMGMT_SERIAL_RATE_BACK       8370h 6Eh  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_SYSMGMT_SERIAL_FLOW_BACK       8378h 6Fh  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_INITIAL_BACK                   8608h C1h  00FFh 0000h   0000h    Yes   No 
	(Input file: BSP\EM\ServerManagement\Serial.ssp)

Q_FRB_RETESTCPU                  1604h C0h  0010h 0000h   0000h    Yes   No 
             (External Function = CheckForCPURetestSupport_FAR)
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_FRB_EARLY                      3605h C0h  00E0h 0001h   0001h    Yes   No 
             (External Function = FRB2_EXT_Func_Far)
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_FRB_LATE                       3610h C2h  0007h 0000h   0000h    Yes   No 
             00h = _str$_FRBDisable                
             01h = _str$_FRB5min                   
             02h = _str$_FRB10min                  
             03h = _str$_FRB15min                  
             04h = _str$_FRB20min                  
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_FRB_OS_HDD                     3613h C2h  0038h 0000h   0000h    Yes   No 
             00h = _str$_FRBDisable                
             01h = _str$_FRB5min                   
             02h = _str$_FRB10min                  
             03h = _str$_FRB15min                  
             04h = _str$_FRB20min                  
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_FRB_OS_PXE                     3618h C3h  0007h 0000h   0000h    Yes   No 
             00h = _str$_FRBDisable                
             01h = _str$_FRB5min                   
             02h = _str$_FRB10min                  
             03h = _str$_FRB15min                  
             04h = _str$_FRB20min                  
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_FRB_OS_POLICY                  2616h C2h  00C0h 0000h   0000h    Yes   No 
             00h = _str$_FRBnoaction               
             01h = _str$_FRBrestart                
             02h = _str$_FRBPoweroff               
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_FRB_BIST_BSP                   12F8h 5Fh  0001h 0000h   0000h    No    Yes
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_FRB4_COUNT                     22FBh 5Fh  0018h 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_LATE_FRB2_FLAG                 12FDh 5Fh  0020h 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_BMC_DEAD                       1279h 4Fh  0002h 0000h   0000h    No    Yes
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_CMOS_IP_FLAGBYTE               8270h 4Eh  00FFh 0000h   0000h    No    Yes
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_WD_TIMER_FAIL_REASON           82D0h 5Ah  00FFh 0000h   0000h    No    Yes
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_FRB2_P80                       8380h 70h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_FRB2_P81                       8388h 71h  00FFh 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_NUM_FRB_FAILURES               22FEh 5Fh  00C0h 0000h   0000h    No    No 
	(Input file: BSP\EM\ServerManagement\FRB.ssp)

Q_CLEAR_ALL_EVENT_LOG            161Bh C3h  0008h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\EM\ServerManagement\Eventlog.ssp)

Q_SMM_EN                         161Ch C3h  0010h 0001h   0001h    Yes   No 
             (External Function = q_smm_en_extfunc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_EVENT_LOGGING                  161Dh C3h  0020h 0001h   0001h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: BSP\EM\ServerManagement\Eventlog.ssp)

Q_INTEL_BoardPartNumber          161Eh C3h  0040h 0000h   0000h    Yes   No 
             (External Function = board_part_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_BoardSerialNumber        161Fh C3h  0080h 0000h   0000h    Yes   No 
             (External Function = board_serial_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_SystemPartNumber         1620h C4h  0001h 0000h   0000h    Yes   No 
             (External Function = system_part_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_SystemSerialNumber       1621h C4h  0002h 0000h   0000h    Yes   No 
             (External Function = system_serial_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_ChassisPartNumber        1622h C4h  0004h 0000h   0000h    Yes   No 
             (External Function = chassis_part_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_ChassisSerialNumber      1623h C4h  0008h 0000h   0000h    Yes   No 
             (External Function = chassis_serial_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_bmcDeviceID              1624h C4h  0010h 0000h   0000h    Yes   No 
             (External Function = bmc_deviceID_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_bmcFirmwareRevision      1625h C4h  0020h 0000h   0000h    Yes   No 
             (External Function = bmc_firmware_revision_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_bmcVersion               1626h C4h  0040h 0000h   0000h    Yes   No 
             (External Function = bmc_version_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_PIARevision              1627h C4h  0080h 0000h   0000h    Yes   No 
             (External Function = bmc_PIA_revision_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_SDRRevision              1628h C5h  0001h 0000h   0000h    Yes   No 
             (External Function = bmc_SDR_revision_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_fpcVersion               1629h C5h  0002h 0000h   0000h    Yes   No 
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_phscVersion              162Ah C5h  0004h 0000h   0000h    Yes   No 
             (External Function = phsc_version_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_shscVersion              162Bh C5h  0008h 0000h   0000h    Yes   No 
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_pscVersion               162Ch C5h  0010h 0000h   0000h    Yes   No 
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_INTEL_hscVersion               162Dh C5h  0020h 0000h   0000h    Yes   No 
             (External Function = hsc_version_proc)
	(Input file: BSP\EM\ServerManagement\BMC.ssp)

Q_SPREAD_SPECTRUM                11C2h 38h  0004h 0001h   0001h    Yes   Yes
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_COM_MODE                       262Eh C5h  00C0h 0000h   0000h    Yes   No 
             (External Function = com_SP_mode_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SP2_CTS_Setting                1630h C6h  0001h 0000h   0000h    Yes   No 
             (External Function = SP2_CTS_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SP2_DSR_Setting                1631h C6h  0002h 0000h   0000h    Yes   No 
             (External Function = SP2_DSR_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SP2_DCD_Setting                1632h C6h  0004h 0000h   0000h    Yes   No 
             (External Function = SP2_DCD_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SI1_RTS_Setting                1633h C6h  0008h 0000h   0000h    Yes   No 
             (External Function = SI1_RTS_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SI1_DTR_Setting                1634h C6h  0010h 0000h   0000h    Yes   No 
             (External Function = SI1_DTR_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SI2_RTS_Setting                1635h C6h  0020h 0000h   0000h    Yes   No 
             (External Function = SI2_RTS_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SI2_DTR_Setting                1636h C6h  0040h 0000h   0000h    Yes   No 
             (External Function = SI2_DTR_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_SIM_TRI_State                  1637h C6h  0080h 0000h   0000h    Yes   No 
             (External Function = SIM_TRI_State_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_COMA_SI2_PORT                  3638h C7h  0007h 0002h   0002h    Yes   No 
             (External Function = com_a_SI2_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_PCIE_POLARITY_INVERSION        328Bh 51h  0038h 0000h   0000h    Yes   Yes
             00h = _str$_DISABLED                  
             01h = _str$_DEVICE_2                  
             02h = STR_RESERVED                    
             03h = STR_RESERVED                    
             04h = STR_RESERVED                    
             05h = _str$_DEVICE_6                  
             06h = _str$_DEVICE_7                  
	(Input file: OEMBOARD\oemboard.ssp)

Q_PCIE_JITTER_TOLERANCE          128Eh 51h  0040h 0000h   0000h    Yes   Yes
             00h = _str$_DISABLED                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_DBI_INVERSION                  128Fh 51h  0080h 0001h   0001h    Yes   Yes
             00h = _str$_DISABLED                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_COMPLIANCE_MODE                1290h 52h  0001h 0000h   0000h    Yes   Yes
             00h = _STR$_DISABLED                  
             01h = _STR$_ENABLED                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_COMPATIBILITY_2                1292h 52h  0004h 0000h   0000h    Yes   Yes
             00h = _STR$_10_A                      
             01h = _STR$_mode10                    
	(Input file: OEMBOARD\oemboard.ssp)

Q_COMPATIBILITY_3                1293h 52h  0008h 0000h   0000h    Yes   Yes
             00h = _STR$_10_A                      
             01h = _STR$_mode10                    
	(Input file: OEMBOARD\oemboard.ssp)

Q_COMPATIBILITY_4                1294h 52h  0010h 0000h   0000h    Yes   Yes
             00h = _STR$_10_A                      
             01h = _STR$_mode10                    
	(Input file: OEMBOARD\oemboard.ssp)

Q_COMPATIBILITY_5                1295h 52h  0020h 0000h   0000h    Yes   Yes
             00h = _STR$_10_A                      
             01h = _STR$_mode10                    
	(Input file: OEMBOARD\oemboard.ssp)

Q_COMPATIBILITY_6                1296h 52h  0040h 0000h   0000h    Yes   Yes
             00h = _STR$_10_A                      
             01h = _STR$_mode10                    
	(Input file: OEMBOARD\oemboard.ssp)

Q_COMPATIBILITY_7                1297h 52h  0080h 0000h   0000h    Yes   Yes
             00h = _STR$_10_A                      
             01h = _STR$_mode10                    
	(Input file: OEMBOARD\oemboard.ssp)

Q_Onboard_SCSI_Function_Mode     263Bh C7h  0018h 0001h   0001h    Yes   No 
             (External Function = SCSI_mode_func_far)
	(Input file: OEMBOARD\oemboard.ssp)

Q_EUSB_TXCTRL                    263Dh C7h  0060h 0002h   0002h    Yes   No 
             00h = _str$_EUSB_TXCTRL_LOW           
             01h = _str$_EUSB_TXCTRL_MIDDLE        
             02h = _str$_EUSB_TXCTRL_FULL          
             03h = _str$_EUSB_TXCTRL_HIGH          
	(Input file: OEMBOARD\oemboard.ssp)

Q_USB2_AFE_Disconnect            2640h C8h  0003h 0002h   0002h    Yes   No 
             00h = _str$_USB2_AFE_Dis_IREF400EN    
             01h = _str$_USB2_AFE_Dis_IREF475EN    
             02h = _str$_USB2_AFE_Dis_IREF450EN    
             03h = _str$_USB2_AFE_Dis_IREF425EN    
	(Input file: OEMBOARD\oemboard.ssp)

Q_USB2_AFE_RCAL                  2642h C8h  000Ch 0002h   0002h    Yes   No 
             00h = _str$_USB2_AFE_RCAL_RCAL400EN   
             01h = _str$_USB2_AFE_RCAL_RCAL475EN   
             02h = _str$_USB2_AFE_RCAL_RCAL450EN   
             03h = _str$_USB2_AFE_RCAL_RCAL425EN   
	(Input file: OEMBOARD\oemboard.ssp)

Q_USB2_AFE_ICAL                  2644h C8h  0030h 0002h   0002h    Yes   No 
             00h = _str$_USB2_AFE_ICAL_ICAL400EN   
             01h = _str$_USB2_AFE_ICAL_ICAL475EN   
             02h = _str$_USB2_AFE_ICAL_ICAL450EN   
             03h = _str$_USB2_AFE_ICAL_ICAL425EN   
	(Input file: OEMBOARD\oemboard.ssp)

Q_BAD_DIMMS_INFO                 8390h 72h  00FFh 0000h   0000h    No    No 
	(Input file: OEMBOARD\oemboard.ssp)

Q_UnUse_DIMMS_INFO               8398h 73h  00FFh 0000h   0000h    No    No 
	(Input file: OEMBOARD\oemboard.ssp)

Q_DIMM4_Status                   163Fh C7h  0080h 0000h   0000h    Yes   No 
             (External Function = imt_DIMM4_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_DIMM5_Status                   1646h C8h  0040h 0000h   0000h    Yes   No 
             (External Function = imt_DIMM5_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_POWER_RESET_SWITCH_INHIBIT     1647h C8h  0080h 0000h   0000h    Yes   No 
             (External Function = MiniBMCPowerandReset)
	(Input file: OEMBOARD\oemboard.ssp)

Q_Slow_Edge_Rates_WA             1648h C9h  0001h 0001h   0001h    Yes   No 
             00h = _STR$_ENABLE                    
             01h = _STR$_DISABLE                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_MCH_ERR_SMI                    1649h C9h  0002h 0000h   0000h    Yes   No 
             00h = _str$_Enabled                   
             01h = _str$_Disabled                  
	(Input file: OEMBOARD\oemboard.ssp)

Q_PXH_PCIXCAP_WA                 164Ah C9h  0004h 0000h   0000h    Yes   No 
             00h = _STR$_Disable                   
             01h = _STR$_Enable                    
	(Input file: OEMBOARD\oemboard.ssp)

Q_HW_MCH_ERR_SMI                 164Bh C9h  0008h 0000h   0000h    Yes   No 
             00h = _str$_Enabled                   
             01h = _str$_Disabled                  
	(Input file: OEMBOARD\oemboard.ssp)

Q_PCIe_Cold_Reset_Fail           11D1h 3Ah  0002h 0000h   0000h    No    Yes
	(Input file: OEMBOARD\oemboard.ssp)

Q_PLLSEL_Done                    11D0h 3Ah  0001h 0000h   0000h    No    Yes
	(Input file: OEMBOARD\oemboard.ssp)

Q_DRC_Filter_Threshold           42A8h 55h  000Fh 0006h   0006h    Yes   Yes
             00h = STR_RESERVED                    
             01h = STR_RESERVED                    
             02h = STR_RESERVED                    
             03h = STR_RESERVED                    
             04h = _STR$_4                         
             05h = _STR$_5                         
             06h = _STR$_6                         
             07h = _STR$_7                         
             08h = _STR$_8                         
             09h = _STR$_9                         
             0Ah = _STR$_10                        
             0Bh = _STR$_11                        
             0Ch = _STR$_12                        
             0Dh = STR_RESERVED                    
             0Eh = STR_RESERVED                    
             0Fh = STR_RESERVED                    
	(Input file: OEMBOARD\oemboard.ssp)

Q_ABS_SYSMGMT_SERIAL_REDIR_mbmc  264Ch C9h  0030h 0000h   0000h    Yes   No 
             (External Function = SerRedirmbmc_extfunc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_MCH_GE_C1                      13A0h 74h  0001h 0000h   0000h    No    No 
             00h = _str$_No                        
             01h = _str$_Yes                       
	(Input file: OEMBOARD\oemboard.ssp)

Q_SATA_Platform                  13A1h 74h  0002h 0000h   0000h    No    No 
             00h = _str$_No                        
             01h = _str$_Yes                       
	(Input file: OEMBOARD\oemboard.ssp)

Q_MCH_BSU_E66                    264Eh C9h  00C0h 0000h   0000h    Yes   No 
             00h = _str$_Mode1                     
             01h = _str$_Mode2                     
             02h = _str$_Mode3                     
             03h = _str$_Mode4                     
	(Input file: OEMBOARD\oemboard.ssp)

Q_SLOT3_SHOW_1_ROM               1650h CAh  0001h 0001h   0001h    Yes   No 
             (External Function = slot3_SHOW_1_rom_proc)
	(Input file: OEMBOARD\oemboard.ssp)

Q_DED_RETRY                      13A8h 75h  0001h 0000h   0000h    Yes   Yes
             00h = _str$_Enabled                   
             01h = _str$_DISABLED                  
	(Input file: OEMBOARD\oemboard.ssp)

Q_Show_Mirror                    1651h CAh  0002h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_PXH_PCI_Priority_Arb           1652h CAh  0004h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_C1E_SUPPORT                    1653h CAh  0008h 0001h   0001h    Yes   No 
	(Input file: OEMBOARD\oemboard.ssp)

Q_PCI_MMIO_64                    1654h CAh  0010h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_ABS_SERIAL_REDIR_BACKUP        2655h CAh  0060h 0000h   0000h    Yes   No 
	(Input file: OEMBOARD\oemboard.ssp)

Q_SBE_DIMMS                      8658h CBh  00FFh 0000h   0000h    No    No 
	(Input file: OEMBOARD\oemboard.ssp)

Q_Mirror_Mode                    11D3h 3Ah  0008h 0000h   0000h    No    Yes
	(Input file: OEMBOARD\oemboard.ssp)

Q_HYPER_MPS                      1657h CAh  0080h 0000h   0000h    Yes   No 
             (External Function = JTinMPSControlFunc_FAR)
	(Input file: OEMBOARD\oemboard.ssp)

Q_CLEAR_ALL_EVENT_LOG_WHEN_FULL  1668h CDh  0001h 0000h   0000h    Yes   No 
             00h = _str$_Disabled                  
             01h = _str$_Enabled                   
	(Input file: OEMBOARD\oemboard.ssp)

Q_EVENT_TIMESTAMP                1669h CDh  0002h 0000h   0000h    Yes   No 
             (External Function = TS_EVENT_LOGGING_PROC)
	(Input file: OEMBOARD\oemboard.ssp)

Q_USB_STOP_HISPEED_HC            166Ah CDh  0004h 0000h   0000h    Yes   No 
             00h = _str$_ENABLED                   
             01h = _str$_DISABLED                  
	(Input file: OEMBOARD\oemboard.ssp)

Q_USB_MASS_CHECKSUM              8670h CEh  00FFh 0000h   0000h    No    No 
	(Input file: OEMBOARD\oemboard.ssp)

Q_CLEAR_CMOS_FP                  13A2h 74h  0004h 0000h   0000h    No    No 
	(Input file: OEMBOARD\oemboard.ssp)

Q_Highest_MEM_Address            166Bh CDh  0008h 0000h   0000h    Yes   No 
             00h = _str$_Enabled                   
             01h = _str$_Disabled                  
	(Input file: OEMBOARD\oemboard.ssp)

Q_CPU_VT                         166Ch CDh  0010h 0001h   0001h    Yes   No 
	(Input file: OEMBOARD\oemboard.ssp)

Q_S5_Setup                       166Dh CDh  0020h 0000h   0000h    Yes   No 
             00h = _str$_Enabled                   
             01h = _str$_Disabled                  
	(Input file: OEMBOARD\oemboard.ssp)

Q_ACPI_IPMI                      166Eh CDh  0040h 0000h   0000h    Yes   No 
             (External Function = ACPI_IPMI_extfunc)
	(Input file: OEMBOARD\oemboard.ssp)

---------------------------------------------------------------


CMOS Map by Location


                                 CMOS  CMOS CMOS  Default Failsafe            
Question                         Token Reg. Mask  Value   Value    CkSum Fixed
------------------------------------------------------------------------------
Q_DATE                           0008h 00h  0000h 0000h   0000h    Yes   No 
Q_TIME                           0008h 00h  0000h 0000h   0000h    Yes   No 
Q_RTC_SECONDS                    8000h 00h  00FFh 0000h   0000h    No    Yes
Q_RTC_SECONDS_ALARM              8008h 01h  00FFh 0000h   0000h    No    Yes
Q_RTC_MINUTES                    8010h 02h  00FFh 0000h   0000h    No    Yes
Q_RTC_MINUTES_ALARM              8018h 03h  00FFh 0000h   0000h    No    Yes
Q_RTC_HOURS                      8020h 04h  00FFh 0000h   0000h    No    Yes
Q_RTC_HOURS_ALARM                8028h 05h  00FFh 0000h   0000h    No    Yes
Q_RTC_DAY_OF_WEEK                8030h 06h  00FFh 0000h   0000h    No    Yes
Q_RTC_DAY                        8038h 07h  00FFh 0000h   0000h    No    Yes
Q_RTC_MONTH                      8040h 08h  00FFh 0000h   0000h    No    Yes
Q_RTC_YEAR                       8048h 09h  00FFh 0000h   0000h    No    Yes
Q_RTC_STATUS_A                   8050h 0Ah  00FFh 0000h   0000h    No    Yes
Q_RTC_STATUS_B                   8058h 0Bh  00FFh 0000h   0000h    No    Yes
Q_RTC_STATUS_C                   8060h 0Ch  00FFh 0000h   0000h    No    Yes
Q_RTC_STATUS_D                   8068h 0Dh  00FFh 0000h   0000h    No    Yes
Q_RTC_DIAG_STATUS                8070h 0Eh  00FFh 0000h   0000h    No    Yes
Q_RTC_SHUTDOWN_STATUS            8078h 0Fh  00FFh 0000h   0000h    No    Yes
Q_FLOPPY_A                       4084h 10h  00F0h 0004h   0004h    Yes   Yes
Q_FLOPPY_B                       4080h 10h  000Fh 0000h   0000h    Yes   Yes
Q_BOOT_FIRST_DEVICE              4088h 11h  000Fh 0000h   0000h    Yes   No 
Q_DISPLAY_MODE                   108Ch 11h  0010h 0000h   0000h    Yes   No 
Q_PM_E_TYPE                      208Dh 11h  0060h 0001h   0001h    Yes   No 
Q_3M_LBA_MODE                    108Fh 11h  0080h 0001h   0001h    Yes   No 
Q_PM_TYPE                        4094h 12h  00F0h 0000h   0000h    Yes   Yes
Q_PS_TYPE                        4090h 12h  000Fh 0000h   0000h    Yes   Yes
Q_PS_E_TYPE                      2098h 13h  0003h 0001h   0001h    Yes   No 
Q_SM_E_TYPE                      209Ah 13h  000Ch 0001h   0001h    Yes   No 
Q_SS_E_TYPE                      209Ch 13h  0030h 0001h   0001h    Yes   No 
Q_3M_E_TYPE                      209Eh 13h  00C0h 0001h   0001h    Yes   No 
Q_DISPLAY_TYPE                   30A3h 14h  0038h 0001h   0001h    Yes   Yes
Q_FLOPPY_COUNT                   20A6h 14h  00C0h 0000h   0000h    Yes   Yes
Q_MATHCO_PRESENT                 10A1h 14h  0002h 0000h   0000h    Yes   Yes
Q_FLOPPY_PRESENT                 10A0h 14h  0001h 0000h   0000h    Yes   Yes
Q_KEYBOARD_PRESENT               10A2h 14h  0004h 0001h   0001h    Yes   Yes
Q_BASE_MEMORY_LSB                80A8h 15h  00FFh 0000h   0000h    Yes   Yes
Q_BASE_MEMORY_MSB                80B0h 16h  00FFh 0000h   0000h    Yes   Yes
Q_EXT_MEMORY_LSB                 80B8h 17h  00FFh 0000h   0000h    Yes   Yes
Q_EXT_MEMORY_MSB                 80C0h 18h  00FFh 0000h   0000h    Yes   Yes
Q_PM_EXT_TYPE                    80C8h 19h  00FFh 0030h   0030h    Yes   Yes
Q_PS_EXT_TYPE                    80D0h 1Ah  00FFh 0030h   0030h    Yes   Yes
Q_PM_CYL                         00D8h 1Bh  FFFFh 0000h   0000h    Yes   Yes
Q_PM_HD                          80E8h 1Dh  00FFh 0000h   0000h    Yes   Yes
Q_PM_WPCOM                       00F0h 1Eh  FFFFh 0000h   0000h    Yes   Yes
Q_PM_SPT                         8100h 20h  00FFh 0000h   0000h    Yes   Yes
Q_PS_CYL                         0108h 21h  FFFFh 0000h   0000h    Yes   Yes
Q_PS_HD                          8118h 23h  00FFh 0000h   0000h    Yes   Yes
Q_PS_WPCOM                       0120h 24h  FFFFh 0000h   0000h    Yes   Yes
Q_PS_SPT                         8130h 26h  00FFh 0000h   0000h    Yes   Yes
Q_SM_TYPE                        8138h 27h  00FFh 0030h   0030h    Yes   Yes
Q_SS_TYPE                        8140h 28h  00FFh 0030h   0030h    Yes   Yes
Q_3S_E_TYPE                      2148h 29h  0003h 0001h   0001h    Yes   No 
Q_4M_E_TYPE                      214Ah 29h  000Ch 0001h   0001h    Yes   No 
Q_4S_E_TYPE                      214Ch 29h  0030h 0001h   0001h    Yes   No 
Q_PM_SMART                       214Eh 29h  00C0h 0000h   0000h    Yes   No 
Q_PM_LBA_MODE                    1150h 2Ah  0001h 0001h   0001h    Yes   Yes
Q_PM_BLOCK_MODE                  1151h 2Ah  0002h 0001h   0001h    Yes   Yes
Q_PM_PIO_MODE                    3153h 2Ah  0038h 0000h   0000h    Yes   Yes
Q_PM_32BIT_XFER                  1152h 2Ah  0004h 0000h   0000h    Yes   Yes
Q_PM_EMULATION_TYPE              2156h 2Ah  00C0h 0000h   0000h    Yes   No 
Q_PS_LBA_MODE                    1158h 2Bh  0001h 0001h   0001h    Yes   Yes
Q_PS_BLOCK_MODE                  1159h 2Bh  0002h 0001h   0001h    Yes   Yes
Q_PS_32BIT_XFER                  115Ah 2Bh  0004h 0000h   0000h    Yes   Yes
Q_PS_PIO_MODE                    315Bh 2Bh  0038h 0000h   0000h    Yes   Yes
Q_PS_SMART                       215Eh 2Bh  00C0h 0000h   0000h    Yes   No 
Q_PS_EMULATION_TYPE              2166h 2Ch  00C0h 0000h   0000h    Yes   No 
Q_SM_LBA_MODE                    1160h 2Ch  0001h 0001h   0001h    Yes   Yes
Q_SM_BLOCK_MODE                  1161h 2Ch  0002h 0001h   0001h    Yes   Yes
Q_SM_PIO_MODE                    3163h 2Ch  0038h 0000h   0000h    Yes   Yes
Q_SM_32BIT_XFER                  1162h 2Ch  0004h 0000h   0000h    Yes   Yes
Q_SM_SMART                       216Eh 2Dh  00C0h 0000h   0000h    Yes   No 
Q_SS_LBA_MODE                    1168h 2Dh  0001h 0001h   0001h    Yes   Yes
Q_SS_BLOCK_MODE                  1169h 2Dh  0002h 0001h   0001h    Yes   Yes
Q_SS_PIO_MODE                    316Bh 2Dh  0038h 0000h   0000h    Yes   Yes
Q_SS_32BIT_XFER                  116Ah 2Dh  0004h 0000h   0000h    Yes   Yes
Q_CHECKSUM_MSB                   8170h 2Eh  00FFh 0000h   0000h    No    Yes
Q_CHECKSUM_LSB                   8178h 2Fh  00FFh 0000h   0000h    No    Yes
Q_POST_EXT_MEMORY_LSB            8180h 30h  00FFh 0000h   0000h    Yes   Yes
Q_POST_EXT_MEMORY_MSB            8188h 31h  00FFh 0000h   0000h    Yes   Yes
Q_CENTURY                        8190h 32h  00FFh 0000h   0000h    Yes   Yes
Q_SCRATCH_33                     8198h 33h  00FFh 0000h   0000h    No    Yes
Q_SCRATCH_34                     81A0h 34h  00FFh 0000h   0000h    No    Yes
Q_SCRATCH_35                     81A8h 35h  00FFh 0000h   0000h    No    Yes
Q_SCRATCH_36                     81B0h 36h  00FFh 0000h   0000h    No    Yes
Q_COLOR                          41B8h 37h  000Fh 0000h   0000h    Yes   Yes
Q_PCI_IDE_CONTROLLER             31BCh 37h  0070h 0004h   0004h    Yes   No 
Q_3M_BLOCK_MODE                  11BFh 37h  0080h 0001h   0001h    Yes   No 
Q_PM_DMA_MODE                    41C3h 38h  0078h 0000h   0000h    Yes   No 
Q_SM_EMULATION_TYPE              21C0h 38h  0003h 0000h   0000h    Yes   No 
Q_3M_32BIT_XFER                  11C7h 38h  0080h 0000h   0000h    Yes   No 
Q_SPREAD_SPECTRUM                11C2h 38h  0004h 0001h   0001h    Yes   Yes
Q_PS_DMA_MODE                    41C8h 39h  000Fh 0000h   0000h    Yes   No 
Q_SM_DMA_MODE                    41CCh 39h  00F0h 0000h   0000h    Yes   No 
Q_PCIe_Cold_Reset_Fail           11D1h 3Ah  0002h 0000h   0000h    No    Yes
Q_PLLSEL_Done                    11D0h 3Ah  0001h 0000h   0000h    No    Yes
Q_Mirror_Mode                    11D3h 3Ah  0008h 0000h   0000h    No    Yes
Q_SS_DMA_MODE                    41D8h 3Bh  000Fh 0000h   0000h    Yes   No 
Q_SS_SMART                       21DCh 3Bh  0030h 0000h   0000h    Yes   No 
Q_SS_EMULATION_TYPE              21DEh 3Bh  00C0h 0000h   0000h    Yes   No 
Q_3M_TYPE                        81E0h 3Ch  00FFh 0030h   0030h    Yes   No 
Q_3M_PIO_MODE                    31E8h 3Dh  0007h 0000h   0000h    Yes   No 
Q_3M_DMA_MODE                    41EBh 3Dh  0078h 0000h   0000h    Yes   No 
Q_3S_LBA_MODE                    11EFh 3Dh  0080h 0001h   0001h    Yes   No 
Q_EXT_CMOS_CHECKSUM_MSB          81F0h 3Eh  00FFh 0000h   0000h    No    Yes
Q_EXT_CMOS_CHECKSUM_LSB          81F8h 3Fh  00FFh 0000h   0000h    No    Yes
Q_SM_CYL                         0200h 40h  FFFFh 0000h   0000h    Yes   Yes
Q_SM_HD                          8210h 42h  00FFh 0000h   0000h    Yes   Yes
Q_SM_WPCOM                       0218h 43h  FFFFh 0000h   0000h    Yes   Yes
Q_SM_SPT                         8228h 45h  00FFh 0000h   0000h    Yes   Yes
Q_SS_CYL                         0230h 46h  FFFFh 0000h   0000h    Yes   Yes
Q_SS_HD                          8240h 48h  00FFh 0000h   0000h    Yes   Yes
Q_SS_WPCOM                       0248h 49h  FFFFh 0000h   0000h    Yes   Yes
Q_SS_SPT                         8258h 4Bh  00FFh 0000h   0000h    Yes   Yes
Q_3M_SMART                       2261h 4Ch  0006h 0000h   0000h    Yes   No 
Q_3M_EMULATION_TYPE              2263h 4Ch  0018h 0000h   0000h    Yes   No 
Q_3S_BLOCK_MODE                  1265h 4Ch  0020h 0001h   0001h    Yes   No 
Q_3S_SMART                       2266h 4Ch  00C0h 0000h   0000h    Yes   No 
Q_L3_CACHE                       1260h 4Ch  0001h 0000h   0000h    Yes   Yes
Q_PASSWORD_CHECKSUM_LOWBYTE      8268h 4Dh  00FFh 0000h   0000h    No    Yes
Q_CMOS_IP_FLAGBYTE               8270h 4Eh  00FFh 0000h   0000h    No    Yes
Q_FORCE_MEM_ONLINE               1278h 4Fh  0001h 0000h   0000h    No    No 
Q_SET_PRESENT                    427Ah 4Fh  003Ch 0000h   0000h    No    No 
Q_PASSWORD_FAILURE_TALLY         227Eh 4Fh  00C0h 0000h   0000h    No    No 
Q_BMC_DEAD                       1279h 4Fh  0002h 0000h   0000h    No    Yes
Q_PASSWORD_CHECKSUM_HIGHBYTE     8280h 50h  00FFh 0000h   0000h    No    Yes
Q_HT_SUPPORT                     1288h 51h  0001h 0001h   0001h    Yes   Yes
Q_MEM_RAS_FEATURE                2289h 51h  0006h 0000h   0000h    Yes   Yes
Q_PCIE_POLARITY_INVERSION        328Bh 51h  0038h 0000h   0000h    Yes   Yes
Q_PCIE_JITTER_TOLERANCE          128Eh 51h  0040h 0000h   0000h    Yes   Yes
Q_DBI_INVERSION                  128Fh 51h  0080h 0001h   0001h    Yes   Yes
Q_3S_32BIT_XFER                  1291h 52h  0002h 0000h   0000h    Yes   No 
Q_COMPLIANCE_MODE                1290h 52h  0001h 0000h   0000h    Yes   Yes
Q_COMPATIBILITY_2                1292h 52h  0004h 0000h   0000h    Yes   Yes
Q_COMPATIBILITY_3                1293h 52h  0008h 0000h   0000h    Yes   Yes
Q_COMPATIBILITY_4                1294h 52h  0010h 0000h   0000h    Yes   Yes
Q_COMPATIBILITY_5                1295h 52h  0020h 0000h   0000h    Yes   Yes
Q_COMPATIBILITY_6                1296h 52h  0040h 0000h   0000h    Yes   Yes
Q_COMPATIBILITY_7                1297h 52h  0080h 0000h   0000h    Yes   Yes
I_CPU_FREQ_RATIO                 8298h 53h  00FFh 00FEh   00FEh    Yes   Yes
I_CPU_VID                        82A0h 54h  00FFh 003Eh   003Eh    Yes   Yes
Q_3S_PIO_MODE                    32ACh 55h  0070h 0000h   0000h    Yes   No 
Q_4M_LBA_MODE                    12AFh 55h  0080h 0001h   0001h    Yes   No 
Q_DRC_Filter_Threshold           42A8h 55h  000Fh 0006h   0006h    Yes   Yes
Q_3S_DMA_MODE                    42B4h 56h  00F0h 0000h   0000h    Yes   No 
Q_4M_BLOCK_MODE                  12B1h 56h  0002h 0001h   0001h    Yes   No 
Q_NX_Support                     12B0h 56h  0001h 0001h   0001h    Yes   Yes
Q_HW_Prefetcher                  12B2h 56h  0004h 0000h   0000h    Yes   Yes
Q_ACL_Prefetch                   12B3h 56h  0008h 0000h   0000h    Yes   Yes
Q_NEC_SERIAL_BOTH                82B8h 57h  00FFh 0000h   0000h    No    No 
Q_NEC_LAN_BOTH                   82C0h 58h  00FFh 0000h   0000h    No    No 
Q_BAD_DIMM_SIGN                  82C8h 59h  00FFh 0000h   0000h    No    No 
Q_WD_TIMER_FAIL_REASON           82D0h 5Ah  00FFh 0000h   0000h    No    Yes
Q_BAD_DIMMS                      82D8h 5Bh  00FFh 0000h   0000h    No    No 
Q_BAD_DIMMS_RETEST               82E0h 5Ch  00FFh 0000h   0000h    No    No 
Q_BAD_DIMMS_PREVIOUS             82E8h 5Dh  00FFh 0000h   0000h    No    No 
Q_VACANT_DIMMS                   82F0h 5Eh  00FFh 0000h   0000h    No    No 
Q_LAN_CHANNEL                    12F9h 5Fh  0002h 0000h   0000h    No    No 
Q_INT19_TRAPPED                  12FAh 5Fh  0004h 0000h   0000h    No    No 
Q_FRB_BIST_BSP                   12F8h 5Fh  0001h 0000h   0000h    No    Yes
Q_FRB4_COUNT                     22FBh 5Fh  0018h 0000h   0000h    No    No 
Q_LATE_FRB2_FLAG                 12FDh 5Fh  0020h 0000h   0000h    No    No 
Q_NUM_FRB_FAILURES               22FEh 5Fh  00C0h 0000h   0000h    No    No 
Q_BAD_DIMM_DRB1                  8300h 60h  00FFh 0000h   0000h    No    No 
Q_BAD_DIMM_DRB3                  8308h 61h  00FFh 0000h   0000h    No    No 
Q_BAD_DIMM_DRB5                  8310h 62h  00FFh 0000h   0000h    No    No 
Q_BAD_DIMM_DRA0                  8318h 63h  00FFh 0000h   0000h    No    No 
Q_BAD_DIMM_DRA1                  8320h 64h  00FFh 0000h   0000h    No    No 
Q_BAD_DIMM_DRA2                  8328h 65h  00FFh 0000h   0000h    No    No 
Q_PROGMTR_COUNT                  8330h 66h  00FFh 0000h   0000h    No    No 
Q_SYSMGMT_BMC                    8338h 67h  00FFh 0000h   0000h    No    No 
Q_F4_SERVPART_CFG                8340h 68h  00FFh 0000h   0000h    No    No 
Q_SERVPART_CFG                   8348h 69h  00FFh 0000h   0000h    No    No 
Q_WHICH_REDIR                    8350h 6Ah  00FFh 0000h   0000h    No    No 
Q_SERIAL_LOCAL_REMOTE            8358h 6Bh  00FFh 0000h   0000h    No    No 
Q_SYSMGMT_SERIAL_REDIR_BACK      8360h 6Ch  00FFh 0000h   0000h    No    No 
Q_SYSMGMT_SERIAL_PORT_BACK       8368h 6Dh  00FFh 0000h   0000h    No    No 
Q_SYSMGMT_SERIAL_RATE_BACK       8370h 6Eh  00FFh 0000h   0000h    No    No 
Q_SYSMGMT_SERIAL_FLOW_BACK       8378h 6Fh  00FFh 0000h   0000h    No    No 
Q_FRB2_P80                       8380h 70h  00FFh 0000h   0000h    No    No 
Q_FRB2_P81                       8388h 71h  00FFh 0000h   0000h    No    No 
Q_BAD_DIMMS_INFO                 8390h 72h  00FFh 0000h   0000h    No    No 
Q_UnUse_DIMMS_INFO               8398h 73h  00FFh 0000h   0000h    No    No 
Q_MCH_GE_C1                      13A0h 74h  0001h 0000h   0000h    No    No 
Q_SATA_Platform                  13A1h 74h  0002h 0000h   0000h    No    No 
Q_CLEAR_CMOS_FP                  13A2h 74h  0004h 0000h   0000h    No    No 
Q_3S_EMULATION_TYPE              23A9h 75h  0006h 0000h   0000h    Yes   No 
Q_4M_PIO_MODE                    33ABh 75h  0038h 0000h   0000h    Yes   No 
Q_4M_SMART                       23AEh 75h  00C0h 0000h   0000h    Yes   No 
Q_DED_RETRY                      13A8h 75h  0001h 0000h   0000h    Yes   Yes
Q_3S_TYPE                        83B0h 76h  00FFh 0030h   0030h    Yes   No 
Q_4M_TYPE                        83B8h 77h  00FFh 0030h   0030h    Yes   No 
Q_4M_DMA_MODE                    43C0h 78h  000Fh 0000h   0000h    Yes   No 
Q_4M_32BIT_XFER                  13C4h 78h  0010h 0000h   0000h    Yes   No 
Q_4M_EMULATION_TYPE              23C5h 78h  0060h 0000h   0000h    Yes   No 
Q_4S_LBA_MODE                    13C7h 78h  0080h 0001h   0001h    Yes   No 
Q_4S_TYPE                        83C8h 79h  00FFh 0030h   0030h    Yes   No 
Q_4S_BLOCK_MODE                  13D0h 7Ah  0001h 0001h   0001h    Yes   No 
Q_4S_PIO_MODE                    33D1h 7Ah  000Eh 0000h   0000h    Yes   No 
Q_4S_DMA_MODE                    43D4h 7Ah  00F0h 0000h   0000h    Yes   No 
Q_4S_SMART                       23D8h 7Bh  0003h 0000h   0000h    Yes   No 
Q_4S_32BIT_XFER                  13DAh 7Bh  0004h 0000h   0000h    Yes   No 
Q_4S_EMULATION_TYPE              23DBh 7Bh  0018h 0000h   0000h    Yes   No 
Q_HDD_ACCESS_CONTROL             13DDh 7Bh  0020h 0000h   0000h    Yes   No 
Q_ATA_80PIN_CABLE_DETECT         23DEh 7Bh  00C0h 0000h   0000h    Yes   No 
Q_ATA_DETECT_TIME_OUT            33E0h 7Ch  0007h 0007h   0007h    Yes   No 
Q_PNP_AWARE_OS                   13E3h 7Ch  0008h 0001h   0001h    Yes   No 
Q_PCI_LATENCY_TIMER              33E4h 7Ch  0070h 0001h   0001h    Yes   No 
Q_PCI_VGA_IRQ                    13E7h 7Ch  0080h 0000h   0000h    Yes   No 
Q_PCI_PALETTE_SNOOP              13E8h 7Dh  0001h 0000h   0000h    Yes   No 
Q_PCI_IDE_BUS_MASTER             13E9h 7Dh  0002h 0001h   0001h    Yes   No 
Q_PCI_OFFBOARD_IDE               33EAh 7Dh  001Ch 0000h   0000h    Yes   No 
Q_PCI_OFFBOARD_IDE_PRI_IRQ       33EDh 7Dh  00E0h 0000h   0000h    Yes   No 
Q_ACPI_S4                        83F0h 7Eh  00FFh 0000h   0000h    No    Yes
Q_PCI_OFFBOARD_IDE_SEC_IRQ       33F8h 7Fh  0007h 0000h   0000h    Yes   No 
Q_IRQ3_USED_BY_ISA               13FBh 7Fh  0008h 0000h   0000h    Yes   No 
Q_IRQ4_USED_BY_ISA               13FCh 7Fh  0010h 0000h   0000h    Yes   No 
Q_IRQ5_USED_BY_ISA               13FDh 7Fh  0020h 0000h   0000h    Yes   No 
Q_IRQ7_USED_BY_ISA               13FEh 7Fh  0040h 0000h   0000h    Yes   No 
Q_IRQ9_USED_BY_ISA               13FFh 7Fh  0080h 0000h   0000h    Yes   No 
Q_IRQ10_USED_BY_ISA              1400h 80h  0001h 0000h   0000h    Yes   No 
Q_IRQ11_USED_BY_ISA              1401h 80h  0002h 0000h   0000h    Yes   No 
Q_IRQ14_USED_BY_ISA              1402h 80h  0004h 0000h   0000h    Yes   No 
Q_IRQ15_USED_BY_ISA              1403h 80h  0008h 0000h   0000h    Yes   No 
Q_DMA0_USED_BY_ISA               1404h 80h  0010h 0000h   0000h    Yes   No 
Q_DMA1_USED_BY_ISA               1405h 80h  0020h 0000h   0000h    Yes   No 
Q_DMA3_USED_BY_ISA               1406h 80h  0040h 0000h   0000h    Yes   No 
Q_DMA5_USED_BY_ISA               1407h 80h  0080h 0000h   0000h    Yes   No 
Q_DMA6_USED_BY_ISA               1408h 81h  0001h 0000h   0000h    Yes   No 
Q_DMA7_USED_BY_ISA               1409h 81h  0002h 0000h   0000h    Yes   No 
Q_MEM_SIZE_USED_BY_ISA           240Ah 81h  000Ch 0000h   0000h    Yes   No 
Q_MEM_BASE_USED_BY_ISA           340Ch 81h  0070h 0002h   0002h    Yes   No 
Q_QUICK_BOOT                     140Fh 81h  0080h 0001h   0001h    Yes   No 
Q_INITIAL_DISPLAY                1410h 82h  0001h 0001h   0001h    Yes   No 
Q_ADDON_ROM_DISPLAY              1411h 82h  0002h 0001h   0001h    Yes   No 
Q_NUM_LOCK                       1412h 82h  0004h 0000h   0000h    Yes   No 
Q_MOUSE_SUPPORT                  2413h 82h  0018h 0002h   0002h    Yes   No 
Q_WAIT_FOR_F1                    1415h 82h  0020h 0001h   0001h    Yes   No 
Q_DISPLAY_HIT_DEL                1416h 82h  0040h 0001h   0001h    Yes   No 
Q_PASSWORD_CHECK                 1417h 82h  0080h 0000h   0000h    Yes   No 
Q_SUPERVISOR_PASSWORD            7418h 83h  00FFh 0000h   0000h    Yes   No 
Q_DENY_SETUP                     2450h 8Ah  0003h 0003h   0003h    Yes   No 
Q_VIRUS_PROTECTION               1452h 8Ah  0004h 0000h   0000h    Yes   No 
Q_I19_TRAP_ALLOW                 1453h 8Ah  0008h 0001h   0001h    Yes   No 
Q_FIRST_BOOT_DRIVE               4454h 8Ah  00F0h 0000h   0000h    Yes   No 
Q_USER_PASSWORD                  7458h 8Bh  00FFh 0000h   0000h    Yes   No 
Q_SECOND_BOOT_DRIVE              4490h 92h  000Fh 0001h   0001h    Yes   No 
Q_THIRD_BOOT_DRIVE               4494h 92h  00F0h 0002h   0002h    Yes   No 
Q_FOURTH_BOOT_DRIVE              4498h 93h  000Fh 0003h   0003h    Yes   No 
Q_FIFTH_BOOT_DRIVE               449Ch 93h  00F0h 0004h   0004h    Yes   No 
Q_SIXTH_BOOT_DRIVE               44A0h 94h  000Fh 0005h   0005h    Yes   No 
Q_SEVENTH_BOOT_DRIVE             44A4h 94h  00F0h 0006h   0006h    Yes   No 
Q_EIGHTH_BOOT_DRIVE              44A8h 95h  000Fh 0007h   0007h    Yes   No 
Q_NINETH_BOOT_DRIVE              44ACh 95h  00F0h 0008h   0008h    Yes   No 
Q_TENTH_BOOT_DRIVE               44B0h 96h  000Fh 0009h   0009h    Yes   No 
Q_ELEVENTH_BOOT_DRIVE            44B4h 96h  00F0h 000Ah   000Ah    Yes   No 
Q_TWELVETH_BOOT_DRIVE            44B8h 97h  000Fh 000Bh   000Bh    Yes   No 
Q_HD_FIRST_BOOT_DRIVE            44BCh 97h  00F0h 0000h   0000h    Yes   No 
Q_HD_SECOND_BOOT_DRIVE           44C0h 98h  000Fh 0001h   0001h    Yes   No 
Q_HD_THIRD_BOOT_DRIVE            44C4h 98h  00F0h 0002h   0002h    Yes   No 
Q_HD_FOURTH_BOOT_DRIVE           44C8h 99h  000Fh 0003h   0003h    Yes   No 
Q_HD_FIFTH_BOOT_DRIVE            44CCh 99h  00F0h 0004h   0004h    Yes   No 
Q_HD_SIXTH_BOOT_DRIVE            44D0h 9Ah  000Fh 0005h   0005h    Yes   No 
Q_HD_SEVENTH_BOOT_DRIVE          44D4h 9Ah  00F0h 0006h   0006h    Yes   No 
Q_HD_EIGHTH_BOOT_DRIVE           44D8h 9Bh  000Fh 0007h   0007h    Yes   No 
Q_HD_NINETH_BOOT_DRIVE           44DCh 9Bh  00F0h 0008h   0008h    Yes   No 
Q_HD_TENTH_BOOT_DRIVE            44E0h 9Ch  000Fh 0009h   0009h    Yes   No 
Q_HD_ELEVENTH_BOOT_DRIVE         44E4h 9Ch  00F0h 000Ah   000Ah    Yes   No 
Q_HD_TWELVETH_BOOT_DRIVE         44E8h 9Dh  000Fh 000Bh   000Bh    Yes   No 
Q_RD_FIRST_BOOT_DRIVE            34ECh 9Dh  0070h 0000h   0000h    Yes   No 
Q_COMB_DUPLEX_MODE               14EFh 9Dh  0080h 0001h   0001h    Yes   No 
Q_RD_SECOND_BOOT_DRIVE           34F0h 9Eh  0007h 0001h   0001h    Yes   No 
Q_RD_THIRD_BOOT_DRIVE            34F3h 9Eh  0038h 0002h   0002h    Yes   No 
Q_FLOPPY_CONTROLLER              24F6h 9Eh  00C0h 0002h   0002h    Yes   No 
Q_RD_FOURTH_BOOT_DRIVE           34F8h 9Fh  0007h 0003h   0003h    Yes   No 
Q_CD_FIRST_BOOT_DRIVE            34FBh 9Fh  0038h 0000h   0000h    Yes   No 
Q_COMB_MODE                      24FEh 9Fh  00C0h 0000h   0000h    Yes   No 
Q_CD_SECOND_BOOT_DRIVE           3500h A0h  0007h 0001h   0001h    Yes   No 
Q_CD_THIRD_BOOT_DRIVE            3503h A0h  0038h 0002h   0002h    Yes   No 
Q_COMB_IRRX_PIN                  1506h A0h  0040h 0001h   0001h    Yes   No 
Q_BU_UPDATE                      1507h A0h  0080h 0001h   0001h    Yes   No 
Q_CD_FOURTH_BOOT_DRIVE           3508h A1h  0007h 0003h   0003h    Yes   No 
Q_COMA_PORT                      350Bh A1h  0038h 0002h   0002h    Yes   No 
Q_CPUID_LIMIT                    150Eh A1h  0040h 0000h   0000h    Yes   No 
Q_REMAP                          150Fh A1h  0080h 0001h   0001h    Yes   No 
Q_COMB_PORT                      3510h A2h  0007h 0003h   0003h    Yes   No 
Q_INTERNAL_CACHE                 2513h A2h  0018h 0002h   0002h    Yes   No 
Q_C0000_SHADOW                   3515h A2h  00E0h 0000h   0000h    Yes   No 
Q_C4000_SHADOW                   3518h A3h  0007h 0000h   0000h    Yes   No 
Q_C8000_SHADOW                   351Bh A3h  0038h 0000h   0000h    Yes   No 
Q_AC97_AUDIO                     151Eh A3h  0040h 0000h   0000h    Yes   No 
Q_MC97_MODEM                     151Fh A3h  0080h 0000h   0000h    Yes   No 
Q_CC000_SHADOW                   3520h A4h  0007h 0000h   0000h    Yes   No 
Q_D0000_SHADOW                   3523h A4h  0038h 0000h   0000h    Yes   No 
Q_CPU_BIST_ENABLE                1526h A4h  0040h 0001h   0001h    Yes   No 
Q_ICH_DELAYED_TRANSACTION        1527h A4h  0080h 0001h   0001h    Yes   No 
Q_D4000_SHADOW                   3528h A5h  0007h 0000h   0000h    Yes   No 
Q_D8000_SHADOW                   352Bh A5h  0038h 0000h   0000h    Yes   No 
Q_ICH_DCB_ENABLE                 152Eh A5h  0040h 0001h   0001h    Yes   No 
Q_PCI_ATA_MODE                   152Fh A5h  0080h 0000h   0000h    Yes   No 
Q_DC000_SHADOW                   3530h A6h  0007h 0000h   0000h    Yes   No 
Q_PCI_PATA_CHANNEL               2533h A6h  0018h 0003h   0003h    Yes   No 
Q_PCI_SATA_CHANNEL               1535h A6h  0020h 0001h   0001h    Yes   No 
Q_SATA_AS_RAID                   1536h A6h  0040h 0000h   0000h    Yes   No 
Q_SATA_MODE                      1537h A6h  0080h 0000h   0000h    Yes   No 
Q_FIRST_CHANNEL                  1538h A7h  0001h 0000h   0000h    Yes   No 
Q_SECOND_CHANNEL                 1539h A7h  0002h 0000h   0000h    Yes   No 
Q_THIRD_CHANNEL                  153Ah A7h  0004h 0001h   0001h    Yes   No 
Q_ACPI_OS                        153Bh A7h  0008h 0001h   0001h    Yes   No 
Q_ACPI_2                         153Ch A7h  0010h 0000h   0000h    Yes   No 
Q_ACPI_APIC_TBL                  153Dh A7h  0020h 0001h   0001h    Yes   No 
Q_APIC_ACPI_IRQ                  153Eh A7h  0040h 0000h   0000h    Yes   No 
Q_ACPI_EXCH_BUF                  153Fh A7h  0080h 0001h   0001h    Yes   No 
Q_ACPI_HEADLESS_MODE             1540h A8h  0001h 0000h   0000h    Yes   No 
Q_REMOTE_ACCESS                  1541h A8h  0002h 0000h   0000h    Yes   No 
Q_RA_COM_NO                      2542h A8h  000Ch 0002h   0002h    Yes   No 
Q_RA_COM_MODE                    3544h A8h  0070h 0002h   0002h    Yes   No 
Q_USB_WAKEUP_FROM_S3S4           1547h A8h  0080h 0000h   0000h    Yes   No 
Q_TERMINAL_TYPE                  2548h A9h  0003h 0000h   0000h    Yes   No 
Q_ECC_EVENT_LOGGING              154Ah A9h  0004h 0001h   0001h    Yes   No 
Q_Hub_Interface_Event_Logging    154Bh A9h  0008h 0001h   0001h    Yes   No 
Q_System_Bus_Event_Logging       154Ch A9h  0010h 0001h   0001h    Yes   No 
Q_Memory_Buffer_Event_Logging    154Dh A9h  0020h 0000h   0000h    Yes   No 
Q_PCI_ERROR_LOGGING              154Eh A9h  0040h 0001h   0001h    Yes   No 
Q_geyserville_type               154Fh A9h  0080h 0000h   0000h    Yes   No 
Q_INTEL_SPEEDSTEP_TECH           3550h AAh  0007h 0003h   0003h    Yes   No 
Q_MPS_REVISION                   1553h AAh  0008h 0001h   0000h    Yes   No 
Q_ASPM_ENABLE                    1554h AAh  0010h 0000h   0000h    Yes   No 
Q_PCIE_ERROR_REPORTING           1555h AAh  0020h 0000h   0000h    Yes   No 
Q_PCIE_PORT2                     2556h AAh  00C0h 0000h   0000h    Yes   No 
Q_PCIE_PORT3                     2558h ABh  0003h 0000h   0000h    Yes   No 
Q_PCIE_PORT4                     255Ah ABh  000Ch 0000h   0000h    Yes   No 
Q_PCIE_PORT5                     255Ch ABh  0030h 0000h   0000h    Yes   No 
Q_PCIE_PORT6                     255Eh ABh  00C0h 0000h   0000h    Yes   No 
Q_PCIE_PORT7                     2560h ACh  0003h 0000h   0000h    Yes   No 
Q_PXH_IO_DECODE                  1562h ACh  0004h 0000h   0000h    Yes   No 
Q_PXH_RASERR_HANDLING            1563h ACh  0008h 0000h   0000h    Yes   No 
Q_PXH_VGA_DECODE                 1564h ACh  0010h 0001h   0001h    Yes   No 
Q_USB_FUNCTION_ENABLE            3565h ACh  00E0h 0003h   0003h    Yes   No 
Q_PXH_PCIX_CLOCK                 4568h ADh  000Fh 0000h   0000h    Yes   No 
Q_USB20_ENABLE                   156Ch ADh  0010h 0000h   0000h    Yes   No 
Q_USB_LEGACY_ENABLE              256Dh ADh  0060h 0002h   0002h    Yes   No 
Q_USB_LEGACY_KEYBOARD            156Fh ADh  0080h 0001h   0001h    Yes   No 
Q_USB_LEGACY_MOUSE               1570h AEh  0001h 0001h   0001h    Yes   No 
Q_USB_6460_EMULATION             1571h AEh  0002h 0000h   0000h    Yes   No 
Q_USB_LEGACY_STORAGE             1572h AEh  0004h 0001h   0001h    Yes   No 
Q_USB_STORAGE_DEVICE_DELAY       2573h AEh  0018h 0001h   0001h    Yes   No 
Q_USB_HISPEED_SUPPORT            1575h AEh  0020h 0001h   0001h    Yes   No 
Q_USB_BEEP                       1576h AEh  0040h 0000h   0000h    Yes   No 
Q_FLOPPY_SWAP                    1577h AEh  0080h 0000h   0000h    Yes   No 
Q_USB_MASS_DEV1_EMULATION        3578h AFh  0007h 0000h   0000h    Yes   No 
Q_USB_MASS_DEV2_EMULATION        357Bh AFh  0038h 0000h   0000h    Yes   No 
Q_Dual_Monitor_Video             157Eh AFh  0040h 0000h   0000h    Yes   No 
Q_ONBOARD_RIDE_ENABLE            157Fh AFh  0080h 0001h   0001h    Yes   No 
Q_USB_MASS_DEV3_EMULATION        3580h B0h  0007h 0000h   0000h    Yes   No 
Q_USB_MASS_DEV4_EMULATION        3583h B0h  0038h 0000h   0000h    Yes   No 
Q_ONBOARD_RIDE_ROM_ENABLE        1586h B0h  0040h 0001h   0001h    Yes   No 
Q_ONBOARD_SCSI_ENABLE            1587h B0h  0080h 0001h   0001h    Yes   No 
Q_USB_MASS_DEV5_EMULATION        3588h B1h  0007h 0000h   0000h    Yes   No 
Q_USB_MASS_DEV6_EMULATION        358Bh B1h  0038h 0000h   0000h    Yes   No 
Q_ONBOARD_SCSI_ROM_ENABLE        158Eh B1h  0040h 0001h   0001h    Yes   No 
Q_ONBOARD_NIC1_ENABLE            158Fh B1h  0080h 0001h   0001h    Yes   No 
Q_LANGUAGE                       0590h B2h  FFFFh 0000h   0000h    Yes   No 
Q_PCI_SLOT1_IRQ                  45A0h B4h  000Fh 0000h   0000h    Yes   No 
Q_PCI_SLOT2_IRQ                  45A4h B4h  00F0h 0000h   0000h    Yes   No 
Q_PCI_SLOT3_IRQ                  45A8h B5h  000Fh 0000h   0000h    Yes   No 
Q_PCI_SLOT4_IRQ                  45ACh B5h  00F0h 0000h   0000h    Yes   No 
Q_ONBOARD_NIC1_ROM_ENABLE        15B0h B6h  0001h 0001h   0001h    Yes   No 
Q_ONBOARD_NIC2_ENABLE            15B1h B6h  0002h 0001h   0001h    Yes   No 
Q_ONBOARD_NIC2_ROM_ENABLE        15B2h B6h  0004h 0001h   0001h    Yes   No 
Q_ONBOARD_VIDEO_ENABLE           15B3h B6h  0008h 0001h   0001h    Yes   No 
Q_SLOT1_ROM                      15B4h B6h  0010h 0001h   0001h    Yes   No 
Q_SLOT2_ROM                      15B5h B6h  0020h 0001h   0001h    Yes   No 
Q_SLOT3_ROM                      15B6h B6h  0040h 0001h   0001h    Yes   No 
Q_SLOT4_ROM                      15B7h B6h  0080h 0001h   0001h    Yes   No 
Q_SLOT5_ROM                      15B8h B7h  0001h 0001h   0001h    Yes   No 
Q_SLOT6_ROM                      15B9h B7h  0002h 0001h   0001h    Yes   No 
Q_SLOT7_ROM                      15BAh B7h  0004h 0001h   0001h    Yes   No 
Q_SLOT8_ROM                      15BBh B7h  0008h 0001h   0001h    Yes   No 
Q_SLOT9_ROM                      15BCh B7h  0010h 0001h   0001h    Yes   No 
Q_SLOT10_ROM                     15BDh B7h  0020h 0001h   0001h    Yes   No 
Q_SLOT11_ROM                     15BEh B7h  0040h 0001h   0001h    Yes   No 
Q_SLOT12_ROM                     15BFh B7h  0080h 0001h   0001h    Yes   No 
Q_BMC_IRQ                        25C0h B8h  0003h 0003h   0003h    Yes   No 
Q_POWER_FAILURE_OPTION           25C2h B8h  000Ch 0000h   0000h    Yes   No 
Q_POST_ERROR_PAUSE               15C4h B8h  0010h 0001h   0001h    Yes   No 
Q_TEMP_SENSOR                    15C5h B8h  0020h 0000h   0000h    Yes   No 
Q_CLEAR_ALL_EVENT_LOG_ABS        15C6h B8h  0040h 0000h   0000h    Yes   No 
Q_MEMFAIL_CLR_ABS                15C7h B8h  0080h 0000h   0000h    Yes   No 
Q_FRB_RETESTCPU_ABS              15C8h B9h  0001h 0000h   0000h    Yes   No 
Q_SCAN_USER_FLASH_AREA           15C9h B9h  0002h 0000h   0000h    Yes   No 
Q_REMOTE_ESC                     15CAh B9h  0004h 0000h   0000h    Yes   No 
Q_REMOTE_F12                     15CBh B9h  0008h 0000h   0000h    Yes   No 
Q_INTEL_MEMORY_TEST_ENABLE       15CCh B9h  0010h 0000h   0000h    Yes   No 
Q_BACKGROUND_TEST                15CDh B9h  0020h 0000h   0000h    Yes   No 
Q_EXTMEMTEST_BUMP                25CEh B9h  00C0h 0003h   0003h    Yes   No 
Q_INTEL_INT15_BITS               85D0h BAh  00FFh 0080h   0083h    Yes   No 
Q_INTEL_MEMORY_REMAP_ENABLE      15D8h BBh  0001h 0000h   0000h    Yes   No 
Q_MEMFAIL_CLR                    15D9h BBh  0002h 0000h   0000h    Yes   No 
Q_DIMM0_Status                   15DAh BBh  0004h 0000h   0000h    Yes   No 
Q_DIMM1_Status                   15DBh BBh  0008h 0000h   0000h    Yes   No 
Q_DIMM2_Status                   15DCh BBh  0010h 0000h   0000h    Yes   No 
Q_DIMM3_Status                   15DDh BBh  0020h 0000h   0000h    Yes   No 
Q_PW_UNATTENDED_START            15DEh BBh  0040h 0000h   0000h    Yes   No 
Q_SECURE_MODE_HOTKEY             15DFh BBh  0080h 0000h   0000h    Yes   No 
Q_SECURE_MODE_TIMEOUT            35E0h BCh  0007h 0000h   0000h    Yes   No 
Q_POWER_SWITCH_INHIBIT           15E3h BCh  0008h 0000h   0000h    Yes   No 
Q_RESET_SWITCH_INHIBIT           15E4h BCh  0010h 0000h   0000h    Yes   No 
Q_NMI_SWITCH_INHIBIT             15E5h BCh  0020h 0000h   0000h    Yes   No 
Q_NMI_PERR                       15E6h BCh  0040h 0001h   0001h    Yes   No 
Q_NMI_SERR                       15E7h BCh  0080h 0001h   0001h    Yes   No 
Q_PEF_SETUP                      15E8h BDh  0001h 0001h   0001h    Yes   No 
Q_SYSMGMT_LAN_REDIR              15E9h BDh  0002h 0001h   0001h    Yes   No 
Q_SYSMGMT_LAN_ALERT              15EAh BDh  0004h 0000h   0000h    Yes   No 
Q_SYSMGMT_LAN_DEV                25EBh BDh  0018h 0001h   0001h    Yes   No 
Q_SYSMGMT_SERIAL_REDIR           15EDh BDh  0020h 0000h   0000h    Yes   No 
Q_SYSMGMT_SERIAL_PORT            25EEh BDh  00C0h 0001h   0001h    Yes   No 
Q_ABS_SYSMGMT_SERIAL_REDIR       25F0h BEh  0003h 0000h   0000h    Yes   No 
Q_SYSMGMT_SERIAL_RATE            35F2h BEh  001Ch 0002h   0002h    Yes   No 
Q_SYSMGMT_SERIAL_FLOW            25F5h BEh  0060h 0001h   0001h    Yes   No 
Q_SYSMGMT_SERIAL_RESET           15F7h BEh  0080h 0000h   0000h    Yes   No 
Q_SYSMGMT_SERIAL_TERM            25F8h BFh  0003h 0002h   0002h    Yes   No 
Q_SYSMGMT_CONTINUE_SERIAL_REDIR  25FAh BFh  000Ch 0002h   0002h    Yes   No 
Q_ACPI_OS_HEADLESS               25FCh BFh  0030h 0000h   0000h    Yes   No 
Q_SYSMGMT_SERIAL_ACPI_RATE       25FEh BFh  00C0h 0001h   0001h    Yes   No 
Q_SYSMGMT_SERIAL_ACPI_FLOW       2600h C0h  0003h 0001h   0001h    Yes   No 
Q_SYSMGMT_SERIAL_ACPI_TERM       2602h C0h  000Ch 0002h   0002h    Yes   No 
Q_FRB_RETESTCPU                  1604h C0h  0010h 0000h   0000h    Yes   No 
Q_FRB_EARLY                      3605h C0h  00E0h 0001h   0001h    Yes   No 
Q_INITIAL_BACK                   8608h C1h  00FFh 0000h   0000h    Yes   No 
Q_FRB_LATE                       3610h C2h  0007h 0000h   0000h    Yes   No 
Q_FRB_OS_HDD                     3613h C2h  0038h 0000h   0000h    Yes   No 
Q_FRB_OS_POLICY                  2616h C2h  00C0h 0000h   0000h    Yes   No 
Q_FRB_OS_PXE                     3618h C3h  0007h 0000h   0000h    Yes   No 
Q_CLEAR_ALL_EVENT_LOG            161Bh C3h  0008h 0000h   0000h    Yes   No 
Q_SMM_EN                         161Ch C3h  0010h 0001h   0001h    Yes   No 
Q_EVENT_LOGGING                  161Dh C3h  0020h 0001h   0001h    Yes   No 
Q_INTEL_BoardPartNumber          161Eh C3h  0040h 0000h   0000h    Yes   No 
Q_INTEL_BoardSerialNumber        161Fh C3h  0080h 0000h   0000h    Yes   No 
Q_INTEL_SystemPartNumber         1620h C4h  0001h 0000h   0000h    Yes   No 
Q_INTEL_SystemSerialNumber       1621h C4h  0002h 0000h   0000h    Yes   No 
Q_INTEL_ChassisPartNumber        1622h C4h  0004h 0000h   0000h    Yes   No 
Q_INTEL_ChassisSerialNumber      1623h C4h  0008h 0000h   0000h    Yes   No 
Q_INTEL_bmcDeviceID              1624h C4h  0010h 0000h   0000h    Yes   No 
Q_INTEL_bmcFirmwareRevision      1625h C4h  0020h 0000h   0000h    Yes   No 
Q_INTEL_bmcVersion               1626h C4h  0040h 0000h   0000h    Yes   No 
Q_INTEL_PIARevision              1627h C4h  0080h 0000h   0000h    Yes   No 
Q_INTEL_SDRRevision              1628h C5h  0001h 0000h   0000h    Yes   No 
Q_INTEL_fpcVersion               1629h C5h  0002h 0000h   0000h    Yes   No 
Q_INTEL_phscVersion              162Ah C5h  0004h 0000h   0000h    Yes   No 
Q_INTEL_shscVersion              162Bh C5h  0008h 0000h   0000h    Yes   No 
Q_INTEL_pscVersion               162Ch C5h  0010h 0000h   0000h    Yes   No 
Q_INTEL_hscVersion               162Dh C5h  0020h 0000h   0000h    Yes   No 
Q_COM_MODE                       262Eh C5h  00C0h 0000h   0000h    Yes   No 
Q_SP2_CTS_Setting                1630h C6h  0001h 0000h   0000h    Yes   No 
Q_SP2_DSR_Setting                1631h C6h  0002h 0000h   0000h    Yes   No 
Q_SP2_DCD_Setting                1632h C6h  0004h 0000h   0000h    Yes   No 
Q_SI1_RTS_Setting                1633h C6h  0008h 0000h   0000h    Yes   No 
Q_SI1_DTR_Setting                1634h C6h  0010h 0000h   0000h    Yes   No 
Q_SI2_RTS_Setting                1635h C6h  0020h 0000h   0000h    Yes   No 
Q_SI2_DTR_Setting                1636h C6h  0040h 0000h   0000h    Yes   No 
Q_SIM_TRI_State                  1637h C6h  0080h 0000h   0000h    Yes   No 
Q_COMA_SI2_PORT                  3638h C7h  0007h 0002h   0002h    Yes   No 
Q_Onboard_SCSI_Function_Mode     263Bh C7h  0018h 0001h   0001h    Yes   No 
Q_EUSB_TXCTRL                    263Dh C7h  0060h 0002h   0002h    Yes   No 
Q_DIMM4_Status                   163Fh C7h  0080h 0000h   0000h    Yes   No 
Q_USB2_AFE_Disconnect            2640h C8h  0003h 0002h   0002h    Yes   No 
Q_USB2_AFE_RCAL                  2642h C8h  000Ch 0002h   0002h    Yes   No 
Q_USB2_AFE_ICAL                  2644h C8h  0030h 0002h   0002h    Yes   No 
Q_DIMM5_Status                   1646h C8h  0040h 0000h   0000h    Yes   No 
Q_POWER_RESET_SWITCH_INHIBIT     1647h C8h  0080h 0000h   0000h    Yes   No 
Q_Slow_Edge_Rates_WA             1648h C9h  0001h 0001h   0001h    Yes   No 
Q_MCH_ERR_SMI                    1649h C9h  0002h 0000h   0000h    Yes   No 
Q_PXH_PCIXCAP_WA                 164Ah C9h  0004h 0000h   0000h    Yes   No 
Q_HW_MCH_ERR_SMI                 164Bh C9h  0008h 0000h   0000h    Yes   No 
Q_ABS_SYSMGMT_SERIAL_REDIR_mbmc  264Ch C9h  0030h 0000h   0000h    Yes   No 
Q_MCH_BSU_E66                    264Eh C9h  00C0h 0000h   0000h    Yes   No 
Q_SLOT3_SHOW_1_ROM               1650h CAh  0001h 0001h   0001h    Yes   No 
Q_Show_Mirror                    1651h CAh  0002h 0000h   0000h    Yes   No 
Q_PXH_PCI_Priority_Arb           1652h CAh  0004h 0000h   0000h    Yes   No 
Q_C1E_SUPPORT                    1653h CAh  0008h 0001h   0001h    Yes   No 
Q_PCI_MMIO_64                    1654h CAh  0010h 0000h   0000h    Yes   No 
Q_ABS_SERIAL_REDIR_BACKUP        2655h CAh  0060h 0000h   0000h    Yes   No 
Q_HYPER_MPS                      1657h CAh  0080h 0000h   0000h    Yes   No 
Q_SBE_DIMMS                      8658h CBh  00FFh 0000h   0000h    No    No 
Q_RAS_FEATURE_SUPPORTED          8660h CCh  00FFh 0000h   0000h    No    Yes
Q_CLEAR_ALL_EVENT_LOG_WHEN_FULL  1668h CDh  0001h 0000h   0000h    Yes   No 
Q_EVENT_TIMESTAMP                1669h CDh  0002h 0000h   0000h    Yes   No 
Q_USB_STOP_HISPEED_HC            166Ah CDh  0004h 0000h   0000h    Yes   No 
Q_Highest_MEM_Address            166Bh CDh  0008h 0000h   0000h    Yes   No 
Q_CPU_VT                         166Ch CDh  0010h 0001h   0001h    Yes   No 
Q_S5_Setup                       166Dh CDh  0020h 0000h   0000h    Yes   No 
Q_ACPI_IPMI                      166Eh CDh  0040h 0000h   0000h    Yes   No 
Q_USB_MASS_CHECKSUM              8670h CEh  00FFh 0000h   0000h    No    No 
Q_EXT_CMOS_PHY_LAYOUT0           8740h E8h  00FFh 0000h   0000h    No    Yes
Q_EXT_CMOS_PHY_LAYOUT1           8748h E9h  00FFh 0000h   0000h    No    Yes
Q_EXT_CMOS_PHY_LAYOUT2           8750h EAh  00FFh 0000h   0000h    No    Yes
Q_EXT_CMOS_PHY_LAYOUT3           8758h EBh  00FFh 0000h   0000h    No    Yes
Q_TYPEMATIC_RATE                 1760h ECh  0001h 0001h   0001h    Yes   No 
Q_PARITY_ERROR                   1761h ECh  0002h 0001h   0001h    Yes   No 
Q_OS2_COMP_MODE                  1762h ECh  0004h 0000h   0000h    Yes   No 
------------------------------------------------------------------------------

StorageType = ROM Tokens:

Q_TYPEMATIC_RATE                
Q_KEYBOARD_PRESENT              
Q_PARITY_ERROR                  
Q_OS2_COMP_MODE                 

------------------------------------------------------------------------------

String Tokens:

                                 CMOS CMOS
Question                         Reg. Bytes
-------------------------------------------
Q_SUPERVISOR_PASSWORD            83h  07
Q_USER_PASSWORD                  8Bh  07

------------------------------------------------------------------------------

CMOS addresses excluded from checksum:
2Eh 2Fh 33h 34h 35h 36h 3Ah 3Eh 3Fh 4Dh 4Eh 4Fh 50h 57h 58h 59h 5Ah 5Bh 5Ch 5Dh 
5Eh 5Fh 60h 61h 62h 63h 64h 65h 66h 67h 68h 69h 6Ah 6Bh 6Ch 6Dh 6Eh 6Fh 70h 71h 
72h 73h 74h 7Eh CBh CCh CEh CFh D0h D1h D2h D3h D4h D5h D6h D7h D8h D9h DAh DBh 
DCh DDh DEh DFh E0h E1h E2h E3h E4h E5h E6h E7h E8h E9h EAh EBh 

Last storage address used    = 0ECh

Last storage address in CMOS = 0ECh
Last storage address in ROM  = 0ECh


;*****************************************************************;
;*****************************************************************;
;**                                                             **;
;**      (C)Copyright 1985-2002, American Megatrends, Inc.      **;
;**                                                             **;
;**                     All Rights Reserved.                    **;
;**                                                             **;
;**           6145-F Northbelt Pkwy, Norcross, GA 30071         **;
;**                                                             **;
;**                     Phone (770)-246-8600                    **;
;**                                                             **;
;*****************************************************************;
;*****************************************************************;
