ServerConductor/Blade Server Manager Description and Reference

### Appendix B.2 System board

Alert ID | Level | Message | Action
--- | --- | --- | ---
0x0561 | Failure | An abnormal temperature was detected on the CPU in the CPU slot (<d>). | Remove dust from the system device's air vent to provide good ventilation. If the same event recurs with good ventilation, contact hardware support or the hardware vendor for the system device.
0x0562 | Caution | The CPU in the CPU slot (<d>) was degraded. | Contact hardware support or the hardware vendor for the system device.
0x0564 | Failure | An error occurred in the CPU in the CPU slot (<d>). | Contact hardware support or hardware vendor for the system device.
0x0569 | Warning | The temperature of the CPU in the CPU slot (<d>) exceeds the warning value. | Remove dust from the system device's air vent to provide good ventilation. If the same event recurs with good ventilation, contact hardware support or the hardware vendor for the system device.
0x0571 | Caution | Part of the installed memory has been started in a degraded state. | Contact hardware support or the hardware vendor for the system device.
0x0572 | Information | The amount of installed memory is different from the last time. | Check if the memory configuration was changed before the system device was started.
0x05B0 | Warning | An error occurred in the I2C bus. [args] | Contact hardware support or the hardware vendor for the system device.
0x0611 | Caution | A correctable memory error occurred. | Contact hardware support or the hardware vendor for the system device.
0x0612 | Failure | An uncorrectable multi-bit error occurred in memory. | Contact hardware support or the hardware vendor for the system device.
0x0613 | Failure | A processor configuration error was detected. | Contact hardware support or the hardware vendor for the system device.
0x0614 | Failure | A memory configuration error was detected. | Contact hardware support or the hardware vendor for the system device.
0x0615 | Failure | A memory module has been started in a degraded state. | Contact hardware support or the hardware vendor for the system device.
0x0616 | Warning | The memory chip has been changed. | No action is required.
0x0617 | Failure | The BMC detected an error. | Contact hardware support or the hardware vendor for the system device.
0x0618 | Warning | A chipset warning was detected. | Contact hardware support or the hardware vendor for the system device.
0x0619 | Failure | A chipset error was detected. | Contact hardware support or the hardware vendor for the system device.
0x061A | Failure | An error occurred in the PCI hot plug slot. | Contact hardware support or the hardware vendor for the system device.
0x061B | Warning | A warning occurred in the PCI hot plug slot. | Contact hardware support or the hardware vendor for the system device.

Legend:
  Information: Alerts that report changes in the server status.
  Caution: Alerts that indicate the possibility of an error.
  Warning: Alerts that indicate the possibility of a failure.
  Failure: Alerts that indicate the necessity of prompt action.

All Rights Reserved. Copyright (C) 2006, Hitachi, Ltd.