ServerConductor/Blade Server Manager Description and Reference

## 11.2 Console service settings

To change or view console service settings:

1. In the Host Management window, from the Setting menu, choose Console Service Setting.
   The Console Service setup dialog box appears:

In this dialog box, you can change or view console service information. To set information, you must have logged on as an administrator. A sub-administrator can only view the information.

For details about acquiring information in the Console Service setup dialog box, see 8.1 Acquiring maintenance information.

Organization of this section
  (1) Network

#### (1) Network

You can set the network information needed to communicate with the manager service.

On this tabbed page, you can set the following information:

Item | Setting
--- | ---
Settings for the Manager Service at the connection destination | Select the manager to which connection is to be made. You can select multiple managers. To register a new manager service at a connection destination or to delete an existing manager service, click the Register/Delete button.
Command timeout value | Set the wait time (in seconds) for a response to a transmission from the console service to manager service. The permitted value range is from 1 to 600. The default is 180 seconds.
Keep alive and its interval | Select this check box if the keep alive function is to be used during transfer operations with the manager service (the default is that this check box is not selected). When you check this box, also set a keep alive interval (in seconds). The permitted value range is from 1 to 3,600. The default is 600 seconds.

##### (a) Register or Delete Manager Service at Connection Destination dialog box

Choosing the Register/Delete button displays the Register or Delete Manager Service at Connection Destination dialog box.

In the Register or Delete Manager Service at Connection Destination dialog box, set the following information:

Item | Setting
--- | ---
Manager Service at connection destination (IP address/Host name) | Set the IP address or host name of the manager service to be connected. If the connection target is a network, specify the IP address or host name used by the source system from which connection is established.
Comments | Set any optional comment about the manager service at the connection destination (such as for identification purposes).
List of registered Manager Services | Clicking the Add to List button registers the manager service at the connection destination in the list. You can register a maximum of 128 manager services. To delete a manager service from the list, select it, and then click the Delete button. When connection is to be established with multiple manager services, connection attempts are made sequentially from the top of this list. To change the priority for establishing connection among multiple managers, select a manager and change its location in the list by pressing the Up and Down buttons.

All Rights Reserved. Copyright (C) 2006, Hitachi, Ltd.