ServerConductor/Blade Server Manager Description and Reference

### Appendix A.3 Network (KASM4nnnn)

Message ID | Message text | Action
--- | --- | ---
KASM42104 | The maximum number of creatable sockets has been reached. Release some connections, and then try again. | Release some of the connections, and then re-execute.
KASM42106 | A connection cannot be established. (connection error) | The connection target may not be active. Make sure that the connection target has started.
KASM42107 | A packet cannot be sent. | Data cannot be transmitted for reasons such as a busy line. Re-execute after a while.
KASM43102 | The specified address is invalid. | Start the environment settings utility, check the connection-target address or host name, and then restart the service.
KASM43201 | A send command timeout was detected. | There is no response to the request. Processing may be too slow at the connection destination. Use the environment settings utility to set a large command timeout value.

All Rights Reserved. Copyright (C) 2006, Hitachi, Ltd.