ServerConductor/Blade Server Manager Description and Reference

### Appendix B.1 Casing and power

Alert ID | Level | Message | Action
--- | --- | --- | ---
0x0501 | Warning | The temperature (<d>) in the frame exceeds the warning value. | Remove dust from the system device's air vent to provide good ventilation. If the same event recurs with good ventilation, contact hardware support or the hardware vendor for the system device.
0x0501 | Warning | The temperature (<d>) in the frame exceeds the warning value. [args] | Remove dust from the system device's air vent to provide good ventilation. If the same event recurs with good ventilation, contact hardware support or the hardware vendor for the system device.
0x0502 | Failure | The temperature (<d>) in the frame has risen to an excessively high level. | Remove dust from the system device's air vent to provide good ventilation. If the same event recurs with good ventilation, contact hardware support or the hardware vendor for the system device.
0x0520 | Warning | The voltage (<d>) on the package has risen above the standard value. | Contact hardware support or the hardware vendor for the system device.
0x0520 | Warning | The voltage (<d>) on the package has risen above the standard value. [args] | Contact hardware support or the hardware vendor for the system device.
0x0521 | Warning | The voltage (<d>) on the package has fallen below the standard value. | Contact hardware support or the hardware vendor for the system device.
0x0521 | Warning | The voltage (<d>) on the package has fallen below the standard value. [args] | Contact hardware support or the hardware vendor for the system device.
0x0530 | Warning | An error occurred in the power unit (<d>). | Contact hardware support or the hardware vendor for the system device.
0x0533 | Caution | The temperature of the air intake into the frame has risen above the standard value. | Contact hardware support or the hardware vendor for the system device.
0x0534 | Caution | The temperature of the air intake into the frame has fallen below the standard value. | Contact hardware support or the hardware vendor for the system device.
0x0536 | Failure | The temperature of the air intake into the frame has risen to an excessively high level. | Contact hardware support or the hardware vendor for the system device.
0x0537 | Failure | An error occurred in the voltage (<d>) on the package. | Contact hardware support or the hardware vendor for the system device.
0x0601 | Failure | The rotational speed of the frame fan <d> is below the standard value. | Contact hardware support or the hardware vendor for the system device.
0x0602 | Failure | A device configuration error was detected. | Contact hardware support or the hardware vendor for the system device.
0x0603 | Warning | The number of fan units is insufficient. | Contact hardware support or the hardware vendor for the system device.

Legend:
  Caution: Alerts that indicate the possibility of an error.
  Warning: Alerts that indicate the possibility of a failure.
  Failure: Alerts that indicate the necessity of prompt action.

All Rights Reserved. Copyright (C) 2006, Hitachi, Ltd.