This release note and the software that accompanies it are copyright (c) 2007, Intel Corporation, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported Storage Systems
==========================
This download supports Intel(R) Storage Server SSR212MC2BR and SSR212MC2RBR

===================
Package Information
===================
version = 3.07.0012
OS supported = Windows* Server 2003, Windows Storage Server 2003-R2, Windows Unified Data Storage Server 2003-R2
This package can be installed on all x86 systems.

=========
Attention
=========
Added/Changed in this release:
N/A

Any source code remains the property of Xyratex* and may only be used within the terms of the license agreement

==================
Known Restrictions
==================
Requires Java* Runtime Environment 1.5 or higher and a web browser.

SSR212MC2R Requires Intel(R) RAID controller SRCSAS144E firmware version 1.03.00-0211 or later.

If you are using Windows* disable/remove Internet Explorer Enhanced Security options (see add/remove programs, windows features)


=======================
Contents of the package
=======================
storview-3.07.0012-jbi-win-en.exe


=========================
Installation Instructions
=========================
StorView is developed for 32 bit environment and works on 64 bit OS in emulation mode. For usage and installation steps please refer to the product's Software User Guide.


Summary of Installation Steps:

1. Download the StorView* self extracting installer

2. Run the installer and select all default options  

3. A shortcut will be set up under the Start button -> All Programs


===========================
Uninstallation Instructions
===========================
The product can be uninstalled using Add/Remove Programs opton in Control Panel.


============
New Features
============
N/A


========================================
Known Issues/Limitations in this version
========================================
1) When using multiple ethernet connections, Storview connects via only one of these. If you disconnect the main cable you must then restart storview on the enclosure having first shut down the 2 storview services.
If this port is disabled (through the system OS) or disconnected, Storview will not be able to start. The error message “Could not connect to service on 127.0.0.1, please ensure that the service is running and try it again" will be displayed.  
Note: if you disable the port through Storview, then Storview will be closed. 

2) SSR212MC2R only - RAID card firmware can occasionally override user settings for drive LEDs. If you use storview to turn drive ident lights on and remove/replace a drive, RAID card can override your ident lights and may turn them off.

3) RAID card firmware can add warnings to the windows/linux event logs about temperature differentials. These messages are erroneous and can be ignored safely.

4) Removing one fan causes all fans to go to 100%. This is a design requirement for failure cases and is correct behaviour.

5) Enclosure firmware upgrade is not supported if an external storage expansion unit is connected to the Intel SRCSAS144e RAID card.

6) Inserting a second (redundant) PSU with no live AC attached has the PSU reported as OK rather than AC Power fault.

7) Direct access to enclosure information via other methods such as IPMI is not supported and may cause system failure. Only SES is supported.

8) Virtual disk may go offline and all the disks of the enclosure may go unconfig-bad after the upgarde of RAID card firmware if I/O is present.

9) Flashing of all disk drive ident LEDs are turned off if a disk is removed. 


=============================
Fixes/Updates in this version
=============================
Fixed: Chassis ident light is too dim to see

Fixed: Raw view decode misses of new vendor unique T10 in page 1 SES

Fixed: StorView displays incorerctly for Power Supplies when one is removed. 

Fixed: raw view p2 does not decode PSu at all or other elements fully

Fixed: Storview settings should not show RAID function/option

Fixed: A Java Swing exception occurred while pulling drives from an enclosure. 

Fixed: Missing drives were shown as present when drives were pulled out of the enclosure. The enclosure was also shown as having an erroneous fault.  

Fixed: login problems after changing the servername in Rhel4

Fixed: System setttings shows raid created on the controller SRCSAS144E. System settings must show only system drives and not the VD on the raid controller.




*Third-party trademarks are the property of their respective owners.



