This release note and the software that accompanies it are copyright (c) 2007, Intel Corporation, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported RAID Controllers
==========================
This package contains the firmware update file for the SRCS16 controller and is not designed for use with any other controller. Please verify that this firmware has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at http://Support.Intel.Com.

===================
Package Information
===================
Version = 713S

=========
Attention
=========
Application of this firmware file requires the use of the irflash utility.  

========
Contents
========
The following files are included in this zip:
Name			Description
713S.rom		firmware binary
FW713S_readme.txt	This file
Web License		License Agreement

==========================
Installation instructions:
==========================
This update can be applied using the irflash utility available for DOS, Windows, Linux, or Netware.
1. Download and extract the irflash utility for your Operating system to a local drive.
2. Download and extract the firmware file to a local drive.
3. Boot the target system to the target OS or EFI shell.  For the purposes of this instruction, DOS will be assumed.  Consult the readme file for the version of irflash you have chosen to use.
4. Change directory to the local drive and directory containing both the irflash utility and the firmware image file.
5. Type "irflash /p"
6. When prompted for the name of the firmware binary file enter the name of the file (713S.rom) and press enter.
7. When prompted, confirm the update.

Help can be obtained with the command "irflash /?"
Multiple controllers installed in the same system can be updated one after the other by following the prompts that are presented.

=============
Fixes/Updates
=============
713N - Incorporated BIOS look and feel changes.
713Q - I2C command timeout cause BSOD and an "MRAID" device timout in the system event log.  Two commands (one via IOCTL) were going to the SAF-TE on the i2c bus resulting in an i2c bus hang.  If the DCDB to the SAFTE with timeout value greater than "I2C_TIMEOUT_BIG_DEFAULT", then I2C_TIMEOUT_BIG_DEFAULT timeout value is used.
713R - Fixes and updates:
1. Fixed the cache line reassignment for XOR of RMW(WB) operation.
2. Fixed Bluescreen and/or Controller hang when Patrol Read finds a media error on Raid 5 in a second span under certain caching configurations.
3. Fixed Controller hang when command ID was used previously as "LOCAL COMMAND" and reused by normal cmdType.
4. Fixed issue with timer function, Declared num_timer_reqs as volatile.
5. Fixed issue supporting a system with more than 4GB memory. 
713S - Fixes and updates:
1. Added the Support  for Vitesse 410 based Intel SAFTE backplanes
2. Fixed Stop error when reboot the system after performing hot rebuild

*Third-party trademarks are the property of their respective owners.


