
Firmware and BIOS Update Package for the Intel(R) Server Board S3200SH, S3210SH
    Intel Corporation 2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA

BIOS: S3200X38.86B.00.00.0033  Build Date :  Nov. 21, 2007
BMC: 	25  (Requires v24 be installed before update)
FRUSDR: FSH1_08

!!Hot swap backplanes (HSC) are not supported at this time.
!!!BIOS must be at R0020 and iBMC FW at v.24 before running this update.

This package may be used with:
 - Intel(R) Deployment Assistant 1.4 (on the CD or from support.intel.com)
 - Intel(R) One-boot Flash Update (OFU) v9.62 or later (support.intel.com)
 - the embedded EFI environment (see EFI.txt) or
 - Windows Preboot Execution Environment (WinPE) - availabe in WinPE folder.

=
Processor supported: 
Conroe    	  A-1,B-2,G-2,L-2, M-0; Conroe-L      A-1
Conroe XE         B-2 ;                 Conroe Xeon   B-2,L-2
Kentsfield/XE/XEON  B-3                 Kentsfield    G-0
Wolfdale          A-1,B-1,C-0           Yorkfield   A-1,B-1,C-0,L-0,M-0

Microcode update versions:
CPUID   Microcode       CPUID   Microcode
06F2h       56h        10671h	   106h
06F6h       C6h        10674h	   404h
06F7h       66h        10676h      606h
06FBh	    B6h        10661h       32h
06FDh	    A1h

Intel (R) Matrix Storage OpROM: v7.5.0.1017 
LSI OpRom:              version 10101641
SATA AHCI BIOS:     Release Date 01-05-2007
NIC : Intel (R) Boot Agent       GE v1.2.60
VGA:                    VBE BIOS V3.8SL
Memory Reference Code 1.00

REVISION INFORMATION RETURNED BY GET DEVICE ID COMMAND:
Operational mode:	v00.25
UBoot mode:		v01.09
Device ID:		0x21 (IBMC 2K7 Firmware)
Manufacturer ID:	0x000157 (Intel Corporation)
Product ID:		0x003A (S3210SH)
Checksum information:     UBoot                 hex
  Region:	0x0000000 - 0x0040000	  0x0000000 - 0x0400000
  MD5: 0x334db8d53f61d67b8dbf52bca4f60ad1 0xfe84e4d587f03960b629c31f025c1f13

Changes:
BIOS Added Wolfdale/Yorkfield support
BMC 25 Fixed: SOL data corruption; close session failure; IERR for sn#OF
FRUSDR:Added FSC records so unused PWMs run at 100%
       Fixed: System Fan3 & Fan4 test failed in BMC Module test
              Fan Speed control 
              Incorrect value of BB Ambient Temp (ipmitool)  

LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2007 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  