================================================================================
Multi-Core Intel(R) Xeon(R) Processor-Based Server BIOS Development
================================================================================
INTEL Enterprise Products and Services Division
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : November 29, 2007
TO      : Multi-Core Intel(R) Xeon(R) Processor-Based Server Platform customers
SUBJECT : BIOS Release notes for version R0085
================================================================================
                           LEGAL INFORMATION
================================================================================

Information in this document is provided in connection with Intel Products
and for the purpose of supporting Intel developed server boards and systems.
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation 
may have patents or pending patent applications, trademarks, copyrights, or
other intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any such
patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 

*Other names and brands are the property of their respective owners.

Copyright (C) 2007 Intel Corporation.

================================================================================
                              ABOUT THIS RELEASE
================================================================================
Build Stamp : S5000.86B.10.00.0085.11292007
Build Date  : November 29, 2007

================================================================================
                           BIOS COMPONENTS/CONTENTS
================================================================================
Processors supported: 
  Dual-Core Intel(R) Xeon(R) Processor 5000 series w/ 533Mhz/667Mhz/1066Mhz FSB
  Dual-Core Intel(R) Xeon(R) Processor 5100 series w/ 1066Mhz/1333Mhz FSB
  Dual-Core Intel(R) Xeon(R) Processor 5200 series w/ 1066Mhz/1333Mhz FSB
  Quad-Core Intel(R) Xeon(R) Processor 5300 series w/ 1066Mhz/1333Mhz FSB
  Quad-Core Intel(R) Xeon(R) Processor 5400 series w/ 1066Mhz/1333Mhz FSB

Microcode update versions:
CPUID   Version Status  
0F64h   02      Production
0F65h   08      Production
06F6h   C9      Production 
06F7h   67      Production 
06FBh   B4      Production 
10676   606     Production


On-Board Component Option ROM Versions:
ATI RN50 VGA    	: BK-ATI YJ20234a VER008.005.023.000
				 YJ18794g (S5000PAL, S5000XAL, S5000PHB)
PXE Ver.        	: Intel(R) Boot Agent GE v1.2.45
ESB2 Option ROM 	: vA.01.07101204I
ESB2 AHCI Option ROM	: iSrc 1.08 09252006

Memory Reference Code Version:  1.32

================================================================================
                       SYSTEM FIRMWARE REQUIREMENTS
================================================================================
BIOS Update Utility: 
IFLASH32 VERSION 1.5.1 Build 7 

Beta/Silver/Gold boards:
  Product		Fab Version		BMC	FRUDSR	EEPROM	HSC 
  S5000PAL, S5000XAL ->	Fabk8->Fab5, Fab4+rwk	62	FAL_46	v03.01	v2.05
  S5000PSL, S5000XSL ->	Fab8->Fab4, Fab3+rwk	62	FSL_45	v03.01	V2.05
  S5000VSA	     ->	Fab7->Fab4		62	FSP_41	v03.01	v2.05
  S5000XVN	     ->	Fab8->Fab4		62	FSL_45	v03.01	V2.05
  SC5400RA	     ->	Fab3, Fab2		62	FSL_45	v03.01	V2.05
  S5000VCL	     ->	Fab6->Fab2		62	FCL_17	v03.01	V2.05

================================================================================
                           INSTALLATION NOTES
================================================================================

WARNING:  It is very important to follow these instructions as they are written.
Failure to update using the proper procedure may cause damage to your system.

Update BIOS using bootable USB Flash Drive:

Updating from BIOS revisions R0038 or earlier:
NOTE:  This operation will update both banks of the flash part.  This is necessary
as the Setup options from R0038 and earlier are not compatible with R0039 and later.

NOTE:  BIOS Bank Select jumper needs for be in Normal mode (2-3) during this whole
procedure.

1)  Download release package and extract contents to USB Flash Drive
2)  Verify that the R0085.CAP, BIOS85.BAT and IFLASH32.EXE files are present
    on the USB Flash drive
3)  Verify that BIOS Bank Select Jumper is set to Normal mode (2-3).
4)  Power system on and boot to USB Flash Drive
5)  At the command prompt type "BIOS85".
6)  Flash update should complete within 3 minutes
7)  Shut down the system but leave it connected to AC power
8)  Clear CMOS by moving the Clear CMOS jumper to the clear position and back.
9)  Boot system and enter BIOS Setup by pressing the F2 Key during POST
10) Verify BIOS string
11) Press F9 to load defaults
12) Press F10 to save and reset the system.
13) Power system on and boot to USB Flash Drive
14) At the command prompt type "BIOS85".
15) Flash update should complete within 3 minutes
16) Reboot system and enter BIOS Setup by pressing the F2 Key during POST
17) Verify BIOS string
 

Updating from BIOS revisions R0039 or later:
NOTE:  This operation will only update one bank in the flash part.  This is
recommended in case of a flash update failure that the system can be easily
recovered.

NOTE:  BIOS Bank Select jumper needs for be in Normal mode (2-3) during this
whole procedure.

1) Download release package and extract contents to USB Flash Drive
2) Verify that the R0085.CAP, BIOS85.BAT and IFLASH32.EXE files are present
   on the USB Flash drive
3) Verify that BIOS Bank Select jumper is set to Normal mode (2-3).
4) Power system on and boot to USB Flash Drive
5) At the command prompt type "BIOS85".
6) Flash update should complete within 3 minutes
7) Reboot system and enter BIOS Setup by pressing the F2 Key during POST
8) Verify BIOS string


================================================================================
                        BIOS RECOVERY INSTRUCTIONS
================================================================================

BIOS Recovery is not supported. 

Rolling BIOS is supported.

================================================================================
                            KNOWN ISSUES/WORKAROUNDS
================================================================================

-Video mode is set to 80x25 until BIOS defaults are loaded

-PAE mode and the equivalent Linux mode must be set to see > 2.5GB of memory.

NOTE:  Dual-Core Intel(R) Xeon(R) Processor 5100 series DO NOT support Hyper-Threading.
       The OS will only show 2 CPU threads per physical processor installed.
       Quad-Core Intel(R) Xeon(R) Processor 5300 series DO NOT support Hyper-Threading.
       The OS will only show 4 CPU threads per physical processor installed.
NOTE:  BIOS Setup shows the number of physical processors installed and not the
       number of processor cores. For example, when 2 Dual-Core Intel(R) Xeon(R)
       Processor 5100 series are installed, BIOS POST and Setup will only show 2 processors. 

-THIS BIOS ONLY SUPPORTS BETA OR LATER HARDWARE.
 DO NOT APPLY THIS BIOS TO ALPHA HARDWARE.

-IF CMOS IS CLEARED, IT MUST BE CLEARED PER THE INSTALLATION INSTRUCTIONS.

-When two Dual-Core Intel(R) Xeon(R) 5100 series processors are installed,
 an NMI error may appear during POST after updating from BIOS R0054 or earlier
 to BIOS releases after R0054.  This is expected and due to a change in the way
 errors are handled in the newer BIOS release. Perform a full DC power cycle
 (front panel power off and power on) to prevent this message from appearing again.

-As of BIOS R0063, may encounter a system reset upon first boot if previous
 NVRAM corruption has been found.

-As of BIOS R0077, Case Sensitivity support has been added to BIOS Admin/User password.
 If a password was installed using previous BIOS release without Case Sensitivity,
 enter old password in all lower case and then re-install password for proper Case Sensitivity.


================================================================================
                              FEATURES ADDED/REMOVED
================================================================================
-As of BIOS R0052, DIMMs with outdated AMB (Advanced Memory Buffer) component
 present are no longer supported. The system will halt with 3 beeps at POST code
 0xEA to indicate an "Unsupported AMB" error.

-As of BIOS R0056, removed support for Pre-production CPU steppings of the
 Dual-Core Intel(R) Xeon(R) Processor 5000 series.
 This includes processors with CPUID 0F61h, 0F62h, 0F63h.

-As of BIOS R0079, removed support for Pre-production CPU steppings of the
 Dual-Core Intel(R) Xeon(R) Processor 5100 series and Quad-Core Intel(R) Xeon(R)
 Processor 5300 series.
 This includes processors with CPUID 06F4h, 06F5h.

-As of BIOS R0081, removed support for Pre-production CPU steppings of the
 Dual-Core Intel(R) Xeon(R) Processor 5100 series and Quad-Core Intel(R) Xeon(R)
 Processor 5300 series.
 This includes processors with CPUID 06F9h.


================================================================================
                              FIXED ISSUES
================================================================================
================================================================================
                                R0085
================================================================================
S5000PAL, S5000XAL:
127782  [x] Disabling NIC opROM and I/O Module opROM disabled console redirection
127822  D1 AMB DIMM component errata must have BIOS MRC workaround
127783  Need to remove SAS SWRAID on MP2 (w/1078 chip)

S5000VSA, S5000PSL, S5000XSL, S5000XVN, SC5400RA, S5000VCL:
32482 	After offline programming R0084, boot bank is not consistant
32371   Processor Cache Size Mismatch Error 192 has typo
31807   BIOS Setup needs to remove/add SATA Port information
30289   Fix 2 blinking cursors when entering setup under quiet boot
31826   Video loss when Serial B is disabled but enabled for console redirection
32403   There is an unknown device under Windows2000+SP4
32307   USB mouse and keyboard detected if USB is <Disabled>

  
OTHER:
  -     Performance anomolies in slot4 with Springports and EIRQ enabled
  -     Northbridge shutting down PCIe link with plx device 8533 installed
  -     Trouble entering opROMs that trap int 19
  -     Genuine M15ERR (Accompanied by M13ERR) should have SEL log
  -     Support for Refresh-2 Board
  -     Use HECBASE to determine PCIE Base Addrs (Fix IBIST errors)
  -     Update Memory Reference code to 1.32
  -     Enable Video controller
  -     CSM Payload changes
================================================================================
                                R0084
================================================================================
32340 	System will not boot with max memory (8x  4gig DIMMs- 32gigs)  

================================================================================
                                R0083
================================================================================
S5000PAL, S5000XAL:

S5000VSA, S5000PSL, S5000XSL, S5000XVN, SC5400RA, S5000VCL:
31123   [X] Problem with PXE Boot with on-board NIC 
32181   [X] Impossible to boot to any boot device with SRCS28X installed
32282   MTRR configuration issue with G-0 processors
31248   TPM not functional on refresh SKU
32207   CLLT configuration reverting back to OLTT after Cntl+Alt+Del

S5000PHB, T5000PAL:
32020   HW RAID configuration not foound after reboot
32192   DMIEDIT failure
  -     MP Table Update

OTHER:
    -	Overheating DIMMs in CLTT
    -   AMIBCP Boot Order Support

================================================================================
                                R0082
================================================================================
S5000PAL, S5000XAL:
127771  Rollback to OLTT does not happen with CLTT incapable DIMM
127774  [X] want to boot PATA above SATA

S5000VSA, S5000PSL, S5000XSL, S5000XVN, SC5400RA, S5000VCL:
30549   Unable to boot to full Linux kernel through Linux payload
31426   GBE can not be detected and trasfer data under DOS 7.0 (NICs fail in DOS)
31818   Duplicate devices in Boot Order after CMOS clear
31701   VMWare 3.0.2 ESX kernel panic during installation

S5000PHB, T5000PAL:
28696   Green status LED driven active in standby (DC Off)
30297   Legacy IRQ routing
31538   Add support for refresh

OTHER:
    -	Add back Altitude Bios Setup Option when OLTT selected
    -   Deep C-State support causes W2K3 without service pack to fail
    -   Add Windows Hardware Error Architecture (WHEA) support
    -   Update Memory Reference code to 1.30
    -   Add Half Ratio support for the processor
    -	Add 10676h C-0 processor microcode patch for DP

================================================================================
                                R0081
================================================================================
S5000PAL, S5000XAL:
172022	EFI shell environment variables running out of buffer space
172178  POST screen shows 2 garbage lines in BMC Forced Update Mode

S5000VSA, S5000PSL, S5000XSL, S5000XVN, SC5400RA, S5000VCL:
30300   [X] Addonics SATA CF Card Reader not recognized by BIOS
30272   S5000XVN reboots instead of resumes from S4
30779   [X] Matrox DSX.io and X.effects card not detected
30558   [X] PME Signal waking up system
30765   BIOS hangs when there is no boot targets available on the system
29228   WHQL UAA test fails in Vista 64bit on S5000XVN
31123   [X] Problem with PXE Boot with on-board NIC in BIOS R0078
31379   W2K8 blue screens during install
31559   Some SATA drives not detected on cold boot


S5000PHB, T5000PAL:
127755  BMC Force Update Mode Does not enter BIOS Setup
127757  [X] SLES10 w/SP1 failed to boot w/PCIE HCA installed
127767  Fail to install WIN 2KADV Server w/SP1 


OTHER:
    -	BIOS String Update "Add new CC3 requirements"
    -   Errata 100: ESB2 PCIe switch mis-formats TLPs
    -   MP Routing/Table Fixes
    -   Fix video corruption on Main tab in BIOS Setup w/console redir enabled
    -   Fix Unrecoverable Error Handling problems
    -   Fix kernel panic in Linux with throttled processors
    -   Loading user defaults loads invalid option on the boot order page
    -   Fixed garbled text in BIOS Setup at 115K baud w/console redir
    -   Workaround for DTX PCI-X add-in card blue screen failure.
    -   TPM Status appears in BIOS Setup on boards without TPM.
    -   Update ESB2 RAID OpRom to vA.01.07101204I
    -   Enable fake MSI for S5000PSL Slot4
    -   Add support of depop SKU based off of S5000PSL
    -   WHQL test failure on I/O Port 161 and 162
    -	Add 06F6h B-2 processor microcode patch M046F6C9 for the Dual-Core
    -	Add 06F7h B-3 processor microcode patch M406F767 for the Quad-Core
    -   Allow B-step/G-step mixed stepping for 5100 and 5300 series processors


[END OF RELEASE NOTES]
