================================================================================
Intel(R) Server Board S3200SH/S3210SH System software Update Package for 
Intel(R) Deployment Assistant, Intel(R)One Boot Flash Update Utility, 
The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation 2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================

BIOS: S3200X38.86B.00.00.0042  Build Date :  April 28th, 2008
Integrated BMC: 29  (Requires v24 be installed before update)
FRUSDR: FSH1_12

This package may be used with:
 - Intel(R) Deployment Assistant 1.4 (on the CD or from support.intel.com)
 - Intel(R) One-boot Flash Update (OFU) v9.62 or later (support.intel.com)
 - the embedded EFI environment 
 - Windows Preboot Execution Environment (WinPE) 
================================================================================
                           SUPPORTED PLATFORMS and Dependency
================================================================================
Intel(R) Server Board S3200SH/S3210SH
Processor supported: 
Quad-Core Intel(R) Xeon(R) Processor 3300 Series
Dual-Core Intel(R) Xeon(R) Processor 3200 Series
Quad-Core Intel(R) Xeon(R) Processor 3100 Series
Dual-Core Intel(R) Xeon(R) Processor 3000 Series
Intel(R) Core(TM) 2 Quad Desktop processors
Intel(R) Core(TM) 2 Duo Desktop processors
Intel(R) Core(TM) 2 Extreme processors

Microcode update versions:

CPUID   Microcode   
06F2h       5Ah
06F6h       CBh
06F7h       68h
06FBh	    B6h
06FDh	    A3h
10661h      38h
10671h	    106h
10674h	    404h
10676h      60Bh
10677h      703h  

Intel (R) Matrix Storage OpROM: v7.5.0.1017 
LSI OpRom:              version 10101641
SATA AHCI BIOS:     Release Date 01-05-2007
NIC : Intel (R) Boot Agent       GE v1.2.60
VGA: VBE BIOS V3.8SL
Memory Reference Code 1.00

REVISION INFORMATION RETURNED BY GET DEVICE ID COMMAND:
Operational mode:	v00.29
UBoot mode:		v01.09
Device ID:		0x21 (Integrated BMC 2K7 Firmware)
Manufacturer ID:	0x000157 (Intel Corporation)
Product ID:		0x003A (S3210SH)
Checksum information:     UBoot                 hex
  Region:	0x0000000 - 0x0040000	  0x0000000 - 0x0400000
  MD5: 0x2b055709d138fd9a2c02ee6593c8b091 0x88db6f644c5f32b4aff11e48bfaf0a68 

Dependency
BIOS must be at R0020 and Integrated BMC FW at v.24 before running this update.
================================================================================
                  System Firmware Update Package Usage Model                   
================================================================================
Intel(R) Deployment Assistant (IDA)

User can use IDA CD to update system firmware with below steps
- Boot server with IDA CD
- Select " Get System Updates " Button at IDA home page
- IDA has three options to get system firmware update package

  . From support.intel.com
    IDA can automatically download system firmware update package from Intel
    supporting web site. 
    Server should have valid Internect conncetion. User can follow the indication
    on IDA GUI to enter local server IP setting and Internect proxy configuration;
    Select "Next" button to start firmware download and update process
    
  . From my network
    IDA can get system firmware update package from a Windows* share folder on LAN.
    User need to download firmware update package from support.intel.com web site
    and copy to a Windows* share folder first;
    Follow the indication on IDA GUI to enter local server IP setting / 
    Windows* file server name / Windows* account name and its password;
    Find the firmware update package in the Windows* share folder from 
    a IDA pop-up window;
    Select "Next" button to start firmware update process
          
  . From USB Disk on key or Hard Disk
    IDA can get system firmware update package from USB storage also.
    User need to download firmware update package from support.intel.com web site
    and copy it to a USB key and insert into server USB port;
    Select option "From USB disk on key or hard disk" and select "Browse" button;
    Select firmware update package ZIP file in a IDA pop-up window;
    Select "Next" to start firmware updating
    
 Note: system firmware update package is .ZIP file format, it doesn't need to
       unzip, directly copy the .ZIP to Windows* share folder or USB disk


Intel(R) One Boot Flash Update Utility

The Intel(R)One-Boot Flash Update Utility (Intel OFU) is used to update the BIOS 
and firmware on the Intel server boards while the operating system is running. 
The utility may be launched from a command prompt in either the Windows*
or Linux* Operating Systems.
User can get Intel OFU from Server system IDA CD or from support.intel.com web site
Please refer Intel OFU user guide about the details of intatllation and usage of OFU

User can use OFU to update system firmware with below steps
- Install OFU on Windows* or Linux* system
- Download Intel server system firmware update package from support.intel.com 
- Unzip package and copy all files to a folder in Windows* or Linux* system
- Run below command in Windows* connamd line window or Linux* terminal windows 
  <OFU install folder name>:\ flashupdt -u  <package folder name>\flashupdt.cfg
  to start firmware update process

                       
EFI Shell

User can update system firmware from Intel server EFI shell with below
steps
- Download Intel server system firmware update package from support.intel.com
- Unzip package and copy all files to a folder in a USB disk key 
- Insert USB disk key to server USB port
- Reboot server to EFI shell
- Run command " map -r " at EFI shell to mount USB disk key
- Run command " fs0:" to change folder to USB disk key, USB key may also mount to
  fs1:. The number of "fs" is dependent on the result of command "map -r"
- Change folder to the folder that store the firmware package
- Run command " startup.nsh " to start firmware update process

Please refer " EFI_deployment.pdf" in this firmware package for the details of 
EFI commands


Windows* Preboot Execution Environment (WinPE)

This Intel server system firmware package can be inserted to Windows* PE customized
image and create a bootable Windows* PE CD. 
User can update system firmware from WinPE CD with below steps
- Boot server with customized WinPE CD
- Run script "WinPE_Update.bat" in this firmware package in customzied WinPE CD 
  to start firmware update process
  
Please refer white paper "WinPE1x_Whitepaper.pdf" in this firmware package for 
detailed steps of building customized WinPE CD   

================================================================================
                              Changes since release
================================================================================
BIOS 
Added: 
      - SLP2.0 support
      - Added Multithreads entry into the MPS table
      - MicroCode update for C1 Stepping processors
      - Optimization for MCH VREF,RCOMP,GTLREF
      - Set the ICH_RCRB_HPTC_AE bit to enable the ACPI HPET table. 
      
Fixed: 
      - BIOS always display HSC version as 0.00
      - Show kernel panic message when install RHEL5U1.
      - Keep boot order when SATA mode change between IDE and RAID
      - Fixed S32000SH/S3210SH UUID empty issue 
      - Fixed the issue of wrong BIOS version when console redirection 
        is enabled
      - Fixed the issue of USB port 5 can't detect the USB1.1 decvice 
        in DOS or EFI shell

BMC 
Added: 
      - Support for Hot Swap Backplane (HSBP)
Fixed: 
      - Post LEDs keep on after POST finished
      - SOL data corruption occurs at 9600, 19200, 38400 baud rate 

FRUSDR
Added: 
      - HSC-related sensor data records
      - Message when detecting HSC for notification of possible long delay
       
Fixed: 
      - Removed possible long delay when checking for HSC
      - FRUSDR.EFI's PROBE "PING" command does not work with HSC
      - Add HSBP support  
=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2007 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]