This release note and the software that accompanies it are copyright (c) 2008, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported RAID Controllers
==========================
This download supports Intel(R) RAID controllers using software stack 2 (SROMBU42E, SRCU42X, SRCU42E, SRCU41L, SRCS16, SRCS28X, & SRCZCRX), please verify that this utility has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at //Support.Intel.Com.
	
================
Package Information
================
Version = 2.03-00  
OS supported = Windows* 2003, Windows 2000, Windows XP

====================
Attention!
====================
This flash utility is a Windows based utility that allows you to update RAID controller firmware.  
This package contains the Windows version of the firmware update (flash) utilityand does not include the RAID controller Firmware. This utility is designed for use with the firmware update file which must be downloaded seperately.

================
Known Restrictions
================
This utility is not compatible with the SRCU21, SRCU31, SRCU31L, SRCMR, SRCZCR, SRCU32, SRCU42L, or SRCS14L RAID controllers.
1.	Image files should be present in the current directory except for GUI mode and for /p and /f option.
2.	Only maximum of 3 files can be specified in ignore(/i) and force(/f) file option.
3.	Only maximum of 10 compatible files will be detected from current directory.

====================
Contents on the package
====================
The following files are included in this package:

Name			Description
irflshw.exe		FLash Utility
FlashGUI.dll		DLL file
Web Licence.rtf		License
irflsh_win_readme.txt	This file

==================
Installation Instructions
==================
Note: A firmware update cannot be performed when a logical drive initialization or rebuild is in progress, please wait until the initialization or rebuils is complete before attempting a firmware update.  Backup all data prior to the firmware update.
1. Download and extract the irflash utility to a floppy diskette or directory.
2. Download and extract the firmware file to a seperate floppy diskette or same directory.
3. Run the irflshw.exe program within Windows with "irflashw /p" command.  
4. If the firmware image is on a diskette Insert the floppy diskette containing irflash utility created in step 1 into the floppy drive.
5. When prompted for the name of the firmware binary file enter the name of the file (eg: 414I) and press enter.
6. When prompted, confirm the update.

Help can be obtained with the command "irflash /?"
Multiple controllers installed in the same system can be updated one after the other by following the prompts that are presented.

================
Component Features
================
a) Supports GUI and CLI (Command Line Interface) modes.
b) Multiple instances of utility are not allowed
c) Multiple adapters can be flashed one after another both in GUI and CLI modes.
d) In CLI mode, image files are searched from the current directory, only for the controllers available in the system. In that case, if multiple valid image files found, users will be asked to choose one image file among the listed valid images.
e) “Forced File Flashing?can be done with some adapters with files given with /f option in CLI mode. This means user can provide some image files by her and can force them to flash with matching controllers.
f) “Don’t Check signature?checkbox is provided in the GUI mode to flash any image without checking the signature (i.e. without validating) of the image file.
g) This utility provides an option to query all valid adapters present in the system and shows their information and then quit in CLI mode.


================
Known Bugs
================
N/A

================
Fixes/Updates
================

1. IRFlash fails to detect the Target if 40 lds are present, fixed.


*Third-party trademarks are the property of their respective owners.


