Intel® Graphics Media Accelerator Driver

Production Version 14.37.64.5009

Release Notes

November 13, 2008

Microsoft Windows* XP Professional x64 Edition

DISCLAIMER: INFORMATION IN THIS DOCUMENT IS PROVIDED IN CONNECTION WITH INTEL PRODUCTS. NO LICENSE, EXPRESS OR IMPLIED, BY ESTOPPEL OR OTHERWISE, TO ANY INTELLECTUAL PROPERTY RIGHTS IS GRANTED BY THIS DOCUMENT. EXCEPT AS PROVIDED IN INTEL'S TERMS AND CONDITIONS OF SALE FOR SUCH PRODUCTS, INTEL ASSUMES NO LIABILITY WHATSOEVER AND INTEL DISCLAIMS ANY EXPRESS OR IMPLIED WARRANTY, RELATING TO SALE AND/OR USE OF INTEL PRODUCTS INCLUDING LIABILITY OR WARRANTIES RELATING TO FITNESS FOR A PARTICULAR PURPOSE, MERCHANTABILITY, OR INFRINGEMENT OF ANY PATENT, COPYRIGHT OR OTHER INTELLECTUAL PROPERTY RIGHT.
UNLESS OTHERWISE AGREED IN WRITING BY INTEL, THE INTEL PRODUCTS ARE NOT DESIGNED NOR INTENDED FOR ANY APPLICATION IN WHICH THE FAILURE OF THE INTEL PRODUCT COULD CREATE A SITUATION WHERE PERSONAL INJURY OR DEATH MAY OCCUR.

Intel may make changes to specifications and product descriptions at any time, without notice. Designers must not rely on the absence or characteristics of any features or instructions marked "reserved" or "undefined." Intel reserves these for future definition and shall have no responsibility whatsoever for conflicts or incompatibilities arising from future changes to them. The information here is subject to change without notice. Do not finalize a design with this information.

The products described in this document may contain design defects or errors known as errata which may cause the product to deviate from published specifications. Current characterized errata are available on request.

Contact your local Intel sales office or your distributor to obtain the latest specifications and before placing your product order.

Other names and brands may be claimed as the property of others.
Copyright © Intel Corporation 2008

Intel® Graphics Media Accelerator Driver

The Intel® Graphics Media Accelerator Driver contains support for the following Intel® Chipsets:

· Intel(R) G31 Express Chipset

· Intel(R) G33 Express Chipset

· Intel(R) G35 Express Chipset

· Intel(R) G41 Express Chipset

· Intel(R) G43 Express Chipset

· Intel(R) G45 Express Chipset

· Intel(R) Q33 Express Chipset

· Intel(R) Q35 Express Chipset

· Intel(R) Q43 Express Chipset

· Intel(R) Q45 Express Chipset

· Mobile Intel(R) GL40 Express Chipset

· Mobile Intel(R) GL960 Express Chipset

· Mobile Intel(R) GLE960 Express Chipset

· Mobile Intel(R) GM45 Express Chipset

· Mobile Intel(R) GM965 Express Chipset

· Mobile Intel(R) GME965 Express Chipset

· Mobile Intel(R) GS45 Express Chipset

New Features

Features Added in Baseline 14.37
Reference No. | Description | Affected Components | Affected Chipset(s)
| Support Embedded DisplayPort* with AUX and DPCD mandatory. | VBIOS, softBIOS, Power Conservation | Mobile Intel® 4 Series Express Chipset Family
| Support 512 MB system memory configuration. | GMM | Intel® 4 Series Chipset Family Mobile Intel® 4 Series Express Chipset Family
| Read color depth from panel EDID. | VBIOS, softBIOS | Mobile Intel® 4 Series Express Chipset Family
| Add DirectX* Query Timestamp and Timestamp_Freq. | Direct3D* | Intel® 4 Series Chipset Family Mobile Intel® 4 Series Express Chipset Family Mobile Intel® 965 Express Chipset Family

Known Issues

Known Issues in Build 5009
Reference No. | Description | Affected Component(s) | Affected Chipset(s)
2559791 | Corruption displayed after rotating the HDTV to 180 degrees and keeping the monitor at 0 degrees (not rotated) while in Intel® Dual Display Clone mode. | Rotation | Mobile Intel® 4 Series Express Chipset Family
2560433 | The external digital display’s resolution changes to 800x600x32bit@ 60Hz after closing and re-opening the laptop’s lid and connecting and disconnecting an analog monitor. | NT - miniport | Mobile Intel® 4 Series Express Chipset Family
2788029 | Need for Speed*: ProStreet* game: When launched, error is seen: “This application has failed to start because the application configuration is incorrect. Reinstalling the application may fix this problem.” | CV | Mobile Intel® 4 Series Express Chipset Family
2807778 | The TV Video Standard is not kept after using hot-keys to switch from the Intel® Dual Display Clone mode to TV-only mode. | CUI2 | Mobile Intel® 4 Series Express Chipset Family

Issues Resolved

Issues Resolved in Build 5009
Reference No. | Description | Affected Component(s) | Affected Chipset(s)
2560107 | Direct3D* error with LockRect | DirectDraw* | Mobile Intel® 965 Express Chipset Family
2787262 | Cannot run FurMark* benchmark. | OpenGL* | Mobile Intel® 4 Series Express Chipset Family
2787834 | When changing from POST to Windows* splash screen, there is a few seconds of corruption on the monitor connected through DisplayPort*. | Video BIOS | Intel® 4 Series Chipset Family
2807587 | World of Warcraft*: Wrath of the Lich King* game crashes after pressing Alt-Tab. | OpenGL* | Intel® 4 Series Chipset Family Mobile Intel® 4 Series Express Chipset Family Mobile Intel® 965 Express Chipset Family
2807790 | Cannot change TV format when TV is the secondary display. | CUI2.5 | Mobile Intel® 4 Series Express Chipset Family
2807859 | 3DMark*06 application: STOP: 0x000000EA error when running in loop mode for 24 hours. | GHAL3D Compiler | Intel® 4 Series Chipset Family
2808086 | The ‘Adapter String’ field is empty under the Windows* Display Properties, Settings tab, Advanced button, Adapter tab. | NT - miniport | Intel® 3 Series Chipset Family
2808087 | After connecting the laptop’s power cord, sometimes the display shows corruption. | Power Conservation | Mobile Intel® 4 Series Express Chipset Family