//****************************************************************************
//                   INTEL CORPORATION PROPRIETARY INFORMATION
//       This software is supplied under the terms of a license agreement or
//       nondisclosure agreement with Intel Corporation and may not be copied
//       or disclosed except in accordance with the terms of that agreement.
//         Copyright (c) 2007 Intel Corporation. All Rights Reserved.
//****************************************************************************
//
// Sensor data based on rev 1.02 SDR spreadsheet
// Do not load this file into SDR Create and then save it to source control.
// SDR Create removes all comments and does not like fields set to indicate 
// IPMI rev 2.0 support.
//

_LF_NAME       '3210SH13.SDR'
_LF_VERSION    '0.13'
_LF_FMT_VER    '1.50'
_IPMI_VERSION  '2.00'

_SDR (
_START_ADDR    0000
_DATA_LEN      0000
_NVS_TYPE      'IMBDEVICE'
_DEV_BUS       FF
_DEV_ADDRESS   20

//*******************************************************
// SDR Type 01 Records
//*******************************************************

_SDR_TYPE      01
_REC_LEN       003B

   // Sensor Record Header
   0100               // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   05                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask    --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask  --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   B8                 // Nominal Reading  (B8h = 1.8V)
   C2                 // Normal Maximum   (C2h = 1.899V)
   AE                 // Normal Minimum   (AEh = 1.701V)
   FF                 // Sensor Maximum Reading  
   00                 // Sensor Minimum Reading  
   00                 // Upper non-recoverable
   CE                 // Upper critical      (CEh = 2.018V) 
   C8                 // Upper non-critical  (C8h = 1.959V)
   00                 // Lower non-recoverable
   A3                 // Lower critical      (A3h = 1.592V) 
   A8                 // Lower non-critical  (A8h = 1.641V)
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'BB +1.8V SM'      // String Bytes

_SDR_TYPE      01
_REC_LEN       0038

   // Sensor Record Header
   0200               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask    --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask  --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   9E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   D0                 // Nominal Reading  (D0h = 3.30V)
   DB                 // Normal Maximum   (DBh = 3.465V)
   C6                 // Normal Minimum   (C6h = 3.135V)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   EC                 // Upper critical      (ECh = 2.310V)
   E5                 // Upper non-critical  (E5h = 2.242V)
   00                 // Lower non-recoverable
   B6                 // Lower critical      (B6h = 1.782V)
   BC                 // Lower non-critical  (BCh = 1.837V)
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'BB +3.3V'         // String Bytes

_SDR_TYPE      01
_REC_LEN       003D

   // Sensor Record Header
   0300               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   07                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   03                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask    --[u,l][c,nc]=8532 
   8532               // Deassertion Event Mask  --[u,l][c,nc]=8532 
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   9E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   D0                 // Nominal Reading  (D0h = 3.30V)
   DB                 // Normal Maximum   (DBh = 3.465V)
   C6                 // Normal Minimum   (C6h = 3.135V)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   EC                 // Upper critical      (ECh = 2.310V)
   E5                 // Upper non-critical  (E5h = 2.242V)
   00                 // Lower non-recoverable
   B6                 // Lower critical      (B6h = 1.782V)
   BC                 // Lower non-critical  (BCh = 1.837V)
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BB +3.3V STBY'    // String Bytes

_SDR_TYPE      01
_REC_LEN       0038

   // Sensor Record Header
   0400               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   08                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   04                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask    --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask  --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   F1                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   CF                 // Nominal Reading  (CFh = 5.00V)
   D9                 // Normal Maximum   (D9h = 5.25V)
   C5                 // Normal Minimum   (C5h = 4.75V)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   EB                 // Upper critical      (EBh = 5.66V)
   E4                 // Upper non-critical  (E4h = 5.49V)
   00                 // Lower non-recoverable
   B5                 // Lower critical      (B5h = 4.36V)
   BA                 // Lower non-critical  (BAh = 4.48V)
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'BB +5.0V'         // String Bytes

_SDR_TYPE      01
_REC_LEN       003D

   // Sensor Record Header
   0500               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0E                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   05                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask    --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask  --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   7A                 // Nominal Reading  (7Ah = 1.20V)
   8F                 // Normal Maximum   (8Fh = 1.40V)
   58                 // Normal Minimum   (58h = 0.86V)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   9A                 // Upper critical      (9Ah = 1.51V)
   95                 // Upper non-critical  (95h = 1.46V)
   00                 // Lower non-recoverable
   4F                 // Lower critical      (4Fh = 0.77V)
   52                 // Lower non-critical  (52h = 0.80V)
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Processor Vcc'    // String Bytes

_SDR_TYPE      01
_REC_LEN       003F

   // Sensor Record Header
   0600               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   06                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask    --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask  --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   26                 // Nominal Reading  (26h = 38 Deg C)
   37                 // Normal Maximum   (37h = 55 Deg C)
   14                 // Normal Minimum   (14h = 20 Deg C)
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   42                 // Upper critical      (42h = 66 Deg C)
   3D                 // Upper non-critical  (3Dh = 61 Deg C)
   00                 // Lower non-recoverable
   05                 // Lower critical      (05h = 5 Deg C)
   0A                 // Lower non-critical  (0Ah = 10 Deg C)
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BB Ambient Temp'  // String Bytes

_SDR_TYPE      01
_SDR_TAG       'SC5299UP'
_REC_LEN       0037

   // Sensor Record Header
   0700               // Record ID
   51                 // SDR Version
   01                 // Record Type
   32                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   09                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask    --[l][c,nc]=0530
   0500               // Deassertion Event Mask  --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   11                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   8D                 // Nominal Reading  (8Dh = 2397 RPM)
   FF                 // Normal Maximum   (FFh = 4335 RPM)
   1C                 // Normal Minimum   (1Ch = 476 RPM)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   13                 // Lower critical      (13h = 323 RPM)
   16                 // Lower non-critical  (16h = 374 RPM)
   00                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C7                 // Type/Length Code
   'CPU Fan'          // String Bytes

_SDR_TYPE      01
_SDR_TAG       'SR1530SH'
_SDR_TAG       'SR1530HSH'
_REC_LEN       003C

   // Sensor Record Header
   0800               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0A                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask    --[l][c,nc]=0530
   0500               // Deassertion Event Mask  --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   1B                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   B8                 // Nominal Reading  (B8h = 4968 RPM)
   FF                 // Normal Maximum   (FFh = 6885 RPM)
   72                 // Normal Minimum   (72h = 3078 RPM)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   50                 // Lower critical      (50h = 2160 RPM)
   5B                 // Lower non-critical  (5Bh = 2457 RPM)
   00                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'System Fan 3'     // String Bytes

_SDR_TYPE      01
_SDR_TAG       'SR1530SH'
_SDR_TAG       'SR1530HSH'
_REC_LEN       003C

   // Sensor Record Header
   0900               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0B                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask    --[l][c,nc]=0530
   0500               // Deassertion Event Mask  --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   1B                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   B8                 // Nominal Reading  (B8h = 4968 RPM)
   FF                 // Normal Maximum   (FFh = 6885 RPM)
   72                 // Normal Minimum   (72h = 3078 RPM)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   50                 // Lower critical      (50h = 2160 RPM)
   5B                 // Lower non-critical  (5Bh = 2457 RPM)
   00                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'System Fan 4'     // String Bytes

_SDR_TYPE      01
_SDR_TAG       'SC5299UP'
_REC_LEN       003C

   // Sensor Record Header
   0A00               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0C                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask    --[l][c,nc]=0530
   0500               // Deassertion Event Mask  --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   0D                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   AB                 // Nominal Reading  (ABh = 2223 RPM)
   FF                 // Normal Maximum   (FFh = 3315 RPM)
   57                 // Normal Minimum   (57h = 1131 RPM)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   3D                 // Lower critical      (3Dh = 793 RPM)
   45                 // Lower non-critical  (45h = 897 RPM)
   00                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'System Fan 1'     // String Bytes

_SDR_TYPE      01
_SDR_TAG       'SC5299UP_OPT'
_REC_LEN       003C

   // Sensor Record Header
   0B00               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0D                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask    --[l][c,nc]=0530
   0500               // Deassertion Event Mask  --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   0D                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   AB                 // Nominal Reading  (ABh = 2223 RPM)
   FF                 // Normal Maximum   (FFh = 3315 RPM)
   57                 // Normal Minimum   (57h = 1131 RPM)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   3D                 // Lower critical      (3Dh = 793 RPM)
   45                 // Lower non-critical  (45h = 897 RPM)
   00                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'System Fan 2'     // String Bytes

_SDR_TYPE      01
_SDR_TAG       'SR1530SH'
_REC_LEN       003C

   // Sensor Record Header
   0C00               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0D                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask    --[l][c,nc]=0530
   0500               // Deassertion Event Mask  --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   32                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   E1                 // Nominal Reading  (E1h = 11250 RPM)
   FF                 // Normal Maximum   (FFh = 12750 RPM)
   C4                 // Normal Minimum   (C4h =  9800 RPM)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   89                 // Lower critical     (89h = 6850 RPM)
   9C                 // Lower non-critical (9Ch = 7800 RPM)
   00                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'System Fan 2'     // String Bytes

_SDR_TYPE      01
_SDR_TAG       'CPUFAN1_TACH0'
_REC_LEN       003D

   // Sensor Record Header
   0D00               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   09                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask    --[l][c,nc]=0530
   0500               // Deassertion Event Mask  --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   46                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   86                 // Nominal Reading  (86h =  9380 RPM)
   FF                 // Normal Maximum   (FFh = 17850 RPM)
   0E                 // Normal Minimum   (0Eh =   980 RPM)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   09                 // Lower critical      (09h = 630 RPM)
   0B                 // Lower non-critical  (0Bh = 770 RPM)
   00                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Chassis Fan 1'    // String Bytes

_SDR_TYPE      01
_SDR_TAG       'CPUFAN2_TACH1'
_REC_LEN       003D

   // Sensor Record Header
   0E00               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0A                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask    --[l][c,nc]=0530
   0500               // Deassertion Event Mask  --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   46                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   86                 // Nominal Reading  (86h =  9380 RPM)
   FF                 // Normal Maximum   (FFh = 17850 RPM)
   0E                 // Normal Minimum   (0Eh =   980 RPM)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   09                 // Lower critical      (09h = 630 RPM)
   0B                 // Lower non-critical  (0Bh = 770 RPM)
   00                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Chassis Fan 2'    // String Bytes

_SDR_TYPE      01
_SDR_TAG       'CPUFAN3_TACH2'
_REC_LEN       003D

   // Sensor Record Header
   0F00               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0B                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask    --[l][c,nc]=0530
   0500               // Deassertion Event Mask  --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   46                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   86                 // Nominal Reading  (86h =  9380 RPM)
   FF                 // Normal Maximum   (FFh = 17850 RPM)
   0E                 // Normal Minimum   (0Eh =   980 RPM)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   09                 // Lower critical      (09h = 630 RPM)
   0B                 // Lower non-critical  (0Bh = 770 RPM)
   00                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Chassis Fan 3'    // String Bytes

_SDR_TYPE      01
_SDR_TAG       'SYSFAN1_TACH3'
_REC_LEN       003D

   // Sensor Record Header
   1000               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0C                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask    --[l][c,nc]=0530
   0500               // Deassertion Event Mask  --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   46                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   86                 // Nominal Reading  (86h =  9380 RPM)
   FF                 // Normal Maximum   (FFh = 17850 RPM)
   0E                 // Normal Minimum   (0Eh =   980 RPM)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   09                 // Lower critical      (09h = 630 RPM)
   0B                 // Lower non-critical  (0Bh = 770 RPM)
   00                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Chassis Fan 4'    // String Bytes

_SDR_TYPE      01
_SDR_TAG       'SYSFAN2_TACH4'
_REC_LEN       003D

   // Sensor Record Header
   1100               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0D                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask    --[l][c,nc]=0530
   0500               // Deassertion Event Mask  --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   46                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   86                 // Nominal Reading  (86h =  9380 RPM)
   FF                 // Normal Maximum   (FFh = 17850 RPM)
   0E                 // Normal Minimum   (0Eh =   980 RPM)
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   09                 // Lower critical      (09h = 630 RPM)
   0B                 // Lower non-critical  (0Bh = 770 RPM)
   00                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Chassis Fan 5'    // String Bytes

_SDR_TYPE      01
_REC_LEN       003F

   // Sensor Record Header
   1200               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   10                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   -- (No Events enabled-0000)
   0000               // Deassertion Event Mask -- (No Events Enabled-0000)
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   F1                 // Nominal Reading  (F1h = -15 Deg C)
   00                 // Normal Maximum   (00h = 0 Deg C)
   BA                 // Normal Minimum   (BAh = -70 Deg C)
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Margin'  // String Bytes


//*******************************************************
// SDR Type 02 Records
//*******************************************************

_SDR_TYPE      02
_REC_LEN       002A

   // Sensor Record Header
   1300               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID
   01                 // Entity Instance
   63                 // Sensor Initialization
   40                 // Sensor Capabilities
   09                 // Sensor Type
   6F                 // Event / Reading Base Type
   3100               // Assertion Event Mask
   3100               // Deassertion Event Mask
   3100               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Power Unit'       // String Bytes

_SDR_TYPE      02
_REC_LEN       002D

   // Sensor Record Header
   1400               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   07                 // Entity Instance
   63                 // Sensor Initialization
   40                 // Sensor Capabilities
   23                 // Sensor Type
   6F                 // Event / Reading Base Type
   0F01               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0F01               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'IPMI Watchdog'    // String Bytes

_SDR_TYPE      02
_SDR_TAG       'CHS_INT'
_SDR_TAG       'SC5299UP'
_REC_LEN       002E

   // Sensor Record Header
   1500               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   63                 // Sensor Initialization
   40                 // Sensor Capabilities
   05                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Assertion Event Mask
   0100               // Deassertion Event Mask
   0100               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Physical Scrty'   // String Bytes

_SDR_TYPE      02
_REC_LEN       0030

   // Sensor Record Header
   1600               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0F                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   63                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   6F                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0300               // Deassertion Event Mask
   0300               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'Processor Status' // String Bytes

//********************************************************
// HSC Type 1 sensors
//********************************************************

_SDR_TYPE      01
_SDR_TAG       'HSC'
_REC_LEN       0039

   // Sensor Record Header
   0135               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   01                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   7D                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask		--[u,l][c,nc]=8532
   8532               // Deassertion Event Mask	--[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   02                 // M, Tolerance
   00                 // B
   2C                 // B, Accuracy
   10                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   1C                 // Nominal Reading (1Ch = 28 degree C)
   2D                 // Normal Maximum (2Dh = 45 degree C)
   0A                 // Normal Minimum (0Ah = 10 degree C)
   7F                 // Sensor Maximum Reading (7Fh = 127 degree C)
   80                 // Sensor Minimum Reading (80h = -128 degree C)
   00                 // Upper non-recoverable (00h = 0 degree C)
   36                 // Upper critical (36h = 54 degree C)
   32                 // Upper non-critical (32h = 50 degree C)
   00                 // Lower non-recoverable (00h = 0 degree C)
   00                 // Lower critical (00h = 0 degree C)
   05                 // Lower non-critical (05h = 05 degree C)
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type Length Code
   'HSBP Temp'        // String Bytes

//********************************************************
// HSC Type 2 Sensors
//********************************************************

//********************************************************
// HSC Disk Drive Status sensors
//********************************************************

_SDR_TYPE      02
_SDR_TAG       'HSC'
_REC_LEN       002A

   // Sensor Record Header
   002C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   02                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 0 Stat'       // String Bytes

_SDR_TYPE      02
_SDR_TAG       'HSC'
_REC_LEN       002A

   // Sensor Record Header
   002D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   03                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 1 Stat'       // String Bytes

_SDR_TYPE      02
_SDR_TAG       'HSC'
_REC_LEN       002A

   // Sensor Record Header
   002E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   04                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 2 Stat'       // String Bytes

_SDR_TYPE      02
_SDR_TAG       'HSC'
_REC_LEN       002A

   // Sensor Record Header
   002F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   05                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 3 Stat'       // String Bytes

_SDR_TYPE      02
_SDR_TAG       'HSC'
_REC_LEN       002A

   // Sensor Record Header
   0030               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   06                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 4 Stat'       // String Bytes

_SDR_TYPE      02
_SDR_TAG       'HSC'
_REC_LEN       002A

   // Sensor Record Header
   0031               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   07                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 5 Stat'       // String Bytes

//********************************************************
// HSC Disk Drive Presence sensors
//********************************************************


_SDR_TYPE      02
_SDR_TAG       'HSC'
_REC_LEN       002A

   // Sensor Record Header
   0034               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   09                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   08                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 0 Pres'       // String Bytes

_SDR_TYPE      02
_SDR_TAG       'HSC'
_REC_LEN       002A

   // Sensor Record Header
   0035               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   0A                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   08                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 1 Pres'       // String Bytes

_SDR_TYPE      02
_SDR_TAG       'HSC'
_REC_LEN       002A

   // Sensor Record Header
   0036               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   0B                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   08                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 2 Pres'       // String Bytes

_SDR_TYPE      02
_SDR_TAG       'HSC'
_REC_LEN       002A

   // Sensor Record Header
   0037               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   0C                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   08                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 3 Pres'       // String Bytes

_SDR_TYPE      02
_SDR_TAG       'HSC'
_REC_LEN       002A

   // Sensor Record Header
   0038               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   0D                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   08                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 4 Pres'       // String Bytes

_SDR_TYPE      02
_SDR_TAG       'HSC'
_REC_LEN       002A

   // Sensor Record Header
   0039               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   0E                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   08                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 5 Pres'       // String Bytes

//*******************************************************
// SDR Type 11 Records
//*******************************************************

_SDR_TYPE      11
_REC_LEN       0019

   // Sensor Record Header
   1700               // Record ID
   51                 // SDR Version
   11                 // Record Type
   14                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   00                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   07                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   C9                 // Type/Length Code
   'Baseboard'        // String Bytes

//*******************************************************
// SDR Type 12 Records
//*******************************************************

_SDR_TYPE      12
_REC_LEN       0020

   // Sensor Record Header
   1800               // Record ID
   51                 // SDR Version
   12                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   20                 // Device Slave Address
   00                 // Channel Number

   // Record Body Bytes
   08                 // Power state notification
   BF                 // Device capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   07                 // Entity ID
   08                 // Entity instance
   00                 // OEM
   D0                 // Type/Length Code
   'Basbrd Mgmt Ctlr' // String Bytes

_SDR_TYPE      12
_SDR_TAG       'HSC'
_REC_LEN       001C

   // Sensor Record Header
   00DD               // Record ID
   51                 // SDR Version
   12                 // Record Type
   17                 // Record Length

   // Record Key Bytes
   C0                 // Device Slave Address
   00                 // Channel Number

   // Record Body Bytes
   84                 // Power state notification
   29                 // Device capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   0F                 // Entity ID
   01                 // Entity instance
   00                 // OEM
   CC                 // Type/Length Code
   'HSBP PRIMARY'     // String Bytes



//********************************************************
// SDR Type C0 Records For Fan Speed Control Configuration
//********************************************************

_SDR_TYPE      C0
_SDR_TAG       'SC5299UP'
_REC_LEN       001A

   // Sensor Record Header
   1900               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record sub-type - Temperature Fan Speed Control Type 2
   00                 // Control Domain Number (PWM0-CPU Fan)
   19                 // Normal Control Value (25%)
   64                 // Sleep Control Value (100%)
   64                 // Boost Control Value (100%)
   04                 // Ramp Step 
   02                 // Scan Rate
   01                 // Flags; profile 1 
   19                 // minimum control value - fail value (25%)
   20                 // sensor owner ID
   10                 // Temperature Sensor Number (PECI)
   64                 // Temp Sensor Failure Control value (100%)
   02                 // Temperature Control Type (clamp type = 2)
   A8                 // Temperature Info [7]-Signed Sensor =1; [6]-Reserved; [5:3]-Negative Hysteresis =5; [2:0]-Positive Hysteresis =0
   01                 // Ramp Contribution (1 %)
   05                 // Scan Rate
   00                 // Temperature 0c
   01                 // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source=1 (use TControl)


_SDR_TYPE      C0
_SDR_TAG       'SC5299UP'
_REC_LEN       0025

   // Sensor Record Header
   1A00               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   20                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record sub-type - Temperature Fan Speed Control Type 2
   01                 // Control Domain Number (PWM1 - Rear Fan)
   2C                 // Normal Control Value (44%)
   64                 // Sleep Control Value (100%)
   64                 // Boost Control Value (100%)
   01                 // Ramp Step 
   02                 // Scan Rate
   01                 // Flags; profile 1 
   19                 // minimum control value - fail value (25%)
   20                 // Sensor Owner ID
   04                 // Temperature Sensor Number (Baseboard Temp)
   64                 // Temp sensor Failue Control value (100%)
   01                 // Temperature Control Type (StepWise=1)
   90                 // Temperature Info [7]-Signed Sensor=1; [6]-Domain Max=0; [5:3]-Negative Hysteresis =2; [2:0]-Positive Hysteresis=0
   07                 // Count of Temperature/Control Value Pairs
   00                 // Temperature 1 (0-37c)
   2E                 // Control Value 1 (46%)
   25                 // Temperature 2 37c
   34                 // Control Value 2 (52%)
   26                 // Temperature 3 38c
   40                 // Control Value 3 (64%)
   27                 // Temperature 4 39c
   49                 // Control Value 4 (73%)
   28                 // Temperature 5 40c
   52                 // Control Value 5 (82%)
   29                 // Temperature 6 41c
   5E                 // Control Value 6 (94%)
   2A                 // Temperature 7 42c - inf
   64                 // Control Value 7 (100%)


_SDR_TYPE      C0
_SDR_TAG       'SC5299UP_OPT'
_REC_LEN       0025

   // Sensor Record Header
   1B00               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   20                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record sub-type - Temperature Fan Speed Control Type 2
   02                 // Control Domain Number (PWM2 - Front HDD Hotswap Bay)
   3C                 // Normal Control Value (60%)
   64                 // Sleep Control Value (100%)
   64                 // Boost Control Value (100%)
   01                 // Ramp Step 
   02                 // Scan Rate
   01                 // Flags; profile 1 
   19                 // minimum control value - fail value (25%)
   20                 // Sensor Owner ID
   04                 // Temperature Sensor Number (Baseboard Temp)
   64                 // Temp sensor Failue Control value (100%)
   01                 // Temperature Control Type (StepWise=1)
   90                 // Temperature Info [7]-Signed Sensor=1; [6]-Domain Max=0; [5:3]-Negative Hysteresis =2; [2:0]-Positive Hysteresis=0
   07                 // Count of Temperature/Control Value Pairs
   00                 // Temperature 1 (0-37c)
   3D                 // Control Value 1 (61%)
   25                 // Temperature 2 37c
   43                 // Control Value 2 (67%)
   26                 // Temperature 3 38c
   49                 // Control Value 3 (73%)
   27                 // Temperature 4 39c
   4F                 // Control Value 4 (79%)
   28                 // Temperature 5 40c
   58                 // Control Value 5 (88%)
   29                 // Temperature 6 41c
   5E                 // Control Value 6 (94%)
   2A                 // Temperature 7 42c - inf
   64                 // Control Value 6 (100%)

_SDR_TYPE      C0
_SDR_TAG       'SC5299UP_NO_OPT'
_REC_LEN       0011

   // Sensor Record Header
   1C00               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0C                 // Record Length

   // Record Body Bytes
   // Unused Domain defaults to 100%
   570100             // Manufacturer ID
   0C                 // Record sub-type - Temperature Fan Speed Control Type 2
   02                 // Control Domain Number (PWM2)
   64                 // Normal Control Value (100%)
   64                 // Sleep Control Value (100%)
   64                 // Boost Control Value (100%)
   04                 // Ramp Step 
   02                 // Scan Rate
   01                 // Flags; profile 1 
   64                 // minimum control value - fail value (100%)

_SDR_TYPE      C0
_SDR_TAG       'SR1530SH'
_REC_LEN       002E

   // Sensor Record Header
   1D00               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   29                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record sub-type - Temperature Fan Speed Control Type 2
   00                 // Control Domain Number (PWM0 - CPU & Memory Blowers)
   28                 // Normal Control Value (40%)
   64                 // Sleep Control Value (100%)
   64                 // Boost Control Value (100%)
   01                 // Ramp Step 
   02                 // Scan Rate
   01                 // Flags; profile 1 
   1E                 // minimum control value (30%)
   20                 // sensor owner ID
   10                 // Temperature Sensor Number (PECI)
   64                 // Temp Sensor Failure Control value (100%)
   02                 // Temperature Control Type (clamp type = 2)
   A8                 // Temperature Info [7]-Signed Sensor=1; [6]-Reserved=0; [5:3]-Negative Hysteresis =5; [2:0]-Positive Hysteresis=0
   01                 // Ramp Contribution (1 %)
   05                 // Scan Rate
   00                 // Temperature 0c
   01                 // Clamp Flags [7:4]-CPU Number=0; [3:1]-Reserved=0; [0]-Temp Source=1 (use TControl)
   20                 // Sensor Owner ID
   04                 // Temperature Sensor Number (Baseboard Temp)
   64                 // Temp sensor Failue Control value (100%)
   01                 // Temperature Control Type (StepWise=1)
   90                 // Temperature Info [7]-Signed Sensor=1; [6]-Domain Max=0; [5:3]-Negative Hysteresis =2; [2:0]-Positive Hysteresis=0
   07                 // Count of Temperature/Control Value Pairs
   00                 // Temperature 1 0-31c
   37                 // Control Value 1 (55%)
   1F                 // Temperature 2 31c
   3B                 // Control Value 2 (59%)
   20                 // Temperature 3 32c
   43                 // Control Value 3 (67%)
   21                 // Temperature 4 33c
   49                 // Control Value 4 (73%)
   22                 // Temperature 5 34c
   4F                 // Control Value 5 (79%)
   23                 // Temperature 6 35c
   57                 // Control Value 6 (87%)
   24                 // Temperature 7 36c - inf
   5B                 // Control Value 6 (91%)


_SDR_TYPE      C0
_SDR_TAG       'SR1530HSH'
_REC_LEN       002E

   // Sensor Record Header
   1E00               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   29                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record sub-type - Temperature Fan Speed Control Type 2
   00                 // Control Domain Number (PWM0 - CPU & Memory Blowers)
   28                 // Normal Control Value (40%)
   64                 // Sleep Control Value (100%)
   64                 // Boost Control Value (100%)
   01                 // Ramp Step 
   02                 // Scan Rate
   01                 // Flags; profile 1 
   1E                 // minimum control value (30%)
   20                 // sensor owner ID
   10                 // Temperature Sensor Number (PECI)
   64                 // Temp Sensor Failure Control value (100%)
   02                 // Temperature Control Type (clamp type = 2)
   A8                 // Temperature Info [7]-Signed Sensor=1; [6]-Reserved=0; [5:3]-Negative Hysteresis =5; [2:0]-Positive Hysteresis=0
   01                 // Ramp Contribution (1 %)
   05                 // Scan Rate
   00                 // Temperature 0c
   01                 // Clamp Flags [7:4]-CPU Number=0; [3:1]-Reserved=0; [0]-Temp Source=1 (use TControl)
   20                 // Sensor Owner ID
   04                 // Temperature Sensor Number (Baseboard Temp)
   64                 // Temp sensor Failue Control value (100%)
   01                 // Temperature Control Type (StepWise=1)
   90                 // Temperature Info [7]-Signed Sensor=1; [6]-Domain Max=0; [5:3]-Negative Hysteresis =2; [2:0]-Positive Hysteresis=0
   07                 // Count of Temperature/Control Value Pairs
   00                 // Temperature 1 0-33c
   37                 // Control Value 1 (55%)
   21                 // Temperature 2 33c
   3B                 // Control Value 2 (59%)
   22                 // Temperature 3 34c
   43                 // Control Value 3 (67%)
   23                 // Temperature 4 35c
   49                 // Control Value 4 (73%)
   24                 // Temperature 5 36c
   4F                 // Control Value 5 (79%)
   25                 // Temperature 6 37c
   57                 // Control Value 6 (87%)
   26                 // Temperature 7 38c - inf
   5B                 // Control Value 6 (91%)

_SDR_TYPE      C0
_SDR_TAG       'SR1530SH'
_SDR_TAG       'SR1530HSH'
_REC_LEN       0011

   // Sensor Record Header
   1F00               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0C                 // Record Length

   // Record Body Bytes
   // Unused Domain defaults to 100%
   570100             // Manufacturer ID
   0C                 // Record sub-type - Temperature Fan Speed Control Type 2
   01                 // Control Domain Number (PWM1)
   64                 // Normal Control Value (100%)
   64                 // Sleep Control Value (100%)
   64                 // Boost Control Value (100%)
   04                 // Ramp Step 
   02                 // Scan Rate
   01                 // Flags; profile 1 
   64                 // minimum control value - fail value (100%)

_SDR_TYPE      C0
_SDR_TAG       'SR1530SH'
_SDR_TAG       'SR1530HSH'
_REC_LEN       0011

   // Sensor Record Header
   2000               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0C                 // Record Length

   // Record Body Bytes
   // Unused Domain defaults to 100%
   570100             // Manufacturer ID
   0C                 // Record sub-type - Temperature Fan Speed Control Type 2
   02                 // Control Domain Number (PWM2)
   64                 // Normal Control Value (100%)
   64                 // Sleep Control Value (100%)
   64                 // Boost Control Value (100%)
   04                 // Ramp Step 
   02                 // Scan Rate
   01                 // Flags; profile 1 
   64                 // minimum control value - fail value (100%)

_SDR_TYPE      C0
_SDR_TAG       'OTHER'
_REC_LEN       0011

   // Sensor Record Header
   2100               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0C                 // Record Length

   // Record Body Bytes
   // Domain defaults to 100%
   570100             // Manufacturer ID
   0C                 // Record sub-type - Temperature Fan Speed Control Type 2
   00                 // Control Domain Number (PWM0)
   64                 // Normal Control Value (100%)
   64                 // Sleep Control Value (100%)
   64                 // Boost Control Value (100%)
   04                 // Ramp Step 
   02                 // Scan Rate
   01                 // Flags; profile 1 
   64                 // minimum control value - fail value (100%)

_SDR_TYPE      C0
_SDR_TAG       'OTHER'
_REC_LEN       0011

   // Sensor Record Header
   2200               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0C                 // Record Length

   // Record Body Bytes
   // Domain defaults to 100%
   570100             // Manufacturer ID
   0C                 // Record sub-type - Temperature Fan Speed Control Type 2
   01                 // Control Domain Number (PWM1)
   64                 // Normal Control Value (100%)
   64                 // Sleep Control Value (100%)
   64                 // Boost Control Value (100%)
   04                 // Ramp Step 
   02                 // Scan Rate
   01                 // Flags; profile 1 
   64                 // minimum control value - fail value (100%)

_SDR_TYPE      C0
_SDR_TAG       'OTHER'
_REC_LEN       0011

   // Sensor Record Header
   2300               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0C                 // Record Length

   // Record Body Bytes
   // Domain defaults to 100%
   570100             // Manufacturer ID
   0C                 // Record sub-type - Temperature Fan Speed Control Type 2
   02                 // Control Domain Number (PWM2)
   64                 // Normal Control Value (100%)
   64                 // Sleep Control Value (100%)
   64                 // Boost Control Value (100%)
   04                 // Ramp Step 
   02                 // Scan Rate
   01                 // Flags; profile 1 
   64                 // minimum control value - fail value (100%)

//*******************************************************
// SDR Type C0 Records For Fan Sensor Scaling
//*******************************************************

_SDR_TYPE      C0
_SDR_TAG       'SC5299UP'
_REC_LEN       001B


  //Sensor Record Header
   2400               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
   9411               // Fan 1 Max RPM (Sensor 09)  **(M = 11)**
   F82A               // Fan 2 Max RPM (Sensor 0A)--------------
   F82A               // Fan 3 Max RPM (Sensor 0B)--------------
   AC0D               // Fan 4 Max RPM (Sensor 0C)  **(M = 0D)**
   AC0D               // Fan 5 Max RPM (Sensor 0D)  **(M = 0D)**
   F82A               // Fan 6 Max RPM -------------------------
   F82A               // Fan 7 Max RPM -------------------------
   F82A               // Fan 8 Max RPM -------------------------

_SDR_TYPE      C0
_SDR_TAG       'SR1530SH'
_REC_LEN       001B


   // Sensor Record Header
   2500               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length


   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution- Bit Field - 1 == 1 PPR, 0 == 2 PPR
   F82A               // Fan 1 Max RPM (Sensor 09)--------------
   BC1B               // Fan 2 Max RPM (Sensor 0A)  **(M = 1B)**
   BC1B               // Fan 3 Max RPM (Sensor 0B)  **(M = 1B)**
   F82A               // Fan 4 Max RPM (Sensor 0C)--------------
   C832               // Fan 5 Max RPM (Sensor 0D)  **(M = 32)**
   F82A               // Fan 6 Max RPM -------------------------
   F82A               // Fan 7 Max RPM -------------------------
   F82A               // Fan 8 Max RPM -------------------------

_SDR_TYPE      C0
_SDR_TAG       'SR1530HSH'
_REC_LEN       001B


   // Sensor Record Header
   2600               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution- Bit Field - 1 == 1 PPR, 0 == 2 PPR
   F82A               // Fan 1 Max RPM (Sensor 09)---------------
   BC1B               // Fan 2 Max RPM (Sensor 0A)   **(M = 1B)**
   BC1B               // Fan 3 Max RPM (Sensor 0B)   **(M = 1B)**
   F82A               // Fan 4 Max RPM (Sensor 0C)---------------
   F82A               // Fan 5 Max RPM (Sensor 0D)---------------
   F82A               // Fan 6 Max RPM --------------------------
   F82A               // Fan 7 Max RPM --------------------------
   F82A               // Fan 8 Max RPM --------------------------


_SDR_TYPE      C0
_SDR_TAG       'OTHER'
_REC_LEN       001B


   // Sensor Record Header
   2700               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution- Bit Field - 1 == 1 PPR, 0 == 2 PPR
   5046               // Fan 1 Max RPM (Sensor 09)   **(M = 46)**
   5046               // Fan 2 Max RPM (Sensor 0A)   **(M = 46)**
   5046               // Fan 3 Max RPM (Sensor 0B)   **(M = 46)**
   5046               // Fan 4 Max RPM (Sensor 0C)   **(M = 46)**
   5046               // Fan 5 Max RPM (Sensor 0D)   **(M = 46)**
   F82A               // Fan 6 Max RPM --------------------------
   F82A               // Fan 7 Max RPM --------------------------
   F82A               // Fan 8 Max RPM --------------------------

//*******************************************************
// SDR Type C0 Records For File & Package Version Info
//*******************************************************

_SDR_TYPE      C0
_REC_LEN       0013

   // Sensor Record Header
   2800               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR File 13'      // String Bytes

_SDR_TYPE      C0
_REC_LEN       0016

   // Sensor Record Header
   2900               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   11                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR Package 13'   // String Bytes

)
