Intel® AP450GX Server Platform
The products you are looking for are no longer manufactured by Intel. Additionally, Intel no longer provides interactive support for these products via telephone or e-mail, nor will Intel provide any future content updates or software updates to support new operating systems or improve compatibility with third party devices and software products. THESE PRODUCT SUPPORT DOCUMENTS ARE PROVIDED FOR HISTORICAL REFERENCE ONLY AND ARE SUBJECT TO THE TERMS SET FORTH IN THE "TERMS OF USE" INFORMATION. Information on currently available Intel products is available at www.intel.com and/or developer.intel.com

Identify your products
  Product Discontinuance Announcement
    Intel® will no longer provide interactive support for these products via telephone or e-mail

Software and drivers
  BIOS/Firmware, drivers and utilities download

Technical specifications
  Technical Product Specifications
    Product overview, including descriptions and diagrams of the integrated features
    Motherboard Technical Product Specifications [PDF]
    AP450GX Platform Technical Product Specifications [PDF]
    AR450GX Platform Technical Product Specifications [PDF]
  Specification Update
    An update to the specifications contained in the Technical Product Specification
    Motherboard Specification Update [PDF]
    Platform Specification Update [PDF]
    Montly Change Summary [PDF]

Installation and use
  System Installation Guide
    Platform overview, descriptions, and diagrams for setup and operation
    System Installation Guide [PDF]
  Installation and Configuration Notes
    Redundant Power
      A pedestal system must have three power supplies for redundancy. A rack system may have two or three.
    Redundant Cooling
      A single system fans can fail without compromising the cooling. The fans are not hot-swappable.
    Fast-20 Drives
      The Adaptec* 7880 chip set supports Fast-20 mode drives with maximum transfer rates of 40 MB/sec. Use the Adaptec SCSI Select utility to configure. Narrow SCSI devices are not supported when in Fast-20 mode.
    Hot-swap Hard Drives
      The included carriers support 80-pin SCA SCSI-2 hot-swap hard drives 3.5" wide and up to 1.6" high.
    Narrow SCSI Drives
      Supported in fast/wide mode only, but not recommended in the 5-1/4" peripheral bay due to EMI considerations. Active bus termination is required on the last device.
    RAID Capabilities
      Add a RAID controller from the list of qualified controllers. Set the jumpers to change the SCSI IDs on the SCSI backplane to change the SCSI IDs if not all hard drives are detected.
    Operating Systems Supported by the Server Management Software
      Microsoft* Windows NT* and Novell NetWare*.
    ECC Memory Support
      Memory ECC is supported via ECC logic in the chipset if using standard parity SIMMs or DIMMs. The chipset will detect double bit errors and correct single bit errors.
  Third Power Supply Requirements
    Ships with two 420 watt power supplies. The system configuration may require more. Please refer to the power table in the Technical Product Specification.
  Novell IntraNetWare* 4.11 limit of 16MB
    See Novell Technical Information Document 1003164 at Novell* Knowledgebase for instructions on editing the AUTOEXEC.NCF
  CPU error messages
    - Missing processor
    - CPU failed
    - "176 previous cpu failure. Slot 1 cpu #01."
    - "177 previous cpu failure. Slot 2 cpu #01"
    - "178 previous cpu failure. Slot 1 cpu #02."
    - "179 previous cpu failure. Slot 2 cpu #02."
    - "180 attempt to boot with failed cpu."
    Run System Configuration Utility and retest processors.
  Identifying Hot-swap Capabilities
    Hot-swap capability is present on Top Assembly numbers whose dash numbers end in 3 (as in -xx3), or if the serial number equal to or higher than:
    Product code ALPC0MB2CPC = S/N Z00088552
    Product code ALPCD166512C = S/N Z00108949
    Product code ALPCD200512C = S/N Z00082658
  SCU Reports "Out Of Memory" Errors
    To workaround this error, set your CONFIG.SYS to:
    device=himem.sys
    dos=high,umb
    stacks=0,0
    lastdrive=b
  Hard drives not recognized by system during OS installation
    Change SCSI jumpers on SCSI backplane to ID 0-5 and reboot the system.
  Server Board system does not power up
    Intel® AR450GX Rack-mount Server System has a magnetic chassis interlock switch under the top cover, at the left front of the chassis. This disables all power to the system. This interlock is not present in the Intel® AP450GX Pedestal-mount system. For normal operation, the cover should always be installed.

Compatibility
  Microprocessor Combinations Supported
    A table showing supported Intel® Pentium® Pro processor combinations by type and stepping is included in the Technical Product Specification.
  Optional 4GB memory module ALMEM4GBM0
    Optional 4GB memory module ALMEM4GBM0 is available, and fits into the 1GB memory module. The additional memory uses TOSP DRAM's packaged in JEDEC standard 16Mx72 60ns DIMMs only. Memory on the module in organized in 8 banks and 4-way interleaves.
  List of operating systems and peripherals tested
    List of operating systems and peripherals tested
    Tested Hardware and Operating System List [PDF]