##
## This is a template multipath-tools configuration file
## Uncomment the lines relevent to your environment
##
#defaults {
#	udev_dir		/dev
#	polling_interval 	10
#	selector		"round-robin 0"
#	path_grouping_policy	multibus
#	getuid_callout		"/sbin/scsi_id -g -u -s /block/%n"
#	prio_callout		/bin/true
#	path_checker		readsector0
#	rr_min_io		100
#	rr_weight		priorities
#	failback		immediate
#	no_path_retry		fail
#	user_friendly_names	no
#}
devnode_blacklist {
	devnode "^(ram|raw|loop|fd|md|dm-|sr|scd|st)[0-9]*"
	devnode "^hd[a-z]"
	devnode "^cciss!c[0-9]d[0-9]*"
}
#blacklist_exceptions {
#       devnode "^dasd[c-d]+[0-9]*"
#       wwid    "IBM.75000000092461.4d00.34"
#}
#multipaths {
#	multipath {
#		wwid			3600508b4000156d700012000000b0000
#		alias			yellow
#		path_grouping_policy	multibus
#		path_checker		readsector0
#		path_selector		"round-robin 0"
#		failback		manual
#		rr_weight		priorities
#		no_path_retry		5
#		rr_min_io		100
#	}
#	multipath {
#		wwid			1DEC_____321816758474
#		alias			red
#	}
#}
devices {
#	device {
#		vendor			"Promise"
#		product			"VTrak"
#		path_grouping_policy	multibus
#		getuid_callout          "/sbin/scsi_id -g -u -s /block/%n"
#		path_checker		tur
#		path_selector		"round-robin 0"
#		hardware_handler		"0"
#		failback			immediate
#		rr_weight			uniform
#		no_path_retry		20
#		rr_min_io			100
#		features			"1 queue_if_no_path"
#	}
	device {
		vendor			"Intel"
		product			"Multi-Flex"
		path_grouping_policy	group_by_prio
		getuid_callout          "/sbin/scsi_id -g -u -s /block/%n"
		prio_callout		"/sbin/mpath_prio_intel /dev/%n"
		path_checker		tur
		path_selector		"round-robin 0"
		hardware_handler		"1 intel"
		failback			immediate
		rr_weight			uniform
		no_path_retry		queue
		rr_min_io			100
		features			"1 queue_if_no_path"
		}
}