EFI System Update Package Install Instructions

The contents of this update package is used to update the System Firmware for 
the following Intel Server Products:

Intel(R) Server Board S5500BC 
Intel(R) Server System SR1630BC
Intel(R) Server Chassis SC5650DP/SC5650BRP
 
System Update Instructions - S5500BC_2

Released - May 6th, 2009


**********************************************************************************
This Update package includes the following system software updates:

System BIOS - R0036
BMC Firmware - R36
FRUSDR Utility - R13 


Important NOTES: 

!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
- The following update process must be followed to ensure a trouble free updating
  of your baseboard.
	1.BMC firmware to 00.36 or later
	2.BIOS R0036 or later
	3.Manageability Engine (ME) firmware 01.10 or later
	4.Latest FRU/SDR package specific to the baseboard.
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!



- The software updates in this update package have only been tested on -40x level hardware. Previous pre-production hardware releases CAN NOT be updated 
with these updates. Intel will not provide support with these software releases on 
pre-production Alpha level hardware.

- All the updates provided in this package are EFI based (unless otherwise noted).
To run these updates, you must boot the system to the embedded EFI shell and then 
access the USB device containing the system software udpates. See instructions
below

- It is highly recommended that you read the Release Notes (.TXT Files) for each 
of the software updates provided to understand what the known issues are, what 
issues were addressed from previous updates, and what new features (if any) were added. 


***********************************************************************************




***********************************************************************************

*********  Standard Update Procedure **************

***********************************************************************************

- Copy all the files to a USB disk-on-key device
- Verify that all jumpers are installed in their default locations.  Switching 
jumpers is not required to properly update the server board, however any jumpers
not set to default may cause unknown behaviors during the update process.

** Booting to the embedded EFI operating environment**
- Plug in your USB device containing the system software updates
- Power on your server
- During POST, hit the F2 key when prompted to access the BIOS Setup Utility
	- Alternatively F6 can be pressed to go directly to the BOOT MANAGER
- In BIOS Setup, move the cursor over to the BOOT MANAGER menu
- Move the cursor down to EFI and hit enter.
- The system will boot to the embedded EFI Shell
- Once the system has booted, and is sitting at a EFI Shell prompt, type 'FS0:' to 
access the USB device. If your USB device is not accessible, type the 'MAP -r' command
to determine which device ID EFI has assigned your USB device, then type in the 
device ID using the same command syntax as before '<device ID>:'.


- Follow the instructions below to perform each software update. Update the system 
software in the sequence specified.  Failure to update in the proper order may result
in the system hanging or restarting on boot.


*** Update BMC Firmware ***

IMPORTANT BMC UPDATE NOTES:

-If an RMM3 is installed in the system, it must be updated along with the BMC.
DO NOT update the RMM3 independent of the BMC.  The BMC may be updated alone if an 
RMM3 is not present.


BMC_36 UPDATE INSTRUCTIONS:

1) Confirm that the BMC Force Update Jumper is in the default location (pins 1-2)
2) Boot the system to EFI and navigate update directory
3) Verify that the following files are present:
BMC36.NSH; BMC_0036.ima; FWPIAUPD.EFI; IPMI.EFI;
4) run the BMC36.nsh script file by typing 'BMC36'
5) If an RMM3 is installed, the RMM3 will be updated automatically.


The BMC update is complete. Either reboot the server or go to the BIOS Update 
described below. 


*** Update System BIOS ***


1)  Verify that the R0036.CAP, IFLASH32.EFI and BIOS36.NSH files are present in the 
directory
2)  At the shell prompt type BIOS36 and press the Enter key


The BIOS update is complete. Either reboot the server or go to the ME FW Update 
described below.  

For BIOS recovery instructions, see the BIOS 36 Release Notes.


*** Management Engine (ME) Firmware Update ***


1)  Verify that the fwpiaupd.efi, ipmi.efi, sps_110_dib.bin, and ME110.nsh files are present in the 
directory
2)  At the shell prompt type ME110 and press the Enter key
3)  The update may take up to 5 minutes to complete

The ME FW update is complete. Either reboot the server or go to the FRUSDR Update 
described below.  


*** Updating the FRU and SDR data on your server ***


1) Boot to EFI shell and confirm that the following files are in the directory:
FRUSDR.efi; IPMI.efi; MASTER.cfg; BC_BMC.fru; BC_BMC.sdr; FUR13.nsh
2) At the EFI Shell prompt type FUR13 and hit the ENTER key to start the utility
3) Answer questions and enter desired information when prompted.
4) When the FRUSDR utility has completed its update, power cycle the server and reboot.


*** Verifying updates ***

1) During POST, hit the F2 Key when prompted to access the BIOS Setup Utility
2) Hit the F9 key to load BIOS Defaults
3) At the MAIN menu verify the BIOS revision is S5500.86B.01.00.0036
4) Move cursor to the SERVER MANAGEMENT Menu
5) Move cursor down to the SYSTEM INFORMATION Option and hit Enter
6) Verify the BMC Firmware revision is 0.36
7) Verify the ME Firmware Revision is 1.10
8) Verify the SDR Revision is 0.13
9) Make any desired BIOS setting changes
10)Hit the F10 Key to save changes and Exit


The System Software Update is Complete.





