Intel® T440BX (NL440BX) Server Board
The products you are looking for are no longer manufactured by Intel. Additionally, Intel no longer provides interactive support for these products via telephone or e-mail, nor will Intel provide any future content updates or software updates to support new operating systems or improve compatibility with third party devices and software products. THESE PRODUCT SUPPORT DOCUMENTS ARE PROVIDED FOR HISTORICAL REFERENCE ONLY AND ARE SUBJECT TO THE TERMS SET FORTH IN THE "TERMS OF USE" INFORMATION. Information on currently available Intel products is available at www.intel.com and/or developer.intel.com

Identify your products
  Product Discontinuance Announcement
    Intel® will no longer provide interactive support for these products via telephone or e-mail

Software and drivers
  BIOS/Firmware, drivers, and utilities

Technical specifications
  Technical Product Specifications
    Product overview, including descriptions and diagrams of the integrated features
    Technical Product Specifications [PDF]
  Specification Update
    An update to the specifications contained in the Technical Product Specification
    Specification Update [PDF]

Installation and use
  AMI MegaRAID* Express 762 Installation and Operating Summary
    Installation and Operating Summary [PDF]
  Beep Code 1-1-1-1
    Unrecognized processor. Reseat or replace
  Beep Code 1-3-3-1
    Memory failure. Try BIOS recovery, or replace memory
  Connecting SCSI Peripherals
    Connect an internal SCSI cable to a SCSI termination card placed in an unused I/O slot of the chassis. From the termination card, use an external SCSI cable to connect external SCSI devices.
    Use an additional SCSI host adapter PCI add-in card. If this option is chosen, Intel does not recommend installing a host adapter in PCI slot one, as the onboard Symbios SCSI controller shares the interrupt with PCI slot one.
  EMP Configuration and Operating
    EMP can be configured for modem mode and either "always active" or "pre-boot only" in BIOS set-up. In "always active" mode, COM2 is not available to the OS. EMP will answer all calls to a modem connected to COM2. In "pre-boot only" mode, EMP will only be active while powered down, and during POST; making COM2 and the modem available to the OS.
    Configuration and Operating Summary [PDF]
  Error: 8101 CPU 1 fail BIST
    Set BIOS Server | Processor Retest to "Yes", and reboot
  Install Pro/100+ Ethernet driver on Unixware* 2.1
    Download and extract the drivers
    Type "sw a:" to extract the Unix drivers to a floppy disk
    Login as root and type "doscp a:eee_uw23.pkg /tmp/eee_uw23.pkg"
    Next type "pkgadd -d /tmp/eee_uw23.pkg"
  Last Known issues
    Wake On LAN requires 0.8A of +5V standby current. Disable the Wake On LAN jumper if your power supply is insufficient.
    USB is not enabled until the operating system is loaded
    Zero-channel RAID adapter must be installed in PCI Slot three
    ISA cards may not work until you set BIOS | Advanced Menu | Reset Configuration Data to "Yes"
    PS/2 port may stop working after a BIOS update. Clear the CMOS by jumper to work around this issue.
  Mylex AcceleRAID* 200 RAID Controller
    Quick Start Guide [PDF]
    Installation Notes [PDF]
  Network Operating System Self-Certification Guidelines
    Self-Certification Guide [PDF]
  NVRAM/CMOS clear
    1. Power the system down. Unplug system from AC
    2. Locate the CMOS CLR jumper at J2J1, then move the jumper to pins 2-3 position.
    3. Boot up, and verify the message indicating NVRAM is clear.
    4. Power down the system, unplug AC, and move jumper back to its initial position, 1-2.
  Product Guide
    Product Guide [PDF]
  Safety and EMC Self-Certification Guidelines
    Self-Certification Guide [PDF]
  Symbios Logic SDMS User's Guide
    User's Guide [PDF]

Compatibility
  Tested Chassis
    The only Intel-designed chassis for the T440BX is Intel® Columbus III Chassis.
    Test Report Summary [PDF]
  Tested Hard Drives
    The Intel® T440BX (NL440BX) server board supports UltraDMA, but does not support LVDS. LVDS drives will only work with the integrated Symbios SCSI controller in Ultra Mode, limited to 40 MB/sec.
    Avoid PCI slot for add-in RAID cards as the Symbios SCSI controller shares its PCI interrupt
  Tested Hardware and Operating System
    The Intel® T440BX Server Board supports the AMI MegaRAID Express* 762, and includes AGP support and slot connector
    Install Microsoft* Windows NT 4.0 from floppy, not CD ROM. Select 'S' during install to manually load SCSI, IDE CD ROM, and NIC drivers
    Disable "Plug-n-Play OS" in the BIOS for Microsoft* Windows NT 4.0
    Supported Hardware and Operating Systems [PDF]
  Tested Memory
    The Intel® T440BX (NL440BX) Server Board has three dual in-line memory module (DIMM) sockets that support up to 384 MB of unbuffered 100 MHz or 66 MHz ECC or non-ECC SDRAM, or 768 MB of registered 100 MHz SDRAM.
    Tested Memory List [PDF]
  Tested Processors
    Select your processor speed in the BIOS under Main Menu | CPU Speed Setting
    All Intel® T440BX server boards support Intel® Pentium® II processors with a 100 MHz Front Side Bus (FSB) running internally at 350, 400 or 450 MHz with 512 KB of integrated L2 cache. All T440BX boards also can be used with the 266, 300 and 333 MHz Pentium II processors, which have a 66 MHz system bus.
    The Intel® Pentium® III processor is supported only on the following versions of the T440BX server board:

    TA* code | Revision | BIOS required | BMC firmware required
    700981 | -004 or higher | BIOS P06 or later | BMC 54 or later

    AA** number | Revision | BIOS required | BMC firmware required
    700980 | -415 or higher | BIOS P06 or later | BMC 54 or later

    PBA** number | Revision | BIOS required | BMC firmware required
    695741 | -415 or higher | BIOS P06 or later | BMC 54 or later

    The T440BX server board does not have the necessary Voltage Regulation Module (VRM) changes needed to support the following processors, although they will physically fit. The below processors are *not* supported on any version of the T440BX board

    Pentium® III Processor | Part number
    733 MHz | BX80526U733256E
    700 MHz | BX80526U700256ES
    667 MHz | BX80526U667256E
    650 MHz | BX80526U650256E
    600EB MHz | BX80526U600256E
    600E MHz | BX80526H600256E
    600B MHz (133-MHz FSB) | BX80525H600512E
    550E MHz | BX80526F550256E
    533EB MHz | BX80526U533256E
    533B MHz (133-MHz FSB) | BX80525U533512E

Technical advisories
  Slot 1-to-Socket 370 Adapters Not Supported
    Technical Advisory [PDF]