=============================================================================
Intel(R) Server Board Platform Confidence Test Release Notes
=============================================================================
Intel Product Collaboration & System Division
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
=============================================================================
DATE:           January, 2014
TO:             Intel(R) server platform customers
SUBJECT:        Unified EFI Platform Confidence Test x64(PCTx64) 
=============================================================================
Information in this document is provided in connection with Intel products.
No license, express or implied, by estoppels or otherwise, to any intellectual
property rights are granted by this document. Except as provided in Intel's
Terms and Conditions of Sale for such products, Intel assumes no liability
whatsoever, and Intel disclaims any express or implied warranty, relating to
sale and/or use of Intel products including liability or warranties relating
to fitness for a particular purpose, merchantability, or infringement of any
patent, copyright or other intellectual property right. Intel Corporation may
have patents or pending patent applications, trademarks, copyrights, or other
intellectual property rights that relate to the presented subject matter. The
furnishing of documents and other materials and information does not provide
any license, express or implied, by estoppels or otherwise, to any such
patents, trademarks, copyrights, or other intellectual property rights. Intel
products are not intended for use in medical, life saving, or life sustaining
applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation.

*Other names and brands are the property of their respective owners.

Copyright (c) 2014 Intel Corporation.


=============================================================================
                              SET UP OF CD/DVD-ROM DRIVE
=============================================================================

Not Supported at this time.

=============================================================================
                              SET UP OF USB FLASH DRIVE
=============================================================================

Unzip efi_pctx64_122.zip to root of USB Flash Drive.  

Insert USB Flash drive and boot the system.
BIOS Settings required for PCT, Press <F2> to enter Setup.
Upon entering BIOS press <F9> to load defaults.
Change the boot order so EFI Shell is the primary (#1) boot device.
Press <F10> to save BIOS setup settings and reboot to EFI.
Test should start automatically.
Pressing <F10> during tests will cause test to terminate.

It is recommended that after the comprehensive or comprehensive looping test 
you do a full AC power cycle (remove power from the system) before retesting.  
The reason for this is to ensure that all controllers are reset and in an 
expected mode.

The network test requires that the server not be plugged into any network.  
You can connect any network port to another port in the same system with 
a cross-over cable to test the NIC ports.

Using Same PCT USB Flash Drive to test multiple systems.
===========================================
If you plan to use the same PCT USB drive to test multiple systems, boot the system
with the USB Flash Drive to start the test in EFI then wait until all the files are copied to the 
RAM drive, and test menu will display automatically, then remove the USB Flash Drive
before you start the PCT test. 
Note:
If the USB key is removed during or after starting the PCT test, it will cause the test to fail.

============================================================================
                              Supported Products
=============================================================================

Product		Date Added	Version of Initial Support
=============================================================================
S5520HC		07/08/2008		1.02
S5520SC		10/23/2008		1.03
S5520UR		11/07/2008		1.04
S5520UR		11/28/2008		1.05
S5520XX		12/05/2008		1.06
S5520XX		01/23/2009		1.07
S5520XX		02/13/2009		1.08
S5520VI		03/09/2009		1.09
S5520XX		03/26/2009		1.10
S5520XX		04/02/2009		1.11
S5500XX		12/08/2009		1.16
S5520XX		12/22/2009		1.17
S55XXXX		02/18/2010		1.18
S55XXXX		02/26/2010		1.19
S55XXXX		10/19/2010		1.20
S55XXXX		01/10/2011		1.21
S55XXXX		01/28/2014		1.22
=============================================================================
                              ABOUT THIS RELEASE
=============================================================================
V1.22 - 01/28/2014
        Updated PCT utilities.

v1.21 - 01/10/2011
	Updated test executive and nicx64.efi
	Changed NIC parameter AUTOCFG_BRD2BRD = NO


v1.20 - 10/19/2010
	Updated PCT utilities.


v1.19 - 02/26/2010
	Updated PCT utilities.


v1.18 - 02/18/2010
	Release to Support S55XX products with the latest Intel test modules and utilites.
	Added support for Westmere CPUs.

v1.17 - 12/22/2009
	Release to Support S5520 products with the latest Intel test modules and utilites.
	Also support using the same USB flash drive to test multiple systems.

v1.16 - 12/08/2009
	Release to Support S5500 products with the latest Intel test modules and utilites.
	Also support using the same USB flash drive to test multiple systems.
	

v1.12 - 07/30/2009
	Release to fixed tracker 26770 'Lose video output from add-in graphics card when run PCT 1.11 in S5520SC'
	Validated on S5520HC, S5520HCV & S5520SC
	

v1.11 - 04/02/2009
	Release to support S5520XX Resource CD Only
	Validated on S5520HC, S5520HCV & S5520SC
	Updated the mkramdrive.efi tools

v1.10 - 03/09/2009
	Release to support S5520XX Resource CD Only
	Validated on S5520UR
	Updated the default package file.


v1.09 - 03/09/2009
	Release to support S5520VI Resource CD Only
	Validated on S5520VI


v1.08 - 02/13/2009
	Release to support S5520XX Resource CD
	Removed "(Gold)" from startup.nsh display (request from CD team)
	Updated DISPSTAT.DAT file
	Validated on S5520UR and S5520WB

v1.07 - 01/23/2009
	Release to support S5520XX Resource CD (Gold).
	Corrected text error in the startup.nsh file
	Added "MaxFanDomain = 2" to COMPREH.PKG
	Enabled NIC EEPROM Checksum test
	Updated DISPSTAT.DAT file
	Validated on S5520UR and S5520WB


v1.06 - 12/05/2008 
	Release to support S5520XX Resource CD (Gold).


v1.05 - 11/07/2008 
	Re-release to support S5520UR Resource CD (Silver).


v1.04 - 11/07/2008 
	Release to support S5520UR Resource CD (Silver).  Removed Comprehensive Loop test due to bug.  Issue being worked.


V1.03 - 10/24/2008
      - 'Comprehensive Test with Continuous Looping' is not supported for this release.
      - Fixed issue found not able to create RAM drive (FSZ:) on S5520SC. 
      - Updated to included the following modules:
	NPTM
	ICHx


v1.02 - 07/08/2008 
	Initial release to support S5520HC.
	 

System requirements:
	
	USB/PS2 Keyboard 
	EFI Shell must be first Boot Option

Known Issue:
- Please use USB flash drive to run PCT, the test will run direct from USB flash drive. 
  UEFIx64 CD image is not available at this time.
- The Comprehensive test and Comprehensive test with looping takes ~1 hour to configure.   

=============================================================================

