Intel® AD450NX Server Platform
The products you are looking for are no longer manufactured by Intel. Additionally, Intel no longer provides interactive support for these products via telephone or e-mail, nor will Intel provide any future content updates or software updates to support new operating systems or improve compatibility with third party devices and software products. THESE PRODUCT SUPPORT DOCUMENTS ARE PROVIDED FOR HISTORICAL REFERENCE ONLY AND ARE SUBJECT TO THE TERMS SET FORTH IN THE "TERMS OF USE" INFORMATION. Information on currently available Intel products is available at www.intel.com and/or developer.intel.com

Identify your products
  Product Discontinuance Announcement
    Intel® will no longer provide interactive support for these products via telephone or e-mail

Software and drivers
  BIOS/Firmware, drivers and utilities download

Technical specifications
  A450NX Board Specification Update
    An update to the specifications contained in the Technical Product Specification
    Specification Update [PDF]
  A450NX Board Technical Product Specifications
    Product overview, including descriptions and diagrams of the integrated features
    Technical Product Specifications [PDF]
  AD450NX System Specification Update
    An update to the specifications contained in the Technical Product Specification
    Specification Update [PDF]
  AD450NX System Technical Product Specifications
    Product overview, including descriptions and diagrams of the integrated features
    Technical Product Specifications [PDF]

Installation and use
  System Event Log Messages
    System Event Log [PDF]
  Quick Start Guide
    Product Guide [PDF]
  SCSI Software User Guide
    User Guide [PDF]
  Storage Solutions
    Storage Solutions [PDF]
  User's Guide
    Product Guide [PDF]

Compatibility
  Tested Hardware and Operating Systems
    Hardware and Software List [PDF]
  Tested Memory
    The system supports up to 8 GB of EDO/ECC system memory using two memory modules
    Tested Memory [PDF]
  Tested Processors
    The Intel® AD450NX Server Platform supports Intel® Pentium® II Xeon® processors (400 MHz or 450 MHz) and Intel® Pentium® III Xeon™ processors (500 MHz or 550 MHz).
    700 MHz Pentium® III Xeon processors are not supported.
    To support 550MHz, close pins 5-6, 7-8, and 9-10 on the Bus ratio jumper block (J31)