Intel® ISP1100 Internet Server Plaform
The products you are looking for are no longer manufactured by Intel. Additionally, Intel no longer provides interactive support for these products via telephone or e-mail, nor will Intel provide any future content updates or software updates to support new operating systems or improve compatibility with third party devices and software products. THESE PRODUCT SUPPORT DOCUMENTS ARE PROVIDED FOR HISTORICAL REFERENCE ONLY AND ARE SUBJECT TO THE TERMS SET FORTH IN THE "TERMS OF USE" INFORMATION. Information on currently available Intel products is available at www.intel.com and/or developer.intel.com

Identify your products
  Product Discontinuance Announcement
    Intel® will no longer provide interactive support for these products via telephone or e-mail

Software and drivers
  BIOS/Firmware, drivers and utilities download

Technical specifications
  Datasheet
    DS [PDF]
  Specification update
    An update to the specifications contained in the Technical Product Specification
    Specification Update [PDF]
  Technical Product Specifications
    Product overview, including descriptions and diagrams of the integrated features
    Technical Product Specifications [PDF]

Installation and use
  BIOS Console Redirection
    CONFIGSC [PDF]
  Front Mount Kit Guide
    FRONT_MOUNT [PDF]
  Headless Network Installation of Red Hat* Linux 6.2 SBE
    RHL6_2 [PDF]
  How to Install an OS by USB Floppy
    BIOS | Advanced | Floppy Configuration | Floppy A: | Disabled
    BIOS | Advanced | Floppy Configuration | Onboard Floppy Controller | Disabled
    BIOS | Advanced | USB Configuration | USB Mass Storage Device Configuration | Emulation type | Floppy
  Product Guide
    Product Guide [PDF]
  Quick Start Guide
    1100_QS [PDF]
  Rail Option Kit Installation Guide
    Rail Option Kit Installation Guide [PDF]
  SCSI Cable Option Kit
    CH_SCSI_KIT [PDF]
  Slimline CD-ROM/Floppy Drive Option Kit Installation Guide
    CH_SLIMLINE_KIT [PDF]

Compatibility
  Tested Hardware and Operating Systems
    Peripherals Manufacturer Model Description
    CD-ROM Teac* CD-224E-AP3 Slimline ATAPI IDE
    Teac CD-224E-AP4 Slimline ATAPI IDE
    Floppy Drive Mitsubishi* MF3555H-348MN Slimline 3.5" 1.44 MB
    Teac FD235HF-A429 3.5" 1.44 MB
    HDD IBM* Ultrastar36LZX 18.6 GB 10k rpm SCSI
    IBM Ultrastar36LZX 36.7 GB 10k rpm SCSI
    IBM Ultrastar DPSS-336950 36.7 GB 10k rpm SCSI
    IBM Ultrastar DPSS-318350 18.6 GB 10k rpm SCSI
    Quantum* Atlas V 9 GB Ultra 2 SCSI HDD
    Quantum Atlas V 18 GB Ultra 2 SCSI HDD
    Quantum LM15AP3E (Fireball) 15 GB EIDE
    Quantum LM30AP3E (Fireball) 30 GB EIDE
    Quantum LC07A011 (LCT15) 7.5 GB EIDE
    Samsung* SP0914D 9.1 GB EIDE
    Seagate* Aspen Barracuda3 20.4 GB, 7.2k rpm Ultra 100 IDE
    Seagate Aspen Barracuda3 30.6 GB, 7.2k rpm Ultra 100 IDE
    Seagate ST318203LW 18 GB Ultra 2 SCSI HDD
    Seagate ST39175LW 18 GB Ultra 2 SCSI HDD
    Seagate ST318275LW 18 GB Ultra 2 SCSI HDD
    Seagate ST310210A 10.2 GB EIDE
    Seagate ST318203LW 10.2 GB EIDE
    Seagate ST320420A 20.4 GB EIDE
    Seagate Barracuda ST310220A 10.2GB 7200 IDE
    Seagate ST330620A 30.6 GB Ultra100 IDE
    Seagate ST320414A 20.4GB 7200 IDE
    Western Digital* AC29100 9.1 GB EIDE
    Western Digital 205AA Caviar 20.5GB IDE
    Western Digital 307AA 30.7 GB IDE
    Graphics Adapter Matrox* Millennium G200 SD 8 MB SDRAM PCI
    ATI* Rage XL (Low Profile) (ACCGRFLP001) 8 MB
    SCSI Adapter Adaptec* AHA-2940U2W Ultra2 SCSI
    Adaptec AHA-3940UW Ultra SCSI
    Adaptec 29160LP Low Profile PCI Ultra 160 SCSI
    LSI Logic* SYM53C896 Dual Channel Ultra2 SCSI
    LSI Logic SYM22910 Dual Channel Ultra2 SCSI
    LSI Logic **SYM22902/2U64M2 Low Profile PCI Ultra2 SCSI dual channel
    LSI Logic **SYM22903/2U364M2 Low Profile PCI Ultra160/M SCSI dual channel
    Qlogic* QLA1040 Ultra SCSI
    Qlogic 29160 Ultra 160 SCSI
    Network Adapter Intel® PRO/100+ 10/100 Ethernet
    Intel PRO/1000 100/1000 Ethernet
    RAID Intel SRCU31L
    Low Profile Raid Adapter
    Mylex* AcceleRAID 160*** Raid Adapter
    Mylex AcceleRAID 170*** Raid Adapter
    Mylex Accele 150 Raid Adapter
    Mylex Accele 250 Raid Adapter
    Fibre Channel Adapter Qlogic QLA2000 Fibre Channel Host Adapter
  Tested PCI Video Adapters
    The PCI video adapters below have been verified to operate in VGA mode during system boot with Red Hat* Linux 6.1 and Windows NT* 4.0.
    Intel has not performed full compatibility, inter-operability, or stress testing on these adapters with the Intel® ISP1100 Internet Server Platform.
    Certain add-in PCI card device drivers require bus mastering to be set by the BIOS.
    ATI Xpert @ Work*, 8MB
    ATI Xpert @ Play 98*, 8MB
    Palit Daytona SiS 6326*, 4MB
    Sparkle* S3 Savage 4 GT*, 8MB
    Matrox* Millenium G200*, 8MB
    Gainward SiS 6326*, 4MB
  Tested Processors
    If using a boxed processor, remove the fan from the heatsink. Processors greater than 800 MHz require a special air baffle.

    Intel® Pentium® III Processors
    Speed | BIOS version
    850 MHz** | P14 or later
    800 MHz** | P14 or later
    750 MHz* | P14 or later
    700 MHz* | P14 or later
    650 MHz | P08 or later
    600 MHz | P08 or later
    550 MHz | P08 or later
    500 MHz | P08 or later
    Intel® Celeron™ Processors
    850 MHz** | P14 or later
    800 MHz** | P14 or later
    766 MHz* | P14 or later
    733 MHz | P08 or later
    700 MHz | P08 or later
    667 MHz | P08 or later
    633 MHz | P08 or later
    600 MHz | P08 or later
    566 MHz | P08 or later
    533 MHz | P08 or later
    500 MHz | P08 or later
    466 MHz | P08 or later
    433 MHz | P08 or later
    400 MHz | P08 or later

    ** An air baffle insert or a specific heat sink is required to support these processors. Please refer to TA-2003-3 and TA-2004-1.
    * An Air Baffle insert may be required to support theses processors. For additional information, see TA-2003-1.

Technical advisories
  Multiple-bit ECC memory errors
    TA-2000-1 [PDF]
  Support for Intel® cD0 Stepping
    TA-2004-1 [PDF]
  Support for Processor Speeds 800/850 MHz
    TA-2003-1 [PDF]
  Support for Processor Speeds above 700 MHz
    TA-2003-3 [PDF]