Intel® ISP2150 Internet Server Platform
The products you are looking for are no longer manufactured by Intel. Additionally, Intel no longer provides interactive support for these products via telephone or e-mail, nor will Intel provide any future content updates or software updates to support new operating systems or improve compatibility with third party devices and software products. THESE PRODUCT SUPPORT DOCUMENTS ARE PROVIDED FOR HISTORICAL REFERENCE ONLY AND ARE SUBJECT TO THE TERMS SET FORTH IN THE "TERMS OF USE" INFORMATION. Information on currently available Intel products is available at www.intel.com and/or developer.intel.com

Identify your products
  Product Discontinuance Announcement
    Intel® will no longer provide interactive support for these products via telephone or e-mail

Software and drivers
  BIOS/Firmware, drivers and utilities download

Technical specifications
  Technical Product Specifications
    Product overview, including descriptions and diagrams of the integrated features
    Technical Product Specifications [PDF]
  Specification Update
    An update to the specifications contained in the Technical Product Specification
    Specification Update [PDF]

Installation and use
  EMP "Always active" mode
    EMP can be configured for modem mode and either "always active" or "pre-boot only" in BIOS set-up. In "always active" mode, COM2 is not available to the OS. EMP will answer all calls to a modem connected to COM2. In "pre-boot only" mode, EMP will only be active while powered down, and during POST; making COM2 and the modem available to the OS.
  External SCSI Cable Installation Instuctions
    SCSI_CABLE [PDF]
  Installation and User Guide
    Installation and User's Guide [PDF]
  Mouse pointer looks like a 1/2" square
    If the mouse pointer looks like a 1/2" square, you cannot set the resolution properly, or there are thin lines throughout the display, use XFree86 3.3.6 or later and add "VideoRam 2048" and "option sw_cursor" to the /etc/X11/XF86Config file | Device | Cirrus Logic 5480
    The graphical installation will remain unusable. Install in TEXT Mode.
    The onboard video RAM chips for previous boards were a pair of 1MB chips. The newer boards use a single 2MB chip. The video chipset does not report the new memory size properly.
  Product Guide
    Product Guide [PDF]
  Quick Start Guide
    Quick Start Guide [PDF]

Compatibility
  Tested Hardware and Operating Systems
    Certain add-in PCI card device drivers require bus mastering to be set by the BIOS
    Tested Operating Systems
    Microsoft Windows* 2000
    Microsoft Windows NT* 4.0
    Red Hat* Linux 6.1
    Solaris* 7
    Tested Hardware [PDF]
  Tested Processors

    Pentium® III Processors
    Speed | BIOS version
    850 MHz | 12.1
    800 MHz | 11.1
    750 MHz | 11.1
    700 MHz | 9.2
    650 MHz | 9.2
    600E MHz | 9.2
    600 MHz | 9.2
    550 MHz | 9.2
    500 MHz | 9.2
    450 MHz | 9.2

Technical advisories
  TA 2002: Serial numbers not included in BIOS
    Chassis and System serial number not included in BIOS
    TA-2002-2 [PDF]
  TA 315: Do not run Server Diagnostic Utility under certain circumstances
    The Intel® Server Diagnostics Utility should not be run on systems configured with an Intel® SCSI RAID controller when installed in an Intel® server chassis having a hot-swap backplane.
    Technical Advisory [PDF]
  TA 402: ICP* RAID Controllers Require New Hot Swap Controller Firmware
    Technical Advisory [PDF]