Intel® OCPRF100 Server Platform
The products you are looking for are no longer manufactured by Intel. Additionally, Intel no longer provides interactive support for these products via telephone or e-mail, nor will Intel provide any future content updates or software updates to support new operating systems or improve compatibility with third party devices and software products. THESE PRODUCT SUPPORT DOCUMENTS ARE PROVIDED FOR HISTORICAL REFERENCE ONLY AND ARE SUBJECT TO THE TERMS SET FORTH IN THE "TERMS OF USE" INFORMATION. Information on currently available Intel products is available at www.intel.com and/or developer.intel.com

Identify your products
  Product Discontinuance Announcement
    Intel® will no longer provide interactive support for these products via telephone or e-mail

Software and drivers
  BIOS/Firmware, drivers, and utilities

Technical specifications
  Board Technical Product Specification
    Product overview, including descriptions and diagrams of the integrated features
    Technical Product Specifications [PDF]
  System Technical Product Specification
    Product overview, including descriptions and diagrams of the integrated features
    Technical Product Specifications [PDF]

Installation and use
  Intel® Server Control Installation Guide
    Installation Guide [PDF]
  Power Cord Specifications
    For North America, the cord must be UL Listed/CSA Certified, 14/3, 75°C type SJT with NEMA 6-15P attachment plug for 110 VAC operation and IEC 320, C19 input connector.
    For outside North America, the cord must be flexible VDE certified or HAR (harmonized) rated 250 V, 0.75 mm minimum conductor size with IEC 320, C19 input connector. The AC wall attachment plug shall be a three conductor grounding type and must be for the configuration in the specific region or country. The AC wall attachment plug must bear the safety agency certification mark for the specific region or country intended for installation.
    The cord must be no longer than 4.5 meters (14.76 ft.).
    The maximum power consumption expectations of the OCPRF100 MP Server System are as follows:
    12 Amp max while operating at 110 VAC.
    7 Amp max while operating at 220 VAC.
  Product Guide
    Product Guide [PDF]
  Quick Start Guide
    Quick Start Guide [PDF]
  Scalable Storage Solutions
    Scalable Storage Solutions [PDF]
  Server Platform Upgrade Procedure
    This document describes the technical procedures to upgrade the system hardware from a 4-way Intel® AC450NX to an 8-way Intel® OCPRF100
    Platform Upgrade Procedure [PDF]
  Symbios Logic SDMS software
    PCI SDMS 4.0 User Guide [PDF]

Compatibility
  Tested Processors
    The Intel® OCPRF100 MP Server Platform supports 500 MHz and 550 MHz Intel® Pentium® III Xeon® processors. It does not support 700 MHz processors.

Technical advisories
  TA 0329: Microsoft* Windows* 2000 may report less than 4GB memory
    TA-0329 [PDF]
  TA 0339: Installing NT 4.0 with more than 4Gb of memory
    TA-0339 [PDF]