This release note and the software that accompanies it are copyright (c) 2010, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

======================
Supported RAID Controllers
======================
Intel(R) Integrated RAID Module RMS2LL080 and RMS2LL040

Intel(R)  RAID Modules RMS2LL080/040 when inserted in below Intel(R) Server Boards and Systems:
 - S5520HC / S5520HCV, S5520SC,S5520UR,S5500WB,S3420GPC,S3420GPX

Please verify that this utility has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at http://support.intel.com.

=================
Package Information
=================
Driver Version = 5.00.02
OS supported = RHEL5(GA-U4), SLES10(GA-SP3), SLES11(GA); (both x86 & x64 versions for these OS versions)

This driver is intended for use with IR RAID 0/1/1E/10E configurations 
====================
Attention!
====================

It is important to follow instructions provided below for successfully installing SLES10/11 or RHEL5 operating systems onto RAID device.

Do not attempt to install the driver for SLES11 on SLES11 SP1. It may not work properly. A future release will contain the driver for SLES with the latest service pack.
SLES11SP1 can use the inbox driver until then.

================
Known Restrictions
================
N/A

====================
Contents in the package
====================
The following files are included in this package:

Driver package:
mpt2sas-05.00.02.00-2-rhel5.i686.rpm
mpt2sas-05.00.02.00-2-rhel5.x86_64.rpm
mpt2sas-05.00.02.00-2-sles10.i586.rpm
mpt2sas-05.00.02.00-2-sles10.x86_64.rpm
mpt2sas-05.00.02.00-2-sles11.i586.rpm
mpt2sas-05.00.02.00-2-sles11.x86_64.rpm

Diver RPM Source files:
mpt2sas-05.00.02.00-2.src.rpm

Floppy disk images for creating Installation disk(s):
mpt2sas-05.00.02.00-2-rhel5.1.i686.dd.gz
mpt2sas-05.00.02.00-2-rhel5.1.x86_64.dd.gz
mpt2sas-05.00.02.00-2-rhel5.2.i686.dd.gz
mpt2sas-05.00.02.00-2-rhel5.2.x86_64.dd.gz
mpt2sas-05.00.02.00-2-rhel5.3.i686.dd.gz
mpt2sas-05.00.02.00-2-rhel5.3.x86_64.dd.gz
mpt2sas-05.00.02.00-2-rhel5.4.i686.dd.gz
mpt2sas-05.00.02.00-2-rhel5.4.x86_64.dd.gz
mpt2sas-05.00.02.00-2-rhel5.5.i686.dd.gz
mpt2sas-05.00.02.00-2-rhel5.5.x86_64.dd.gz
mpt2sas-05.00.02.00-2-rhel5.i686.dd.gz
mpt2sas-05.00.02.00-2-rhel5.x86_64.dd.gz
mpt2sas-05.00.02.00-2-sles10.i586.dd.gz
mpt2sas-05.00.02.00-2-sles10.x86_64.dd.gz
mpt2sas-05.00.02.00-2-sles10sp1.i586.dd.gz
mpt2sas-05.00.02.00-2-sles10sp1.x86_64.dd.gz
mpt2sas-05.00.02.00-2-sles10sp2.i586.dd.gz
mpt2sas-05.00.02.00-2-sles10sp2.x86_64.dd.gz
mpt2sas-05.00.02.00-2-sles10sp3.i586.dd.gz
mpt2sas-05.00.02.00-2-sles10sp3.x86_64.dd.gz
mpt2sas-05.00.02.00-2-sles11.i586.dd.gz
mpt2sas-05.00.02.00-2-sles11.x86_64.dd.gz

================
Driver Installation Instructions
================

This updated driver can be applied using the normal OS installation options.

1 The purpose of this document is to provide clear instructions on how to install OS on drives attached to the Intel(R) IT/IR RAID controller or device.

2 Prepare Installation disk(s)
2.1 Driver files are available on the CD that shipped with the product or can be downloaded from http://support.intel.com. 
2.2 Create install disk(s)
The driver is provided as driver update disk (DUD) image (file extension is .img). To prepare the installation driver diskette, if user has a system with Microsoft Windows* operating system installed, a third party utility must be used to extract the DUD image to a floppy disk, for example, using rawrite utility; or users can use ĄźddĄŻ command under Linux or Sun Solaris* operating system to extract the DUD image to a floppy diskette. Below is the command format.

 dd if=<image_file_name> of= path-to-media 

On most systems, path-to-media is /dev/fd0, which is the floppy drive special file. User must identify the path-to-media if using USB floppy drive.


3 Installation methods
There are different types of installation possible with the installation package provided. Those are explained in different sections.

3.1 OS installation on RAID

This mode of installation is selected when user needs to install the Operating system on a fresh RAID configuration. For this kind of installation the driver update disc is used at the starting of the installation and the installer will update the system with driver images for the required kernels. Follow the procedure given below to install Intel(R) IT/IR RAID Stack at the time of Installation.

-----------------
3.1.1 Installing RHEL5 on RAID
-----------------

a) Insert floppy diskette created in step 2 into floppy drive
a) Boot to CD-ROM or DVD-ROM with OS Disk 1.
b) At the Linux installation prompt type: linux dd
c) Press <Enter> at the boot prompt on the Welcome screen.
d) Copy the Linux driver image from the Universal Driver Suite CD to diskette.
	Insert the diskette with driver image.
e) Select Yes. 
f) Scroll down to select the Intel RAID adapter driver. 
g) The utility locates and loads the driver for your device. 
h) Follow the Red Hat Linux installation procedure to complete the installation.
i) Reboot the system.

-----------------
3.1.2 Installing SLES10/11 on RAID
-----------------

a) Boot to CD-ROM or DVD-ROM with OS Disk 1.
b) When first screen come up press F5 key for SLES 10 or F6 key for SLES 9 to load a driver, then select installation menu option 
c) Insert DUD when it is prompted 
d) Follow the installation procedure to continue the OS installation. 
   Tips: press ALT+CTRL+F4 to see whether the driver is loaded. 

-----------------
3.2 Updating RHEL or SLES RAID driver on already installed system
-----------------

This method is used to update IT/IR RAID driver in a system, which is already installed with an older (or OS embedded) driver version. Here this procedure explains the manual process of updating the driver.  Follow the steps given to update driver.

1) Create RAID array on RAID Controller using Intel(R) IT/IR RAID Console Utility.
2) Boot the OS from primary controller/Disk.
3) Copy mptlinux rpm files to a temporary directory in the OS.
4) Query which version of the MPT driver is installed by running the command
	#rpm -qa | grep mpt2sas
5) (If result of step#4 is null, then skip this step.)Remove the bundled version of the MPT driver by running the command
	#rpm -e mpt2sas-<version>-<os>
6) Install the new version of the MPT driver by running the command
	#rpm -ivh mpt2sas-<version>-<release>-<os>.<arch>.rpm
7) Run command line
	#lsmod
to check if mptsas has been loaded successfully.
8) Run command line
	#modinfo mptsas
to make sure that the mptsas driver version has been updated
9) Completed.

================
Known Bugs
================
N/A

================
Fixes/Updates
================
Version 5.00.02
Initial release for RMS2LL080 and RMS2LL040 modules


*Other names and brands may be claimed as the property of others.
