================================================================================
Intel(R) Server Boards S5000PAL and S5000XAL BIOS RELEASE NOTES
================================================================================
INTEL Enterprise Products and Services Division
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : April 23, 2010
TO      : Intel(R) Xeon(R) Processor-Based Server Platform customers
SUBJECT : BIOS Release notes for version R0099
================================================================================
                           LEGAL INFORMATION
================================================================================

Information in this document is provided in connection with Intel Products
and for the purpose of supporting Intel developed server boards and systems.
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation 
may have patents or pending patent applications, trademarks, copyrights, or
other intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any such
patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 

*Other names and brands are the property of their respective owners.

Copyright (C) 2010 Intel Corporation.

================================================================================
                              ABOUT THIS RELEASE
================================================================================
Build Stamp : S5000.86B.14.00.0099.03092010
Build Date  : March 09, 2010

================================================================================
                           BIOS COMPONENTS/CONTENTS
================================================================================
Processors supported: 
 Intel(R) Xeon(R) Processor 5000 series w/ 533Mhz/667Mhz/1066Mhz FSB
 Intel(R) Xeon(R) Processor 5100 series w/ 1066Mhz/1333Mhz FSB
 Intel(R) Xeon(R) Processor 5200 series w/ 1066Mhz/1333Mhz FSB
 Intel(R) Xeon(R) Processor 5300 series w/ 1066Mhz/1333Mhz FSB
 Intel(R) Xeon(R) Processor 5400 series w/ 1066Mhz/1333Mhz FSB

Microcode update versions:
CPUID   Version Status  
0F64h   02      Production
0F65h   08      Production
06F6h   CD      Production 
06F7h   69      Production 
06FBh   B9      Production 
10676   60C     Production
1067A   A07     Production

On-Board Component Option ROM Versions:
ATI RN50 VGA    	: BK-ATI YJ20234a VER008.005.023.000	 
PXE Ver.        	: Intel(R) Boot Agent GE v1.2.45
ESB2 Option ROM 	: v A.08.09161334I
ESB2 AHCI Option ROM	: iSrc 1.08 09252006

Memory Reference Code Version:  1.32

================================================================================
                       SYSTEM FIRMWARE REQUIREMENTS
================================================================================
BMC 66
S5000PAL, S5000XAL	FRUDSR FAL_48
EEPROM v03.01
HSC V2.08
================================================================================
                           INSTALLATION NOTES
================================================================================

WARNING:  It is very important to follow these instructions as they are written.
Failure to update using the proper procedure may cause damage to your system.

Update BIOS using bootable USB Flash Drive:

Updating from BIOS revisions R0038 or earlier:
NOTE:  This operation will update both banks of the flash part.  This is necessary
as the Setup options from R0038 and earlier are not compatible with R0039 and later.

NOTE:  BIOS Bank Select jumper needs for be in Normal mode (2-3) during this whole
procedure.

1)  Download release package and extract contents to USB Flash Drive
2)  Verify that the R0099.CAP, BIOS99.BAT and IFLASH32.EXE files are present
    on the USB Flash drive
3)  Verify that BIOS Bank Select Jumper is set to Normal mode (2-3).
4)  Power system on and boot to USB Flash Drive
5)  At the command prompt type "BIOS99".
6)  Flash update should complete within 3 minutes
7)  Shut down the system but leave it connected to AC power
8)  Clear CMOS by moving the Clear CMOS jumper to the clear position and back.
9)  Boot system and enter BIOS Setup by pressing the F2 Key during POST
10) Verify BIOS string
11) Press F9 to load defaults
12) Press F10 to save and reset the system.
13) Power system on and boot to USB Flash Drive
14) At the command prompt type "BIOS99".
15) Flash update should complete within 3 minutes
16) Reboot system and enter BIOS Setup by pressing the F2 Key during POST
17) Verify BIOS string
 

Updating from BIOS revisions R0039 or later:
NOTE:  This operation will only update one bank in the flash part.  This is
recommended in case of a flash update failure that the system can be easily
recovered.

NOTE:  BIOS Bank Select jumper needs for be in Normal mode (2-3) during this
whole procedure.

1) Download release package and extract contents to USB Flash Drive
2) Verify that the R0099.CAP, BIOS99.BAT and IFLASH32.EXE files are present
   on the USB Flash drive
3) Verify that BIOS Bank Select jumper is set to Normal mode (2-3).
4) Power system on and boot to USB Flash Drive
5) At the command prompt type "BIOS99".
6) Flash update should complete within 3 minutes
7) Reboot system and enter BIOS Setup by pressing the F2 Key during POST
8) Verify BIOS string


================================================================================
                        BIOS RECOVERY INSTRUCTIONS
================================================================================

BIOS Recovery is not supported. 

Rolling BIOS is supported.

================================================================================
                            KNOWN ISSUES/WORKAROUNDS
================================================================================

-Video mode is set to 80x25 until BIOS defaults are loaded

-PAE mode and the equivalent Linux mode must be set to see > 2.5GB of memory.

NOTE:  Intel(R) Xeon(R) Processor 5100 series DO NOT support Hyper-Threading.
       The OS will only show 2 CPU threads per physical processor installed.
       Intel(R) Xeon(R) Processor 5300 series DO NOT support Hyper-Threading.
       The OS will only show 4 CPU threads per physical processor installed.
NOTE:  BIOS Setup shows the number of physical processors installed and not the
       number of processor cores. For example, when 2 Intel(R) Xeon(R)
       Processor 5100 series are installed, BIOS POST and Setup will only show 2 processors. 

-THIS BIOS ONLY SUPPORTS BETA OR LATER HARDWARE.
 DO NOT APPLY THIS BIOS TO ALPHA HARDWARE.

-IF CMOS IS CLEARED, IT MUST BE CLEARED PER THE INSTALLATION INSTRUCTIONS.

-When two Intel(R) Xeon(R) 5100 series processors are installed,
 an NMI error may appear during POST after updating from BIOS R0054 or earlier
 to BIOS releases after R0054.  This is expected and due to a change in the way
 errors are handled in the newer BIOS release. Perform a full DC power cycle
 (front panel power off and power on) to prevent this message from appearing again.

-As of BIOS R0065, may encounter a system reset upon first boot if previous
 NVRAM corruption has been found.

-As of BIOS R0077, Case Sensitivity support has been added to BIOS Admin/User password.
 If a password was installed using previous BIOS release without Case Sensitivity,
 enter old password in all lower case and then re-install password for proper Case Sensitivity.


================================================================================
                              FEATURES ADDED/REMOVED
================================================================================
-As of BIOS R0052, DIMMs with outdated AMB (Advanced Memory Buffer) component
 present are no longer supported. The system will halt with 3 beeps at POST code
 0xEA to indicate an "Unsupported AMB" error.

-As of BIOS R0056, removed support for Pre-production CPU steppings of the
 Dual-Core Intel(R) Xeon(R) Processor 5000 series.
 This includes processors with CPUID 0F61h, 0F62h, 0F63h.

-As of BIOS R0077, removed support for Pre-production CPU steppings of the
 Dual-Core Intel(R) Xeon(R) Processor 5100 series and Quad-Core Intel(R) Xeon(R)
 Processor 5300 series.
 This includes processors with CPUID 06F4h, 06F5h.

-As of BIOS R0081, removed support for Pre-production CPU steppings of the
 Dual-Core Intel(R) Xeon(R) Processor 5100 series and Quad-Core Intel(R) Xeon(R)
 Processor 5300 series.
 This includes processors with CPUID 06F9h.


================================================================================
                              FIXED ISSUES
================================================================================

================================================================================
                                R0099
================================================================================
 - Fixed "power -on -console" command cannot work for SOL
 - Fixed BIOS98 boot order issue 
 - Fixed BIOS Flash Corruption Exposure

OTHER:
 - Fixed System Date does not revert to year 2000 with invalid date set.
 - Microcode Update - CTN/WDC - G-Step
 - SMRR Implementation 
 - Update to CSM v2.60

================================================================================
                               R0098
================================================================================
 - Fixed PCI SERR, device 0x10, function 2, pn PCI Bus 0

OTHER:
 - Updated SMM memory utilization
 - Corrected some SMRR bit locks
 - Increase PCIe completion timeouts for supported devices.
 
================================================================================
                                R0096
================================================================================
 - Fixed BIOS88/91 incorrect UQI value for new BIOS setting.
 - Fixed Microsoft* Windows* 2008 Blue Screen with mixed stepping Intel(R) Xeon(R) Processor 5400 Sequence (C0 & E0).
 - Fixed "Kernel-Processor-Power" System Event Viewer Errors (if Geyserville is disabled).

OTHER:
 - Fixed APs contending for Semaphore during microcode load.
 - Added update to LSI SATA SW RAID OpRom v A.08.09161334I.

================================================================================
                                R0094
================================================================================
 - Fixed Midplane2 beep sound during POST for S5000PAL/S5000XAL.
 - Fixed System won't POST with some Gigabit LAN adapters installed in x8 slots.
 - Fixed Fixed BIOS89 failure on Platform Compatibility Test (PCT) for S5000PSL and S5000PAL.
 - Fixed Issue with BIOS91 and the Intel Xeon Processors 5400 Series E-0.
 - Fixed Intel Xeon Processor E5405 power down issue.
 - Fixed NMI and SEL log policy for Fatal and Non Fatal Memory Errors.

OTHER:
 - Added workaround for the board signal integrity issue requiring a manufacturing change for some products.  Note this workaround may be used on both older and newer motherboards.
 - Add Qimonda* AMB patch to MRC 1.32 in efforts to reduce M1Err(s).
 - Improve remote console performance at 9600 baud rate.
 - Update to LSI* SATA SW RAID OpRom v A.07.05151334I.

================================================================================
                                R0091_6
================================================================================
S5000PAL, S5000XAL:
- Fixed: NMIs seen during POST with BIOS91 and E0 Intel Xeon Processor L5400 Series 
================================================================================
                                R0091
================================================================================
================================================================================
S5000PAL, S5000XAL:
  - Fixed "Kernel-Processor-Power" System Event Viewer Errors
  - Fixed: Serial Console redirection is available even if COM ports are disabled
  - Fixed: Event Log in  OS Displays PPM Disabled Error Event with E5310  
  - Fixed: Serial Over LAN (SOL) corruption on BIOS R0086->R0089

OTHER:
  -      Added E-0  Intel Xeon Processor L5400 Series/ Intel  Xeon DP Processor  microcode (A07)
  -      Updated  Intel Xeon Processor L5400 Series/ Intel  Xeon DP Processor microcode (60C)
  -      Add BIOS selectable option to do a hard reset on NMI
  -      Serial Over LAN (SOL) corruption on BIOS R0086->R0089 

================================================================================
                                R0089
================================================================================
S5000PAL, S5000XAL:
  -   Server fails to NMI on Uncorrectable Errors

OTHER:
  -      Enable QR Support in MRC
  -      Added Verb Table for RealTek Alc262 Audio Codec
  -      BIOS menuing issue with listbox
  -      Update Copyright Year in BIOS Setup Screen
  -      Update LSI SATA SW RAID OpRom v. a_02151557i
  -      Mask replay timeout errors for ATI Video Card
  -      NVRAM corruption problem with boutil /f
  -      Fix WinPE Boot from USB key failure
================================================================================
                                R0088
================================================================================
S5000PAL, S5000XAL:
  -      [X] BIOS84 Incorrect MP table entries
  -   BIOS needs to program SSVID on LSI 1078 MP2



OTHER:
  -     Add setup option to enable/disable USB device moving to top of Boot Order
  -     CCB 481 - ID for files modified with AMIBCP
  -     Add FW_VERSION structure to NV Storage area
  -     Support changing OEMID and OEM TableID with AMIBCP
  -     WBINVD issue, need to increase AP timeout

================================================================================
                                R0087
================================================================================
S5000PAL, S5000XAL:
 -  [WHQL] Windows Server 2008 OS Install fails with BIOS 86


================================================================================
                                R0086
================================================================================
S5000PAL, S5000XAL:
 -  [x] want to boot Pata over Sata (Legacy Mode)



OTHER:
  -     Add SLP 2.0 Support
  -     Add AMISLP support for SLP 2.0
  -     WHEA - Error Record Serialization misinterpreted by WS 2008
  -     Overlapping Memory Area fixed in PCI 3.0 implementation
  -     Support Infiniband Boot Type
  -     Not all possible P-states made available for 
  -     Sync SLIC (SLP) Table ID with Platfrom ID
  -     Boot Order Retrofit (internal CCB)
  -     Server hangs under certain COM connection conditions
  -     Microcode Update(s)
	06F6h   CD 
	06F7h   69
	06FBh   B7
	10676   60B

================================================================================
                                R0085
================================================================================
S5000PAL, S5000XAL:
 -      [x] Disabling NIC opROM and I/O Module opROM disabled console redirection
 -      D1 AMB DIMM component errata must have BIOS MRC workaround
 -      Need to remove SAS SWRAID on MP2 (w/1078 chip)
  
OTHER:
  -     Performance anomolies in slot4 with Springports and EIRQ enabled
  -     Northbridge shutting down PCIe link with plx device 8533 installed
  -     Trouble entering opROMs that trap int 19
  -     Genuine M15ERR (Accompanied by M13ERR) should have SEL log
  -     Support for Harbison Refresh-2 Board
  -     Use HECBASE to determine PCIE Base Addrs (Fix IBIST errors)
  -     Update Memory Reference code to 1.32
  -     Enable Video controller
  -     CSM Payload changes
================================================================================
                                R0084
================================================================================
32340 	System will not boot with max memory (8x  4gig DIMMs- 32gigs)  

================================================================================
                                R0083
================================================================================
S5000PAL:
 -     HW RAID configuration not found after reboot
 -     DMIEDIT failure
 -     MP Table Update

OTHER:
    -	Overheating DIMMs in CLTT
    -   AMIBCP Boot Order Support

================================================================================
                                R0082
================================================================================
S5000PAL, S5000XAL:
  -     Rollback to OLTT does not happen with CLTT incapable DIMM
  -     [X] want to boot PATA above SATA

S5000PHB, T5000PAL:
   -    Green status LED driven active in standby (DC Off)
   -    Harbison Ophir Legacy IRQ routing
   -   Add DP support for Harbson refresh

OTHER:
    -	Add back Altitude Bios Setup Option when OLTT selected
    -   Deep C-State support causes W2K3 without service pack to fail
    -   Add Windows Hardware Error Architecture (WHEA) support
    -   Update Memory Reference code to 1.30
    -   Add Half Ratio support for the processor
    -	Add 10676h C-0 processor microcode patch for DP

================================================================================
                                R0081
================================================================================
S5000PAL, S5000XAL:
  -	EFI shell environment variables running out of buffer space
  -     POST screen shows 2 garbage lines in BMC Forced Update Mode

S5000PHB, T5000PAL:
 -     BMC Force Update Mode Does not enter BIOS Setup
 -     [X] SLES10 w/SP1 failed to boot w/PCIE HCA installed
 -     Fail to install WIN 2KADV Server w/SP1 


OTHER:
    -	BIOS String Update "Add new CC3 requirements"
    -   Errata 100: ESB2 PCIe switch mis-formats TLPs
    -   MP Routing/Table Fixes
    -   Fix video corruption on Main tab in BIOS Setup w/console redir enabled
    -   Fix Unrecoverable Error Handling problems
    -   Fix kernel panic in Linux with throttled processors
    -   Loading user defaults loads invalid option on the boot order page
    -   Fixed garbled text in BIOS Setup at 115K baud w/console redir
    -   Workaround for DTX PCI-X add-in card blue screen failure.
    -   TPM Status appears in BIOS Setup on boards without TPM.
    -   Update ESB2 RAID OpRom to vA.01.07101204I
    -   Enable fake MSI for S5000PSL Slot4
    -   Add support of depop SKU based off of S5000PSL
    -   WHQL test failure on I/O Port 161 and 162
    -	Add 06F6h B-2 processor microcode patch M046F6C9 
    -	Add 06F7h B-3 processor microcode patch M406F767 
    -   Allow B-step/G-step mixed stepping for 5100 and 5300 series processors


[END OF RELEASE NOTES]



[END OF RELEASE NOTES]
