//****************************************************************************
//                   INTEL CORPORATION PROPRIETARY INFORMATION
//       This software is supplied under the terms of a license agreement or
//       nondisclosure agreement with Intel Corporation and may not be copied
//       or disclosed except in accordance with the terms of that agreement.
//         Copyright (c) 2009-2010 Intel Corporation. All Rights Reserved.
//****************************************************************************
//
// Sensor data based on the rev 2.2 SDR spreadsheet
// Do not load this file into SDR Create and then save it to source control.
// SDR Create removes all comments and does not like fields indicating
// IPMI rev 2.0 support.
//


//
// File Header Information
//

_LF_NAME       'BC_BMC.SDR'
_LF_VERSION    '0.21'
_LF_FMT_VER    '1.50'
_IPMI_VERSION  '2.00'

//
// SDR Header Information
//

_SDR (
_START_ADDR    0000
_DATA_LEN      0000
_NVS_TYPE      'IMBDEVICE'
_DEV_BUS       FF
_DEV_ADDRESS   20


//====================================================================//
// (1) Fans
//====================================================================//
// _SDR_TAG       'CPU1_TACH' // This is the option process 1 FAN tech/present for SC5650DP/SC5650BRP chassis.
// _SDR_TAG       'CPU2_TACH' // This is the standard process 2 FAN tech/present for SC5650DP/SC5650BRP chassis.

// _SDR_TAG       'SYS_1_TACH_PP5' // This is the standard system 1 FAN tech/present for SC5650DP/SC5650BRP chassis.
// _SDR_TAG       'SYS_2_TACH_PP5' // This is the standard system 2 FAN tech/present for SC5650DP/SC5650BRP chassis.
// _SDR_TAG       'SYS_3_TACH_PP5' // This is the standard system 3 FAN tech/present for SC5650DP/SC5650BRP chassis.

// _SDR_TAG       'SYS_1_TACH_HJ2' // This is the standard system FAN 1 tech/present for SR1630BC chassis.
// _SDR_TAG       'SYS_2_TACH_HJ2' // This is the standard system FAN 2 tech/present for SR1630BC chassis.

// _SDR_TAG       'SYS_1_TACH_Other' // This is the standard system FAN 1 tech/present for Other chassis.
// _SDR_TAG       'SYS_2_TACH_Other' // This is the standard system FAN 2 tech/present for Other chassis.
// _SDR_TAG       'SYS_3_TACH_Other' // This is the standard system FAN 3 tech/present for Other chassis.

// _SDR_TAG       'SYS_1_TACH_FCT' // This is the standard system FAN 1 tech/present for FCT.
// _SDR_TAG       'SYS_2_TACH_FCT' // This is the standard system FAN 2 tech/present for FCT.
// _SDR_TAG       'SYS_3_TACH_FCT' // This is the standard system FAN 3 tech/present for FCT.


//====================================================================//
// (2) Temperature Sensors
//====================================================================//
// _SDR_TAG	  'FP_TEMP' // This is the option front panel temperature sensor for SR1630BC, SC5650DP and SC5650BRP chassis.

// _SDR_TAG       'PROC_1_TEMP' // This is the detect Processor 1 Therm Margin sensor/Prochot Sensor 1 for SR1630BC,SC5650DP and SC5650BRP chassis.
// _SDR_TAG       'PROC_2_TEMP' // This is the detect Processor 2 Therm Margin sensor/Prochot Sensor 2 for SR1630BC,SC5650DP and SC5650BRP chassis.



//====================================================================//
// (3) Chassis Intrusion
//====================================================================//
// _SDR_TAG       'INTRUSION' // chassis intrusion
// _SDR_TAG       'NO_INTRUSION' // no chassis intrusion

//====================================================================//
// (4) Processor Detection
//====================================================================//
// _SDR_TAG       'PROC_1'  // This is the +1.1V P1 Vccp/+1.5V P1 DDR3/P1 Status/P1 VRD Temp/MEM P1 THRM MRGN sensors for SR1630BC,SC5650DP and SC5650BRP chassis.
// _SDR_TAG       'PROC_2'  // This is the +1.1V P2 Vccp/+1.5V P2 DDR3/MEM P2 THRM MRGN /P2 Therm Margin/P2 Therm Ctrl %/P2 Status/P2 VRD Temp sensors for SR1630BC,SC5650DP and SC5650BRP chassis.


//====================================================================//
// (5) Power supply
//====================================================================//
// _SDR_TAG       'SC5650BRP_PS1' // This is the standard power supply 1 status/input power/Output Current/Temperature sensor for SC5650BRP chassis.
// _SDR_TAG       'SC5650BRP_PS2' // This is the standard power supply 2 status/input power/Output Current/Temperature sensor for SC5650BRP chassis.

// _SDR_TAG       'REDUNDANT_PS2' // This is the option power unit redundancy sensor for SC5650BRP chassis.


//====================================================================//
// (6) FRU 
//====================================================================//
// _SDR_TAG       'FP_FRU' // This is the standard front panel FRU record for SR1630BC,SC5650DP and SC5650BRP chassis.
// _SDR_TAG       'PDB_FRU' // This is the PDB FRU record for SC5650BRP chassis.
// _SDR_TAG       'PS1_FRU' // This is the Power supply 1 FRU record for SC5650BRP chassis.
// _SDR_TAG       'PS2_FRU' // This is the Power supply 2 FRU record for SC5650BRP chassis.


//====================================================================//
// (7) backplane temp 
//====================================================================//
// _SDR_TAG       'P_R26BPE' // This is using for P_R26BPE HSC backplane temp/status/present sensors.
// _SDR_TAG       'P_R26BP' // This is using for P_R26BP HSC backplane temp/status/present sensors.

//====================================================================//
// (8) Factory sensors
//====================================================================//
// _SDR_TAG       'SHIP'                // SDRs for Shippings
// _SDR_TAG       'FCT'                 // SDRs for Functional Test (FCT)

//====================================================================//
// (9) Interrupt sensors
//====================================================================//
// _SDR_TAG       'FP_NMI'             //Front panel NMI button


//*******************************************************
// SDR Type 01&02 Records
//*******************************************************
_SDR_TYPE      02
_REC_LEN       002F

   // Sensor Record Header
   0001               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID
   01                 // Entity Instance
   63                 // Sensor Initialization
   40                 // Sensor Capabilities
   09                 // Sensor Type
   6F                 // Event / Reading Base Type
   7100               // Assertion Event Mask
   7100               // Deassertion Event Mask
   7100               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Pwr Unit Status'  // String Bytes
//=========================================================================//

_SDR_TYPE      02
_SDR_TAG       'REDUNDANT_PS2'
_REC_LEN       002F

   // Sensor Record Header
   0002               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   02                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   09                 // Sensor Type
   0B                 // Event / Reading Base Type
   FF00               // Assertion Event Mask
   FF00               // Deassertion Event Mask
   FF00               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Pwr Unit Redund' // String Bytes
//=========================================================================//
_SDR_TYPE      02
_REC_LEN       002D

   // Sensor Record Header
   0003               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   63                 // Sensor Initialization
   40                 // Sensor Capabilities
   23                 // Sensor Type
   6F                 // Event / Reading Base Type
   0F01               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0F01               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'IPMI Watchdog'    // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG       'NO_INTRUSION'
_REC_LEN       002E

   // Sensor Record Header
   0004               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   05                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask
   1000               // Deassertion Event Mask
   1000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Physical Scrty'   // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG       'INTRUSION'
_REC_LEN       002E

   // Sensor Record Header
   0005               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   05                 // Sensor Type
   6F                 // Event / Reading Base Type
   1100               // Assertion Event Mask   --Chassis intrusion/LAN leash lost 1 =1100
   1100               // Deassertion Event Mask --Chassis intrusion/LAN leash lost 1 =1100
   1100               // Reading Mask & Settable / Readable Threshold Masks --Chassis intrusion/LAN leash lost 1 =1100
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Physical Scrty'   // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG       'FP_NMI'
_REC_LEN       002F

   // Sensor Record Header
   0006               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   05                 // Sensor Number 

   // Record Body Bytes
   0C                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   13                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0100               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'FP NMI Diag Int'  // String Bytes
//=========================================================================//
_SDR_TYPE      02
_REC_LEN       002B

   // Sensor Record Header
   0007               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   41                 // Sensor Capabilities
   F3                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'SMI Timeout'      // String Bytes
//=========================================================================//
_SDR_TYPE      02
_REC_LEN       0030

   // Sensor Record Header
   0008               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   07                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   03                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   10                 // Sensor Type
   6F                 // Event / Reading Base Type
   0400               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0400               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'System Event Log' // String Bytes
//=========================================================================//   
_SDR_TYPE      02
_REC_LEN       002C

   // Sensor Record Header
   0009               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   08                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   04                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   12                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   1000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'System Event'     // String Bytes
//=========================================================================//      
_SDR_TYPE      02
_REC_LEN       0026

   // Sensor Record Header
   000A               // Record ID
   51                 // SDR Version
   02                 // Record Type
   21                 // Record Length
 
   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   09                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   05                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   14                 // Sensor Type
   6F                 // Event / Reading Base Type
   0500               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0500               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'Button'           // String Bytes
//=========================================================================// 
_SDR_TYPE      01
_REC_LEN       003C

   // Sensor Record Header
   000B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   10                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID				-- (system board)
   06                 // Entity Instance
   7B                 // Sensor Initialization			-- (7B = Initial All)
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   B8                 // M
   40                 // M, Tolerance
   44                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   B2                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   EB                 // Nominal Reading			-- (E7h = 1.085 Volt)
   F2                 // Normal Maximum				-- (EEh = 1.118 Volt)
   E3                 // Normal Minimum				-- (EOh = 1.052 Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = Volt)
   00                 // Sensor Minimum Reading			-- (0h = 0Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable			
   FC                 // Upper critical				-- (F8h = 1.165 Volt)
   F5                 // Upper non-critical			-- (F1h = 1.132 Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable				
   DA                 // Lower critical				-- (D6h = 1.005 Volt) 
   E0                 // Lower non-critical			-- (DDh = 1.038 Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'BB +1.1V IOH'     // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'PROC_1'
_REC_LEN       0040

   // Sensor Record Header
   000C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   11                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   07                 // Entity Instance
   7B                 // Sensor Initialization			-- (7B = Initial All)
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   3D                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   B3                 // Nominal Reading			-- (BOh = 1.091Volt)
   F2                 // Normal Maximum				-- (EEh = 1.475Volt)
   74                 // Normal Minimum				-- (73h = 0.713Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = 1.581Volt)
   00                 // Sensor Minimum Reading			-- (00h = 0 Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable			
   FC                 // Upper critical				-- (F8h = 1.538Volt)
   F5                 // Upper non-critical			-- (F1h = 1.494Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   6F                 // Lower critical				-- (6Dh = 0.675Volt)
   73                 // Lower non-critical			-- (71h = 0.700Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.1V P1 Vccp' // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'PROC_2'
_SDR_TAG       'FCT'
_REC_LEN       0040

   // Sensor Record Header
   000D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   12                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   08                 // Entity Instance
   7B                 // Sensor Initialization			-- (7B = Initial All)
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   3D                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   B3                 // Nominal Reading			-- (BOh = 1.091Volt)
   F2                 // Normal Maximum				-- (EEh = 1.475Volt)
   74                 // Normal Minimum				-- (73h = 0.713Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = 1.581Volt)
   00                 // Sensor Minimum Reading			-- (00h = 0 Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable			
   FC                 // Upper critical				-- (F8h = 1.538Volt)
   F5                 // Upper non-critical			-- (F1h = 1.494Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   6F                 // Lower critical				-- (6Dh = 0.675Volt)
   73                 // Lower non-critical			-- (71h = 0.700Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.1V P2 Vccp' // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'PROC_1'
_REC_LEN       0040

   // Sensor Record Header
   000E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   13                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   09                 // Entity Instance
   3E                 // Sensor Initialization			-- (7B = Initial All)
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   41                 // M
   00                 // M, Tolerance
   BA                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   CF                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   E6                 // Nominal Reading			-- (E3h = 1.498Volt)
   F2                 // Normal Maximum				-- (EEh = 1.570Volt)
   DB                 // Normal Minimum				-- (D7h = 1.419Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = Volt)
   00                 // Sensor Minimum Reading			-- (h = Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   FC                 // Upper critical				-- (F8h = 1.636Volt)
   F5                 // Upper non-critical			-- (F1h = 1.590Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   D2                 // Lower critical				-- (CEh = 1.359Volt)
   D8                 // Lower non-critical			-- (D5h = 1.405Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5V P1 DDR3' // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'PROC_2'
_SDR_TAG       'FCT'
_REC_LEN       0040

   // Sensor Record Header
   000F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   14                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   0A                 // Entity Instance
   3E                 // Sensor Initialization			-- (7B = Initial All)
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   41                 // M
   00                 // M, Tolerance
   BA                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   CF                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   E6                 // Nominal Reading			-- (E3h = 1.498Volt)
   F2                 // Normal Maximum				-- (EEh = 1.570Volt)
   DB                 // Normal Minimum				-- (D7h = 1.419Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = Volt)
   00                 // Sensor Minimum Reading			-- (h = Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   FC                 // Upper critical				-- (F8h = 1.636Volt)
   F5                 // Upper non-critical			-- (F1h = 1.590Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   D2                 // Lower critical				-- (CEh = 1.359Volt)
   D8                 // Lower non-critical			-- (D5h = 1.405Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5V P2 DDR3' // String Bytes
//=========================================================================//
_SDR_TYPE      01
_REC_LEN       003C

   // Sensor Record Header
   0010               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   15                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   0B                 // Entity Instance
   7B                 // Sensor Initialization			
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   4D                 // M
   00                 // M, Tolerance
   7F                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   EB                 // Nominal Reading			-- (E8h = 1.786Volt)
   F2                 // Normal Maximum				-- (EFh = 1.840Volt)
   E4                 // Normal Minimum				-- (E1h = 1.732Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = Volt)
   00                 // Sensor Minimum Reading			-- (0h = 0Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   FC                 // Upper critical				-- (F8h = 1.909Volt)
   F5                 // Upper non-critical			-- (F1h = 1.855Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   DB                 // Lower critical				-- (D8h = 1.663Volt)
   E1                 // Lower non-critical			-- (DEh = 1.709Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'BB +1.8V AUX'     // String Bytes
//=========================================================================//
_SDR_TYPE      01
_REC_LEN       0038

   // Sensor Record Header
   0011               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   16                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   0C                 // Entity Instance
   7B                 // Sensor Initialization			
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   8F                 // M
   00                 // M, Tolerance
   D7                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   E5                 // Nominal Reading			-- (E1h = 3.285Volt)
   F0                 // Normal Maximum				-- (EDh = 3.460Volt)
   D9                 // Normal Minimum				-- (D6h = 3.1244Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = Volt)
   00                 // Sensor Minimum Reading		
//------------------------------------------------------------------//	
   00                 // Upper non-recoverable
   FC                 // Upper critical				-- (F8h = 3.620Volt)
   F5                 // Upper non-critical			-- (F1h = 3.518Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   CF                 // Lower critical				-- (CCh = 2.9781Volt)
   D5                 // Lower non-critical			-- (D2h = 3.066Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'BB +3.3V'         // String Bytes
//=========================================================================//
_SDR_TYPE      01
_REC_LEN       003D

   // Sensor Record Header
   0012               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   17                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   0D                 // Entity Instance
   7B                 // Sensor Initialization			
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   8F                 // M
   00                 // M, Tolerance
   D7                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   E5                 // Nominal Reading			-- (E1h = 3.285Volt)
   F0                 // Normal Maximum				-- (EDh = 3.460Volt)
   D9                 // Normal Minimum				-- (D6h = 3.1244Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = Volt)
   00                 // Sensor Minimum Reading		
//------------------------------------------------------------------//	
   00                 // Upper non-recoverable
   FC                 // Upper critical				-- (F8h = 3.620Volt)
   F5                 // Upper non-critical			-- (F1h = 3.518Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   CF                 // Lower critical				-- (CCh = 2.9781Volt)
   D5                 // Lower non-critical			-- (D2h = 3.066Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BB +3.3V STBY'    // String Bytes
//=========================================================================//
_SDR_TYPE      01
_REC_LEN       003D

   // Sensor Record Header
   0013               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   18                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   0E                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   82                 // M
   00                 // M, Tolerance
   41                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   E6                 // Nominal Reading			-- (E2h = 2.983Volt)
   F1                 // Normal Maximum				-- (EDh = 3.128Volt)
   C3                 // Normal Minimum				-- (C0h = 2.534Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = Volt)
   00                 // Sensor Minimum Reading			-- (00h = 0Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   FC                 // Upper critical				-- (F8h = 3.273Volt)
   F5                 // Upper non-critical			-- (F1h = 3.181Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   A7                 // Lower critical				-- (A4h = 2.164Volt)
   C0                 // Lower non-critical			-- (BDh = 2.494Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BB +3.3V Vbat'          // String Bytes
//=========================================================================//   
_SDR_TYPE      01
_REC_LEN       0038

   // Sensor Record Header
   0014               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   19                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   0F                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   E3                 // M
   00                 // M, Tolerance
   4A                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   E4                 // Nominal Reading			-- (E0h = 4.995Volt)
   EF                 // Normal Maximum				-- (ECh = 5.262Volt)
   D9                 // Normal Minimum				-- (D5h = 4.750Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = Volt)
   00                 // Sensor Minimum Reading			-- (0h = 0Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   FC                 // Upper critical				-- (F8h = 5.530Volt)
   F5                 // Upper non-critical			-- (F1h = 5.374Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   CD                 // Lower critical				-- (CAh = 4.504Volt)
   D4                 // Lower non-critical			-- (D0h = 4.638Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'BB +5.0V'         // String Bytes
//=========================================================================//
_SDR_TYPE      01
_REC_LEN       003D

   // Sensor Record Header
   0015               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   1A                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   10                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   E3                 // M
   00                 // M, Tolerance
   4A                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   E4                 // Nominal Reading			-- (E4h = 5.36Volt)
   EF                 // Normal Maximum				-- (EFh = 5.61Volt)
   D9                 // Normal Minimum				-- (D9h = 5.12Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = 5.97Volt)
   00                 // Sensor Minimum Reading			-- (00h = 0.18Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   FC                 // Upper critical				-- (FCh = 5.90Volt)
   F5                 // Upper non-critical			-- (F5h = 5.74Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   CD                 // Lower critical				-- (CDh = 4.84Volt)
   D4                 // Lower non-critical			-- (D4h = 4.99Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BB +5.0V STBY'    // String Bytes
//=========================================================================//
_SDR_TYPE      01
_REC_LEN       0039

   // Sensor Record Header
   0016               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   1B                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   11                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   34                 // M
   00                 // M, Tolerance
   B7                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   D0                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   E3                 // Nominal Reading			-- (DFh = 11.81Volt)
   EE                 // Normal Maximum				-- (EAh = 12.40Volt)
   D7                 // Normal Minimum				-- (D4h = 11.23Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = Volt)
   00                 // Sensor Minimum Reading			-- (0h = 0Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   FC                 // Upper critical				-- (F8h = 13.14Volt)
   F5                 // Upper non-critical			-- (F1h = 12.77Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   CB                 // Lower critical				-- (C8h = 10.6Volt)
   D2                 // Lower non-critical			-- (CEh = 10.91Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'BB +12.0V'        // String Bytes
//=========================================================================//
_SDR_TYPE      01
_REC_LEN       0039

   // Sensor Record Header
   0017               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   1C                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   12                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   AE                 // M
   00                 // M, Tolerance
   6B                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C3                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   A8                 // Nominal Reading			-- (A8h = -12.42Volt)
   ED                 // Normal Maximum				-- (EDh = -13.62Volt)
   63                 // Normal Minimum				-- (63h = -11.22Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = -13.94Volt)
   00                 // Sensor Minimum Reading			-- (00h = -9.50Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   FC                 // Upper critical				-- (FCh = -13.88Volt)
   F5                 // Upper non-critical			-- (F5h = -13.76Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   5C                 // Lower critical				-- (5Ch = -11.10Volt)
   5F                 // Lower non-critical			-- (5Fh = -11.15Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'BB -12.0V'        // String Bytes
//=========================================================================//

//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'PROC_1'
_REC_LEN       0040

   // Sensor Record Header
   0018               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   1D                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   13                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   3B                 // M
   00                 // M, Tolerance
   DB                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   CF                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   E6                 // Nominal Reading			-- (E6h = 1.35Volt)
   F2                 // Normal Maximum				-- (F2h = 1.42Volt)
   DB                 // Normal Minimum				-- (DBh = 1.29Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = 1.50Volt)
   00                 // Sensor Minimum Reading			-- (00h = 0.00Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   FC                 // Upper critical				-- (FCh = 1.48Volt)
   F5                 // Upper non-critical			-- (F5h = 1.44Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   D2                 // Lower critical				-- (D2h = 1.24Volt)
   D8                 // Lower non-critical			-- (D8h = 1.27Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35V P1DDR3'        // String Bytes
//=========================================================================//


//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'PROC_2'
_SDR_TAG       'FCT'
_REC_LEN       0040

   // Sensor Record Header
   0019               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   1E                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   14                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type				-- (Voltage)
   01                 // Event / Reading Base Type		-- (Threshold)
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2				-- (Volts)
   00                 // Sensor Units 3
   00                 // Linearization
   3B                 // M
   00                 // M, Tolerance
   DB                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   CF                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   E6                 // Nominal Reading			-- (E6h = 1.35Volt)
   F2                 // Normal Maximum				-- (F2h = 1.42Volt)
   DB                 // Normal Minimum				-- (DBh = 1.29Volt)
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading			-- (FFh = 1.50Volt)
   00                 // Sensor Minimum Reading			-- (00h = 0.00Volt)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   FC                 // Upper critical				-- (FCh = 1.48Volt)
   F5                 // Upper non-critical			-- (F5h = 1.44Volt)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   D2                 // Lower critical				-- (D2h = 1.24Volt)
   D8                 // Lower non-critical			-- (D8h = 1.27Volt)
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35V P2DDR3' // String Bytes
//=========================================================================//

_SDR_TYPE      01
_REC_LEN       003E

   // Sensor Record Header
   001A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   20                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   13                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   30                 // Nominal Reading			-- (30h = 48 degree C)
   4B                 // Normal Maximum				-- (4Bh = 75 degree C)
   14                 // Normal Minimum				-- (14h = 20 degree C)
//------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading			-- (7fh = 127 degree C)
   80                 // Sensor Minimum Reading			-- (80h = -128 degree C)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   5A                 // Upper critical				-- (5Ah = 90 degree C)
   53                 // Upper non-critical			-- (53h = 83 degree C)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable			
   05                 // Lower critical				-- (5h = 5 degree C)
   0A                 // Lower non-critical			-- (0Ah = 10 degree C)
//------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Baseboard Temp'   // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'FP_TEMP'
_REC_LEN       0040

   // Sensor Record Header
   001B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   21                 // Sensor Number

   // Record Body Bytes
   0C                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask			-- [u,l][c,nc]=8532
   8532               // Deassertion Event Mask			-- [u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks	--[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   19                 // Nominal Reading			-- ( 19h = 25 degree C)
   28                 // Normal Maximum				-- ( 28h = 40 degree C)
   0A                 // Normal Minimum				-- ( 0Ah = 10degree C)
//------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading			-- ( 7fh = 127 degree C)
   80                 // Sensor Minimum Reading			-- ( 80h = -128 degree C)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   30                 // Upper critical				-- (30h = 48 degree C)
   2C                 // Upper non-critical			-- (2Ch = 44 degree C)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical				-- (00h =  0 degree C)
   05                 // Lower non-critical			-- (05h =  5 degree C)
//------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'Front Panel Temp' // String Bytes
//=========================================================================//
_SDR_TYPE      01
_REC_LEN       0040

   // Sensor Record Header
   001C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   22                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   14                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask			-- [u][c,nc]=8002
   8032               // Deassertion Event Mask			-- [u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks	--[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   EC                 // Nominal Reading			-- (00h = 00 degree C)
   00                 // Normal Maximum				-- (00h = 00 degree C)
   D8                 // Normal Minimum				-- (00h = 00 degree C)
//------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading			-- (7Fh = 127 degree C)
   80                 // Sensor Minimum Reading			-- (80h = -128 degree C)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   0A                 // Upper critical				-- (00h = 00 degree C)
   05                 // Upper non-critical			-- (00h = 00 degree C)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical				-- (00h =  0 degree C)
   00                 // Lower non-critical			-- (00h =  00 degree C)
//------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   D0                 // Type/Length Code
   'IOH Therm Margin' // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'PROC_1'
_REC_LEN       0040

   // Sensor Record Header
   001D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   23                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   15                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask                     -- [u][c,nc]=8002
   8032               // Deassertion Event Mask                   -- [u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks    --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   EC                 // Nominal Reading			-- ( 00h = 00 degree C)
   00                 // Normal Maximum				-- ( 00h = 00 degree C)
   D8                 // Normal Minimum				-- ( 00h = 10 degree C)
//------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading			-- ( 7Fh = 127 degree C)
   80                 // Sensor Minimum Reading			-- ( 80h = -128 degree C)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   0A                 // Upper critical				-- ( h =  degree C)
   05                 // Upper non-critical			-- ( h =  degree C)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical				-- ( h =  degree C)
   00                 // Lower non-critical			-- ( h =  degree C)
//------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   D0                 // Type/Length Code
   'Mem P1 Thrm Mrgn' // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'PROC_2'
_REC_LEN       0040

   // Sensor Record Header
   001E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   24                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   16                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask                    -- [u][c,nc]=8002
   8032               // Deassertion Event Mask                  -- [u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks     --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   EC                 // Nominal Reading			-- ( 00h = 00 degree C)
   00                 // Normal Maximum				-- ( 00h = 00 degree C)
   D8                 // Normal Minimum				-- ( 00h = 10 degree C)
//------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading			-- ( 7Fh = 127 degree C)
   80                 // Sensor Minimum Reading			-- ( 80h = -128 degree C)
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   0A                 // Upper critical				-- ( h =  degree C)
   05                 // Upper non-critical			-- ( h =  degree C)
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical				-- ( h =  degree C)
   00                 // Lower non-critical			-- ( h =  degree C)
//------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   D0                 // Type/Length Code
   'Mem P2 Thrm Mrgn' // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'CPU2_TACH'
_REC_LEN       003F

   // Sensor Record Header
   001F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask			--[l][c,nc]=0530
   0500               // Deassertion Event Mask			--[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks	--[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   1F                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   8F                 // Nominal Reading			-- = 5000	
   FF                 // Normal Maximum				-- = 9000
   1F                 // Normal Minimum				-- = 1000
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   16                 // Lower critical				-- = 700
   19                 // Lower non-critical			-- = 800
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 2 Mean (avg) [4:0]=5 Sample Count
   CF                 // Type/Length Code
   'Processor 2 FAN'  // String Bytes
//=========================================================================//    
_SDR_TYPE      01
_SDR_TAG       'CPU1_TACH'
_REC_LEN       003F

   // Sensor Record Header
   0020               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask			--[l][c,nc]=0530
   0500               // Deassertion Event Mask			--[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks	--[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   1F                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   8F                 // Nominal Reading			-- = 5000	
   FF                 // Normal Maximum				-- = 9000
   1F                 // Normal Minimum				-- = 1000
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   16                 // Lower critical				-- = 700
   19                 // Lower non-critical			-- = 800
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 2 Mean (avg) [4:0]=5 Sample Count
   CF                 // Type/Length Code
   'Processor 1 FAN'  // String Bytes
//=========================================================================//    
_SDR_TYPE      01
_SDR_TAG       'SYS_1_TACH_PP5'
_SDR_TAG       'SYS_1_TACH_Other'
_SDR_TAG       'SYS_1_TACH_FCT'
_REC_LEN       003C

   // Sensor Record Header
   0021               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask			--[l][c,nc]=0530
   0500               // Deassertion Event Mask			--[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks	--[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   10                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   8F                 // Nominal Reading			-- = 2300
   FF                 // Normal Maximum				-- = 4100
   1F                 // Normal Minimum				-- = 500
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   15                 // Lower critical				-- = 400
   18                 // Lower non-critical			-- = 350
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 2 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 1'     // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'SYS_1_TACH_HJ2'
_REC_LEN       003C

   // Sensor Record Header
   0022               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask			--[l][c,nc]=0530
   0500               // Deassertion Event Mask			--[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks	--[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   1B                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   88                 // Nominal Reading			-- = 4000
   FF                 // Normal Maximum				-- = 7000
   12                 // Normal Minimum				-- = 1000
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   0C                 // Lower critical				-- = 800
   0E                 // Lower non-critical			-- = 700
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 2 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 1'     // String Bytes  
//=========================================================================//   
_SDR_TYPE      01
_SDR_TAG       'SYS_2_TACH_PP5'
_SDR_TAG       'SYS_2_TACH_Other'
_SDR_TAG       'SYS_2_TACH_FCT'
_REC_LEN       003C

   // Sensor Record Header
   0023               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask			--[l][c,nc]=0530
   0500               // Deassertion Event Mask			--[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks	--[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   0C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   92                 // Nominal Reading			-- = 1900
   FF                 // Normal Maximum				-- = 3300
   26                 // Normal Minimum				-- = 500
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   1B                 // Lower critical				-- = 400
   1E                 // Lower non-critical			-- = 350
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 2 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 2'     // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'SYS_2_TACH_HJ2'
_REC_LEN       003C

   // Sensor Record Header
   0024               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask			--[l][c,nc]=0530
   0500               // Deassertion Event Mask			--[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks	--[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   1B                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   88                 // Nominal Reading			-- = 4000
   FF                 // Normal Maximum				-- = 7000
   12                 // Normal Minimum				-- = 1000
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   0C                 // Lower critical				-- = 800
   0E                 // Lower non-critical			-- = 700
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 2 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 2'     // String Bytes  
//=========================================================================//     
_SDR_TYPE      01
_SDR_TAG       'SYS_3_TACH_PP5'
_SDR_TAG       'SYS_3_TACH_Other'
_SDR_TAG       'SYS_3_TACH_FCT'
_REC_LEN       003C

   // Sensor Record Header
   0025               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7B                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask			--[l][c,nc]=0530
   0500               // Deassertion Event Mask			--[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks	--[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   16                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   8A                 // Nominal Reading			-- = 3350
   FF                 // Normal Maximum				-- = 5700
   16                 // Normal Minimum				-- = 1000
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   0F                 // Lower critical				-- = 800
   11                 // Lower non-critical			-- = 700
//------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 2 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 3'     // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG       'SC5650BRP_PS1'
_REC_LEN       002A

   // Sensor Record Header
   0026               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   50                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type 
   4F00               // Assertion Event Mask
   4F00               // Deassertion Event Mask
   4F00               // Reading Mask &  Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00		          // Reserved
   00		          // Reserved
   00		          // Reserved
   00		          // OEM
   CA                 // Type/Length Code
   'PS1 Status'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG       'SC5650BRP_PS2'
_REC_LEN       002A

   // Sensor Record Header
   0027               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   51                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   4F00               // Assertion Event Mask
   4F00               // Deassertion Event Mask
   4F00               // Reading Mask &  Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00		          // Reserved
   00		          // Reserved
   00		          // OEM
   CA                 // Type/Length Code
   'PS2 Status'       // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'SC5650BRP_PS1'
_REC_LEN       003C

   // Sensor Record Header
   0028               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   52                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   03                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask			--[u][c,nc]=8002
   8032               // Deassertion Event Mask			--[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   04                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   56                 // Nominal Reading
   AC                 // Normal Maximum
   00                 // Normal Minimum
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   BE                 // Upper critical
   B5                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
//------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS1 Power In'     // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'SC5650BRP_PS2'
_REC_LEN       003C

   // Sensor Record Header
   0029               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   53                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   04                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask			--[u][c,nc]=8002
   8032               // Deassertion Event Mask			--[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   04                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   56                 // Nominal Reading
   AC                 // Normal Maximum
   00                 // Normal Minimum
//------------------------------------------------------------------//
   00                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   BE                 // Upper critical
   B5                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
//------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS2 Power In'     // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'SC5650BRP_PS1'
_REC_LEN       003E

   // Sensor Record Header
   002A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   05                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask			--[u][c,nc]=8002
   8032               // Deassertion Event Mask			--[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   32                 // Nominal Reading
   64                 // Normal Maximum
   00                 // Normal Minimum
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   6E                 // Upper critical
   64                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
//------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'  // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'SC5650BRP_PS2'
_REC_LEN       003E

   // Sensor Record Header
   002B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   06                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask			--[u][c,nc]=8002
   8032               // Deassertion Event Mask			--[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   32                 // Nominal Reading
   64                 // Normal Maximum
   00                 // Normal Minimum
//------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   6E                 // Upper critical
   64                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
//------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'SC5650BRP_PS1'
_REC_LEN       003F

   // Sensor Record Header
   002C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   56                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   07                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   08                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask			--[u][c,nc]=8002
   8032               // Deassertion Event Mask			--[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   19                 // Nominal Reading
   32                 // Normal Maximum
   05                 // Normal Minimum
//------------------------------------------------------------------//
   00                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   3C                 // Upper critical
   37                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
//------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 Temperature'  // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'SC5650BRP_PS2'
_REC_LEN       003F

   // Sensor Record Header
   002D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   57                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   08                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   08                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask			--[u][c,nc]=8002
   8032               // Deassertion Event Mask			--[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   19                 // Nominal Reading
   32                 // Normal Maximum
   05                 // Normal Minimum
//------------------------------------------------------------------//
   00                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   3C                 // Upper critical
   37                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
//------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 Temperature'  // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG       'PROC_1'
_REC_LEN       0029

   // Sensor Record Header
   002E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   24                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   60                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   6F                 // Event / Reading Base Type
   A301               // Assertion Event Mask
   A301               // Deassertion Event Mask
   A301               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'P1 Status'        // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG       'PROC_2'
_REC_LEN       0029

   // Sensor Record Header
   002F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   24                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   61                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   6F                 // Event / Reading Base Type
   A301               // Assertion Event Mask
   A301               // Deassertion Event Mask
   A301               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'P2 Status'        // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'PROC_1_TEMP'
_REC_LEN       003F

   // Sensor Record Header
   0030               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   62                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   F1                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
//------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
//------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Margin'  // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'PROC_2_TEMP'
_REC_LEN       003F

   // Sensor Record Header
   0031               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   63                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   F1                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
//------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
//------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P2 Therm Margin'  // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'PROC_1_TEMP'
_REC_LEN       003F

   // Sensor Record Header
   0032               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   64                 // Sensor Number 

   // Record Body Bytes
   03                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask			--[u][nc,c]=8002
   8032               // Deassertion Event Mask			--[u][nc,c]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks	--[u][nc,c]=1818
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   00                 // Nominal Reading
   14                 // Normal Maximum
   00                 // Normal Minimum
//------------------------------------------------------------------//
   64                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   32                 // Upper critical
   1E                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
//------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Ctrl %'  // String Bytes
//=========================================================================//
_SDR_TYPE      01
_SDR_TAG       'PROC_2_TEMP'
_REC_LEN       003F

   // Sensor Record Header
   0033               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   65                 // Sensor Number 

   // Record Body Bytes
   03                 // Entity ID
   06                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask			--[u][nc,c]=8002
   8032               // Deassertion Event Mask			--[u][nc,c]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks	--[u][nc,c]=1818
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   00                 // Nominal Reading
   14                 // Normal Maximum
   00                 // Normal Minimum
//------------------------------------------------------------------//
   64                 // Sensor Maximum Reading          
   00                 // Sensor Minimum Reading 
//------------------------------------------------------------------//         
   00                 // Upper non-recoverable           
   32                 // Upper critical
   1E                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
//------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P2 Therm Ctrl %'  // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG       'PROC_1'
_REC_LEN       002A

   // Sensor Record Header
   0034               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   66                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   07                 // Entity Instance
   67                 // Sensor Initialization
   28                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'P1 VRD Hot'       // String Bytes
//=========================================================================//   
_SDR_TYPE      02
_SDR_TAG       'PROC_2'
_REC_LEN       002A

   // Sensor Record Header
   0035               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   67                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   08                 // Entity Instance
   67                 // Sensor Initialization
   28                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'P2 VRD Hot'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_REC_LEN       0026

   // Sensor Record Header
   0036               // Record ID
   51                 // SDR Version
   02                 // Record Type
   21                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   68                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   09                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00		              // Reserved
   00		              // Reserved
   00		              // Reserved
   00		              // OEM
   C6                 // Type/Length Code
   'CATERR'           // String Bytes
//=========================================================================//
_SDR_TYPE      02
_REC_LEN       002B

   // Sensor Record Header
   0037               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   69                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   0A                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'CPU Missing'      // String Bytes
//=========================================================================//
_SDR_TYPE      02
_REC_LEN       002E

   // Sensor Record Header
   0038               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   6A                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   17                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00		              // Reserved
   00		              // Reserved
   00		              // Reserved
   00		              // OEM
   CE                 // Type/Length Code
   'IOH Therm Trip' // String Bytes
//=========================================================================//


// ********************************************************************
// HSBP SDR Record Primary HSC controller at address 0xC0
// ********************************************************************
_SDR_TYPE      01
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       003B

   // Sensor Record Header
   0039               // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   C0                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   7D                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   02                 // M, Tolerance
   00                 // B
   2C                 // B, Accuracy
   10                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
//------------------------------------------------------------------//
   17                 // Nominal Reading
   2D                 // Normal Maximum
   0A                 // Normal Minimum
//------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
//------------------------------------------------------------------//
   00                 // Upper non-recoverable
   37                 // Upper critical
   32                 // Upper non-critical
//------------------------------------------------------------------//
   00                 // Lower non-recoverable
   05                 // Lower critical
   09                 // Lower non-critical
//------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'HSC0 BP Tmp'      // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       002A

   // Sensor Record Header
   003A               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   02                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   02                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 0 Stat'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       002A

   // Sensor Record Header
   003B               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   03                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   03                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 1 Stat'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       002A

   // Sensor Record Header
   003C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   04                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   04                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 2 Stat'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       002A

   // Sensor Record Header
   003D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   05                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   05                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 3 Stat'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       002A

   // Sensor Record Header
   003E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   06                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   06                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 4 Stat'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       002A

   // Sensor Record Header
   003F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   07                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   07                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 5 Stat'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       002A

   // Sensor Record Header
   0040               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   09                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   08                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   08                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 0 Pres'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       002A

   // Sensor Record Header
   0041               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   0A                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   09                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   08                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 1 Pres'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       002A

   // Sensor Record Header
   0042               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   0B                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   0A                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   08                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 2 Pres'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       002A

   // Sensor Record Header
   0043               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   0C                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   0B                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   08                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 3 Pres'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       002A

   // Sensor Record Header
   0044               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   0D                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   0C                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   08                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 4 Pres'       // String Bytes
//=========================================================================//
_SDR_TYPE      02
_SDR_TAG    'P_R26BPE'
_SDR_TAG    'P_R26BP'
_REC_LEN       002A

   // Sensor Record Header
   0045               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   C0                 // Sensor ID
   00                 // Sensor LUN
   0E                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   0D                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   08                 // Event / Reading Base Type
   0300               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'Drv 5 Pres'       // String Bytes
//=========================================================================//

//*******************************************************
// SDR Type 03 - Event Only Record for BIOS 
//*******************************************************
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   0046               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   01                 // Entity Instance
   0C                 // Sensor Type
   0B                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mem Mirr Sensor'   // Memory Mirroring Sensor 
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   0047               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   11                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   02                 // Entity Instance
   0C                 // Sensor Type
   0B                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mem Spar Sensor'  // Memory Spare Sensor
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   0048               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   01                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mmry ECC Sensor'  // Memory ECC Error Sensor 
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   0049               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   30                 // Entity ID = PCI
   01                 // Entity Instance
   13                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCI Lgcy Sensor'  // Legacy PCI Sensor
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   004A               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   01                 // Entity Instance
   13                 // Sensor Type
   70                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Fat Sensor'  // PCI Express Fatal Error Sensor
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   004B               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   05                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   02                 // Entity Instance
   13                 // Sensor Type
   71                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Cor Sensor'  // PCI Express Correctable Error Sensor
//=========================================================================//

//********************************************************
// SDR Type 03 - Event Only Record for BIOS Boot Events 
//********************************************************   
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   004C               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   12                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   03                 // Entity Instance
   0C                 // Sensor Type
   09                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mirr Mod Sensor'  // Memory Mirroring Mode Enable/Presence Sensor
//=========================================================================// 
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   004D               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   13                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   04                 // Entity Instance
   0C                 // Sensor Type
   09                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Spar Mod Sensor'  // Memory Sparing Mode Enable/Presence Sensor
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   004E               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   05                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // BIOS Boot Event Sensor
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   004F               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   17                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   06                 // Entity Instance
   13                 // Sensor Type
   74                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Fatl Sensor'   // QPI Fatal Error Sensor
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   0050               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   07                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   07                 // Entity Instance
   13                 // Sensor Type
   73                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI NonF Sensor'  // QPI Non-fatal Event Sensor
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   0051               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   08                 // Entity Instance
   13                 // Sensor Type
   72                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Corr Sensor'  // QPI Correctable Event Sensor
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   0052               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   18                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   09                 // Entity Instance
   13                 // Sensor Type
   74                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Fatl Sensor'  // QPI fatal Event Sensor (extended)
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   0053               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   14                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   0A                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mem Parity Snsr'  // Memory Parity Error Event Sensor
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       0020

   // Sensor Record Header
   0054               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

    // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

    // Record Body Bytes
   2B                 // Entity ID-BIOS POST
   00                 // Entity Instance
   0F                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'POST Err Sensor'  // POST Error Sensor
//=========================================================================//


//************************************************************************
// SDR Type 03 - Event Only Record for Management Engine (ME controller) 
//************************************************************************
_SDR_TYPE      03
_REC_LEN       001E

   // Sensor Record Header
   0055               // Record ID
   51                 // SDR Version
   03                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   17                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor type 
   75                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'SPS FW Health'    // String Bytes
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       001D

   // Sensor Record Header
   0056               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   18                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   02                 // Entity Instance
   DC                 // Sensor type 
   72                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'NM Exception'     // String Bytes
//=========================================================================//
_SDR_TYPE      03
_REC_LEN       001A

   // Sensor Record Header
   0057               // Record ID
   51                 // SDR Version
   03                 // Record Type
   15                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   19                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   03                 // Entity Instance
   DC                 // Sensor type 
   73                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'NM Health'        // String Bytes
//=========================================================================//
_SDR_TYPE      02
_REC_LEN       002F

   // Sensor Record Header
   0058               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   1A                 // Sensor Number (Node Manager Operational Capabilities Change Event)

   // Record Body Bytes
   2E                 // Entity ID
   04                 // Entity Instance
   41                 // Sensor Initialization
   C3                 // Sensor Capabilities
   DC                 // Sensor Type
   74                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0700               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0000               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'NM Capabilities'  // String Bytes    
//=========================================================================//  
_SDR_TYPE      03
_REC_LEN       001D

   // Sensor Record Header
   0059               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   1B                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   05                 // Entity Instance
   DC                 // Sensor type 
   72                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'NM Threshold'     // String Bytes
//=========================================================================//

   
//*******************************************************
// SDR Type 11 Records
//*******************************************************
_SDR_TYPE      11
_REC_LEN       0019

   // Sensor Record Header
   005A               // Record ID
   51                 // SDR Version
   11                 // Record Type
   14                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address (20h for BMC)
   00                 // FRU Device ID / Device Slave Address ( 0 for ID 0)
   80                 // Access LUN / Bus ID (A8h for Baseboard FRU device)
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   07                 // FRU Entity ID
   18                 // FRU Entity Instance
   00                 // OEM
   C9                 // Type/Length Code
   'Baseboard'        // String Bytes
//=========================================================================//
_SDR_TYPE      11
_SDR_TAG       'PDB_FRU'
_REC_LEN       0020


   // Sensor Record Header
   005B               // Record ID
   51                 // SDR Version
   11                 // Record Type
   1B                 // Record Length
   // Record Key Bytes
   20                 // Device Access Address
   01                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number
   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   15                 // FRU Entity ID
   03                 // FRU Entity Instance
   00                 // Reserved for OEM use
   D0                 // Type/Length Code
   'Power Dist Board' // String Bytes   
//=========================================================================//
_SDR_TYPE      11
_SDR_TAG       'PS1_FRU'
_REC_LEN       0020
 
   // Sensor Record Header
   005C               // Record ID
   51                 // SDR Version
   11                 // Record Type
   1B                 // Record Length
   // Record Key Bytes
   20                 // Device Access Address
   02                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number
   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0A                 // FRU Entity ID
   09                 // FRU Entity Instance
   00                 // Reserved for OEM use
   D0                 // Type/Length Code
   'Pwr Supply 1 FRU' // String Bytes
//=========================================================================//
_SDR_TYPE      11
_SDR_TAG       'PS2_FRU'
_REC_LEN       0020

   // Sensor Record Header
   005D               // Record ID
   51                 // SDR Version
   11                 // Record Type
   1B                 // Record Length
   // Record Key Bytes
   20                 // Device Access Address
   03                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number
   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0A                 // FRU Entity ID
   0A                 // FRU Entity Instance
   00                 // Reserved for OEM use
   D0                 // Type/Length Code
   'Pwr Supply 2 FRU' // String Bytes
//=========================================================================//


//*******************************************************
// SDR Type 12 Records
//*******************************************************
_SDR_TYPE      12
_REC_LEN       0020

   // Sensor Record Header
   005E               // Record ID
   51                 // SDR Version
   12                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   20                 // Device Slave Address
   00                 // Channel Number

   // Record Body Bytes
   08                 // Power state notification
   BF                 // Device capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   07                 // Entity ID
   19                 // Entity instance
   00                 // OEM
   D0                 // Type/Length Code
   'Basbrd Mgmt Ctlr' // String Bytes
//=========================================================================//
_SDR_TYPE      12
_SDR_TAG       'HSC0'
_REC_LEN       001C

   // Sensor Record Header
   005F               // Record ID
   51                 // SDR Version
   12                 // Record Type
   17                 // Record Length

   // Record Key Bytes
   C0                 // Device Slave Address
   00                 // Channel Number

   // Record Body Bytes
   84                 // Power state notification
   29                 // Device capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   0F                 // Entity ID
   0E                 // Entity instance
   00                 // OEM
   CC                 // Type/Length Code
   'HSBP PRIMARY'     // String Bytes
//=========================================================================//
_SDR_TYPE      12
_SDR_TAG       'LCP'
_REC_LEN       0020

   // Sensor Record Header
   0060               // Record ID
   51                 // SDR Version
   12                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   22                 // Device Slave Address
   00                 // Channel Number

   // Record Body Bytes
   84                 // Power state notification
   29                 // Device capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   0C                 // Entity ID
   03                 // Entity instance
   00                 // OEM
   D0                 // Type/Length Code
   'Local Ctrl Panel' // String Bytes
//=========================================================================//
_SDR_TYPE      12
_REC_LEN       0012

   // Sensor Record Header
   0061               // Record ID
   51                 // SDR Version
   12                 // Record Type
   0D                 // Record Length

   // Record Key Bytes
   2C                 // Device Slave Address
   06                 // Channel number

   // Record Body Bytes
   06                 // Power State Notification
   21                 // Device Capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   2E                 // Entity ID
   06                 // Entity Instance
   00                 // OEM
   C2                 // Type/Length Code
   'ME'               // String Bytes    
//=========================================================================//


//*******************************************************
// SDR Type C0 Records - OEM
//*******************************************************

//*******************************************************
// SDR Type C0/02 Record for Power Unit Map 
//*******************************************************
_SDR_TYPE      C0
_SDR_TAG       'REDUNDANT_PS2'
_REC_LEN       000E

   // Sensor Record Header
   0062               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   09                 // Record Length
   
   // Record Body Bytes
   570100             // Manufacturer ID
   02                 // Record Subtype Value
   02                 // Power Unit Redundancy sensor number
   00                 // Bits [7:1]-Reserved; Bit [0]-1=No monitor able supplies present
   01                 // the number of present and operational
   50                 // Power Supply Status 1 Sensor Number
   51                 // Power Supply Status 2 Sensor Number 

//*******************************************************
// SDR Type C0/09 Records For Voltage Sensor Scaling
//*******************************************************
_SDR_TYPE      C0
_REC_LEN       0037

   // Sensor Record Header
   0063               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   32                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   09                 // Record sub-type - Voltage Sensor Scaling
   0F                 // Number of entries following
   10                 // Voltage Sensor Number
   5414               // Scale Factor (LSB MSB)
   11                 // Voltage Sensor Number
   880F               // Scale Factor (LSB MSB)
   12                 // Voltage Sensor Number
   880F               // Scale Factor (LSB MSB)
   13                 // Voltage Sensor Number
   A50E               // Scale Factor (LSB MSB)
   14                 // Voltage Sensor Number
   A50E               // Scale Factor (LSB MSB)
   15                 // Voltage Sensor Number
   730C               // Scale Factor (LSB MSB)
   16                 // Voltage Sensor Number
   B60A               // Scale Factor (LSB MSB)
   17                 // Voltage Sensor Number
   B60A               // Scale Factor (LSB MSB)
   18                 // Voltage Sensor Number
   D509               // Scale Factor (LSB MSB)
   19                 // Voltage Sensor Number
   BB0A               // Scale Factor (LSB MSB)
   1A                 // Voltage Sensor Number
   BB0A               // Scale Factor (LSB MSB)
   1B                 // Voltage Sensor Number
   D50A               // Scale Factor (LSB MSB)
   1C                 // Voltage Sensor Number
   391E               // Scale Factor (LSB MSB)
   1D                 // Voltage Sensor Number
   4410               // Scale Factor (LSB MSB)
   1E                 // Voltage Sensor Number
   4410               // Scale Factor (LSB MSB)   
//=========================================================================//

//*******************************************************
// SDR Type C0/0A Records For Fan Sensor Scaling
//*******************************************************
//For SC5650DP/SC5650BRP Chassis
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_SDR_TAG       'Other'
_SDR_TAG       'FCT'
_REC_LEN       0015

  //Sensor Record Header
   0064               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
   FF1F               // Placeholder for CPU fan 1(SN:0x30), Max RPM: 8191RPM == 0xFF1F (the order is LSB, MSB)
   FF1F               // Placeholder for CPU fan 2(SN:0x31), Max RPM: 8191RPM == 0xFF1F (the order is LSB, MSB)
   FF10               // Placeholder for Sys Fan 1(SN:0x32), Max RPM: 4351RPM == 0xFF10 (the order is LSB, MSB)
   FF0C               // Placeholder for Sys Fan 2(SN:0x33), Max RPM: 3327RPM == 0xFF0C (the order is LSB, MSB)
   FF16               // Placeholder for Sys Fan 3(SN:0x34), Max RPM: 5887RPM == 0xFF16 (the order is LSB, MSB)
//=========================================================================//
//For SR1630BC Chassis
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0015

  //Sensor Record Header
   0065               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
   0001               // NULL(SN:0x30)
   0001               // NULL(SN:0x31)
   FF1B               // Placeholder for Sys Fan 1(SN:0x32), Max RPM: 7167RPM == 0xFF1B (the order is LSB, MSB)
   FF1B               // Placeholder for Sys Fan 2(SN:0x33), Max RPM: 7167RPM == 0xFF1B (the order is LSB, MSB)
   0001               // NULL(SN:0x34)
//=========================================================================//


// ***************************************************************************
// SDR Type C0/0B Records For Thermal Profile Data, Open Loop
// ***************************************************************************

//=========================================================================//
// For SC5650DP/SC5650BRP Chassis
//========================================================================//
// SC5650DP/SC5650BRP Chassis Thermal Profile 0 data SDR Record in OLTT
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   0066               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   01                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   58                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   2C01               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// SC5650DP/SC5650BRP Chassis Thermal Profile 1 data SDR Record in OLTT   
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   0067               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   02                 // Profile Support Bitmap
   42                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   4E                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   8403               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// SC5650DP/SC5650BRP Chassis Thermal Profile 2 data SDR Record in OLTT
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   0068               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   04                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   52                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   9001               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// SC5650DP/SC5650BRP Chassis Thermal Profile 3 data SDR Record in OLTT 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   0069               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   08                 // Profile Support Bitmap
   42                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   4A                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   E803               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// SC5650DP/SC5650BRP Chassis Thermal Profile 4 data SDR Record in OLTT   
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   006A               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   10                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   50                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   BC02               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1

//=========================================================================//
// SC5650DP/SC5650BRP Chassis Thermal Profile 5 data SDR Record in OLTT 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   006B               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   20                 // Profile Support Bitmap
   42                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   48                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   B004               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// SC5650DP/SC5650BRP Chassis Thermal Profile 6 data SDR Record in OLTT   
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   006C               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   40                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   4C                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   7805               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1  

//=========================================================================//
// SC5650DP/SC5650BRP Chassis Thermal Profile 7 data SDR Record in OLTT 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   006D               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   80                 // Profile Support Bitmap
   38                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   46                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   B80B               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1    

//=========================================================================//
// SC5650DP/SC5650BRP Chassis Thermal Profile 0-7 data SDR Record in CLTT 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   006E               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   02                 // Flags - Throttling Mode (CLTT)
   FF                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   3C                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   9001               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   03                 // Throttle Mode (03=EXTTS CLTT).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
//=========================================================================//

//=========================================================================//
// For SR1630BC Chassis
//========================================================================//
// SR1630BC Chassis Thermal Profile 0 data SDR Record in OLTT  
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0013

   // Sensor Record Header
   006F               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   01                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   58                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   2C01               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1

//=========================================================================//
// SR1630BC Chassis Thermal Profile 1 data SDR Record in OLTT  
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0013

   // Sensor Record Header
   0070               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   02                 // Profile Support Bitmap
   42                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   4E                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   8403               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// SR1630BC Chassis Thermal Profile 2 data SDR Record in OLTT  
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0013

   // Sensor Record Header
   0071               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   04                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   52                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   9001               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1

//=========================================================================//
// SR1630BC Chassis Thermal Profile 3 data SDR Record in OLTT  
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0013

   // Sensor Record Header
   0072               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   08                 // Profile Support Bitmap
   42                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   4A                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   E803               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// SR1630BC Chassis Thermal Profile 4 data SDR Record in OLTT  
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0013

   // Sensor Record Header
   0073               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   10                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   50                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   BC02               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1

//=========================================================================//
// SR1630BC Chassis Thermal Profile 5 data SDR Record in OLTT  
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0013

   // Sensor Record Header
   0074               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   20                 // Profile Support Bitmap
   42                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   48                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   B004               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
      
//=========================================================================//
// SR1630BC Chassis Thermal Profile 6 data SDR Record in OLTT  
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0013

   // Sensor Record Header
   0075               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   40                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   4C                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   7805               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1

//=========================================================================//
// SR1630BC Chassis Thermal Profile 7 data SDR Record in OLTT  
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0013

   // Sensor Record Header
   0076               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   80                 // Profile Support Bitmap
   38                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   46                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   B80B               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// SR1630BC Chassis Thermal Profile 0-7 data SDR Record in CLTT  
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0013

   // Sensor Record Header
   0077               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   02                 // Flags - Throttling Mode (CLTT)
   FF                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   3C                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   9001               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9001               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   03                 // Throttle Mode (03=EXTTS CLTT).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
//=========================================================================//

//=========================================================================//
// For Other Chassis/FCT/SHIP
//========================================================================//
// Other Chassis/FCT/SHIP Thermal Profile 0 data SDR Record in OLTT
_SDR_TYPE      C0
_SDR_TAG       'Other'
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       0013

   // Sensor Record Header
   0078               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   01                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   2C                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   EF03               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9301               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// Other Chassis/FCT/SHIP Thermal Profile 1 data SDR Record in OLTT   
_SDR_TYPE      C0
_SDR_TAG       'Other'
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       0013

   // Sensor Record Header
   0079               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   02                 // Profile Support Bitmap
   42                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   2A                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   E804               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9301               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// Other Chassis/FCT/SHIP Thermal Profile 2 data SDR Record in OLTT
_SDR_TYPE      C0
_SDR_TAG       'Other'
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       0013

   // Sensor Record Header
   007A               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   04                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   2B                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   5404               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9301               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// Other Chassis/FCT/SHIP Thermal Profile 3 data SDR Record in OLTT 
_SDR_TYPE      C0
_SDR_TAG       'Other'
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       0013

   // Sensor Record Header
   007B               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   08                 // Profile Support Bitmap
   42                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   29                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   6305               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9301               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// Other Chassis/FCT/SHIP Thermal Profile 4 data SDR Record in OLTT   
_SDR_TYPE      C0
_SDR_TAG       'Other'
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       0013

   // Sensor Record Header
   007C               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   10                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   2A                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   BB04               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9301               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1

//=========================================================================//
// Other Chassis/FCT/SHIP Thermal Profile 5 data SDR Record in OLTT 
_SDR_TYPE      C0
_SDR_TAG       'Other'
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       0013

   // Sensor Record Header
   007D               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   20                 // Profile Support Bitmap
   42                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   28                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   E205               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9301               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
   
//=========================================================================//
// Other Chassis/FCT/SHIP Thermal Profile 6 data SDR Record in OLTT   
_SDR_TYPE      C0
_SDR_TAG       'Other'
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       0013

   // Sensor Record Header
   007E               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   40                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   28                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   C805               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9301               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1  

//=========================================================================//
// Other Chassis/FCT/SHIP Thermal Profile 7 data SDR Record in OLTT 
_SDR_TYPE      C0
_SDR_TAG       'Other'
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       0013

   // Sensor Record Header
   007F               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   01                 // Flags - Throttling Mode (OLTT)
   80                 // Profile Support Bitmap
   38                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   26                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   2C07               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9301               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   01                 // Throttle Mode (01=VTS Only(OLTT)).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1    

//=========================================================================//
// Other Chassis/FCT/SHIP Thermal Profile 0-7 data SDR Record in CLTT 
_SDR_TYPE      C0
_SDR_TAG       'Other'
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       0013

   // Sensor Record Header
   0080               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0B                 // Record Subtype Value (Thermal Profile Data)
   02                 // Flags - Throttling Mode (CLTT)
   FF                 // Profile Support Bitmap
   32                 // TempInlet: Temperature at chassis inlet in units of 0.5 degrees C
		                  // (i. e. 90 units = 45 C) applied to SYS.TempInlet
   2C                 // TempRise: Temperature rise from chassis inlet to dimm local ambient in units
		                  // of 0.5 degrees C (i. e. 90 units = 45 C) applied to SYS.TempRise
   EF03               // AirFlow: Average air flow velocity in dim channel in units of mm/sec
		                  // (i.e. 1500 units = 1.5 m/s) applied to SYS.AirFlow.
   9301               // DimmPitch: The pitch between DIMMs in units of 1/1000 inch
		                  // (i.e. 410 units = 0.41 in) applied SYS.DimmPitch.
   03                 // Throttle Mode (03=EXTTS CLTT).
   08                 // [0]-Therm_Reg_Lock=0, [1-2]-Hysteresis=0, [3]-Control Event# mode=1
//=========================================================================//

// ***************************************************************************
// SDR Type C0/0C Records For Fan Speed Control
// ***************************************************************************
// **********************************************
// Stepwise Fan Speed Control Records
// **********************************************
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   0081               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   03                 // Fan Profile Support = 00000011

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   38                 // Temp Sensor failure control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   1A                 // Control Value 1 (Percentage) (1Ah = PWM 26%)
   
   0F                 // Temperature 2 15c
   1A                 // Control Value 2 (Percentage) (1Ah = PWM 26%)
   
   19                 // Temperature 3 25c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   23                 // Temperature 4 35c
   2B                 // Control Value 5 (Percentage) (2Bh = PWM 43%)
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 2,3 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   0082               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0C                 // Fan Profile Support = 00001100

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   38                 // Temp Sensor failure control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   1D                 // Control Value 1 (Percentage) (1Dh = PWM 29%)
   
   0F                 // Temperature 2 15c
   1D                 // Control Value 2 (Percentage) (1Dh = PWM 29%)
   
   19                 // Temperature 3 25c
   23                 // Control Value 3 (Percentage) (23h = PWM 35%)
   
   23                 // Temperature 4 35c
   2D                 // Control Value 5 (Percentage) (2Dh = PWM 45%)
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3 for Maximum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   0083               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   38                 // Temp Sensor failure control Value (38h = PWM 56%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   38                 // Control Value 1 (Percentage) (38h = PWM 56%)
   
   0F                 // Temperature 2 15c
   38                 // Control Value 2 (Percentage) (38h = PWM 56%)
   
   19                 // Temperature 3 25c
   38                 // Control Value 3 (Percentage) (38h = PWM 56%)
     
   23                 // Temperature 5 35c
   38                 // Control Value 5 (Percentage) (38h = PWM 56%)
   
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 4,5 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F
  
   // Sensor Record Header
   0084               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   38                 // Temp Sensor failure control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   21                 // Control Value 1 (Percentage) (21h = PWM 33%)
   
   0F                 // Temperature 2 15c
   21                 // Control Value 2 (Percentage) (21h = PWM 33%)
   
   19                 // Temperature 3 25c
   26                 // Control Value 3 (Percentage) (26h = PWM 38%)
   
   21                 // Temperature 4 33c
   2D                 // Control Value 4 (Percentage) (2Dh = PWM 45%)
   
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 4,5 for Maximum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F
   
   // Sensor Record Header
   0085               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   38                 // Temp Sensor failure control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   38                 // Control Value 1 (Percentage) (38h = PWM 56%)
   
   0F                 // Temperature 2 15c
   38                 // Control Value 2 (Percentage) (38h = PWM 56%)
   
   19                 // Temperature 3 25c
   38                 // Control Value 3 (Percentage) (38h = PWM 56%)
   
   21                 // Temperature 4 33c
   38                 // Control Value 4 (Percentage) (38h = PWM 56%)
   
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 6,7 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F
   
   // Sensor Record Header
   0086               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   38                 // Temp Sensor failure control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)

   00                 // Temperature 1 0c
   28                 // Control Value 1 (Percentage) (28h = PWM 40%)
   
   0F                 // Temperature 2 15c
   28                 // Control Value 2 (Percentage) (28h = PWM 40%)
   
   19                 // Temperature 3 25c
   2D                 // Control Value 3 (Percentage) (2Dh = PWM 45%)
   
   1C                 // Temperature 4 28c
   2F                 // Control Value 4 (Percentage) (2Fh = PWM 47%)
   
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 6,7 for Maximum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F
   // Sensor Record Header
   0087               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   38                 // Temp Sensor failure control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   38                 // Control Value 1 (Percentage) (38h = PWM 56%)
   
   0F                 // Temperature 2 15c
   38                 // Control Value 2 (Percentage) (38h = PWM 56%)
   
   19                 // Temperature 3 25c
   38                 // Control Value 3 (Percentage) (38h = PWM 56%)
   
   1C                 // Temperature 4 28c
   38                 // Control Value 4 (Percentage) (38h = PWM 56%)
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3 for Minimum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F

   // Sensor Record Header
   0088               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   0F                 // Temperature 2 15c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   19                 // Temperature 3 25c
   1E                 // Control Value 3 (Percentage) (1Eh = PWM 30%)
   
   23                 // Temperature 4 35c
   32                 // Control Value 4 (Percentage) (32h = PWM 50%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3 for Maximum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F

   // Sensor Record Header
   0089               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   50                 // Control Value 1 (Percentage) (50h = PWM 80%)
   
   0F                 // Temperature 2 15c
   50                 // Control Value 2 (Percentage) (50h = PWM 80%)
   
   19                 // Temperature 3 25c
   50                 // Control Value 3 (Percentage) (50h = PWM 80%)
     
   23                 // Temperature 5 35c
   50                 // Control Value 5 (Percentage) (50h = PWM 80%)
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 4,5 for Minimum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
   // Sensor Record Header
   008A               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   0F                 // Temperature 2 15c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   19                 // Temperature 3 25c
   1E                 // Control Value 3 (Percentage) (1Eh = PWM 30%)
   
   21                 // Temperature 4 33c
   32                 // Control Value 4 (Percentage) (32h = PWM 50%)
   
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 4,5 for Maximum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
   // Sensor Record Header
   008B               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   50                 // Control Value 1 (Percentage) (50h = PWM 80%)
   
   0F                 // Temperature 2 15c
   50                 // Control Value 2 (Percentage) (50h = PWM 80%)
   
   19                 // Temperature 3 25c
   50                 // Control Value 3 (Percentage) (50h = PWM 80%)
   
   21                 // Temperature 4 33c
   50                 // Control Value 4 (Percentage) (50h = PWM 80%)   
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 6,7 for Minimum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
// Sensor Record Header
   008C               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)

   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   0F                 // Temperature 2 15c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   19                 // Temperature 3 25c
   1E                 // Control Value 3 (Percentage) (1Eh = PWM 30%)
   
   1C                 // Temperature 4 28c
   32                 // Control Value 4 (Percentage) (32h = PWM 50%)
   
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 6,7 for Maximum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
   // Sensor Record Header
   008D               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   50                 // Control Value 1 (Percentage) (50h = PWM 80%)
   
   0F                 // Temperature 2 15c
   50                 // Control Value 2 (Percentage) (50h = PWM 80%)
   
   19                 // Temperature 3 25c
   50                 // Control Value 3 (Percentage) (50h = PWM 80%)
   
   1C                 // Temperature 4 28c
   50                 // Control Value 4 (Percentage) (50h = PWM 80%)
       


//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3 for Minimum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F

   // Sensor Record Header
   008E               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   14                 // Temperature 2 20c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   1E                 // Temperature 3 30c
   19                 // Control Value 3 (Percentage) (19h = PWM 25%)
   
   3C                 // Temperature 4 60c
   32                 // Control Value 4 (Percentage) (32h = PWM 50%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3 for Maximum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F

   // Sensor Record Header
   008F               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 4,5 for Minimum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   0090               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   14                 // Temperature 2 20c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   1E                 // Temperature 3 30c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   3C                 // Temperature 4 60c
   39                 // Control Value 4 (Percentage) (39h = PWM 57%)    
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 4,5 for Maximum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   0091               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 6,7 for Minimum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   0092               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   33                 // Control Value 1 (Percentage) (33h = PWM 51%)
   
   14                 // Temperature 2 20c
   33                 // Control Value 2 (Percentage) (33h = PWM 51%)
   
   1E                 // Temperature 3 30c
   33                 // Control Value 3 (Percentage) (33h = PWM 51%)
   
   3C                 // Temperature 4 60c
   4C                 // Control Value 4 (Percentage) (4Ch = PWM 76%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 6,7 for Maximum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   0093               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3 for Minimum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F

   // Sensor Record Header
   0094               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   14                 // Temperature 2 20c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   1E                 // Temperature 3 30c
   19                 // Control Value 3 (Percentage) (19h = PWM 25%)
   
   3C                 // Temperature 4 60c
   4B                 // Control Value 5 (Percentage) (4Bh = PWM 75%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3 for Maximum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F

   // Sensor Record Header
   0095               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   3C                 // Temperature 4 60c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 4,5 for Minimum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
   // Sensor Record Header
   0096               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   14                 // Temperature 2 20c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   1E                 // Temperature 3 30c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   3C                 // Temperature 4 60c
   52                 // Control Value 4 (Percentage) (52h = PWM 82%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 4,5 for Maximum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
   // Sensor Record Header
   0097               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 6,7 for Minimum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
// Sensor Record Header
   0098               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   33                 // Control Value 1 (Percentage) (33h = PWM 51%)
   
   14                 // Temperature 2 20c
   33                 // Control Value 2 (Percentage) (33h = PWM 51%)
   
   1E                 // Temperature 3 30c
   33                 // Control Value 3 (Percentage) (33h = PWM 51%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 6,7 for Maximum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
   // Sensor Record Header
   0099               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3 for Minimum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F

   // Sensor Record Header
   009A               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   14                 // Temperature 2 20c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   1E                 // Temperature 3 30c
   19                 // Control Value 3 (Percentage) (19h = PWM 25%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3 for Maximum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F

   // Sensor Record Header
   009B               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   3C                 // Temperature 4 60c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 4,5 for Minimum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
   // Sensor Record Header
   009C               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   14                 // Temperature 2 20c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   1E                 // Temperature 3 30c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 4,5 for Maximum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
   // Sensor Record Header
   009D               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 6,7 for Minimum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
// Sensor Record Header
   009E               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   33                 // Control Value 1 (Percentage) (33h = PWM 51%)
   
   14                 // Temperature 2 20c
   33                 // Control Value 2 (Percentage) (33h = PWM 51%)
   
   1E                 // Temperature 3 30c
   33                 // Control Value 3 (Percentage) (33h = PWM 51%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 6,7 for Maximum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
   // Sensor Record Header
   009F               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00A0               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
    
   00                 // Temperature 1 0c
   32                 // Control Value 1 (Percentage) (32h = PWM 50%)
     
   0F                 // Temperature 2 15c
   32                 // Control Value 2 (Percentage) (32h = PWM 50%)
   
   19                 // Temperature 3 25c
   46                 // Control Value 3 (Percentage) (46h = PWM 70%)
    
   23                 // Temperature 4 35c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)

  
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3 for Maximum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00A1               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0C
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
    
   23                 // Temperature 5 35c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
 
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 4,5 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00A2               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2))
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   32                 // Control Value 1 (Percentage) (32h = PWM 50%)
   
   0F                 // Temperature 2 15c
   32                 // Control Value 2 (Percentage) (32h = PWM 50%)
   
   19                 // Temperature 3 25c
   46                 // Control Value 3 (Percentage) (46h = PWM 70%)
   
   21                 // Temperature 4 33c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 4,5 for Maximum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00A3               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
     
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   21                 // Temperature 4 33c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 6,7 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00A4               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support   = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
  
   00                 // Temperature 1 0c
   32                 // Control Value 1 (Percentage) (32h = PWM 50%)
   
   0F                 // Temperature 2 15c
   32                 // Control Value 2 (Percentage) (32h = PWM 50%)
   
   19                 // Temperature 3 25c
   46                 // Control Value 3 (Percentage) (46h = PWM 70%)
   
   1C                 // Temperature 4 28c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 6,7 for Maximum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00A5               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support   = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
    
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   1C                 // Temperature 4 28c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1 for Minimum
// For SR1630BC Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F

   // Sensor Record Header
   00A6               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   03                 // Fan Profile Support   = 00000011

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   28                 // Control Value 1 (Percentage) (28h = PWM 40%)
   
   0F                 // Temperature 2 15c
   28                 // Control Value 2 (Percentage) (28h = PWM 40%)
   
   19                 // Temperature 3 25c
   37                 // Control Value 3 (Percentage) (37h = PWM 55%)
      
   23                 // Temperature 5 35c
   41                 // Control Value 5 (Percentage) (41h = PWM 65%)
   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 2,3 for Minimum
// For SR1630BC Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F

   // Sensor Record Header
   00A7               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0C                 // Fan Profile Support   = 00001100

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   28                 // Control Value 1 (Percentage) (28h = PWM 40%)
   
   0F                 // Temperature 2 15c
   28                 // Control Value 2 (Percentage) (28h = PWM 40%)
   
   19                 // Temperature 3 25c
   37                 // Control Value 3 (Percentage) (37h = PWM 55%)
      
   23                 // Temperature 5 35c
   4B                 // Control Value 5 (Percentage) (4Bh = PWM 75%)
      
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3 for Maximum
// For SR1630BC Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F

   // Sensor Record Header
   00A8               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support   = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   23                 // Temperature 5 35c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 4,5 for Minimum
// For SR1630BC Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F
   // Sensor Record Header
   00A9               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   32                 // Control Value 1 (Percentage) (32h = PWM 50%)
   
   0F                 // Temperature 2 15c
   32                 // Control Value 2 (Percentage) (32h = PWM 50%)
   
   19                 // Temperature 3 25c
   41                 // Control Value 3 (Percentage) (41h = PWM 65%)
   
   21                 // Temperature 4 33c
   50                 // Control Value 4 (Percentage) (50h = PWM 80%)

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 4,5 for Maximum
// For SR1630BC Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F
   // Sensor Record Header
   00AA               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   21                 // Temperature 4 33c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 6,7 for Minimum
// For SR1630BC Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F
// Sensor Record Header
   00AB               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support  = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
  
   00                 // Temperature 1 0c
   46                 // Control Value 1 (Percentage) (46h = PWM 70%)
   
   0F                 // Temperature 2 15c
   46                 // Control Value 2 (Percentage) (46h = PWM 70%)
   
   19                 // Temperature 3 25c
   55                 // Control Value 3 (Percentage) (55h = PWM 85%)
   
   1C                 // Temperature 4 28c
   5A                 // Control Value 4 (Percentage) (5Ah = PWM 90%)

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 6,7 for Maximum
// For SR1630BC Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F
   // Sensor Record Header
   00AC               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support   = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   1C                 // Temperature 4 28c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3 for Minimum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F

   // Sensor Record Header
   00AD               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   23                 // Temperature 4 35c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3 for Maximum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F

   // Sensor Record Header
   00AE               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   23                 // Temperature 5 35c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 4,5 for Minimum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
   // Sensor Record Header
   00AF               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   21                 // Temperature 4 33c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 4,5 for Maximum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
   // Sensor Record Header
   00B0               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   21                 // Temperature 4 33c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 6,7 for Minimum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
// Sensor Record Header
   00B1               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)

   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   1C                 // Temperature 4 28c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 6,7 for Maximum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #1 (PWM1: System Fan2)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
   // Sensor Record Header
   00B2               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   1C                 // Temperature 4 28c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3 for Minimum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F

   // Sensor Record Header
   00B3               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   14                 // Temperature 2 20c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   1E                 // Temperature 3 30c
   19                 // Control Value 3 (Percentage) (19h = PWM 25%)
   
   3C                 // Temperature 4 60c
   32                 // Control Value 4 (Percentage) (32h = PWM 50%) 
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3 for Maximum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F

   // Sensor Record Header
   00B4               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 4,5 for Minimum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   00B5               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   14                 // Temperature 2 20c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   1E                 // Temperature 3 30c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   3C                 // Temperature 4 60c
   39                 // Control Value 4 (Percentage) (39h = PWM 57%) 
      
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 4,5 for Maximum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   00B6               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 6,7 for Minimum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
// Sensor Record Header
   00B7               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   33                 // Control Value 1 (Percentage) (33h = PWM 51%)
   
   14                 // Temperature 2 20c
   33                 // Control Value 2 (Percentage) (33h = PWM 51%)
   
   1E                 // Temperature 3 30c
   33                 // Control Value 3 (Percentage) (33h = PWM 51%)
   
   3C                 // Temperature 4 60c
   4C                 // Control Value 4 (Percentage) (4Ch = PWM 76%) 
   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 6,7 for Maximum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   00B8               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3 for Minimum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F

   // Sensor Record Header
   00B9               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   14                 // Temperature 2 20c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   1E                 // Temperature 3 30c
   19                 // Control Value 3 (Percentage) (19h = PWM 25%)
   
   3C                 // Temperature 4 60c
   4B                 // Control Value 5 (Percentage) (4Bh = PWM 75%) 
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3 for Maximum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F

   // Sensor Record Header
   00BA               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   3C                 // Temperature 4 60c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 4,5 for Minimum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
   // Sensor Record Header
   00BB               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   14                 // Temperature 2 20c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   1E                 // Temperature 3 30c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   3C                 // Temperature 4 60c
   52                 // Control Value 4 (Percentage) (52h = PWM 82%) 
      
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 4,5 for Maximum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
   // Sensor Record Header
   00BC               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 6,7 for Minimum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
// Sensor Record Header
   00BD               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   33                 // Control Value 1 (Percentage) (33h = PWM 51%)
   
   14                 // Temperature 2 20c
   33                 // Control Value 2 (Percentage) (33h = PWM 51%)
   
   1E                 // Temperature 3 30c
   33                 // Control Value 3 (Percentage) (33h = PWM 51%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 6,7 for Maximum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
   // Sensor Record Header
   00BE               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3 for Minimum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F

   // Sensor Record Header
   00BF               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   14                 // Temperature 2 20c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   1E                 // Temperature 3 30c
   19                 // Control Value 3 (Percentage) (19h = PWM 25%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3 for Maximum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F

   // Sensor Record Header
   00C0               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   3C                 // Temperature 4 60c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 4,5 for Minimum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
   // Sensor Record Header
   00C1               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   14                 // Temperature 2 20c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   1E                 // Temperature 3 30c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
      
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 4,5 for Maximum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
   // Sensor Record Header
   00C2               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 6,7 for Minimum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
// Sensor Record Header
   00C3               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   33                 // Control Value 1 (Percentage) (33h = PWM 51%)
   
   14                 // Temperature 2 20c
   33                 // Control Value 2 (Percentage) (33h = PWM 51%)
   
   1E                 // Temperature 3 30c
   33                 // Control Value 3 (Percentage) (33h = PWM 51%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 6,7 for Maximum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
   // Sensor Record Header
   00C4               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00C5               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support   = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
      
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   0F                 // Temperature 2 15c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   19                 // Temperature 3 25c
   23                 // Control Value 3 (Percentage) (23h = PWM 35%)

   23                 // Temperature 4 35c
   46                 // Control Value 4 (Percentage) (46h = PWM 70%)  
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3 for Maximum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00C6               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support   = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
     
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   23                 // Temperature 5 35c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 4,5 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00C7               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A               // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
    
   00                 // Temperature 1 0c
   23                 // Control Value 1 (Percentage) (23h = PWM 35%)
    
   0F                 // Temperature 2 15c
   23                 // Control Value 2 (Percentage) (23h = PWM 35%)
   
   19                 // Temperature 3 25c
   37                 // Control Value 3 (Percentage) (37h = PWM 55%)
   
   21                 // Temperature 4 33c
   4B                 // Control Value 4 (Percentage) (4Bh = PWM 75%)

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 4,5 for Maximum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F
   // Sensor Record Header
   00C8               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
     
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   21                 // Temperature 4 33c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 6,7 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00C9               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support   = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   37                 // Control Value 1 (Percentage) (37h = PWM 55%)
   
   0F                 // Temperature 2 15c
   37                 // Control Value 2 (Percentage) (37h = PWM 55%)
   
   19                 // Temperature 3 25c
   48                 // Control Value 3 (Percentage) (48h = PWM 72%)
   
   1C                 // Temperature 4 28c
   50                 // Control Value 4 (Percentage) (50h = PWM 80%) 
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 6,7 for Maximum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00CA               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support   = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
  
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   1C                 // Temperature 4 28c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)    
   

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3 for Minimum
// For SR1630BC Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F

   // Sensor Record Header
   00CB               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support   = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
  
   00                 // Temperature 1 0c
   37                 // Control Value 1 (Percentage) (37h = PWM 55%)
   
   0F                 // Temperature 2 15c
   37                 // Control Value 2 (Percentage) (37h = PWM 55%)
   
   19                 // Temperature 3 25c
   41                 // Control Value 3 (Percentage) (41h = PWM 65%)
     
   23                 // Temperature 5 35c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
   
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3 for Maximum
// For SR1630BC Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F

   // Sensor Record Header
   00CC               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support   = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   23                 // Temperature 5 35c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 4,5 for Minimum
// For SR1630BC Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F

   // Sensor Record Header
   00CD               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   41                 // Control Value 1 (Percentage) (41h = PWM 65%)
   
   0F                 // Temperature 2 15c
   41                 // Control Value 2 (Percentage) (41h = PWM 65%)
   
   19                 // Temperature 3 25c
   50                 // Control Value 3 (Percentage) (50h = PWM 80%)
   
   21                 // Temperature 4 33c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 4,5 for Maximum
// For SR1630BC Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F

   // Sensor Record Header
   00CE               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM1: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
    
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
    
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   21                 // Temperature 4 33c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 6,7 for Minimum
// For SR1630BC Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F

   // Sensor Record Header
   00CF               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support   = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
  
   00                 // Temperature 1 0c
   4B                 // Control Value 1 (Percentage) (4Bh = PWM 75%)
   
   0F                 // Temperature 2 15c
   4B                 // Control Value 2 (Percentage) (4Bh = PWM 75%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   1C                 // Temperature 4 28c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 6,7 for Maximum
// For SR1630BC Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       001F

   // Sensor Record Header
   00D0               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support   = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   1C                 // Temperature 4 28c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3 for Minimum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F

   // Sensor Record Header
   00D1               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   23                 // Temperature 4 35c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3 for Maximum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F

   // Sensor Record Header
   00D2               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   23                 // Temperature 5 35c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 4,5 for Minimum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
   // Sensor Record Header
   00D3               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   21                 // Temperature 4 33c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
   
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 4,5 for Maximum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
   // Sensor Record Header
   00D4               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   21                 // Temperature 4 33c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)   
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 6,7 for Minimum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
// Sensor Record Header
   00D5               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)

   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   1C                 // Temperature 4 28c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
   
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 6,7 for Maximum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #2 (PWM2: System Fan1)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
   // Sensor Record Header
   00D6               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   1C                 // Temperature 4 28c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
   
   
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3 for Minimum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F

   // Sensor Record Header
   00D7               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   14                 // Temperature 2 20c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   1E                 // Temperature 3 30c
   19                 // Control Value 3 (Percentage) (19h = PWM 25%)
   
   3C                 // Temperature 4 60c
   32                 // Control Value 4 (Percentage) (32h = PWM 50%) 
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3 for Maximum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F

   // Sensor Record Header
   00D8               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 4,5 for Minimum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   00D9               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   14                 // Temperature 2 20c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   1E                 // Temperature 3 30c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   3C                 // Temperature 4 60c
   39                 // Control Value 4 (Percentage) (39h = PWM 57%) 
      
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 4,5 for Maximum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   00DA               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 6,7 for Minimum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
// Sensor Record Header
   00DB               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   33                 // Control Value 1 (Percentage) (33h = PWM 51%)
   
   14                 // Temperature 2 20c
   33                 // Control Value 2 (Percentage) (33h = PWM 51%)
   
   1E                 // Temperature 3 30c
   33                 // Control Value 3 (Percentage) (33h = PWM 51%)
   
   3C                 // Temperature 4 60c
   4C                 // Control Value 4 (Percentage) (4Ch = PWM 76%) 
   
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 6,7 for Maximum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   00DC               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3 for Minimum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F

   // Sensor Record Header
   00DD               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   14                 // Temperature 2 20c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   1E                 // Temperature 3 30c
   19                 // Control Value 3 (Percentage) (19h = PWM 25%)
   
   3C                 // Temperature 4 60c
   4B                 // Control Value 5 (Percentage) (4Bh = PWM 75%) 
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3 for Maximum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F

   // Sensor Record Header
   00DE               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   3C                 // Temperature 4 60c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 4,5 for Minimum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
   // Sensor Record Header
   00DF               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   14                 // Temperature 2 20c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   1E                 // Temperature 3 30c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   3C                 // Temperature 4 60c
   52                 // Control Value 4 (Percentage) (52h = PWM 82%) 
      
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 4,5 for Maximum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
   // Sensor Record Header
   00E0               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 6,7 for Minimum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
// Sensor Record Header
   00E1               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   33                 // Control Value 1 (Percentage) (33h = PWM 51%)
   
   14                 // Temperature 2 20c
   33                 // Control Value 2 (Percentage) (33h = PWM 51%)
   
   1E                 // Temperature 3 30c
   33                 // Control Value 3 (Percentage) (33h = PWM 51%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 6,7 for Maximum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
   // Sensor Record Header
   00E2               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3 for Minimum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F

   // Sensor Record Header
   00E3               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   14                 // Temperature 2 20c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   1E                 // Temperature 3 30c
   19                 // Control Value 3 (Percentage) (19h = PWM 25%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3 for Maximum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F

   // Sensor Record Header
   00E4               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   3C                 // Temperature 4 60c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 4,5 for Minimum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
   // Sensor Record Header
   00E5               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   14                 // Temperature 2 20c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   1E                 // Temperature 3 30c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
      
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 4,5 for Maximum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
   // Sensor Record Header
   00E6               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 6,7 for Minimum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
// Sensor Record Header
   00E7               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   33                 // Control Value 1 (Percentage) (33h = PWM 51%)
   
   14                 // Temperature 2 20c
   33                 // Control Value 2 (Percentage) (33h = PWM 51%)
   
   1E                 // Temperature 3 30c
   33                 // Control Value 3 (Percentage) (33h = PWM 51%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 6,7 for Maximum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
   // Sensor Record Header
   00E8               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #3 (PWM3: System Fan3)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00E9               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3 )
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support   = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   46                 // Temp Sensor failure control Value (46h = PWM 70%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
     
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   0F                 // Temperature 2 15c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   19                 // Temperature 3 25c
   23                 // Control Value 3 (Percentage) (23h = PWM 35%)
     
   23                 // Temperature 4 35c
   32                 // Control Value 4 (Percentage) (32h = PWM 50%)
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3 for Maximum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #3 (PWM3: System Fan3)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00EA               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support   = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   46                 // Temp Sensor failure control Value (46h = PWM 70%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
     
   00                 // Temperature 1 0c
   46                 // Control Value 1 (Percentage) (46h = PWM 70%)
    
   0F                 // Temperature 2 15c
   46                 // Control Value 2 (Percentage) (46h = PWM 70%)
   
   19                 // Temperature 3 25c
   46                 // Control Value 3 (Percentage) (46h = PWM 70%)
     
   23                 // Temperature 4 35c
   46                 // Control Value 4 (Percentage) (46h = PWM 70%)

//=========================================================================//
// Chassis Fan Control Domain 3 with profile 4,5 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #3 (PWM3: System Fan3)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00EB               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3 )
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   46                 // Temp Sensor failure control Value (46h = PWM 70%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   28                 // Control Value 1 (Percentage) (28h = PWM 40%)
   
   0F                 // Temperature 2 15c
   28                 // Control Value 2 (Percentage) (28h = PWM 40%)
   
   19                 // Temperature 3 25c
   2D                 // Control Value 3 (Percentage) (2Dh = PWM 45%)
   
   21                 // Temperature 4 33c
   38                 // Control Value 4 (Percentage) (38h = PWM 56%)
   
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 4,5 for Maximum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #3 (PWM3: System Fan3)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00EC               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   46                 // Temp Sensor failure control Value (46h = PWM 70%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
  
   00                 // Temperature 1 0c
   46                 // Control Value 1 (Percentage) (46h = PWM 70%)
   
   0F                 // Temperature 2 15c
   46                 // Control Value 2 (Percentage) (46h = PWM 70%)
   
   19                 // Temperature 3 25c
   46                 // Control Value 3 (Percentage) (46h = PWM 70%)
   
   21                 // Temperature 4 33c
   46                 // Control Value 4 (Percentage) (46h = PWM 70%)

//=========================================================================//
// Chassis Fan Control Domain 3 with profile 6,7 for Minimum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #3 (PWM3: System Fan3)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00ED               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3 )
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support   = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   46                 // Temp Sensor failure control Value (46h = PWM 70%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   2D                 // Control Value 1 (Percentage) (2Dh = PWM 45%)
   
   0F                 // Temperature 2 15c
   2D                 // Control Value 2 (Percentage) (2Dh = PWM 45%)
   
   19                 // Temperature 3 25c
   38                 // Control Value 3 (Percentage) (38h = PWM 56%)
   
   1C                 // Temperature 4 28c
   3C                 // Control Value 4 (Percentage) (3Ch = PWM 60%)

//=========================================================================//
// Chassis Fan Control Domain 3 with profile 6,7 for Maximum
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #3 (PWM3: System Fan3)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       001F

   // Sensor Record Header
   00EE               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support   = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   21                 // Temperature Sensor Number -- (FP Amb)
   46                 // Temp Sensor failure control Value (46h = PWM 70%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//   
   04                 // Count of Temperature/Control Value Pairs (04h=4)
    
   00                 // Temperature 1 0c
   46                 // Control Value 1 (Percentage) (46h = PWM 70%)
     
   0F                 // Temperature 2 15c
   46                 // Control Value 2 (Percentage) (46h = PWM 70%)
   
   19                 // Temperature 3 25c
   46                 // Control Value 3 (Percentage) (46h = PWM 70%)
   
   1C                 // Temperature 4 28c
   46                 // Control Value 4 (Percentage) (46h = PWM 70%)

//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3 for Minimum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #3 (PWM3: System Fan3)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F

   // Sensor Record Header
   00EF               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   23                 // Temperature 4 35c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3 for Maximum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #3 (PWM3: System Fan3)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F

   // Sensor Record Header
   00F0               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   23                 // Temperature 5 35c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 4,5 for Minimum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #3 (PWM3: System Fan3)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
   // Sensor Record Header
   00F1               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   21                 // Temperature 4 33c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
   
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 4,5 for Maximum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #3 (PWM3: System Fan3)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
   // Sensor Record Header
   00F2               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   21                 // Temperature 4 33c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)   
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 6,7 for Minimum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #3 (PWM3: System Fan3)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
// Sensor Record Header
   00F3               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)

   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   1C                 // Temperature 4 28c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
   
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 6,7 for Maximum
// For Other Chassis (Full Speed)
// Fan Control Domain Number #3 (PWM3: System Fan3)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001F
   // Sensor Record Header
   00F4               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   0F                 // Temperature 2 15c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   19                 // Temperature 3 25c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   1C                 // Temperature 4 28c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
   
   
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3 for Minimum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F

   // Sensor Record Header
   00F5               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   14                 // Temperature 2 20c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   1E                 // Temperature 3 30c
   19                 // Control Value 3 (Percentage) (19h = PWM 25%)
   
   3C                 // Temperature 4 60c
   32                 // Control Value 4 (Percentage) (32h = PWM 50%) 
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3 for Maximum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F

   // Sensor Record Header
   00F6               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 4,5 for Minimum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   00F7               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   14                 // Temperature 2 20c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   1E                 // Temperature 3 30c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   3C                 // Temperature 4 60c
   39                 // Control Value 4 (Percentage) (39h = PWM 57%) 
      
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 4,5 for Maximum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   00F8               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 6,7 for Minimum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
// Sensor Record Header
   00F9               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   33                 // Control Value 1 (Percentage) (33h = PWM 51%)
   
   14                 // Temperature 2 20c
   33                 // Control Value 2 (Percentage) (33h = PWM 51%)
   
   1E                 // Temperature 3 30c
   33                 // Control Value 3 (Percentage) (33h = PWM 51%)
   
   3C                 // Temperature 4 60c
   4C                 // Control Value 4 (Percentage) (4Ch = PWM 76%) 
   
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 6,7 for Maximum
// For Other Chassis (Slow ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_REC_LEN       001F
   // Sensor Record Header
   00FA               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 

//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3 for Minimum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F

   // Sensor Record Header
   00FB               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   14                 // Temperature 2 20c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   1E                 // Temperature 3 30c
   19                 // Control Value 3 (Percentage) (19h = PWM 25%)
   
   3C                 // Temperature 4 60c
   4B                 // Control Value 5 (Percentage) (4Bh = PWM 75%) 
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3 for Maximum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F

   // Sensor Record Header
   00FC               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   3C                 // Temperature 4 60c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 4,5 for Minimum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
   // Sensor Record Header
   00FD               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   14                 // Temperature 2 20c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   1E                 // Temperature 3 30c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   3C                 // Temperature 4 60c
   52                 // Control Value 4 (Percentage) (52h = PWM 82%) 
      
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 4,5 for Maximum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
   // Sensor Record Header
   00FE               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 6,7 for Minimum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
// Sensor Record Header
   00FF               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   33                 // Control Value 1 (Percentage) (33h = PWM 51%)
   
   14                 // Temperature 2 20c
   33                 // Control Value 2 (Percentage) (33h = PWM 51%)
   
   1E                 // Temperature 3 30c
   33                 // Control Value 3 (Percentage) (33h = PWM 51%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 6,7 for Maximum
// For Other Chassis (Medium ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_MR'
_REC_LEN       001F
   // Sensor Record Header
   0100               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3 for Minimum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F

   // Sensor Record Header
   0101               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   19                 // Control Value 1 (Percentage) (19h = PWM 25%)
   
   14                 // Temperature 2 20c
   19                 // Control Value 2 (Percentage) (19h = PWM 25%)
   
   1E                 // Temperature 3 30c
   19                 // Control Value 3 (Percentage) (19h = PWM 25%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3 for Maximum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F

   // Sensor Record Header
   0102               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   0F                 // Fan Profile Support = 00001111

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value (NA)
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------//
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
     
   3C                 // Temperature 4 60c
   64                 // Control Value 5 (Percentage) (64h = PWM 100%)
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 4,5 for Minimum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
   // Sensor Record Header
   0103               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support   = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   20                 // Control Value 1 (Percentage) (20h = PWM 32%)
   
   14                 // Temperature 2 20c
   20                 // Control Value 2 (Percentage) (20h = PWM 32%)
   
   1E                 // Temperature 3 30c
   20                 // Control Value 3 (Percentage) (20h = PWM 32%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
      
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 4,5 for Maximum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
   // Sensor Record Header
   0104               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   30                 // Fan Profile Support = 00110000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 6,7 for Minimum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================//  
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
// Sensor Record Header
   0105               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   10                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=0; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   33                 // Control Value 1 (Percentage) (33h = PWM 51%)
   
   14                 // Temperature 2 20c
   33                 // Control Value 2 (Percentage) (33h = PWM 51%)
   
   1E                 // Temperature 3 30c
   33                 // Control Value 3 (Percentage) (33h = PWM 51%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 6,7 for Maximum
// For Other Chassis (Fast ramp)
// Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
//====================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FR'
_REC_LEN       001F
   // Sensor Record Header
   0106               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   C0                 // Fan Profile Support = 11000000

   // Stepwise Linear type Temperature Sensor Sub-record
   20                 // Sensor Owner ID
   20                 // Temperature Sensor Number -- (BB Amb)
   64                 // Temp Sensor failure control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   41                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (001b=Stepwise linear)
   50                 // Temperature Info [7]-Reserved; [6]-Domain Maximum=1; [5:3]-Negative Hysteresis=2; [2:0]-Positive Hysteresis=0
//------------------------------------------------------------------// 
   04                 // Count of Temperature/Control Value Pairs (04h=4)
   
   00                 // Temperature 1 0c
   64                 // Control Value 1 (Percentage) (64h = PWM 100%)
   
   14                 // Temperature 2 20c
   64                 // Control Value 2 (Percentage) (64h = PWM 100%)
   
   1E                 // Temperature 3 30c
   64                 // Control Value 3 (Percentage) (64h = PWM 100%)
   
   3C                 // Temperature 4 60c
   64                 // Control Value 4 (Percentage) (64h = PWM 100%) 
   
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SC5650DP/SC5650BRP Chassis with one/two CPU(NHM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_PROC_NHM'
_SDR_TAG       'SC5650BRP_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   0107               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   38                 // Temp Sensor Fail Control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SC5650DP/SC5650BRP Chassis with one/two CPU(WSM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_PROC_WSM'
_SDR_TAG       'SC5650BRP_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   0108               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   38                 // Temp Sensor Fail Control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)
    
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SC5650DP/SC5650BRP Chassis with two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_2P_PROC_NHM'
_SDR_TAG       'SC5650BRP_2P_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   0109               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   38                 // Temp Sensor Fail Control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)  
   
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SC5650DP/SC5650BRP Chassis with two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_2P_PROC_WSM'
_SDR_TAG       'SC5650BRP_2P_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   010A               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   38                 // Temp Sensor Fail Control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)
   
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SC5650DP/SC5650BRP Chassis with one/two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (IOH Temp)
//=========================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_1P'
_SDR_TAG       'SC5650DP_2P'
_SDR_TAG       'SC5650BRP_1P'
_SDR_TAG       'SC5650BRP_2P'
_REC_LEN       001A

   // Sensor Record Header
   010B               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   22                 // Temperature Sensor Number -- (IOH Temp)
   38                 // Temp Sensor Fail Control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   F8                 // NHM/WSM Clamp Temperature (F8h = -8 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)  
  
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,2,4,6 (CLTT only)
// For SC5650DP/SC5650BRP Chassis with one/two CPU(NHM/WSM)
// Clamp Fan Speed Control Records (MEM A)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_1P'
_SDR_TAG       'SC5650DP_2P'
_SDR_TAG       'SC5650BRP_1P'
_SDR_TAG       'SC5650BRP_2P'
_REC_LEN       001A

   // Sensor Record Header
   010C               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support   = 01010101 CLTT-only
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   23                 // Temperature Sensor Number -- (MEM A)
   38                 // Temp Sensor Fail Control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   3A                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 2
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   FB                 // NHM/WSM Clamp Temperature (FBh = -5 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
     
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,2,4,6 (CLTT only)
// For SC5650DP/SC5650BRP Chassis with NHM/WSM CPU
// Clamp Fan Speed Control Records (MEM B)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_2P'
_SDR_TAG       'SC5650BRP_2P'
_REC_LEN       001A

   // Sensor Record Header
   010D               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support   = 01010101 CLTT-only
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   24                 // Temperature Sensor Number -- (MEM B)
   38                 // Temp Sensor Fail Control Value (38h = PWM 56%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   3A                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 2
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   FB                 // NHM/WSM Clamp Temperature (FBh = -5 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)  
     
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with one/two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_PROC_NHM'
_SDR_TAG       'OTHER_SR_PROC_NHM'
_SDR_TAG       'OTHER_MR_PROC_NHM'
_SDR_TAG       'OTHER_FR_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   010E               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with one/two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_PROC_WSM'
_SDR_TAG       'OTHER_SR_PROC_WSM'
_SDR_TAG       'OTHER_MR_PROC_WSM'
_SDR_TAG       'OTHER_FR_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   010F               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)
   
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_2P_PROC_NHM'
_SDR_TAG       'OTHER_SR_2P_PROC_NHM'
_SDR_TAG       'OTHER_MR_2P_PROC_NHM'
_SDR_TAG       'OTHER_FR_2P_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   0110               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_2P_PROC_WSM'
_SDR_TAG       'OTHER_SR_2P_PROC_WSM'
_SDR_TAG       'OTHER_MR_2P_PROC_WSM'
_SDR_TAG       'OTHER_FR_2P_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   0111               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)
   
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with one/two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (IOH Temp)
//=========================================================================//
_SDR_TYPE      C0
_SDR_TAG       'Other_1P'
_SDR_TAG       'Other_2P'
_REC_LEN       001A

   // Sensor Record Header
   0112               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   22                 // Temperature Sensor Number -- (IOH Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   FC                 // NHM/WSM Clamp Temperature (FCh = -4 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
  
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,2,4,6 (CLTT only)
// For Other Chassis with one/two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM A)
//=========================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001A

   // Sensor Record Header
   0113               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support   = 01010101 CLTT-only
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   23                 // Temperature Sensor Number -- (MEM A)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   32                 // NHM/WSM Clamp Temperature (32h = 50 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0) 
   
   
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,2,4,6 (CLTT only)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with one/two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM A)
//=========================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR'
_SDR_TAG       'OTHER_MR'
_SDR_TAG       'OTHER_FR'
_REC_LEN       001A

   // Sensor Record Header
   0114               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support   = 01010101 CLTT-only
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   23                 // Temperature Sensor Number -- (MEM A)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   FD                 // NHM/WSM Clamp Temperature (FDh = -3 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0) 
   
     
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,2,4,6 (CLTT only)
// For Other Chassis with two CPUs (NHM/WSM)
// Clamp Fan Speed Control Records (MEM B)
//=========================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_2P_PROC_WSM'
_SDR_TAG       'OTHER_FS_2P_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   0115               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support   = 01010101 CLTT-only
    
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   24                 // Temperature Sensor Number -- (MEM B)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   32                 // NHM/WSM Clamp Temperature (32h = 50 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)

//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,2,4,6 (CLTT only)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with two CPUs (NHM/WSM)
// Clamp Fan Speed Control Records (MEM B)
//=========================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_SR_2P_PROC_NHM'
_SDR_TAG       'OTHER_SR_2P_PROC_WSM'
_SDR_TAG       'OTHER_MR_2P_PROC_NHM'
_SDR_TAG       'OTHER_MR_2P_PROC_WSM'
_SDR_TAG       'OTHER_FR_2P_PROC_NHM'
_SDR_TAG       'OTHER_FR_2P_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   0116               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support   = 01010101 CLTT-only
    
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   24                 // Temperature Sensor Number -- (MEM B)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   FD                 // NHM/WSM Clamp Temperature (FDh = -3 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
   
   
   
//=========================================================================//
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For FCT/SHIP (FULL SPEED)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       001A

   // Sensor Record Header
   0117               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 
   64                 // Normal Control Value (64h = PWM 100%)
   64                 // Boost Control Value  (64h = PWM 100%)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   64                 // Sleep Control Value            (64h = PWM 100%)
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   00                 // NHM/WSM Clamp Temperature (00h = 0 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #1 (PWM1: System Fan2)
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SR1630BC Chassis with one CPU or two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   0118               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)
   
 //=========================================================================//
// Fan Control Domain Number #1 (PWM1: System Fan2)
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SR1630BC Chassis with one CPU or two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   0119               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)
   
//=========================================================================//
// Fan Control Domain Number #1 (PWM1: System Fan2)
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SR1630BC Chassis with one CPU or two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (IOH Temp)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC_1P'
_SDR_TAG       'SR1630BC_2P'
_REC_LEN       001A

   // Sensor Record Header
   011A               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM0: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   22                 // Temperature Sensor Number -- (IOH Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   F8                 // NHM/WSM Clamp Temperature (F8h = -8 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
   
//=========================================================================//
// Fan Control Domain Number #1 (PWM1: System Fan2)
// Chassis Fan Control Domain 1 with profile 0,2,4,6 (CLTT only)
// For SR1630BC Chassis with one CPU or two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM A)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC_1P'
_SDR_TAG       'SR1630BC_2P'
_REC_LEN       001A

   // Sensor Record Header
   011B               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support  = 01010101 CLTT-only
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   23                 // Temperature Sensor Number -- (MEM A)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   FB                 // NHM/WSM Clamp Temperature (FBh = -5 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)

//=========================================================================//
// Fan Control Domain Number #1 (PWM1: System Fan2)
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with one/two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   011C               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #1 (PWM1: System Fan2)
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with one/two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   011D               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)
  
//=========================================================================//
// Fan Control Domain Number #1 (PWM1: System Fan2)
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_2P_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   011E               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #1 (PWM1: System Fan2)
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_2P_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   011F               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)
   
//=========================================================================//
// Fan Control Domain Number #1 (PWM1: System Fan2)
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with one/two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (IOH Temp)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'Other_1P'
_SDR_TAG       'Other_2P'
_REC_LEN       001A

   // Sensor Record Header
   0120               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   22                 // Temperature Sensor Number -- (IOH Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   FC                 // NHM/WSM Clamp Temperature (FCh = -4 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0) 
     
//=========================================================================//
// Fan Control Domain Number #1 (PWM1: System Fan2)
// Chassis Fan Control Domain 1 with profile 0,2,4,6 (CLTT only)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with one/two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM A Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'Other_1P'
_SDR_TAG       'Other_2P'
_REC_LEN       001A

   // Sensor Record Header
   0121               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support   = 01010101 CLTT-only
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   23                 // Temperature Sensor Number -- (MEM A)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   FD                 // NHM/WSM Clamp Temperature (FDh = -3 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
   
   
//=========================================================================//
// Fan Control Domain Number #1 (PWM1: System Fan2)
// Chassis Fan Control Domain 1 with profile 0,2,4,6 (CLTT only)
// For SC5650DP/SC5650BRP/ Chassis with two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM B Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_2P_PROC_NHM'
_SDR_TAG       'OTHER_FS_2P_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   0122               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support   = 01010101 CLTT-only
    
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   24                 // Temperature Sensor Number -- (MEM B)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   FD                 // NHM/WSM Clamp Temperature (FDh = -3 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
 
//=========================================================================//
// Fan Control Domain Number #1 (PWM1: System Fan2)
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For FCT/SHIP (FULL SPEED)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       001A

   // Sensor Record Header
   0123               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 
   64                 // Normal Control Value (64h = PWM 100%)
   64                 // Boost Control Value  (64h = PWM 100%)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   64                 // Sleep Control Value            (64h = PWM 100%)
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   00                 // NHM/WSM Clamp Temperature (00h = 0 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)  
 
//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SC5650DP/SC5650BRP Chassis with two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_2P_PROC_NHM'
_SDR_TAG       'SC5650BRP_2P_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   0124               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SC5650DP/SC5650BRP Chassis with two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_2P_PROC_WSM'
_SDR_TAG       'SC5650BRP_2P_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   0125               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)   
   
//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,2,4,6 (CLTT only)
// For SC5650DP/SC5650BRP Chassis with two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM B Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_2P'
_SDR_TAG       'SC5650BRP_2P'
_REC_LEN       001A

   // Sensor Record Header
   0126               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support  = 01010101 CLTT-only
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   24                 // Temperature Sensor Number -- (MEM B)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   3A                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 2
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   FB                 // NHM/WSM Clamp Temperature (FBh = -5 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
  
//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,2,4,6 (CLTT only)
// For SR1630BC Chassis with two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC_2P_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   0127               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   F7                 // NHM Clamp Temperature (F7h = -9 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,2,4,6 (CLTT only)
// For SR1630BC Chassis with two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC_2P_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   0128               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   F7                 // WSM Clamp Temperature (F7h = -9 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)
   
//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,2,4,6 (CLTT only)
// For SR1630BC Chassis with two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM B Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC_2P'
_REC_LEN       001A

   // Sensor Record Header
   0129               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support  = 01010101 CLTT-only
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   24                 // Temperature Sensor Number -- (MEM B)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   FB                 // NHM/WSM Clamp Temperature (FBh = -5 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
 
//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with one/two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   012A               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with one/two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   012B               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)
      
//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_2P_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   012C               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)

 //=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other Chassis with two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_2P_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   012D               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)
   
//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with one/two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (IOH Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'Other_1P'
_SDR_TAG       'Other_2P'
_REC_LEN       001A

   // Sensor Record Header
   012E               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   22                 // Temperature Sensor Number -- (IOH Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   FC                 // NHM/WSM Clamp Temperature (FCh = -4 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
 
//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,2,4,6 (CLTT only)
// For Other Chassis with one/two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM A Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS'
_REC_LEN       001A

   // Sensor Record Header
   012F               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support   = 01010101 CLTT-only
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   23                 // Temperature Sensor Number -- (MEM A)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   FD                 // NHM/WSM Clamp Temperature (FDh = -3 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
   
   
//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,2,4,6 (CLTT only)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM B Temp)
//=========================================================================//    
_SDR_TYPE      C0
_SDR_TAG       'Other_2P'
_REC_LEN       001A

   // Sensor Record Header
   0130               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support   = 01010101 CLTT-only
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   24                 // Temperature Sensor Number -- (MEM B)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   FD                 // NHM/WSM Clamp Temperature (FDh = -3 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
   
//=========================================================================//
// Fan Control Domain Number #2 (PWM2: System Fan1)
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For FCT/SHIP (FULL SPEED)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//       
_SDR_TYPE      C0
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       001A

   // Sensor Record Header
   0131               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 
   64                 // Normal Control Value (64h = PWM 100%)
   64                 // Boost Control Value  (64h = PWM 100%)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   64                 // Sleep Control Value            (64h = PWM 100%)
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   00                 // NHM/WSM Clamp Temperature (00h = 0 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1) 
 
//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SC5650DP/SC5650BRP Chassis with one/two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//       
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_PROC_NHM'
_SDR_TAG       'SC5650BRP_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   0132               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   46                 // Temp Sensor Fail Control Value (46h = PWM 70%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)

 //=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SC5650DP/SC5650BRP Chassis with one/two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//       
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_PROC_WSM'
_SDR_TAG       'SC5650BRP_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   0133               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   46                 // Temp Sensor Fail Control Value (46h = PWM 70%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)
     
//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SC5650DP/SC5650BRP Chassis with two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//       
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_2P_PROC_NHM'
_SDR_TAG       'SC5650BRP_2P_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   0134               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   46                 // Temp Sensor Fail Control Value (46h = PWM 70%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SC5650DP/SC5650BRP Chassis with two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//       
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_2P_PROC_WSM'
_SDR_TAG       'SC5650BRP_2P_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   0135               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   46                 // Temp Sensor Fail Control Value (46h = PWM 70%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For SC5650DP/SC5650BRP Chassis with two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (IOH Temp)
//=========================================================================//       
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_1P'
_SDR_TAG       'SC5650DP_2P'
_SDR_TAG       'SC5650BRP_1P'
_SDR_TAG       'SC5650BRP_2P'
_REC_LEN       001A

   // Sensor Record Header
   0136               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   22                 // Temperature Sensor Number -- (IOH Temp)
   46                 // Temp Sensor Fail Control Value (46h = PWM 70%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   F8                 // NHM/WSM Clamp Temperature (F8h = -8 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
   
//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,2,4,6 (CLTT only)
// For SC5650DP/SC5650BRP Chassis with one/two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM A Temp)
//=========================================================================//       
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_1P'
_SDR_TAG       'SC5650DP_2P'
_SDR_TAG       'SC5650BRP_1P'
_SDR_TAG       'SC5650BRP_2P'
_REC_LEN       001A
   // Sensor Record Header
   0137               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support  = 01010101 CLTT-only
  
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   23                 // Temperature Sensor Number -- (MEM A)
   46                 // Temp Sensor Fail Control Value (46h = PWM 70%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   3A                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 2
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   FB                 // NHM/WSM Clamp Temperature (FBh = -5 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
   
//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,2,4,6 (CLTT only)
// For SC5650DP/SC5650BRP Chassis with two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM B Temp)
//=========================================================================//       
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP_2P'
_SDR_TAG       'SC5650BRP_2P'
_REC_LEN       001A
   // Sensor Record Header
   0138               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support  = 01010101 CLTT-only

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   24                 // Temperature Sensor Number -- (MEM B)
   46                 // Temp Sensor Fail Control Value (46h = PWM 70%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   3A                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 2
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   FB                 // NHM/WSM Clamp Temperature (FBh = -5 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0) 
   
//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with one/two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_PROC_NHM'
_SDR_TAG       'OTHER_SR_PROC_NHM'
_SDR_TAG       'OTHER_MR_PROC_NHM'
_SDR_TAG       'OTHER_FR_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   0139               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with one/two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_PROC_WSM'
_SDR_TAG       'OTHER_SR_PROC_WSM'
_SDR_TAG       'OTHER_MR_PROC_WSM'
_SDR_TAG       'OTHER_FR_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   013A               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)

//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with two CPUs(NHM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_2P_PROC_NHM'
_SDR_TAG       'OTHER_SR_2P_PROC_NHM'
_SDR_TAG       'OTHER_MR_2P_PROC_NHM'
_SDR_TAG       'OTHER_FR_2P_PROC_NHM'
_REC_LEN       001A

   // Sensor Record Header
   013B               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // NHM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)
  
//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with two CPUs(WSM)
// Clamp Fan Speed Control Records (Processor 2 Temp)
//=========================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'OTHER_FS_2P_PROC_WSM'
_SDR_TAG       'OTHER_SR_2P_PROC_WSM'
_SDR_TAG       'OTHER_MR_2P_PROC_WSM'
_SDR_TAG       'OTHER_FR_2P_PROC_WSM'
_REC_LEN       001A

   // Sensor Record Header
   013C               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   63                 // Temperature Sensor Number -- (Processor 2 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   06                 // WSM Clamp Temperature (06h = +6 degree C)
   11                 // Clamp Flag  (CPU number = 1; temp source = 1)
    
//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with one/two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (IOH Temp)
//=========================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'Other_1P'
_SDR_TAG       'Other_2P'
_REC_LEN       001A

   // Sensor Record Header
   013D               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support= 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   22                 // Temperature Sensor Number -- (IOH Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   FC                 // NHM/WSM Clamp Temperature (FCh = -4 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
     
//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,2,4,6 (CLTT only)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with one/two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM A Temp)
//=========================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'Other_1P'
_SDR_TAG       'Other_2P'
_REC_LEN       001A

   // Sensor Record Header
   013E               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support   = 01010101 CLTT-only
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   23                 // Temperature Sensor Number -- (MEM A)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   FD                 // NHM/WSM Clamp Temperature (FDh = -3 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0)
   
//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,2,4,6 (CLTT only)
// For Other/Slow ramp/Medium ramp/Fast ramp Chassis with two CPUs(NHM/WSM)
// Clamp Fan Speed Control Records (MEM B Temp)
//=========================================================================//   
_SDR_TYPE      C0
_SDR_TAG       'Other_2P'
_REC_LEN       001A

   // Sensor Record Header
   013F               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   55                 // Fan Profile Support   = 01010101 CLTT-only
   
   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   24                 // Temperature Sensor Number -- (MEM B)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   00                 // Sleep Control Value 
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   38                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 7; [2:0]-Positive Hysteresis = 0
   00                 // Ramp Coefficient (LSB) (00h)
   01                 // Ramp Coefficient (MSB) (01h)
   FD                 // NHM/WSM Clamp Temperature (FDh = -3 degree C)
   00                 // Clamp Flag  (no CPU number; temp source = 0) 
   
//=========================================================================//
// Fan Control Domain Number #3 (PWM3: System Fan3)
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7 (OLTT and CLTT)
// For FCT/SHIP (FULL SPEED)
// Clamp Fan Speed Control Records (Processor 1 Temp)
//=========================================================================//     
_SDR_TYPE      C0
_SDR_TAG       'FCT'
_SDR_TAG       'SHIP'
_REC_LEN       001A
   // Sensor Record Header
   0140               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 
   64                 // Normal Control Value (64h = PWM 100%)
   64                 // Boost Control Value  (64h = PWM 100%)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support   = 11111111

   // Clamp Type Temperature Sensor sub-record
   20                 // Sensor Owner ID
   62                 // Temperature Sensor Number -- (Processor 1 Temp)
   64                 // Temp Sensor Fail Control Value (64h = PWM 100%)
   64                 // Sleep Control Value            (64h = PWM 100%)
   42                 // [7:6]-Supported in S1 (1=yes); [5:3]-Reserved; [2:0]-Control Type (010b=Clamp)
   28                 // Temperature Info [7:6]-Reserved; [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40                 // Ramp Coefficient (LSB) (40h)
   00                 // Ramp Coefficient (MSB) (00h)
   00                 // NHM/WSM Clamp Temperature (00h = 0 degree C)
   01                 // Clamp Flag  (CPU number = 0; temp source = 1)
//=========================================================================//  
 
   
// ***************************************************************************
// Sensor failure exclusion Sub-record (sub-record type: 0xFD)
// ***************************************************************************
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   0141               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Sensor failure exclusion Sub-record
   FD                 // Sub Record Type (Sensor failure exclusion Sub-record)
   00                 // Sensor Count
   00                 // Sensor Number

//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7
// For Other Chassis
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'Other'
_REC_LEN       0013

   // Sensor Record Header
   0142               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Sensor failure exclusion Sub-record
   FD                 // Sub Record Type (Sensor failure exclusion Sub-record)
   00                 // Sensor Count
   00                 // Sensor Number

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   0143               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Sensor failure exclusion Sub-record
   FD                 // Sub Record Type (Sensor failure exclusion Sub-record)
   01                 // Sensor Count
   04                 // Sensor Number

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7
// For SR1630BC Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0013

   // Sensor Record Header
   0144               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Sensor failure exclusion Sub-record
   FD                 // Sub Record Type (Sensor failure exclusion Sub-record)
   00                 // Sensor Count
   00                 // Sensor Number

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7
// For Other Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'Other'
_REC_LEN       0013

   // Sensor Record Header
   0145               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Sensor failure exclusion Sub-record
   FD                 // Sub Record Type (Sensor failure exclusion Sub-record)
   00                 // Sensor Count
   00                 // Sensor Number
     
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   0146               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Sensor failure exclusion Sub-record
   FD                 // Sub Record Type (Sensor failure exclusion Sub-record)
   01                 // Sensor Count
   04                 // Sensor Number

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7
// For SR1630BC Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0013

   // Sensor Record Header
   0147               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Sensor failure exclusion Sub-record
   FD                 // Sub Record Type (Sensor failure exclusion Sub-record)
   00                 // Sensor Count
   00                 // Sensor Number
 
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7
// For Other Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'Other'
_REC_LEN       0013

   // Sensor Record Header
   0148               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Sensor failure exclusion Sub-record
   FD                 // Sub Record Type (Sensor failure exclusion Sub-record)
   00                 // Sensor Count
   00                 // Sensor Number
        
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #3 (PWM3: System Fan3)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0013

   // Sensor Record Header
   0149               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Sensor failure exclusion Sub-record
   FD                 // Sub Record Type (Sensor failure exclusion Sub-record)
   00                 // Sensor Count
   00                 // Sensor Number

//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7
// For Other Chassis
// Fan Control Domain Number #3 (PWM3: System Fan3)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'Other'
_REC_LEN       0013

   // Sensor Record Header
   014A               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Sensor failure exclusion Sub-record
   FD                 // Sub Record Type (Sensor failure exclusion Sub-record)
   00                 // Sensor Count
   00                 // Sensor Number
      
// ***************************************************************************
// Boost value Sub-record (sub-record type: 0xFF)
// *************************************************************************** 
//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0015

   // Sensor Record Header
   014B               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Boost value Sub-record
   FF                 // Sub Record Type (Boost value sub record type)
   38                 // Fan Fault Boost Value (38h = PWM 56%)
   38                 // Critical Temp Boost Value (38h = PWM 56%)
   FF                 // Chassis Intrusion Boost Value (FFh = disableboost for this failure)
   00                 // Reserved

//=========================================================================//
// Chassis Fan Control Domain 0 with profile 0,1,2,3,4,5,6,7
// For Other Chassis
// Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'Other'
_REC_LEN       0015

   // Sensor Record Header
   014C               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   00                 // Fan Control Domain Number #0 (PWM0: Processor1&2 Fan)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Boost value Sub-record
   FF                 // Sub Record Type (Boost value sub record type)
   64                 // Fan Fault Boost Value (64h = PWM 100%)
   64                 // Critical Temp Boost Value (64h = PWM 100%)
   64                 // Chassis Intrusion Boost Value (64h = PWM 100%)
   00                 // Reserved
   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0015

   // Sensor Record Header
   014D               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Boost value Sub-record
   FF                 // Sub Record Type (Boost value sub record type)
   64                 // Fan Fault Boost Value (64h = PWM 100%)
   64                 // Critical Temp Boost Value (64h = PWM 100%)
   64                 // Chassis Intrusion Boost Value (64h = PWM 100%)
   00                 // Reserved  
   
//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7
// For SR1630BC Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0015

   // Sensor Record Header
   014E               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Boost value Sub-record
   FF                 // Sub Record Type (Boost value sub record type)
   64                 // Fan Fault Boost Value (64h = PWM 100%)
   64                 // Critical Temp Boost Value (64h = PWM 100%)
   FF                 // Chassis Intrusion Boost Value (FFh = disableboost for this failure)
   00                 // Reserved   

//=========================================================================//
// Chassis Fan Control Domain 1 with profile 0,1,2,3,4,5,6,7
// For Other Chassis
// Fan Control Domain Number #1 (PWM1: System Fan2)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'Other'
_REC_LEN       0015

   // Sensor Record Header
   014F               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   01                 // Fan Control Domain Number #1 (PWM1: System Fan2)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Boost value Sub-record
   FF                 // Sub Record Type (Boost value sub record type)
   64                 // Fan Fault Boost Value (64h = PWM 100%)
   64                 // Critical Temp Boost Value (64h = PWM 100%)
   64                 // Chassis Intrusion Boost Value (64h = PWM 100%)
   00                 // Reserved   
   
//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0015

   // Sensor Record Header
   0150               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Boost value Sub-record
   FF                 // Sub Record Type (Boost value sub record type)
   64                 // Fan Fault Boost Value (64h = PWM 100%)
   64                 // Critical Temp Boost Value (64h = PWM 100%)
   64                 // Chassis Intrusion Boost Value (64h = PWM 100%)
   00                 // Reserved  

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7
// For SR1630BC Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0015

   // Sensor Record Header
   0151               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Boost value Sub-record
   FF                 // Sub Record Type (Boost value sub record type)
   64                 // Fan Fault Boost Value (64h = PWM 100%)
   64                 // Critical Temp Boost Value (64h = PWM 100%)
   FF                 // Chassis Intrusion Boost Value (FFh = disableboost for this failure)
   00                 // Reserved  

//=========================================================================//
// Chassis Fan Control Domain 2 with profile 0,1,2,3,4,5,6,7
// For Other Chassis
// Fan Control Domain Number #2 (PWM2: System Fan1)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'Other'
_REC_LEN       0015

   // Sensor Record Header
   0152               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   02                 // Fan Control Domain Number #2 (PWM2: System Fan1)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Boost value Sub-record
   FF                 // Sub Record Type (Boost value sub record type)
   64                 // Fan Fault Boost Value (64h = PWM 100%)
   64                 // Critical Temp Boost Value (64h = PWM 100%)
   64                 // Chassis Intrusion Boost Value (64h = PWM 100%)
   00                 // Reserved  
       
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7
// For SC5650DP/SC5650BRP Chassis
// Fan Control Domain Number #3 (PWM3: System Fan3)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_SDR_TAG       'SC5650BRP'
_REC_LEN       0015

   // Sensor Record Header
   0153               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Boost value Sub-record
   FF                 // Sub Record Type (Boost value sub record type)
   46                 // Fan Fault Boost Value (46h = PWM 70%)
   46                 // Critical Temp Boost Value (46h = PWM 70%)
   FF                 // Chassis Intrusion Boost Value (FFh = disableboost for this failure)
   00                 // Reserved     
 
//=========================================================================//
// Chassis Fan Control Domain 3 with profile 0,1,2,3,4,5,6,7
// For Other Chassis
// Fan Control Domain Number #3 (PWM3: System Fan3)
// OLTT&CLTT
//====================================================================//
_SDR_TYPE      C0
_SDR_TAG       'Other'
_REC_LEN       0015

   // Sensor Record Header
   0154               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0C                 // Record Subtype Value (Fan Speed Control SDR Record, rev 2)

   // Temperature Fan Control Record
   01                 // Record Version
   03                 // Fan Control Domain Number #3 (PWM3: System Fan3)
   14                 // Normal Control Value (14h = PWM 20%)
   FF                 // Boost Control Value (FFh = use boost sub record)
   01                 // Ramp Step (1=1%)
   02                 // Scan Rate (2 Cycles)
   FF                 // Fan Profile Support = 11111111

   // Boost value Sub-record
   FF                 // Sub Record Type (Boost value sub record type)
   64                 // Fan Fault Boost Value (64h = PWM 100%)
   64                 // Critical Temp Boost Value (64h = PWM 100%)
   64                 // Chassis Intrusion Boost Value (64h = PWM 100%)
   00                 // Reserved  
      
//*******************************************************
// SDR Type C0/0D Records For Management Engine (ME controller)
//*******************************************************
_SDR_TYPE      C0
_REC_LEN       0010

   // Sensor Record Header
   0155               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0B                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0D                 // Record subtype - NM Discovery
   01                 // Version number of record subtype
   2C                 // NM Device Slave Address ([7:1] - 7-bit address; [0] - reserved)
   60                 // [7:4] - channel number (0 for primary) [3:2] - reserved (b'00) [1:0] - sensor owner LUN
   19                 // Node Manager Health Event sensor   
   18                 // Node Manager Exception Event sensor   
   1A                 // Node Manager Operational Capabilities sensor   
   1B                 // Node Manager Alert Threshold Exceeded sensor   
//=========================================================================// 
 
 
// ***************************************************************************
// SDR Type C0/0E Chassis ID and FAN FRU LED Mapping
// ***************************************************************************
_SDR_TYPE      C0
_SDR_TAG       'SC5650DP'
_REC_LEN       0017
 
   // Sensor Record Header
   0156               // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0E             // Record Subtype Value (Chassis ID & FRU LED Mapping)
   01             // Record Version
   0C             // Chassis ID number = 0x0C (SC5650DP)

   // LED mapping sub-records
   01             // LED Group = 1 (Fan Fault LED)
//------------------------------------------------------------------//
   05             // Number of mapping pairs = 5
   
   30             // 1st fan sensor number = 0x30
   2A             // 1st fan fault LED GPIO number = 42
   
   31             // 2nd fan sensor number = 0x31
   36             // 2nd fan fault LED GPIO number = 54
   
   32             // 3rd fan sensor number = 0x32
   2B             // 3rd fan fault LED GPIO number = 43
   
   33             // 4th fan sensor number = 0x33
   37             // 4th fan fault LED GPIO number = 55
   
   34             // 5th fan sensor number = 0x34
   34             // 5th fan fault LED GPIO number = 52
   
//=========================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SC5650BRP'
_REC_LEN       0017
 
   // Sensor Record Header
   0157               // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0E             // Record Subtype Value (Chassis ID & FRU LED Mapping)
   01             // Record Version
   0B             // Chassis ID number = 0x0B (SC5650BRP)

   // LED mapping sub-records
   01             // LED Group = 1 (Fan Fault LED)
//------------------------------------------------------------------//
   05             // Number of mapping pairs = 5
   
   30             // 1st fan sensor number = 0x30
   2A             // 1st fan fault LED GPIO number = 42
   
   31             // 2nd fan sensor number = 0x31
   36             // 2nd fan fault LED GPIO number = 54
   
   32             // 3rd fan sensor number = 0x32
   2B             // 3rd fan fault LED GPIO number = 43
   
   33             // 4th fan sensor number = 0x33
   37             // 4th fan fault LED GPIO number = 55
   
   34             // 5th fan sensor number = 0x34
   34             // 5th fan fault LED GPIO number = 52
   
//=========================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'SR1630BC'
_REC_LEN       0011
 
   // Sensor Record Header
   0158               // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0E             // Record Subtype Value (Chassis ID & FRU LED Mapping)
   01             // Record Version
   03             // Chassis ID number = 0x03 (SR1630BC)

   // LED mapping sub-records
   01             // LED Group = 1 (Fan Fault LED)
//------------------------------------------------------------------//
   02             // Number of mapping pairs = 2
   
   32             // 1rd fan sensor number = 0x32
   2B             // 1rd fan fault LED GPIO number = 43
   
   33             // 2th fan sensor number = 0x33
   37             // 2th fan fault LED GPIO number = 55
//=========================================================================// 
_SDR_TYPE      C0
_SDR_TAG       'Other'
_SDR_TAG       'FCT'
_REC_LEN       0017
 
   // Sensor Record Header
   0159               // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0E             // Record Subtype Value (Chassis ID & FRU LED Mapping)
   01             // Record Version
   0E             // Chassis ID number = 0x0E (OTHER)

   // LED mapping sub-records
   01             // LED Group = 1 (Fan Fault LED)
//------------------------------------------------------------------//
   05             // Number of mapping pairs = 5
   
   30             // 1st fan sensor number = 0x30
   2A             // 1st fan fault LED GPIO number = 42
   
   31             // 2nd fan sensor number = 0x31
   36             // 2nd fan fault LED GPIO number = 54
   
   32             // 3rd fan sensor number = 0x32
   2B             // 3rd fan fault LED GPIO number = 43
   
   33             // 4th fan sensor number = 0x33
   37             // 4th fan fault LED GPIO number = 55
   
   34             // 5th fan sensor number = 0x34
   34             // 5th fan fault LED GPIO number = 52
   

//=========================================================================// 
// SDR Type C0 Records For File & Package Revisions
//=========================================================================// 
_SDR_TYPE      C0
_REC_LEN       0015

   // Sensor Record Header
   015A               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR File 0.21'    // String Bytes
//=========================================================================//
_SDR_TYPE      C0
_REC_LEN       0018

   // Sensor Record Header
   015B               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   13                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR Package 0.21' // String Bytes
   
)