Intel® Server Board S875WP1-E
The products you are looking for are no longer manufactured by Intel. Additionally, Intel no longer provides interactive support for these products via telephone or e-mail, nor will Intel provide any future content updates or software updates to support new operating systems or improve compatibility with third party devices and software products. THESE PRODUCT SUPPORT DOCUMENTS ARE PROVIDED FOR HISTORICAL REFERENCE ONLY AND ARE SUBJECT TO THE TERMS SET FORTH IN THE "TERMS OF USE" INFORMATION. Information on currently available Intel products is available at www.intel.com and/or developer.intel.com

Identify your products
  Product Discontinuance Announcement
    Intel® will no longer provide interactive support for these products via telephone or e-mail

Software and drivers
  BIOS/Firmware, drivers and utilities download

Technical specifications
  Technical Product Specifications
    Product overview, including descriptions and diagrams of the integrated features
    Technical Product Specifications [PDF]

Installation and use
  Adaptec* SATA RAID User Guide
    ata_rug.pdf
  Board Order Codes

    Order Code | MM | AA or PBA | Decription
    S875WP1 | 853263 | C28366-xxx | C28368-xxx 2-port Serial ATA with RAID 0 or 1
    S875WP1LX | 853264 | C26812-xxx | C26813-xxx 2-port Serial ATA with RAID 0 or 1, 4-port SATA with RAID 0, 1, and 10

  Degraded Array, or Hang at "Preparing Network Connections"
    Intel® Server Boards may show a "Degraded Array" with both drives healthy, may hang on the "Preparing Network Connections" screen in Microsoft* Windows, or both.
    Ensure your RAM is on the tested list.
    Go into BIOS - Advanced - USB Configuration - Legacy USB support and set it to Disabled.
    If you are using the LX version of the Intel® Entry Server Board S875WP1-E, and are not booting from the onboard Promise* controller, disable the Promise* option ROM in the BIOS.
  Enabling SATA RAID
    The SATARAID.EXE utility should only be used before the operating system is loaded, or to return the SATA mode to the previous state. Once the operating system is loaded, DO NOT switch modes. This may result in a non-functioning system.
  Error: CMOS Checksum Bad
    Clear the CMOS after a BIOS update
  File x caused an unexpected error at line y in d:\nt\private\ntos\boot\...
    When copying SATA [Serial ATA] RAID drivers from floppy during an install of Microsoft Windows* 2000 or 2003, an error message may appear:
    File \win32\aarich.sys caused an unexpected error (4101) at line 1211 in d:\nt\private\ntos\boot\setup\oemdisk.c
    Certain floppy diskettes have read issues. Try a floppy from a different manufacturer.
  Installing OS Using USB Floppy
    BIOS | Advanced | Floppy Configuration | Floppy A: | Disabled BIOS | Advanced | Floppy Configuration | Onboard Floppy Controller | Disabled BIOS | Advanced | USB Configuration | USB Mass Storage Device Configuration | Emulation | Floppy
  Product Guide
    pguide.pdf
  Promise* RAID Console SCSI Processor Device In "Other devices"
    If no Serial ATA hard drives are attached to the Promise Serial ATA controller, disable the controller.
  Promise* SATA RAID User Guide
    PDC20319.PDF
    If installing Windows 2000, press F6 to Specify Drivers and choose "Win2000 Promise FastTrak S150 TX4 (tm) Controller"
  Quick Start Guide
    Front S875WP1-E_QSG_FRONT.PDF
    Back S875WP1-E_QSG_BACK.PDF
  RAID 0+1 (S875WP1LX only) Configuration Requirements
    RAID 0+1 requires all four Serial ATA drives to be connected.
  Rebuild Degraded Adaptec Array
    Logical Devices | Task | New Task | Rebuild | Start Now | Apply
  SATA drives appear to be non-functioning
    Disable PM2 and SSC features on the SATA hard drive.
  Troubleshooting Guide
    TSG.PDF

Compatibility
  Tested Chassis
    Intel® SC5200
    Intel® SC5250-E
    AIC* RMC1H2-0-XP
    AIC* RMC1D2-XPSS
    Apex* TU-150
    Casedge* TN-152-3G
    Chenbro* SR107
    Chenbro* SR205
    Chenbro* RM214
    Chenbro* PC611
    CiDesign* RS2100
    Evercase* E4252B-PCT
    Inwin* J508
    Yeong Yang* YY-R236
    Yeong Yang* YY-5408
  Tested Hardware and Operating Systems
    Supports AGP. Does not support dual SCSI hot-swap backplanes
    Microsoft Windows* Server 2003, Enterprise Edition Compatibility & Stress
    Microsoft Windows* Small Business Server 2003 Install Only
    Microsoft Windows* 2000 Advanced Server, Service Pack 3 Compatibility & Stress
    Microsoft Small Business Server 2000* Install Only
    Microsoft Windows* XP Professional, Service Pack 1 Compatibility & Stress
    THOL.PDF
  Tested Memory
    Tested Memory List [PDF]
  Tested Processors

    sSpec | CPU speed | Bus speed | Mfg. Tech | Stepping | Cache size | Package Type
    SL793 | 3.4 GHz | 800 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA
    SL7E6 | 3.4 GHz | 800 MHz | 90 nm | D0 | 1 MB | 478 pin PPGA
    SL7B9 | 3.40E GHz | 800 MHz | 90 nm | C0 | 1 MB | 478 pin PPGA
    SL7E5 | 3.2 GHz | 800 MHz | 90 nm | D0 | 1 MB | 478 pin PPGA
    SL7B8 | 3.20E GHz | 800 MHz | 90 nm | C0 | 1 MB | 478 pin PPGA
    SL6WG | 3.2 GHz | 800 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6QC | 3.06 GHz | 533 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6PG | 3.06 GHz | 533 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6SM | 3.06 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6JJ | 3.06 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6S5 | 3.06 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6K7 | 3.06 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL7E4 | 3 GHz | 800 MHz | 90 nm | D0 | 1 MB | 478 pin PPGA
    SL79L | 3E GHz | 800 MHz | 90 nm | C0 | 1 MB | 478 pin PPGA
    SL6WK | 3 GHz | 800 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL7E3 | 2.8 GHz | 800 MHz | 90 nm | D0 | 1 MB | 478 pin PPGA
    SL7E2 | 2.8 GHz | 533 MHz | 90 nm | D0 | 1 MB | 478 pin PPGA
    SL6PF | 2.8 GHz | 533 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6WJ | 2.8 GHz | 800 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6S4 | 2.8 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6WT | 2.8 GHz | 800 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6QB | 2.8 GHz | 533 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6K6 | 2.8 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6HL | 2.8 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6Z5 | 2.8 GHz | 800 MHz | 0.13 micron | M0 | 512 KB | 478 pin PPGA FC-PGA2
    SL79K | 2.80E GHz | 800 MHz | 90 nm | C0 | 1 MB | 478 pin PPGA
    SL6SL | 2.8 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6SK | 2.66 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6EH | 2.66 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6S3 | 2.66 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6PE | 2.66 GHz | 533 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6QA | 2.66 GHz | 533 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6DX | 2.66 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6SB | 2.6 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6HB | 2.6 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6GU | 2.6 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6WH | 2.6 GHz | 800 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6PP | 2.6 GHz | 400 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6QR | 2.6 GHz | 400 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6WS | 2.6 GHz | 800 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6PD | 2.53 GHz | 533 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6S2 | 2.53 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6Q9 | 2.53 GHz | 533 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6EG | 2.53 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6SJ | 2.53 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6DW | 2.53 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6QQ | 2.5 GHz | 400 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6SA | 2.5 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6EB | 2.5 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6PN | 2.5 GHz | 400 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6GT | 2.5 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6EF | 2.4 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6PM | 2.4 GHz | 400 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6Q8 | 2.4 GHz | 533 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6QP | 2.4 GHz | 400 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6E9 | 2.4 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6RZ | 2.4 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6PC | 2.4 GHz | 533 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6S9 | 2.4 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6SH | 2.4 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6SR | 2.4 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6WF | 2.4 GHz | 800 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6WR | 2.4 GHz | 800 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6GS | 2.4 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6DV | 2.4 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6Z3 | 2.4 GHz | 800 MHz | 0.13 micron | M0 | 512 KB | 478 pin PPGA FC-PGA2
    SL6PB | 2.26 GHz | 533 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6DU | 2.26 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6EE | 2.26 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6Q7 | 2.26 GHz | 533 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6RY | 2.26 GHz | 533 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6E8 | 2.2 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6GR | 2.2 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6PL | 2.2 GHz | 400 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6QN | 2.2 GHz | 400 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6S8 | 2.2 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6E7 | 2 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6GQ | 2 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6PK | 2 GHz | 400 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6QM | 2 GHz | 400 MHz | 0.13 micron | D1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6S7 | 2 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL6SP | 2 GHz | 400 MHz | 0.13 micron | C1 | 512 KB | 478 pin PPGA FC-PGA2
    SL7AA | 3.2 GHz | 800 MHz | 90nm | M0 | 2 MB | 478 pin PPGA FC-PGA2 3,4
    SL7CH | 3.4 GHz | 800 MHz | 90nm | M0 | 2 MB | 478 pin PPGA FC-PGA2 3,4
    SL7C7 | 2.8 GHz | 533 MHz | 90nm | C0 | 256KB | 478 pin PPGA
    SL7C6 | 2.66 GHz | 533 MHz | 90nm | C0 | 256KB | 478 pin PPGA
    SL7C5 | 2.53 GHz | 533 MHz | 90nm | C0 | 256KB | 478 pin PPGA
    SL7C4 | 2.4 GHz | 533 MHz | 90nm | C0 | 256KB | 478 pin PPGA
    SL77T | 2.8 GHz | 400 MHz | 0.13 micron | D1 | 128 KB | 478 pin PPGA
    SL77V | 2.8 GHz | 400 MHz | 0.13 micron | D1 | 128 KB | 478 pin PPGA
    SL77U | 2.7 GHz | 400 MHz | 0.13 micron | D1 | 128 KB | 478 pin PPGA
    SL77S | 2.7 GHz | 400 MHz | 0.13 micron | D1 | 128 KB | 478 pin PPGA
    SL6VV | 2.6 GHz | 400 MHz | 0.13 micron | D1 | 128 KB | 478 pin PPGA
    SL6ZY | 2.5 GHz | 400 MHz | 0.13 micron | D1 | 128 KB | 478 pin PPGA
    SL72B | 2.5 GHz | 400 MHz | 0.13 micron | D1 | 128 KB | 478 pin PPGA

Technical advisories
  TA 0680: Two Capacitors May Prevent Installation of Boxed Intel® Processor Fan Heatsink
    ta680.pdf
  TA 0733: PXE and SATARAID Configuration Errors
    ta73301.pdf