EFI System Update Package Install Instructions

The contents of this update package is used to update the System Firmware for 
the following Intel Server Products:

Intel(R) Server Board S5400SF 
Intel(R) Server System SR1560SF
 
System Update Instructions - S5400SF_PR12 (Production Release)

Released - Dec 8, 2010


**********************************************************************************
This Update package includes the following system software updates:

System BIOS - R0033 (Production Release)
BMC Firmware - R011 (Production Release)
FRUSDR Utility - R011 (Production Release)
HSC Firmware - R2.09 (Production Release) Used for Hot Swap SR1560SF Systems only


Important NOTES: 

- All the updates provided in this package are EFI based.
To run these updates, you must boot the system to the embedded EFI shell and then 
access the USB device containing the system software udpates. See instructions
below

- The System BIOS revision provided in this Software Update Package does not
include processor microCode to support any pre-production Intel(R) Xeon(R) 
processors 

- It is highly recommended that you read the Release Notes (.TXT Files) for each 
of the software updates provided to understand what the known issues are, what 
issues were addressed from previous updates, and what new features (if any) were added. 


***********************************************************************************




***********************************************************************************

*********  Standard Update Procedure **************

***********************************************************************************

- Copy all the files to a USB disk-on-key device
- Verify that the BIOS Select jumper on the server board is set to its default 
postion on pins 2-3. If this jumper is set on pins 1-2, you must move it back to its
normal position before updating the BIOS.


** Booting to the embedded EFI operating environment**
- Plug in your USB device containing the system software updates
- Power on your server
- During POST, hit the F2 key when prompted to access the BIOS Setup Utility
- In BIOS Setup, move the cursor over to the BOOT MANAGER menu
- Move the cursor down to EFI and hit enter.
- The system will boot to the embedded EFI Shell
- Once the system has booted, and is sitting at a EFI Shell prompt, type FS0: to 
access the USB device. If your USB device is not accessible, type the MAP command
to determine which device ID EFI has assigned your USB device, then type in the 
device ID using the same command syntax as before <device ID>:


- Follow the instructions below to perform each software update. Update the system 
software in the sequence specified:


*** Update System BIOS ***


IMPORTANT BIOS UPDATE NOTEs: 

- The following procedure will update the BIOS twice in order to load it into each 
bank of the rolling BIOS feature.


BIOS Update Instructions:

1)  Verify that the R0033.CAP, IFLASH32.EFI and BIOS33.NSH files are present in the 
directory
2)  At the shell prompt type BIOS33 and press the Enter key
3)  The update should complete within 3 minutes
4)  Shut down the system but leave it connected to AC power
5)  Clear CMOS by moving the Clear CMOS jumper on the baseboard to the clear position 
(pins 2-3). wait a few seconds, and move the jumper back to pins 1-2.
6)  Boot the system and enter BIOS Setup by pressing the F2 Key during POST
7)  Verify the BIOS string shows the BIOS revision as S5400.86B.06.00.0033
8) Press F9 to load defaults
9) Press F10 to save and reset the system.
10) Reboot the system to the EFI SHELL (See Booting to EFI Above)
11) Access the USB device 
12) At the command prompt type BIOS33 and press the Enter key
13) The update should complete within 3 minutes

The BIOS update is complete. Either reboot the server or go to the BMC Firmware Update 
described below.  



*** Update BMC Firmware ***


1) Verify that the following files are present in the directory:
BMC11.NSH; FWPIAUPD.EFI; SFBMC11.HEX; IPMI.EFI
2) At the EFI command prompt type BMC11 and hit enter

The update should take approximately 3-5 minutes to complete

When the BMC Firmware update is complete, either reboot the server, or update
the HSC Firmware, or go to the FRUSDR update section described below




*** Update HSC Firmware ***

Only perform this update if you are using an Intel Server System SR1560SF and
you have a hot swap backplane installed.


1) Verify that the following files are present in the directory:
HSC209.NSH; FWPIAUPD.EFI; DOW209.HEX; IPMI.EFI
2) At the EFI command prompt type HSC209 and hit enter
3) When prompted to select the 'P'(Primary) or 'S'(Secondary) controller, select 'P'
4) When prompted to CONTINUE (y/N), enter 'y' (yes)

NOTE: The HSC update may take over 10 minutes to complete

When the HSC Firmware update is complete, either reboot the server, or go to 
the FRUSDR update described below




*** Updating the FRU and SDR data on your server ***

1) At the EFI Shell prompt type FRUSDR11 and hit the ENTER key to start the utility
2) Answer questions and enter desired information when prompted.
3) When the FRUSDR utility has completed its update, power cycle the server and reboot.


*** Verifying updates ***

1) During POST, hit the F2 Key when prompted to access the BIOS Setup Utility
2) Hit the F9 key to load BIOS Defaults
3) At the MAIN menu verify the BIOS revision is S5400.86B.06.00.0033
3) Move cursor to the SERVER MANAGEMENT Menu
4) Move cursor down to the SYSTEM INFORMATION Option and hit Enter
5) Verify the BMC Firmware revision is 11
6) Verify the SDR Revision is 11
7) (IF PRESENT) Verify the HSC Revision is 2.09
7) Hit the F10 Key to save changes and Exit


The System Software Update is Complete.





