                  FRUSDR Load Utility - Release Notes
                 Copyright (c) 2008 Intel Corporation
                          All Rights Reserved
                           March 26, 2008


RELEASE NOTES FOR FRUSDR LOAD UTILITY VERSION 1.0.4 Build 7

This document describes some specifics of the WinPE and 
EFI-32(Extensible Firmware Interface - 32 bit version) version 
of FRU & SDR Load Utility.


This utility is used for updating or modifying the server management
subsystem's product level Field Replacement Unit (FRU), Sensor Data 
Record (SDR) repository, displaying the System Management 
BIOS (SMB) non-volatile storage components (previously known as the Desktop 
Management Interface (DMI) non-volatile storage components).

Through the use of a configuration file, added features allow the user to
control the execution path by probing hardware, requesting user input, and 
setting tags to provide filtering of FRU and SDR data. Multiple 
FRU and SDR files may also be processed at once through the configuration file.

The FRUSDR utility fully supports IPMI 1.5 and IPMI 2.0 specifications.

       Important Notes

	A. Install
	B. Parse the Command Line
	C. Display FRU, SDR and SMB Information
	D. Temporary Files
	E. Limitation:
	F. DEPENDENCIES:
	G. SUPPORTED PLATFORMS:
	H. Documentation:
	I. Required Files
	J. Changes Since Last Release
	K. Errata Items
	L. Legal Information


 				Important Notes

A. Install
==========

a. For WinPE 1.5/1.6

The FRUSDR Loader is meant to be used as a WinPE application on a Microsoft 
Windows Preinstallation Environment* server. 

The frusdr utiliy requires IMBdriver to be installed as a pre-requisite. 

To install IMBdriver:
	
	1. Go to the command prompt.
	2. Change directory to the path where FRUSDR package is present.
	3. Run the following command.

install.cmd [Full path where FRUSDR Loader utility is present.]

The IMBdriver and memory map driver installation is not needed 
if the customized WinPE CD, containing the Intel drivers is used.

The FRUSDR utility needs to be executed from the same directory, in the 
command prompt with one of the command line options below.

Normal Command Line Use:

	C:> FRUSDR /CFG MASTER.CFG

	Upon completion of programming the FRU/SDR reboot the server. 

b. For WinPE 2.0 and 2.1

   	1. Boot to the WinPE 2.0/2.1 environment using a WinPE HDD/CD/UFD/DVD.
   	2. FRUSDR utility requires the FRUSDR update drivers (IBSMUtil.sys and imbdrv.sys)
	   to be installed on the WinPE environment as a pre-requisite.

	To install FRUSDR update driver:	

		a. Go to the command prompt.
		b. Change directory to the path where FRUSDR package is present.
		c. Run the following command.

	FOR WINPE 2.1 (x64)	IBSMUtilDrvInstall.exe and SetupIMB64.exe
	[NOTE: THIS WILL NOT DISPLAY ANY MESSAGE ON SCREEN.]

	FOR WINPE 2.0 (32bit) install.cmd .

   	3. Run the FRUSDR utility on the prompt
	     C:\FRUSDR [Options] [file Name ]


c. For EFI

The FRUSDR Loader is meant to be used as an EFI-32 application that runs 
on EFI- Shell.

The frusdr utiliy requires IPMI driver file (IPMI.efi) to be present in the 
same directory from which the utility is run. 

The FRUSDR utility needs to be executed in the EFI-Shell command prompt with 
one of the command line options below.

Normal Command Line Use:

	fs0:\> FRUSDR /CFG MASTER.CFG

Upon completion of programming the FRU/SDR reboot the server.  

   
B.  Parsing the Command Line
============================


The FRUSDR Loader utility provides the following command line options:

	Usage: 

      		/? or /h Displays usage information.
      		/d {smb,fru,sdr} Only displays requested area.
      		/cfg filename.cfg Uses custom CFG file.
      		/p Pause between blocks of data.

      	Users may alternatively use '-' instead of the '/'. 


C. Display FRU, SDR and SMB Information
=======================================


The SDR, FRU & SMB area can be displayed using the respective commands. Example 
for each of these has been listed below.

The /D FRU parameter will display the IMM module FRU area by default. To view 
other FRU areas, additional addressing information must be provided:

The /D FRU optional addresses are used to view different FRU areas, instead 
of the default displaying of the IMM module FRU.  The parameters following the 
/D FRU are in the order: NVS_TYPE, DEVICE_ID, DEV_CNTR, NVS_LUN, DEV_BUS and 
DEV_ADDRESS. The NVS LUN address and Device Controller address are optional. 
If the LUN address is used, it must start with a "L". Only LUN addresses of 0,
1, 2, & 3 are allowed. If the Controller address is used, it must start with a
"C". There are two basic ways of addressing most FRU devices, Direct Addressing
and Indirect Addressing (IMM module logical device). Using Direct Addressing, 
after the NVS type you must supply the correct Device Controller, LUN, bus and 
slave address. When using Indirect Addressing,after the NVS type only the Device 
ID (IMM module logical device) is necessary.

      Usage for Direct Addressing:
      FRUSDR /D FRU [NVS type] [dev ctlr] [lun] [bus] [addr] 
      Example for IMM module: 
      FRUSDR /D FRU IMBDEVICE C20 L00 FF 20
      
      Usage for Indirect Addressing:
      FRUSDR /D FRU [NVS type] [device id]
      Example: FRUSDR /D FRU IMBDEVICE 00


Examples for the S5000PSL Server board:

	1. To display the SM BIOS area:
   		fs0:\> FRUSDR /D SMB  
   		C:> FRUSDR /D SMB  

	2. To display the SDRs:
   		fs0:\> FRUSDR /D SDR 
   		C:> FRUSDR /D SDR 

	3. To display the Starlake IMM module FRU:
   		fs0:\> FRUSDR /D FRU 
   		C:> FRUSDR /D FRU 

Note: 

   If your system does not display information on any particular FRU device, then 
   it probably does not contain the device.


D. Temporary Files:
===================


If you desire to create temporary files, you must use the undocumented "/tmp"
switch on the command line. When the FRUSDR Loader is executed, it 
creates temporary files that may be used to aid in recreating a problem, 
should one arise.  The FRUSDR Loader does not remove the temporary files, the
temporary files may be erased by the user after the FRUSDR Loader has 
completed.


E. Limitation:
==============


The FRUSDR utility currently doesn't support programming FRUs and SDRs on any 
mBMC systems.


F. DEPENDENCIES:
================


   1. Executes under the WinPE/EFI command Shell.
   2. The WinPE image on which the utility to run should have support for WMI.
   3. The IPMI driver file, IPMI.EFI should be present in the same directory as 
      the utility.
  

G. SUPPORTED PLATFORMS:
=======================


   1. S5000, S5400, s5300, S3200 and S7000 Server boards.

H. Documentation:
=================


Additional information on the FRUSDR Loader utility may be found in the 
External Product Specification.


I. Required Files:
==================


The FRUSDR utility SHOULD contain the following files in the directory from 
which it is run.

For WinPE
	FRUSDR Loader utility program 
	install.cmd
	imbdrv.inf
	imbdrv.sys
	imbapi.dll 
	ibsmutil.inf
	ibsmutil.sys
	Win2kInstall.exe
	Win2kUninstall.exe

For EFI
	FRUSDR Loader utility program 
	IPMI.EFI


J. Changes Since Last Release:
==============================
   Bug fixes from last release.


K. Errata Items:
================

	NONE
   				
L. LEGAL INFORMATION:
=====================

Information in this document is provided in connection with Intel Products

and for the purpose of supporting Intel developed server boards and systems.

No license, express or implied, by estoppel or otherwise, to any intellectual 

property rights is granted by this document. Except as provided in Intel's 

Terms and Conditions of Sale for such products, Intel assumes no liability 

whatsoever, and Intel disclaims any express or implied warranty, relating to 

sale and/or use of Intel products including liability or warranties relating 

to fitness for a particular purpose, merchantability, or infringement of any 

patent, copyright or other intellectual property right. Intel Corporation may 

have patents or pending patent applications, trademarks, copyrights, or other 

intellectual property rights that relate to the presented subject matter.  

The furnishing of documents and other materials and information does not 

provide any license, express or implied, by estoppel or otherwise, to any 

such patents, trademarks, copyrights, or other intellectual property rights.  

Intel products are not intended for use in medical, life saving, or life 

sustaining applications. Intel may make changes to specifications and product 

descriptions at any time, without notice.

 

Intel is a registered trademark of Intel Corporation. 

 

*Other names and brands are the property of their respective owners.

 

Copyright (c) 2007 Intel Corporation.
