================================================================================
Intel(R) Server System S5400SF System Firmware Update Package for 
Intel(R) Deployment Assistant, Intel(R) One Boot Flash Update Utility, 
The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : November 09, 2010
TO      : Intel(R) Server System S5400SF customers
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : S5400.86B.07.00.0033.11092010   Build Date  : December 09, 2010
BMC    : v11
FRUSDR : 11  
HSC    : v2.09
================================================================================
                           Support Platform and Dependency
================================================================================
Intel(R) Server System S5400SF Processors supported: 
  Intel(R) Xeon(R) Processor 5100 series w/ 1066Mhz/1333Mhz FSB
  Intel(R) Xeon(R) Processor 5200 series w/ 1066Mhz/1333Mhz/1600Mhz FSB
  Intel(R) Xeon(R) Processor 5300 series w/ 1066Mhz/1333Mhz/1600Mhz FSB
  Intel(R) Xeon(R) Processor 5400 series w/ 1333Mhz/1600Mhz FSB 
    
Microcode update versions:
CPUID   Version Status  
06F6h   D2      Production 
06F7h   6B      Production 
06FBh   BC      Production 
10676   60F     Production
1067A   A0B     Production

On-Board Component Option ROM Versions:
ATI RN50 VGA    	: BK-ATI YJ21797a VER008.005.031.000
PXE Ver.        	: Intel(R) Boot Agent GE v1.2.45
ESB2 Option ROM 	: v A_02151557I
ESB2 AHCI Option ROM	: iSrc 1.08 09252006
Memory Reference Code Version:  1.2
ESB2 BSU: v1.01
SNB BSU: v0.84
Self test tool version tested: 5.19.14

Dependency:
Intel(R) Server Board S5400SF with the PBA revisions -401 (or higher)
BIOS revision:   R0025 or higher
BMC version:     BMC07 or higher
FRU/SDR package: FSF_11 or higher
================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - The embedded EFI shell
 - Intel(R) Deployment Assistant
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   v9.70 Build3.4 or later)
 - Windows* Preboot Execution Environment (WinPE)

To Update from the embedded EFI Shell

update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from support.intel.com
- Unzip package and copy all files to a folder in USB disk on key 
- Insert USB disk on key to server USB port
- Reboot server to EFI shell
- Run command "map -r" in EFI shell to mount USB disk on key
- Run command "fs0:" to change folder to USB disk on key, USB key may also mount to
  fs1:. The number of "fs" is dependent on the result of command "map -r"
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process

Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the of EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment toolkit" CD shipped with the system.
User can download the latest version IDA CD ISO image from support.intel.com
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From support.intel.com
    Automatically downloads the latest Firmware Update Package from Intel 
    It requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from support.intel.com and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB Disk on Key or Hard Disk
    Download the latest Firmware Update Package from support.intel.com and copy it 
    to a USB key, then insert the key into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB disk.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from support.intel.com
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from support.intel.com
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE20_x86_Update.bat" (name may be varied depends on your own customization)
  
Note: 
1. In this SFUP package, Intel only provide batch file "WinPE20_x86_Update.bat"
for WinPE2.0 32 bit solution as an example. Please refer to white paper "White 
Paper-Intel Server Utilities Procedure for WinPE.pdf" for details on building 
your own customized WinPE CD.

2. Windows PE 2.0 - built from Windows Vista, 32 bit.   
================================================================================
                           BIOS Changes in release R33
================================================================================
Issues Fixed:
- None

Added:
- Added	Micrcode Update to Production Distribution SRV_P_96 to address the following:

	Intel?Xeon?Processor 5100 Series Specification Update, Erratum AG131
	Intel?Xeon?Processor 5200 Series Specification Update, Erratum AY76
	Intel?Xeon?Processor 5300 Series Specification Update, Erratum AJ127
	Intel?Xeon?Processor 5400 Series Specification Update, Erratum AX76

================================================================================
                           BMC Changes in release BMC11
================================================================================
Issues Fixed:
- BMC fails to respond during reboot testing.
- BMC MAC Address becomes zero during the power cycle test.
- DIMM D4 presence check error during validation in BMC09
================================================================================
                     FRUSDR Changes in release FRUSDR11
================================================================================    
Issue Fixed:
- Changed TempLoGB for CLTT mode from 14h to 24h
================================================================================
                       HSC FW Changes in release V2.09
================================================================================
Issues Fixed:
- FP LED going Amber blinking for Drive Fault doesn't work.
- HSC update takes around 25mins to update because of 16 bytes updates.
- EFI FWPIAUPD 4.0.2 Build 3 doesn't work for HSC update. Please use the one
  provided with the package.
================================================================================
                           LEGAL INFORMATION
================================================================================

Information in this document is provided in connection with Intel Products
and for the purpose of supporting Intel developed server boards and systems.
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation 
may have patents or pending patent applications, trademarks, copyrights, or
other intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any such
patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 

*Other names and brands are the property of their respective owners.

Copyright (C) 2010 Intel Corporation.
================================================================================


[END OF RELEASE NOTES]