=============================================================================
Intel(R) Server Platforms S5000PSL and S5000XSL BMC RELEASE NOTES
=============================================================================
INTEL Enterprise Platform & Services Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
=============================================================================
DATE:       Dec 09, 2010
TO:         Intel(R) server platform S5000PSL/S5000XSL customers
SUBJECT:    BMC(R) 00.68 Release Notes


=============================================================================
                               LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel Products
and for the purpose of supporting Intel developed server boards and systems.
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 

*Other names and brands are the property of their respective owners.

Copyright (c) 2010 Intel Corporation.


=============================================================================
                              ABOUT THIS RELEASE
=============================================================================
REVISION INFORMATION RETURNED BY GET DEVICE ID COMMAND:

Operational code:       v00.68
Boot code:              v00.43
PIA data:               v00.03
Manufacturer ID:        0x000157 (Intel)
Product ID:             0x0029   (Starlake)

Checksum Information:
Operational Code
  Region 	     : 	 0x00020000 -> 0x0012d2b2
  Checksum (HEX File):              0xc85d 

Boot Block
  Region:               0x00000000 -> 0x00005616
  Checksum (HEX file):             0x573b

=============================================================================
			SYSTEM HARDWARE REQUIREMENTS/REVISIONS
=============================================================================
-None
=============================================================================
		       SYSTEM SOFTWARE REQUIREMENTS/REVISIONS
=============================================================================

- MS-DOS v6.22 (or later)

- FRU/SDR package:
      FSL_48

- Starlake BIOS revision:
      R0099 BIOS

- STARLAKE SEEPROM Image
    v04.00 (SDRAM disabled - Use of any other SEEPROM image is not supported at this time)

=============================================================================
                         IMPORTANT INSTALLATION NOTES
=============================================================================
- Executing the batch files can be done from any media (Hard disk, USB disk-on-
  key, shared network drive or floppy).

=============================================================================
                         INSTALLATION PROCEDURES
=============================================================================


-----------------------------------------------------
   If a BMC has previously been installed
-----------------------------------------------------
1) Update the BMC firmware using BMC68.bat.

2) Update the SDR & FRUs with the FRU/SDR package.

=============================================================================
                           KNOWN ISSUES/WORKAROUNDS
=============================================================================

1) SIO3 Contention is resolved in this Release
   --------------------------------------------
     This release is for Beta base board (or equivalent) only.  Equivalent HW must contain SIO and GPIO rework.  
	Otherwise system will not function correctly.  True Beta HW must have EEPROM V02.09
	installed to match A1/C0 ESB2/Gilgal on board.


2) Serial/Modem is defeatured for Bensley Platforms.
  
=============================================================================
                           FEATURES ADDED
=============================================================================

BMC 00.68:
Fixed - BMC Memory Leak under certain conditions

BMC 00.66:
N/A

BMC 00.65:
Fixed - FAN_TACH going low issue on S5000PSL

BMC00.64
Fixed - 82563GB network/BMC interface contention issue.
Fixed - BMC checksum mismatches

BMC00.63
Fixed - BMC sometimes hangs if SOL sessions are terminated  
Fixed - BIOS/BMC hang issue

BMC00.62
Fixed - System reverts to OLTT after ctrl+alt+del

BMC 00.61
Added - S5000PSL/S5000XSL/S5000XVN/SC5400RA Refresh Release with CLTT integration
Added - the new FWPIAUPD which supports 128 bytes of flash update.
Fixed - Fans fail to boost after crossing DIMM aggregate temp UC.
Fixed - Get thermal profile data shows success for profile 0 and error for profile 2
Fixed - BMC FW not supporting 128 bytes write. 
Fixed - BMC slow to respond or stops responding completely
Fixed - Direct Serial Connection is not working from sysconfig
Fixed - The event type of system reconfigured event are incorrect
Fixed - SOL can't activate by OpenSource IPMITOOL
Fixed - There are two duplicate assertion/de-assertion events for Power Unit Redundancy sensor after DC Power Cycle.
Fixed - [SYS BOOT -F NORMAL & SERVICE] terminal mode command can't set the needed boot flags.
Fixed - Unnecessary SEL events are getting logged in AC and DC cycle 
Fixed - PEF configuration will be lost after AC or DC cycle 
Fixed - Irregular Chassis ID LED blinking 

BMC 00.59
Fixed - BIOS Setup screen is observed as garbled data on remote machine.
Fixed - Power on console comand is not working
Fixed - GPO61 not supported by PC87427/SIO3 driver 
Fixed - SDK - BMC cmd "Set Processor State" Unsupported state settable and unclearable. 
Fixed - BMC SEL log contains inaccurate timestamp
Fixed - BMC failed to respond during Sx sleep state cycling test.
Fixed - Unable to read SEL entries

BMC 00.58:
Fixed - Wrong status LED behaviour observed for Power restore policy.
Fixed - Status LED color irregularity observed when power restore policy is "Prior state"  
Fixed - Get ACPI State command returns "Legacy Power Off" when in S4 state (Hibernation)
Fixed - Status Led turns to solid amber color after doing a bmc refresh from OS 
Fixed - The 'Get ACPI power state' returns wrong status in Hibernate(S4) mode  
Fixed - BMC is not tracking the correct sleep states

BMC 00.57:
Fixed - The firmware allowed a invalid password to log in.
Fixed - IPMI 1.5 session can be made with any password  

BMC 00.56:

Fixed - BIOS not responding to BMC SetSystemBootOption command - Note: At this point of time this issue
        is resolved only for Intel XEON Series 5100 processors.
Fixed - ACPI issue: When Get ACPI Status command is executed even beofre DC is on, BMC responds as S0/G0 working.
Fixed - After system goes into shutdown, then the system will auto-reboot when comport 2 is connected to loopback
Fixed - System will automatically boot up with RJ45-RS232 convert and RS232 Loopback.
Fixed - Windows 32 or 64-bit will not shutdown with loopback connector on COM Port 2
Fixed - TPT module is not including FML Header/FML Status/TPT Status as part of read buffer 
Fixed - Switching Serial MUX from System to TMODE truncates "[TMODE OK] message  
Fixed - TMode will not maintain connection in standby

BMC 00.55: 

Future processor PECI Support is added.

BMC 00.54: 
	
- SC5400RA Support is added.
- Feature Enhancement - Support for Email Alerts VIA ESB2/BMC on all S5000 Series products is added

Fixed - The boot code version in SLBMC53 does not match that of the BMC release note.
Fixed - Deasserted sel event for chassis intrusion.
Fixed - Unnecessary Characters are displayed in SOL redirection
Fixed - Updating to BIOS R0038 got error 92AB serial port B is being used by BMC as EMP port
Fixed - T-Mode Auto Detect Message  "[TMODE OK]" response is truncated  
Fixed - The CPU failure LEDs on the server board are not lit for processor disabling.

BMC 00.53:

Fixed - BMC stops responding (Error message in BIOS)  - D/C power cycle over RMCPP (dpccli) session
Fixed - Suspend BMC ARP command is not working as expected. 
Fixed - Fully Fan redundant event [deasserted, asserted]is getting logged in DC cycle
Fixed - System hangs if processor disabled thru "set proc state" command 
Fixed - In PIA file PECI Poller Imager Type is incorrect 
Fixed - Power Redundancy event [deasserted, asserted] is getting logged in DC cycle 


BMC 00.52:
  
Fixed - SEL event for S3 ACPI power state is not getting logged when system goes to S3 

BMC 00.51:
       First production Release




[END OF RELEASE NOTES]
