echo -off
# + ============================================================== +
#  Copyright (c) 2010 - 2011, Intel Corporation.

#  This source code and any documentation accompanying it ("Material") is furnished
#  under license and may only be used or copied in accordance with the terms of that
#  license.  No license, express or implied, by estoppel or otherwise, to any
#  intellectual property rights is granted to you by disclosure or delivery of these
#  Materials.  The Materials are subject to change without notice and should not be
#  construed as a commitment by Intel Corporation to market, license, sell or support
#  any product or technology.  Unless otherwise provided for in the license under which
#  this Material is provided, the Material is provided AS IS, with no warranties of
#  any kind, express or implied, including without limitation the implied warranties
#  of fitness, merchantability, or non-infringement.  Except as expressly permitted by
#  the license for the Material, neither Intel Corporation nor its suppliers assumes
#  any responsibility for any errors or inaccuracies that may appear herein.  Except
#  as expressly permitted by the license for the Material, no part of the Material
#  may be reproduced, stored in a retrieval system, transmitted in any form, or
#  distributed by any means without the express written consent of Intel Corporation.

#  Module Name:  startup.nsh

#  Abstract:  Script file for invoking iflash.

# + ============================================================== +
#    Program all blocks of BIOS from capsule file 
# + ============================================================== +

@echo -off
mode 80 25
;foundimage section is simply to locate the correct drive
cls
if exist .\ipmi.efi then
 goto FOUNDIMAGE
endif
if exist fs0:\ipmi.efi then
 fs0:
 echo Found Update Packages on fs0:
 goto FOUNDIMAGE
endif
if exist fs1:\ipmi.efi then
 fs1:
 echo Found Update Packages on fs1:
 goto FOUNDIMAGE
endif
if exist fs2:\ipmi.efi then
 fs2:
 echo Found Update Packages on fs2:
 goto FOUNDIMAGE
endif
 echo "Unable to find Update Packages".  
 echo "Please mount the drive with the update package".
 echo ""
 goto END
:FOUNDIMAGE
echo ==========================================================================
echo "This utility will allow you to update the BMC, BIOS, ME firmware, "
echo "and FRUSDR in the Intel(R) Server Boards S5500WB,S5500WB12V,S5500WBR and S5500WB12VR"
echo "and Intel(R) Server System Boards SR1690WB and SR1695WB"
echo ""
echo "If you want to do all these functions, press Enter. If not, hit 'q'."
echo ""
echo "if you want to update single components like BMC/BIOS separately,"
echo "please execute the individual scripts separately (e.g. BIOSxx.nsh),"
echo "and follow below update process to ensure trouble free update"
echo "from BIOS R0038, BMC 00.40:"
echo "  1): BMC firmware update to 00.56;"
echo "  2): BIOS update to R0057;"
echo "  3): Manageability Engine (ME) Firmware update to 01.12;"
echo "  4): FRUSDR update to 16"
echo ""
echo "Do NOT reboot during this process until you see Updates completed."

echo ==========================================================================
pause

echo ""
echo Integrated BMC and Intel Remote Management Module 3 firmware update rev 00.56
echo ""
Fwpiaupd -u -bin -o -pia -ni BMC_0056.ima 
echo ""
echo "BMC 00.56 Update completed"

echo ""
echo Flashing BIOS R0057...
IFlash32.efi R0057.cap /u /ni
echo ""
echo "BIOS R0057 update completed..."

echo ""
echo "ME Firmware Update rev: Production Release - 01.12"
fwpiaupd -u -o -b -address=2c -bin -ni SPS_01_01_02_007_ME_FW_DIB.bin
echo ""
echo "ME Firmware Update completed..."


echo ""
echo "Update FRUSDR using FRUSDR utility"
frusdr -cfg master.cfg
echo ""
echo "FRUSDR Update completed..."
echo ""
echo ""
echo "Updates completed. Please reboot using the front panel button."
:END

