================================================================================
Intel(R) Server Board S3420GPV System Firmware Update Package for 
Intel(R) Deployment Assistant (3.5.2 or later), 
The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : Jul 14, 2011
TO      : Intel(R) Server Board S3420GPV customers
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : S3420GP.86B.01.00.0049
================================================================================
                           SUPPORTED PLATFORMS and Dependency
================================================================================
Processor supported:
Intel(R) Xeon(R) Processor 3400 Series
Intel(R) Processor i3-500 Series
Intel(R) Pentium(R) Processor G6950

On-Board Component Option ROM Versions: N/A
LSI SWRAID Oprom                	: ESRT2 A.09.08061549I
Intel(R) Matrix RAID Oprom	        : 8.9.0.1023
IBMC Matrox VGA				: VBE BIOS V3.8SL
82574L PXE Version			: Intel(R) Boot Agent GE v1.3.24
82578DM PXE Version			: Intel(R) Boot Agent GE v1.3.35
82578DM EEPROM Version			: v3.1
82574L EEPROM Version			: v1.0
Management Engine Firmware Version 	: 6.0.30.1199

Dependency:

Production boards with belowing minimum BIOS/BMC version:
  Product		BIOS           		   
  S3420GPV		S3420GP.86B.01.00.0030

================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
IMPORTANT!
 - ME FW Update does not work on WINPE (x86) or (x64), OFU, IDA; it is only 
   supported on the embedded EFI shell.


This package can be updated using one of the following methods:
 - The embedded EFI shell
 - Intel(R) Deployment Assistant
 - Windows* Preboot Execution Environment (WinPE)

To Update from the embedded EFI Shell

update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from support.intel.com
- Unzip package and copy all files to a folder in USB disk on key 
- Insert USB disk on key to server USB port
- Reboot server to EFI shell
- Run command "map -r" in EFI shell to mount USB disk on key
- Run command "fs0:" to change folder to USB disk on key, USB key may also mount to
  fs1:. The number of "fs" is dependent on the result of command "map -r"
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process

Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the of EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment toolkit" CD shipped with the system.
User can download the latest version IDA CD ISO image from support.intel.com
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From support.intel.com
    Automatically downloads the latest Firmware Update Package from Intel 
    It requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from support.intel.com and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB Disk on Key or Hard Disk
    Download the latest Firmware Update Package from support.intel.com and copy it 
    to a USB key, then insert the key into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB disk.
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.1 32 bit solution as an example. Please refer to white paper "White 
Paper-Intel Server Utilities Procedure for WinPE.pdf" for details on building 
your own customized WinPE CD.

2. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T

3. Windows PE 3.1 - built from Windows Windows Server 2008 R2


================================================================================
                              BIOS Changes from release 49
================================================================================
IMPORTANT Notice: 
  -  Please use EEUPDATE v5.14.57.1 or later version to update 82578's EEPROM
  -  Intel(R) Core(TM) Processor i3 series must work with Ignition ME FW 6.0.20.1185
     or later version.
  -  Please clear CMOS after BIOS update to activate ME-FW 1185 or later version
     if the onboard ME version is before 6.0.20.1185.
  -  Please use Iflash32 version 2.6 build 15 or later version to support Microsoft*
     OEM Activation 2.0 process.
 
Added:
  - N/A
  
Fixed:
  
  - Fixed: AJA* Kona3* PCIe card has blue screen randomly and triggers PCIE error
           event in SEL
 
================================================================================ 
                           LEGAL INFORMATION
================================================================================

Information in this document is provided in connection with Intel Products
and for the purpose of supporting Intel developed server boards and systems.
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation 
may have patents or pending patent applications, trademarks, copyrights, or
other intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any such
patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 

*Other names and brands are the property of their respective owners.

Copyright (C) 2011 Intel Corporation.

[END OF RELEASE NOTES]

