================================================================================
Intel(R) Server Boards S5500WB,S5500WBR,S5500WB12V and S5500WB12VR
Intel(R) Server System SR1690WB and SR1695WB System Firmware Update Package
for Intel(R) Deployment Assistant, Intel(R) One Boot Flash Update Utility, 
The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : July 27, 2011
TO      : Intel(R) Server Boards S5500WB,S5500WBR,S5500WB12V and S5500WB12VR
	  Intel(R) Server System SR1690WB and SR1695WB customers
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : S5500.86B.01.00.0059.08232011  1421   Build Date  : Aug. 23, 2011
BMC    : 57
FRUSDR : 16
ME     : SPS_01.01.02.007.0_Production
================================================================================
                           Support Platforms and Dependency
================================================================================
Processors supported: 
  Intel(R) Xeon(R) Processor 5500 series and Intel(R) Xeon(R) Processor 5600 series
    w/ <= 6.40GT/s Max Intel(R) QuickPath Interconnect Speed

Microcode update versions:
CPUID     Version      Status
0x106A4   0x00000011   Production (Intel(R) Xeon(R) Processor 5500 series C0/C1)
0x106A5   0x00000015   Production (Intel(R) Xeon(R) Processor 5500 series D0)
0x206C2   0x00000013   Production (Intel(R) Xeon(R) Processor 5600 series B1)

On-Board Component Option ROM Versions:
IBMC Matrox VGA                : VBE BIOS V3.8SM
ICH9R/ICH10 AHCI Option ROM    : iSrc 1.18_E 05012008
ICH10 SATA SW-RAID Option ROM  : vA.09.08061549I
82575EB iSCSI Boot Option ROM  : v2.2.96
82567LM, 82571EB, 82574L,
  82575EB, & 82576 PXE Version : Intel(R) Boot Agent GE v1.3.71
82599EB PXE Version            : Intel(R) Boot Agent XG v2.1.30 Alpha-3

Intel(R) QPI Reference Code Version : 1.85
Memory Reference Code Version       : 2.21

Management Engine Firmware Version  : SPS_01.01.02.007.0 Production #3

Dependency:

Production boards:
  Product		    Fab Version	      BMC	     FRUDSR		EEPROM	  HSC
  S5500WB		    Fab3 or above     00.34	   FWB_08		TBD	      N/A
  S5500WB12V		    Fab3 or above     00.34	   FWB_08		TBD	      N/A
  S5500WBR		    Fab3 or above     00.34	   FWB_08		TBD	      N/A
  S5500WB12VR		    Fab3 or above     00.34	   FWB_08		TBD	      N/A

The following update process must be followed to ensure a trouble free update from 
the BIOS R0033, BMC00.40 releases.
1.	BMC firmware to 00.40 or later
2.	BIOS R0033 or later
3.	Manageability Engine (ME) firmware 01.10 or later
4.	Latest FRU/SDR package specific to the baseboard.
================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - The embedded EFI shell
 - Intel(R) Deployment Assistant 3.5.3 or latest
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   v9.70 Build 17 or later)
 - Windows* Preboot Execution Environment (WinPE)

To Update from the embedded EFI Shell

update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from support.intel.com
- Unzip package and copy all files to a folder in USB disk on key 
- Insert USB disk on key to server USB port
- Reboot server to EFI shell
- Run command "map -r" in EFI shell to mount USB disk on key
- Run command "fs0:" to change folder to USB disk on key, USB key may also mount to
  fs1:. The number of "fs" is dependent on the result of command "map -r"
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process

Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the of EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment toolkit" CD shipped with the system.
User can download the latest version IDA CD ISO image from support.intel.com
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From support.intel.com
    Automatically downloads the latest Firmware Update Package from Intel 
    It requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from support.intel.com and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB Disk on Key or Hard Disk
    Download the latest Firmware Update Package from support.intel.com and copy it 
    to a USB key, then insert the key into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB disk.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from support.intel.com
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from support.intel.com
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB key from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB key manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x86 or x64 OS, you have to read
OFU releaenotes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.0 32 bit solution "WinPE_x64_Update.bat" for WinPE2.1/3.0 64 bit 
solution as an example. Please refer to white paper "White Paper-Intel Server 
Utilities Procedure for WinPE.pdf" for details on building your own customized 
WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 32bit or EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.0 - built from Windows Server 2008R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.
================================================================================
                      BIOS Changes in release R0057
================================================================================
- Fixed: CPU frequency in BIOS setup is not shown correctly with BIOS58 on some platforms
- Fixed: It takes more than 50s to stay at Windows 2003 R2 SP2 login page on RAID ESRTII with Intel(R) Server Board S5500BC.
- Fixed: L1 Cache Size is not correct in SMBIOS when plug 2 Intel(R) Xeon(R) Processor E5620.
- Fixed: [X] USB Stick Hangs POST on Intel(R) Server Board S5520UR
- Fixed: Wrong hard disk capacity reported in BIOS setup and SATA RAID configuration page

Other:
- Added: RMM3 password via BIOS setup will accept special characters
- Added: NSG Passive: Support 2U 4X PCIe Riser on Intel(R) Server Board S5520UR.
- Added: Support 2U Butterfly Passive Riser on Intel(R) Server Board S5520UR.
- Update: EFI NIC Driver to version 4.5.14 
- Update: PXE Boot Agent OPROM to version 1.3.71
- Update: Intel(R) Xeon(R) Processor 5500 series D0 microcode to version 0x15

================================================================================
                     BMC Changes in release 00.56
================================================================================
- Fixed: Authentication error  - Found during stress test of KVM and web session sensor test
- Fixed: Error opening Video Socket after disconnecting network cable
- Fixed: BMC/RMM3 hangs intermittently with KVM activity
- Fixed: Multiple issues with Win7/IE8/Java 6 Update 22, RMM connection/remote access.
- Fixed: KVM session no response to keyboard when first opened in BIOS setup and EFI.
- Fixed: KVM connection getting Connection Failure - Error reading Video data! pop-up window.
- Fixed: Activate Payload Command - Response data maximum inbound & outbound payload size invalid.
- Fixed: Set Channel Access - Changing non-volatile channel field immediately changes volatile.
- Fixed: MEM Fan1 lost control at 100% speed by using FRUSDR26.
- Fixed: When a redundant supply is removed RMM3 Web GUI FRU info page gets an error.

================================================================================
                    FRUSDR Changes in release FWB_15
================================================================================    
- FRUSDR - Request for pause on error for FP sensor.
- Fan speed control SDR record refers to nonexistent sensor 
- Issue regarding the GID and the Sensor Type w.r.t to SDR data on S5500 Platform.
- "Get Thermal Profile Data" command for fan profile 1 and CLTT should be denied
 
================================================================================
                   ME Changes in release SPS_01.01.02.007.0
================================================================================
Issues Fixed:
- N/A
=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2010 - 2011 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
