This is an update to the REAL subdirectory for the DIGPAK & MIDPAK
developers kit.

It includes two major changes.	In PEND.C there is now an assembly routine
to allow you to change the volume of a sound buffer during playback.  It
has been called to my attention that the SetPCMVolume call for DIGPAK locks
up on SoundBlaster16.  This was written by a senior engineer at Creative
Labs, and I was not aware it didn't work.

Regardless, you are better modulating the volume in software anyway since
that will work on all sound cards.

The other change was a demonstration program on how to RECORD audio in
real-time and write the results to disk.  This is in the deliciously
short and simple program called RECORD

Have Fun and Happy Holidays!

John W. Ratcliff
747 Napa Lane
St. Charles, MO 63304
BBS: 1-314-939-0200
CIS: 70253,3237
INTERNET: 70253.3237@compuserve.com

