If you are having a problem with SER5, *FIRST* read the SER5.TXT and SER5.HLP
files to see if those tips help to solve your problem.  If you still need 
help, please fill out this form completely and E-mail it to:

Paul Hermann <hermann@poly-eng.uakron.edu>
-or-
Russell Gilbert <b804683@csc1.ftw.bnr.com>

Hardware
--------
CPU:                            (I.E. 486 DX2-66)
AMOUNT OF RAM:                  (I.E. 8MB)
BRAND OF MODEM:                 (I.E. ZOOM 14.4 INTERNAL -or- NULL MODEM)
COM PORT OF MODEM:              (I.E. COM 2)
IRQ OF MODEM:                   (I.E. IRQ 3)
PORT ADDRESS OF MODEM:          (I.E. PORT 0x3F8)
UART TYPE:                      (I.E. 8250 or 16550)

*NOTE* :The hardware information is to be exactly as the hardware is
	configured, and NOT a copy of the information in the SER5.CFG file.

SOFTWARE
--------
DOOM VERSION:                   (I.E. DOOM v 1.666)


SER5.CFG: (Please attach your complete SR5.CFG file at this point)


DESCRIPTION OF PROBLEM: (Please include as much detail as you can when 
			reporting a problem.  Include exactly what you
			did to cause the problem. If the problem can be
			reproduced on our end, it will be easier to 
			diagnose.)
