TulliCom - the terminal program for Windows 3.x or WINOS/2

It supports the following emulations: TTY, ANSI, VT-52 and VT-100, the protocoles:X-, Y- and ZModem, ASCII and CompuServe B+, and transmission speeds from 300 to 128000 bauds.
Right now, TulliCom is available in three languages (english, french and german). It is very well adapted to beginners in this field.
TulliCom has a character set filter that always sends the right special characters, even to DOS mailboxes or DOS terminal programs and offers the possibility to direct the maibox with the mouse. Ten quick keys can be according to  your needs. They give a fast access to the character strings you often use, such as user's name, password... With the telephone book, you can automatically or manually several numbers in a row.
Of course, you can redial a number automatically or manually. A login recorder stocks different login procedures, if you wish so, and will do these operations alone in the future, when you want to call these numbers.
Protocol files, you may select as you please, stock, in the ASCII format, everything displayed in the communication windows, if you wish so. All data send or received and the telephonebook can be printed as well. Up- and downloads run also in the background so that you can use other Windows programs in the mean time.
Data transfer demands are recognized automatically by the corresponding protocoles such as ZModem or Batch.
Turning the port on and off allows a modem sharing with other applications.
The use of TulliCom corresponds to the Windows program's conventional use and doesn't need to be explained in its details.

TulliCom is a full version program. Exclusively on CD-ROM by ROMWARE.

SYSTEM REQUIRED:

IBM compatible PC
CD-ROM drive
1 MB RAM
Windows 3.0 or higher WINOS/2 2.0 or higher
2 MB free HDD
Mouse recommanded

Language: English, French, German