[System]
cpu=3
dos=5.00
ram=580
ems=1600
xms=0
mouse=1
cdrom=0
diskspace=8600000

[Game]
gametitle="Microprose - 1942: The Pacific Air War v1.4"
gamedir=UPDATE
gamebatname=NONE
gameexename=1942.EXE
gamewadname=1942
gameconfig=CONFIG.FT

[Special]
sound=NONE
bootdisk=bootdisk.exe

[MinInstall]
mininstalldir=NONE

[MaxInstall]
maxinstalldir=NONE

[Search]
numfiles=10
file00=INSTALL.EXE
file01=1942.EXE
file02=3D.CDF
file03=MAP.CDF
file04=DATA.CDF
file05=LAND.MOD
file06=CONFIG.FT
file07=HALLFAME.DAT
file08=PILOTS.DAT
file09=SETUP.DAT

[Spawn]
numfiles=1
file0=update.exe

[Execute]
file=NONE

[MusicCard]
numcards=18
sound=9
card00="No Sound",                      0, N,   0, 0, 0, NoAddr,    NoIRQ,      NoDRQ
card01="AdLib",                        16, A, 904, 0, 0, AdLibAddr, NoIRQ,      NoDRQ
card02="AdLib Gold",                   34, P, 904, 7, 0, AdLibAddr, NoIRQ,      NoDRQ
card03="Covox Sound Master II",        17, A, 544, 7, 1, CovoxAddr, NoIRQ,      NoDRQ
card04="General MIDI via MPU-401",     64, G, 816, 2, 0, MIDIAddr,  MIDIIRQ,    NoDRQ
card05="Pro Audio Spectrum",           25, A, 904, 7, 1, AdLibAddr, NoIRQ,      NoDRQ
card06="PAS Plus/16/Studio",           33, P, 904, 5, 3, AdLibAddr, NoIRQ,      NoDRQ
card07="Sound Blaster",                18, A, 544, 3, 1, SB1Addr,   NoIRQ,      NoDRQ
card08="Sound Blaster Pro  (OPL-2)",   24, A, 544, 7, 1, SB2Addr,   NoIRQ,      NoDRQ
card09="Sound Blaster Pro2 (OPL-3)",   32, P, 544, 7, 1, SB2Addr,   NoIRQ,      NoDRQ
card10="Sound Blaster 16",             35, P, 544, 5, 1, SB16Addr,  NoIRQ,      NoDRQ
card11="Sound Blaster 16 ASP",         36, P, 544, 5, 1, SB16Addr,  NoIRQ,      NoDRQ
card12="Sound Blaster AWE (w/TSR)",    65, G, 816, 2, 0, SBAWEAddr, SB16IRQ,    NoDRQ
card13="Roland MT-32",                 48, R, 816, 2, 0, MIDIAddr,  MIDIIRQ,    NoDRQ
card14="Roland LAPC-1/CM-32L",         49, R, 816, 2, 0, MIDIAddr,  MIDIIRQ,    NoDRQ
card15="Roland RAP-10",                69, G, 816, 2, 0, RAPAddr,   RAPIRQ,     NoDRQ
card16="Ensoniq Soundscape",           70, G, 816, 2, 0, SSAddr,    SSIRQ,      NoDRQ
card17="Turtle Beach Maui",            68, G, 816, 2, 0, MauiAddr,  MauiIRQ,    NoDRQ


[DigitalCard]
numcards=13
sound=0
card00="No Sound",                      0, N,   0, 0, 0, NoAddr,    NoIRQ,      NoDRQ
card01="AdLib Gold",                   34, P, 904, 7, 1, AdLibAddr, GOLDIRQ,    GOLDDRQ
card02="Covox Sound Master II",        17, A, 904, 7, 1, CovoxAddr, CovoxIRQ,   CovoxDRQ
card03="Pro Audio Spectrum",           25, A, 904, 7, 1, AdLibAddr, PASIRQ,     PASDRQ
card04="PAS Plus/16/Studio",           33, P, 904, 5, 3, AdLibAddr, PAS16IRQ,   PAS16DRQ
card05="Roland RAP-10",                69, G, 816, 2, 5, RAPAddr,   RAPIRQ,     RAPDRQ
card06="Sound Blaster",                18, A, 544, 3, 1, SB1Addr,   SB1IRQ,     SB1DRQ
card07="Sound Blaster Pro  (OPL-2)",   24, A, 544, 7, 1, SB2Addr,   SB2IRQ,     SB2DRQ
card08="Sound Blaster Pro2 (OPL-3)",   32, P, 544, 7, 1, SB2Addr,   SB2IRQ,     SB2DRQ
card09="Sound Blaster 16",             35, P, 544, 5, 1, SB16Addr,  SB16IRQ,    SB16DRQ
card10="Sound Blaster 16 ASP",         36, P, 544, 5, 1, SB16Addr,  SB16IRQ,    SB16DRQ
card11="Sound Blaster AWE",            65, G, 544, 5, 1, SB16Addr,  SB16IRQ,    SB16DRQ
card12="Ensoniq Soundscape",           70, G, 816, 2, 1, SSAddr,    SSIRQ,      SSDRQ

[NoAddr]
addr=   -1
[NoIRQ]
irq=    -1
[NoDRQ]
drq=    -1

[AdLibAddr]
addr=   904

[CovoxAddr]
addr=   544,576,640,704

[CovoxIRQ]
irq=    3,4,5,6,7
[CovoxDRQ]
drq=    1,3

[SB1Addr]
addr=   528,544,560,576,592,608
[SB1IRQ]
irq=    2,3,5,7
[SB1DRQ]
drq=    1

[SB2Addr]
addr=   544,576
[SB2IRQ]
irq=    2,5,7,10
[SB2DRQ]
drq=    0,1,3

[SB16Addr]
addr=   544,576,608,640
[SB16IRQ]
irq=    2,5,7,10
[SB16DRQ]
drq=    0,1,2,3
[SBAWEAddr]
addr=   768,816

[MIDIAddr]
addr=   768,784,800,816,818,820,822,832
[MIDIIRQ]
irq=    2,3,4,5,6,7
[MIDIDRQ]
drq=    -1

[RAPAddr]
addr=   544,560,576,592,800,816,832,848
[RAPIRQ]
irq=    2,5,7,10,11
[RAPDRQ]
drq=    5,6,7

[SSAddr]
addr=   800, 816, 832, 848
[SSIRQ]
irq=    2,5,7,10,12
[SSDRQ]
drq=    0,1,3

[PASIRQ]
irq=    3,4,5,6,7
[PASDRQ]
drq=    1,2,3

[PASplusIRQ]
irq=    2,3,5,7,10,11,12,15
[PASplusDRQ]
drq=    0,2,3,4,5,6,

[PAS16IRQ]
irq=    2,3,5,7,10,11,12,15
[PAS16DRQ]
drq=    0,2,3,5,6,7

[GOLDIRQ]
irq=    3,4,5,7,10,11,12,15
[GOLDDRQ]
drq=    0,1,2,3

[MauiAddr]
addr=   528,560,608,656,768,800,816,824
[MauiIRQ]
irq=    2,5,12,15
