                        MGA MILLENIUM 3DR DRIVER
                            Version: 1.00.001    
                             October 19, 1995

A) Description.
--------------

        This directory contains the Matrox Hardware Accelerated 3DR driver.
        For now, the driver runs on 3DR 2.0.15 only.

        To use the driver you must choose ModeSwitch with QCDP and a 3D video 
        mode with the MGA Millenium Control Panel.

B) Installation procedure.
--------------------------

        1. From the Windows file menu choose run and execute the install.exe
           program in the /3DR/ directory of the MGA CD-ROM. This installs 3DR
	   2.0.15. Run "install.exe win32s" if you need to install win32s.
           Refer to the Readme.Wri file for more information.

        2. Copy mga32.3dr, sx16x64.dll and sx32x64.dll to your windows
           directory on your system. This installs the Matrox driver.

        3. Modify the 3dr.ini file in your windows directory as follows:

                The line IHV_DISPLAY=GEN32.3DR must be commented out by 
                adding a semicolon at the beginning of the line.

                The line ihv_display=mga32.3dr must be added below the
                commented line.

C) Known bugs.
--------------

        1. No support for ModeSwitch feature of our Windows Driver.
           You must close all 3DR applications before switching video
           mode.

        2. This driver does not work in 8 bpp video modes.
        
        3. Shaded objects may have bad colored pixels in them.

        4. Under Truespace 2.0:

                a. Sometimes when painting an object with a texture map some
                   triangles are missing from the object. Move the object or
                   click on the 3DR icon to fix the problem.
