



             ŚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄæ
             ³             CYBERBOARD KID             ³
             ³     TROUBLESHOOTING AND HELP GUIDE     ³
             ĄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄŁ





ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

                      TABLE OF CONTENTS
                      ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

                  1. THE SETUP PROGRAM
                  2. GENERAL TROUBLE SHOOTING
                  3. SOUND CARD TROUBLE SHOOTING
                  4. FREQUENTLY ASKED QUESTIONS

ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

1. THE SETUP PROGRAM
ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
  SETUP.EXE must be run before you can start playing CYBERBOARD KID.
  The menu options and their uses are described below:

  1.1 AUDIO CARD
  ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    You must select your sound card from the list, and choose the
    appropriate sound card settings ( BASE I/O PORT, IRQ, DMA ).

    SOUND QUALITY: The higher the sound quality, the more work the
                   computer must do. So if CYBERBOARD KID is running
                   slowly on your machine, select low sound quality.

    SOUND CHANNELS: This is the number of sound effect that can play
                    simultaneously. One again the higher this value,
                    the more work your computer has to perform.

    TEST SOUND & MUSIC: This just enables you test if your sound card
                        is configured correctly.

  1.2 SOUND & MUSIC
  ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    Use this menu if you wish to disable sound effects and/or music.

  1.3 DETAIL LEVEL
  ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    If CYBERBOARD KID is running slowly or the scrolling seems jerky
    at times, you can try dropping the detail level.

    HIGH DETAIL   : Everything on
    MEDIUM DETAIL : Status bar animations off
    LOW DETAIL    : MEDIUM + foregrounds off, certain animations off,
                    smoke trails on the hoverboard off.

  1.4 INPUT DEVICE
  ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    This is where you select how you wish to control CYBERBOARD KID.
    Remember if you choose JOYSTICK or GRAVIS GAMEPAD you must
    calibrate it first using the CALIBRATE JOYSTICK option in the
    SETTINGS menu in the game.

  1.5 WINDOWS 95 SETUP
  ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    This menu option sets up the directories in the CK.PIF file.

    CYBERBOARD KID is a DOS based game, therefore we strongly
    recommend you run it from DOS ( If you are running Windows 95
    then DOS MODE ), BUT it does run under Windows 95. We have
    therefore included an ICON and PIF.

    To run CYBERBOARD KID from WINDOWS 95, enter the file explorer
    and navigate to your CYBERBOARD KID drive and directory.
    Double click on CK.PIF.

    You can create a shortcut to CYBERBOARD KID by dragging CK.PIF
    onto your desktop.

    If you run CYBERBOARD KID from a DOS window or you wish to
    create your own PIF, make sure you run it with -WIN95 command
    line parameter:

    e.g.: CK -WIN95

    When CYBERBOARD KID starts we automatically turn numlock OFF.
    Sometimes WINDOWS 95 may turn it back on, this will be easily
    noticed as the cursor keys will not work in the menus and
    CYBERBOARD KID is in permanent FAST MODE in the game. Just press
    NUMLOCK once to remedy this.

    NOTE: On slower computers running under WINDOWS 95 may cause the
          music to sound staggered during level loading and some
          comic cut-scenes.

  1.6 COMPATIBILITY
  ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    LOW MEMORY (4 Mb) MODE:
      If your computer has 4Mb of memory you must set this to ON.
      Because of the large amount of sprites and scenery in
      CYBERBOARD KID, the memory usage of the game is very high,
      therefore you may have to perform a clean boot or create a
      boot disk to free up enough memory. See the BOOT DISK section
      of GENERAL TROUBLE SHOOTING.

    ATI MACH COMPATIBILITY:
      Certain VGA cards such as the ATI MACH32 and MACH64 do not
      support PEL-PANNING ( A technique we use to make the scrolling
      smooth ). If you have such a card ( or if the horizontal
      scrolling shudders badly ) then switch this option ON.

      Unfortunately the scrolling with this option ON is not as
      smooth as it would be with a PEL-PANNING compatible video card.

  1.7 SAVE AND EXIT
  ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    Once you have correctly setup and configured CYBERBOARD KID
    choose this option to save the settings.

    Then type CK and have fun!

ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

2. GENERAL TROUBLESHOOTING
ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

  2.1 MEMORY MANAGERS
  ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    CYBERBOARD KID can be unstable in the presence of a memory
    manager, such as EMM386 or QEMM. We recommend removing these from
    memory before playing. Alternatively, if you are having trouble,
    try disabling EMS support, and remove any memory inclusions /
    exclusions.

    e.g.  DEVICE=C:\DOS\EMM386.EXE NOEMS

  2.2 CREATING A BOOT DISK
  ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    1. Insert a new disk into your A drive ( floppy or stiffy - drive
       dependant )

    2. At the DOS prompt type: FORMAT A: /S and press ENTER
       This will format the disk and place the system files onto
       it.

    3. At the DOS prompt type: A: and press ENTER

    4. Type copy con autoexec.bat
       You will now be entering the contents of your autoexec.bat.
       To cancel at any time press CTRL-BREAK.
       To save the file in its current state and exit press CTRL-Z.

       Type in your SOUND driver environment variable and any
       initialization commands it needs:

       Example for SOUND BLASTER 16 with PORT 220, IRQ 7, DMA 1,5

         SET BLASTER=A220 I7 D1 H5 P330 T6
         C:\SB16\SB16SET /M:240 /VOC:240 /TREBLE:220 /OPGAIN:8,8
         C:\SB16\SBCONFIG.EXE /S

       Example for GUS MAX with PORT 220, IRQ 7, DMA 1

         SET ULTRASND=220,1,1,7,7
         C:\ULTRASND\ULTRINIT.EXE -ej

       Once you have completed this press CTRL-Z

    5. Type copy con config.sys
       Enter the following:

        DEVICE=C:\DOS\HIMEM.SYS
        DEVICE=C:\DOS\EMM386.EXE NOEMS
        FILES=20
        BUFFERS=20,0
        DOS=HIGH,UMB

       Press CTRL-Z

     6. You should now reboot your computer.

     7. Goto the CYBERBOARD KID directory on your hard drive
        Example: Type C: and press ENTER
                 Type CD \CK and press ENTER
                 Type CK and press ENTER

     NOTE: If you have an DOS text editor, use this to create
           your bootup files. ( It's much easier than COPY CON )

ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

3. SOUND CARD TROUBLE SHOOTING
ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

  3.1 SOUND CARD SUPPORT
  ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

  CYBERBOARD KID supports most popular sound cards on the
  market, including:

    ž Sound Blaster 1.x
    ž Sound Blaster 2.x
    ž Sound Blaster Pro
    ž Sound Blaster 16/16ASP
    ž Sound Blaster AWE32 and WaveBlaster
    ž Pro Audio Spectrum
    ž Pro Audio Spectrum+
    ž Pro Audio Spectrum 16
    ž Logitech SoundMan
    ž Windows Sound System
    ž Gravis UltraSound
    ž Gravis UltraSound Max


 3.2 SOUND RELATED PROBLEMS AND THEIR SOLUTIONS
 ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

 ž  THE COMPUTER LOCKS UP OR REBOOTS
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    Run SETUP and verify that your sound card settings are correct:

    - Check your I/O port address, IRQ line and DMA channel settings.
      If you don't know your sound's settings, consult your
      manual for details.

    - Make sure your sound card has no conflicts with other cards in
      your system. If your sound card works properly with other
      programs, you can assume that there are no such conflicts.

    If this doesn't solve the problem, try booting clean --- usually
    memory managers like QEMM, EMM386, etc. and/or TSRs loaded in
    memory may cause problems.


 ž  THE SOUND AND MUSIC RUNS SLOWLY ON MY COMPUTER
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    Your computer is not fast enough. You can speed up the system by
    running SETUP and setting a lower quality.


 ž  THE SYSTEM DOES NOT RECOGNIZE MY SOUND CARD
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    You have selected the wrong sound card or I/O port address. Run
    SETUP again and select the right settings.

    If you are using a Sound Blaster 16 then you must check that the
    right drivers are loaded in your AUTOEXEC.BAT and CONFIG.SYS
    files.

    If the problems persist, check that you have enough conventional
    memory ( maybe the system was unable to allocate conventional
    memory required for a DMA buffer used to communicate with your
    sound card ).


 ž  I DON'T HEAR ANY SOUND
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    First check that your speakers/headphones are plugged in. If they
    are make sure the VOLUME CONTROL on your sound card is up.

    If that is not the problem then check that your IRQ and/or DMA
    settings are correct. You must run the SETUP program to select
    the right settings, it is highly recommended to reboot your
    computer before trying the new settings.


 ž  MUSIC IS FINE WHEN I START, BUT GETS CUT OFF AFTER A FEW SECONDS
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    This is what happens when you select a wrong IRQ line for your
    sound card. Run SETUP again and select the correct IRQ number.


 ž  MY SOUND BLASTER CLONE IS NOT RECOGNIZED
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    Run the SETUP program and set the right hardware parameters.
    Choose the plain Sound Blaster. If this does not fix the problem,
    your Sound Blaster clone may not be 100 % compatible.


 ž  THE MUSIC SOUNDS SLOW ON MY SOUND BLASTER
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    Run SETUP again and select plain Sound Blaster. You were possibly
    using the Sound Blaster 2.0 / Pro driver and your card does not
    support high speed DMA transfers.


 ž  THE SYSTEM HANGS WITH MY SOUND BLASTER 16
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    Your system's motherboard cannot handle high DMA at full speed.
    On some machines, the DMA controller does not function properly
    during high DMA transfer. To solve this problem, use a 8-bit DMA
    channel for high DMA transfers. See your SB16 manual for details.


 ž  I HEAR STATIC WITH MY SOUND BLASTER
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    Try turning the MIC and LINE volumes to zero.
    If you still hear static try disconnecting your parallel port
    devices.


 ž  I ONLY HEAR SOUND EFFECTS, NO MUSIC
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    If you are running in LOW MEMORY MODE music is automatically
    disabled to save memory.

    If your aren't running in LOW MEMORY MODE check that MUSIC is
    ON in the SETUP program, then check your music volume in the
    SETTINGS menu in the game.

    If you have a GUS card the IRQ setting is probably incorrect
    Run SETUP again and set the correct settings.


 ž  SOUND BLASTER 16 SPECIFIC NOTES
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    You must select the high DMA channel in the SETUP program, this
    is because the system uses 16-bit playback mode. See your SB16
    manual for details.

    Make sure that the right SB16 drivers are loaded in the
    AUTOEXEC.BAT and CONFIG.SYS files. If you don't want to waste
    memory loading these drivers, you may want to try the following:

    Edit your AUTOEXEC.BAT file and insert the following lines:

      REM
      REM These lines will setup your SB16 sound card at port 220h
      REM using IRQ 5, low DMA 1, high DMA 5 and MIDI port 330h.
      REM
      SET BLASTER=A220 I5 D1 H5 P330 T6
      DIAGNOSE /S

    The above lines will set your SB16 hardware configuration based
    on the BLASTER environment variable. Make sure that the above
    lines are setting the BLASTER variable with the right parameters.
    See your manual for details about the BLASTER environment
    variable.


 ž  PRO AUDIO SPECTRUM SPECIFIC NOTES
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    Make sure that the right PAS drivers are properly loaded in your
    AUTOEXEC.BAT and CONFIG.SYS files. Without these drivers the
    system won't recognize your PAS sound card. If you have a PAS+ or
    PAS16 and the system does not work properly, you may want to try
    running SETUP and tell it that you have a Sound Blaster sound
    card.


 ž  GRAVIS ULTRASOUND SPECIFIC NOTES
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
    You must choose the GF1 IRQ line and Playback DMA channel in the
    SETUP program. Make sure that the right GUS drivers are loaded in
    your AUTOEXEC.BAT and CONFIG.SYS files. However, the sound system
    should work without loading any of these drivers.

    Notice that some SB emulators (SBOS) may conflict with the sound
    system, so if you experience problems try disabling these
    emulators.

    Because of the nature of the GUS, the sound effects are uploaded
    to the card using a caching system. This may cause slight slow
    downs from time to time during gameplay.

ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

4. FREQUENTLY ASKED QUESTIONS
ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

  4.1 TROUBLE SHOOTING RELATED
  ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

  Q. I can't enter the CALIBRATE JOYSTICK option on the setup menu.

  A. You must first set your input device to JOYSTICK or GRAVIS
     GAMEPAD. This is set in the INPUT DEVICE menu of the SETUP
     program.

  Q. I selected JOYSTICK and KEYBOARD as my input device, but in the
     game CYBERBOARD KID doesn't react to the JOYSTICK or KEYBOARD ?

  A. Before you can use a JOYSTICK or GRAVIS GAMEPAD in the game
     you must calibrate it using the CALIBRATE JOYSTICK option
     in the SETTINGS MENU. You only need to calibrate it once
     as the settings are automatically saved.

  Q. The cursor keys don't work in the menu. Why ?
                          OR
  Q. CYBERBOARD KID is permanently in TURBO mode even though I
     haven't pressed 'T' for TURBO ?

  A. Either WINDOWS 95 has set numlock ON or it was pressed on
     your keyboard. Just press NUMLOCK once to fix this.

  Q. Moving around in the menus is painfully slow.

  A. Your are running under WINDOWS 95 without starting CYBERBOARD
     KID with -WIN95 parameter. Type CK -WIN95 at the DOS prompt or
     setup the parameter in your PIF for CYBERBOARD KID.

  Q. Moving around in the menus is ridiculously fast!

  A. You have started CYBERBOARD KID with -WIN95 command line
     parameter, but you are running from normal DOS.

  Q. The scrolling shudders badly horizontally, but is OK diagonally
     and vertically ?

  A. Your video card does not support PEL-PANNING. This is prevalent
     in the ATI MACH range. Set the ATI MACH support option ON in
     the compatibility menu of the SETUP program.

  Q. I get a MEMORY ALLOCATION ERROR when I try run CYBERBOARD KID.

  A. Set the LOW MEMORY MODE option ON in the compatibility menu of
     the SETUP program. If you already have this ON, you must free
     up more memory to run CYBERBOARD KID. See the BOOTDISK section
     of GENERAL TROUBLE SHOOTING.

  Q. The music skips or sounds staggered.

  A. Your computer can't handle such a high music quality. Try
     dropping the music quality in the AUDIO SETUP menu of the
     SETUP program. This may also happen when running under
     Windows 95.


  4.2 GENERAL
  ÄÄÄÄÄÄÄÄÄÄÄ

  Q. What is extra in the FULL REGISTERED version ?

  A. 23 new levels and 3 secret levels. 32 levels all in all!
     10 new enemies, bosses and the mega boss.
     16 new songs.
     23 MEGS of story art and 19 MEGS of total game art.
     Higher quality sound effects.
     A level editor to make your own CYBERBOARD KID levels.

  Q. Where can I get the FULL VERSION ?

  A. Select ORDERING INFO from the HELP utility, or check out the
     ORDERING INFO in the main menu of the game to see where
     you can get it.


ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

   All trademarks are the property of their respective owners.

ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

