DEC OSF/1 will run in GXemul 0.3 and earlier. It may have problems running in
later versions due to bugs in the dyntrans CPU emulation, which was introduced 
in 0.4.0. It is not possible to install OSF/1 from tape in GXemul due to bugs in
the tape emulation. You must copy all the packages to a fake CD image. Format a 
hard drive image as UFS under an ULTRIX or DEC OSF/1 system, make a directory 
called RISC in the root directory of the image, make directories for each of the
package groups (see the table below), copy the packages (all tape files after
the first 4 are packages) from the tapes into the corresponding directories 
(rename them so that the filenames match those that the installer expects; for
example, f04.OSFBASE200.tar.Z should be renamed to OSFBASE200), make an 
"instctrl" directory in each package-group directory, and extract the
instctrl.tar file for each tape into the instctrl directory. Boot the install
system from the emulated tape, install the miniroot, boot the miniroot, change 
"TK50 tz" in /.minidevice to "RZ58 rz", and install OSF/1 normally.

Package groups:

tape			directory on CD image
Tin0Install		MPK
Tin1Kits		BASE
Tin1Kits		BASE
Tin3RT			RT
