
        Instructions for installing Select 5i2
        --------------------------------------

To install and use this upgrade you MUST already have Select 5i1 (RISC
OS 6.14) installed and running on your computer. DO NOT attempt to use
this ROM if you are using any other version of RISC OS.

To install the new ROM proceed as follows.

Drag the skeleton !Boot in this archive over !Boot on your hard drive. A
window will open asking you if you wish to upgrade your existing !Boot.
Click on the button labelled 'Merge'. The new components will be
installed in your existing !Boot but at this stage will not be run.

To use RISC OS 6.16 click on 'Softload' in the Configure window. The
Configure window will already have been opened when you merged !Boot but
if you have closed it then ADJUST-click on the RISC OS 6 icon at the
right hand end of the icon bar to re-open it.

In the window which opens you will see two new ROM images. These are
Select5i2 and Select5i2na. If you have a CD ROM drive connected to the
motherboard IDE interface then choose 'Select5i2'. If your CD ROM drive
is connected to a third party IDE or SCSI interface then choose
'Select5i2na'.

You can now either click on 'Set and Reboot' to choose the new ROM and
reboot your computer immediately or 'Set' in which case the new ROM will
be used the next time your computer starts up.

The 'DevTools' directory contains undated versions of !ResEd and
!ResTest. If you installed earlier versions of these tools then you
should replace them with these new versions.
