Plustek-PARPORT-TODO.txt (2003-29-10) Gerhard Jäger <gerhard@gjaeger.de>
========================================================================

TODO (in general):
    - more documentation/comments on the different functions
    - remove/check the CHECK marks
    - add additional button handler
    - adding adjustment of the scan area
    - checking timeout conditions (MiscCheckTimer !) and handle them correctly
    - let the 96001/3 based models work with the highest available
      phys. resolution
    - Create the modes out of the capability list of each device

(USER-MODE):
    - line by line feedback to the backend


KNOWN BUGS/Limitations:

Model                    Description                           Workaround
------------------------------------------------------------------------------

OpticPro P9636           detected as OP12000                   none
Genius VividPro II Film  Halftone/Gray > 450 dpi didn't work   none
OpticPro P4830           binary scanning does not work         none
OpticPro A3I             bad picture quality                   none
Genius HR6               negative scanning not okay            none

********************************* DONE ***************************************

- PS/2 bidi does not work (libieee1284)                          
- Update the IOCTL interface and remove some old structs (CmdBlk)

******************************** SKIPPED *************************************

better dither maps                             nobody needs halftone scanning
make the backtrace work for ASIC 96001/3       not possible due to ASIC limits
based models
