# SANE: Supported Devices

The following table summarizes the devices supported by sane-backends-1.0.24.

This is only a summary! Please consult the manpages and the author-supplied webpages for more detailed (and usually important) information concerning each backend.

If you have new information or corrections, please file a bug report with as many details as possible. Also please tell us if your scanner isn't mentioned in this list at all.

For an explanation of the tables, see the legend.

## Summary

Device type | Number of devices
--- | ---
Total | Supported | Untested | Unsupported
Sum | Complete | Good | Basic | Minimal
Scanners | 2042 | 1221 | 418 | 672 | 105 | 26 | 337 | 484
Still cameras | 5 | 5 | 1 | 2 | 2 | 0 | 0 | 0
Video Cameras | 8 | 3 | 0 | 1 | 0 | 2 | 3 | 2
Meta backends | 2 | n/a
APIs | 6 | n/a

## Scanners

Manufacturers: Abaton, Acer Peripherals, Across Technologies, Actown, Adlib, Advent, AGFA, Ambir, Apple, Aries, ArmorPlate, Artec/Ultima, Avigramm, Avision, Bell and Howell, Bell+Howell, BenQ, Benq (Acer), BlackWidow, Boeder, BrightScan, Brother, C-Channel, Canon, Chinon, Compaq, Compeye, Corex, Cybercom, DCT, Dell, Devcom, Dextra, Dexxa, E-Lux, EDGE, EDT (Electronic Document Technology), Enhans, Epson, Escom, Escort, Fujitsu, Gallery, Genius, Googlegear, Guillemot, Guillemot / Hercules, Hercules, Hewlett-Packard, IBM, IOMagic, Iris, iVina, Kodak, Komodo, KONICA MINOLTA, Kyocera, LEO, Lexmark, Linotype Hell, Logitech, Medion/Lifetec/Tevion/Cytron, Memorex, Micromaxx, Microstar, Microtek, Minolta, Minolta-QMS, Mitsubishi, Mustek, NeatReceipts, NEC, Network, Nikon, Nortek, OKI, Olivetti, Olympus, Optoelectronics, Optrox, Packard Bell, Panasonic, Pentax, PIE, PIOTECH, PLANon, Plustek, Portable Peripheral Co., Ltd., Primax, Prolink, Quato, Reflecta, Relisys, RevScan, Ricoh, Samsung, Scanport, Scanshell, Sceptre, Sharp, Sicos, Siemens, SmartDisk, Spot Technology, Syscan, Tamarack, Targa, TCE, Teco, TemPlate, Tiny, TriGem, Trust, UMAX, Vantas, Visioneer, Viviscan, Vobis, Vuego, Xerox, Yakumo

### Manufacturer: Abaton

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Scan 300/GS | SCSI |  | Complete | All known modes and functions supported | abaton (unmaintained) | sane-abaton
Scan 300/S | SCSI |  | Untested | Untested, use with caution | abaton (unmaintained) | sane-abaton

### Manufacturer: Acer Peripherals

Comment: Company was renamed to Benq.

### Manufacturer: Across Technologies

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
FS-1130 | SCSI |  | Good | FCC ID LUZFS1130 | leo (1.0-10) | sane-leo

### Manufacturer: Actown

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
ACT Scan I 30 | SCSI |  | Untested | sub model VM3520A | teco1 (1.0-10) | sane-teco1

### Manufacturer: Adlib

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
JetScan630 | SCSI |  | Good |  | pie (1.0) | sane-pie
JetScan636PRO | SCSI |  | Untested |  | pie (1.0) | sane-pie

### Manufacturer: Advent

Link(s): http://www.adventcomputers.co.uk

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
AW10 | USB | 0x040a/0x4060 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio

### Manufacturer: AGFA

Link(s): http://www.agfa.com/, http://www.agfa.com

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Arcus 1200 | SCSI |  | Good | Optional transparency unit supported. | SnapScan (1.4) | sane-snapscan
Arcus II | SCSI |  | Good | Arcus *II*, not Arcus! | microtek (0.13.1) | sane-microtek
DuoScan | SCSI |  | Basic |  | microtek (0.13.1) | sane-microtek
DuoScan f40 | USB IEEE-1394 | 0x06bd/0x02bf | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
DuoScan T2000XL | SCSI |  | Unsupported | Unsupported. Same as Microtek ArtixScan 2020? | unsupported (2010-06-09) | ?
DuoScan T2500 | SCSI IEEE-1384 |  | Unsupported | Unsupported. Same as Microtek Artixscan 2500f | unsupported (2010-06-09) | ?
Focus Color | SCSI |  | Good | 3-pass | agfafocus (unmaintained) | sane-agfafocus
Focus Color Plus | SCSI |  | Good | 3-pass | agfafocus (unmaintained) | sane-agfafocus
Focus GS Scanner | SCSI |  | Untested | 6 bit gray | agfafocus (unmaintained) | sane-agfafocus
Focus II | SCSI |  | Untested | gray only | agfafocus (unmaintained) | sane-agfafocus
Focus Lineart Scanner | SCSI |  | Untested | Lineart only? Untested. | agfafocus (unmaintained) | sane-agfafocus
SnapScan | SCSI |  | Good |  | SnapScan (1.4) | sane-snapscan
SnapScan 300 | SCSI |  | Good |  | SnapScan (1.4) | sane-snapscan
SnapScan 310 | SCSI |  | Good |  | SnapScan (1.4) | sane-snapscan
SnapScan 310P | Parport |  | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
SnapScan 600 | SCSI |  | Good | Optional ADF supported. | SnapScan (1.4) | sane-snapscan
SnapScan 1200P | Parport |  | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
SnapScan 1212P | Parport |  | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
SnapScan 1212U | USB | 0x06bd/0x0001 | Good |  | SnapScan (1.4) | sane-snapscan
SnapScan 1212U_2 | USB | 0x06bd/0x2061 | Good |  | SnapScan (1.4) | sane-snapscan
SnapScan 1236s | SCSI |  | Good | Optional ADF and transparency unit supported. | SnapScan (1.4) | sane-snapscan
SnapScan 1236u | USB | 0x06bd/0x0002 | Good | Optional ADF and transparency unit supported. | SnapScan (1.4) | sane-snapscan
SnapScan e10 | USB | 0x06bd/0x2093 | Good |  | SnapScan (1.4) | sane-snapscan
SnapScan e20 | USB | 0x06bd/0x2091 | Good |  | SnapScan (1.4) | sane-snapscan
SnapScan e25 | USB | 0x06bd/0x2095 | Good |  | SnapScan (1.4) | sane-snapscan
SnapScan e26 | USB | 0x06bd/0x2097 | Good |  | SnapScan (1.4) | sane-snapscan
SnapScan e40 | USB | 0x06bd/0x208d | Good |  | SnapScan (1.4) | sane-snapscan
SnapScan e42 | USB | 0x06bd/0x20ff | Good |  | SnapScan (1.4) | sane-snapscan
SnapScan e50 | USB | 0x06bd/0x208f | Good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
SnapScan e52 | USB | 0x06bd/0x20fd | Good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
SnapScan e60 | USB |  | Untested |  | SnapScan (1.4) | sane-snapscan
SnapScan EZ | Parport |  | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
Snapscan Touch | USB | 0x06bd/0x0100 | Complete |  | niash (0.3) | sane-niash
StudioScan | SCSI |  | Good |  | microtek (0.13.1) | sane-microtek
StudioScan II | SCSI |  | Good |  | microtek (0.13.1) | sane-microtek
StudioScan IIsi | SCSI |  | Good |  | microtek (0.13.1) | sane-microtek
Studiostar | SCSI |  | Minimal | Is detected but scans are very dark | microtek (0.13.1) | sane-microtek

### Manufacturer: Ambir

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Visigo A4 | USB | 0x0a82/0x4600 | Complete | Rebaged Travelscan 464 | plustek (0.52) | sane-plustek

### Manufacturer: Apple

Link(s): http://developer.apple.com/, http://www.apple.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Apple Scanner | SCSI |  | Good | 4bit, 16 shades of gray | apple (unmaintained) | sane-apple
Color OneScanner | SCSI |  | Minimal | truecolor (needs much work) but it scans in non color modes. | apple (unmaintained) | sane-apple
Color OneScanner 600/27 | SCSI |  | Good | Rebadged CanoScan 300 | canon (1.12) | sane-canon
OneScanner | SCSI |  | Basic | 8bit, 256 shades of gray. The backend needs work especially in the quantization code but it may work. | apple (unmaintained) | sane-apple

### Manufacturer: Aries

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Scan-It Pro 4800 | Parport (SPP, EPP) |  | Complete | use driver-switch mov=2 | plustek_pp (0.43) | sane-plustek_pp

### Manufacturer: ArmorPlate

Link(s): http://www.armorplate.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
AmplScan II | SCSI |  | Complete | AmplScan *II*, not AmplScan! | template (0.42, NEW!) | sane-template

### Manufacturer: Artec/Ultima

Link(s): http://www.artecusa.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
1236 USB | USB | 0x05d8/0x4001 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
A6000C | SCSI |  | Complete | all modes working | artec (unmaintained) | sane-artec
A6000C PLUS | SCSI |  | Complete | f/w <= v1.92 basic, f/w >= v1.93 OK | artec (unmaintained) | sane-artec
AM12e+ | Parport |  | Unsupported | Unsupported. Chips found inside: AT015, AD9816JS. Maybe similar to SCSI version or as6e? | unsupported (2010-06-09) | ?
AM12S | SCSI |  | Complete | all modes working | artec (unmaintained) | sane-artec
AS6E | Parport |  | Basic | Requires the program 'as6edriver' to run. | as6e (0.5) | sane-as6e
AT3 | SCSI |  | Complete | all modes working | artec (unmaintained) | sane-artec
AT6 | SCSI |  | Good | Scan head needs to return home before another scan can be started. | artec (unmaintained) | sane-artec
AT12 | SCSI |  | Complete | all modes working | artec (unmaintained) | sane-artec
E+ 48U | USB | 0x05d8/0x4003 | Good | CIS scanner based on the GT6816 chip. Apparently all other devices are re-badged Artec scanners. | artec_eplus48u (unmaintained) | sane-artec_eplus48u
E+ Pro | USB | 0x05d8/0x4004 | Minimal | Works up to 600dpi, but not 1200. Needs better calibration. See bug #310490 | artec_eplus48u (unmaintained) | sane-artec_eplus48u
Ultima 2000 | USB | 0x05d8/0x4002 | Good | Works, only product id 0x4002 is supported | gt68xx (1.0-84) | sane-gt68xx
Ultima 2000 (0x4001) | USB | 0x05d8/0x4001 | Unsupported | Same name, but different ids: This scanner is not supported. The scanner with product id 0x4002 is supported by the gt68xx backend, however. | unsupported (2010-06-09) | ?
Ultima 2000 e+ | USB | 0x05d8/0x4002 | Good | Works, however 12 bit mode doesn't seem to be supported | gt68xx (1.0-84) | sane-gt68xx

### Manufacturer: Avigramm

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Minidoc | USB Parport | 0x05cb/0x1483 | Unsupported | Not supported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Avision

Link(s): http://www.avision.com, http://www.avision.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
@V2500 | USB | 0x0638/0x0aa1 | Untested |  | avision (Build: 296) | sane-avision
@V5100 | USB | 0x0638/0x0a45 | Good | 1 pass, 1200 dpi, A3 - duplex!, LCD screen, paper sensors | avision (Build: 296) | sane-avision
AM3000 Series | USB | 0x0638/0x0a41 | Basic | MFD | avision (Build: 296) | sane-avision
AV100CS | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
AV100IIICS | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
AV100S | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
AV120 | USB | 0x0638/0x0a27 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
AV121 | USB | 0x0638/0x0a3c | Good | sheetfed scanner | avision (Build: 296) | sane-avision
AV122 | USB | 0x0638/0x0a33 | Good | sheetfed duplex scanner | avision (Build: 296) | sane-avision
AV122 C2 | USB | 0x0638/0x0a93 | Good | sheetfed duplex scanner | avision (Build: 296) | sane-avision
AV210 | USB | 0x0638/0x0a25 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
AV210 | USB | 0x0638/0x0a24 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
AV210C2 | USB | 0x0638/0x0a3a | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
AV210C2-G | USB | 0x0638/0x0a2f | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
AV210D2+ | USB | 0x0638/0x1a35 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
AV220 | USB | 0x0638/0x0a23 | Complete | duplex! sheetfed scanner | avision (Build: 296) | sane-avision
AV220+ | USB | 0x0638/0x0a2c | Complete | duplex! sheetfed scanner | avision (Build: 296) | sane-avision
AV220-G | USB | 0x0638/0x0a94 | Complete | duplex! sheetfed scanner | avision (Build: 296) | sane-avision
AV220C2 | USB | 0x0638/0x0a2a | Complete | duplex! sheetfed scanner | avision (Build: 296) | sane-avision
AV220C2-B | USB | 0x0638/0x0a2e | Complete | duplex! sheetfed scanner | avision (Build: 296) | sane-avision
AV220C2-G | USB | 0x0638/0x0a2d | Complete | duplex! sheetfed scanner | avision (Build: 296) | sane-avision
AV220D2 | USB | 0x0638/0x0a2b | Complete | duplex! sheetfed scanner | avision (Build: 296) | sane-avision
AV240SC | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
AV260CS | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
AV360CS | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
AV363CS | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
AV420CS | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
AV600U | USB | 0x0638/0x0a13 | Good | 1 pass, 600 dpi | avision (Build: 296) | sane-avision
AV600U Plus | USB | 0x0638/0x0a18 | Good |  | avision (Build: 296) | sane-avision
AV610 | USB | 0x0638/0x0a18 | Good |  | avision (Build: 296) | sane-avision
AV610C2 | USB | 0x0638/0x0a5e | Good |  | avision (Build: 296) | sane-avision
AV620CS | SCSI |  | Complete | 1 pass, 600 dpi | avision (Build: 296) | sane-avision
AV620CS Plus | SCSI |  | Complete | 1 pass, 1200 dpi | avision (Build: 296) | sane-avision
AV630CS | SCSI |  | Complete | 1 pass, 1200 dpi | avision (Build: 296) | sane-avision
AV630CSL | SCSI |  | Untested | 1 pass, 1200 dpi | avision (Build: 296) | sane-avision
AV660S | SCSI |  | Untested | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV680S | SCSI |  | Untested | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV690U | SCSI |  | Untested | 1 pass, 2400 dpi | avision (Build: 296) | sane-avision
AV800S | SCSI |  | Untested | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV810C | SCSI |  | Untested | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV820 | SCSI |  | Untested | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV820C | SCSI |  | Complete | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV820C Plus | SCSI |  | Complete | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV830C | SCSI |  | Complete | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV830C Plus | SCSI |  | Untested | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV880 | SCSI |  | Untested | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV880C | SCSI |  | Untested | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV3200C | SCSI |  | Complete | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV3200SU | USB | 0x0638/0x0a4e | Complete | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV3730SU | USB | 0x0638/0x0a4f | Complete | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV3750SU | USB | 0x0638/0x0a65 | Complete | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV3800C | SCSI |  | Complete | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV3850SU | USB | 0x0638/0x0a66 | Complete | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV6120 | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
AV6240 | SCSI |  | Complete | 1 pass, ??? dpi | avision (Build: 296) | sane-avision
AV8000S | SCSI |  | Complete | 1 pass, 1200 dpi, A3 | avision (Build: 296) | sane-avision
AV8050U | USB | 0x0638/0x0a4d | Complete | 1 pass, 1200 dpi, A3 - duplex! | avision (Build: 296) | sane-avision
AV8300 | USB | 0x0638/0x0a40 | Complete | 1 pass, 1200 dpi, A3 - duplex! | avision (Build: 296) | sane-avision
AV8350 | USB | 0x0638/0x0a68 | Complete | 1 pass, 1200 dpi, A3 - duplex! | avision (Build: 296) | sane-avision
AVA3 | SCSI |  | Basic | 1 pass, 600 dpi, A3 | avision (Build: 296) | sane-avision
DS310F | Parport |  | Unsupported | Probably not supported. Scanner/printer/copier combination. | unsupported (2010-06-09) | ?
DS610CU Scancopier | USB | 0x0638/0x0a16 | Good | 1 pass, 600 dpi, A4 | avision (Build: 296) | sane-avision
FB2080E | USB | 0x0638/0x0a84 | Basic | 1 pass, 600 dpi, zero-edge | avision (Build: 296) | sane-avision
FB6000E | SCSI |  | Complete | 1 pass, 1200 dpi, A3 - duplex! - zero edge! | avision (Build: 296) | sane-avision
FB6080E | USB | 0x0638/0x0a82 | Complete | 1 pass, 1200 dpi, A3 - duplex! - zero edge! | avision (Build: 296) | sane-avision
IT8300 | USB | 0x0638/0x0a61 | Good | 1 pass, 1200 dpi, A3 - duplex!, LCD screen, paper sensors | avision (Build: 296) | sane-avision
iVina 1600 | USB | 0x0638/0x0a10 | Unsupported | GL646 based, to be added to genesys backend. Same as UMAX Astra 4500. | unsupported (2010-06-09) | ?
iVina FB1800 | USB | 0x0638/0x0a20 | Unsupported | GL646/GL660 based. Same as UMAX Astra 4700. | unsupported (2010-06-09) | ?
iVina FB2400 | USB |  | Unsupported | Not supported. No chipset information available. Same as UMAX Astra 6700. | unsupported (2010-06-09) | ?

### Manufacturer: Bell and Howell

Link(s): http://www.bhscanners.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
COPISCAN II 2135 | SCSI |  | Untested | Simplex Scanner | bh (1.0-4) | sane-bh
COPISCAN II 2137(A) | SCSI |  | Good | Simplex Scanner (with ACE) - limited testing | bh (1.0-4) | sane-bh
COPISCAN II 2138A | SCSI |  | Untested | Simplex Scanner with ACE | bh (1.0-4) | sane-bh
COPISCAN II 3238 | SCSI |  | Untested | Simplex Scanner | bh (1.0-4) | sane-bh
COPISCAN II 3338(A) | SCSI |  | Untested | Simplex Scanner (with ACE) | bh (1.0-4) | sane-bh
COPISCAN II 6338 | SCSI |  | Good | Duplex Scanner with ACE - development model | bh (1.0-4) | sane-bh

### Manufacturer: Bell+Howell

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
2000F | SCSI |  | Basic | 1 pass, ??? dpi, A4 | avision (Build: 296) | sane-avision

### Manufacturer: BenQ

Link(s): http://www.benq.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
5550 | USB | 0x04a5/0x2211 | Minimal | developing yet | hp3900 (0.12) | sane-hp3900

### Manufacturer: Benq (Acer)

Link(s): http://www.benq.com
Comment: Formerly Acer Peripherals

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
300f | SCSI |  | Good |  | SnapScan (1.4) | sane-snapscan
310P | Parport |  | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
310s | SCSI |  | Good |  | SnapScan (1.4) | sane-snapscan
310U | USB | 0x04a5/0x1a20 | Good |  | SnapScan (1.4) | sane-snapscan
320P | Parport |  | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
320U | USB | 0x04a5/0x2022 | Good |  | SnapScan (1.4) | sane-snapscan
340P | Parport |  | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
340U | USB | 0x04a5/0x2022 | Good |  | SnapScan (1.4) | sane-snapscan
610P | Parport |  | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
610plus | SCSI |  | Good |  | SnapScan (1.4) | sane-snapscan
610PT | Parport |  | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
610s | SCSI |  | Good |  | SnapScan (1.4) | sane-snapscan
620P | Parport |  | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
620PT | Parport |  | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
620s | SCSI |  | Good |  | SnapScan (1.4) | sane-snapscan
620U | USB | 0x04a5/0x1a2a | Good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
620UT | USB | 0x04a5/0x2040 | Good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
640BT | USB | 0x04a5/0x20be | Good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
640bu | USB | 0x04a5/0x207e | Good |  | SnapScan (1.4) | sane-snapscan
640P | Parport |  | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
640U | USB | 0x04a5/0x2060 | Good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
1240 | USB | 0x04a5/0x20c0 | Good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
3300 | USB | 0x04a5/0x20de | Good |  | SnapScan (1.4) | sane-snapscan
3300 | USB | 0x04a5/0x20b0 | Good |  | SnapScan (1.4) | sane-snapscan
4300 | USB | 0x04a5/0x20de | Good |  | SnapScan (1.4) | sane-snapscan
4300 | USB | 0x04a5/0x20b0 | Good |  | SnapScan (1.4) | sane-snapscan
5000 | USB | 0x04a5/0x20f8 | Good | USB ID 0x04a5,0x20f8: Color / grayscale scans working up to 1200 DPI | SnapScan (1.4) | sane-snapscan
5000E | USB | 0x04a5/0x20fc | Basic | Same as 5000U, working up to 600 DPI | SnapScan (1.4) | sane-snapscan
5000U | USB | 0x04a5/0x20fc | Basic | Same as 5000E, working up to 600 DPI | SnapScan (1.4) | sane-snapscan
5150 | USB | 0x04a5/0x2137 | Basic | Calibration algorithm unknown | SnapScan (1.4) | sane-snapscan
5250 | USB | 0x04a5/0x2137 | Basic | Same hardware as 5150 (?), Calibration algorithm unknown | SnapScan (1.4) | sane-snapscan
5300 | USB | 0x04a5/0x20fe | Basic | Problems with firmware upload reported | SnapScan (1.4) | sane-snapscan
5450 | USB | 0x04a5/0x211e | Unsupported | Unsupported. | unsupported (2010-06-09) | ?
5550 | USB | 0x04a5/0x2211 | Unsupported | Unsupported, see link for details. | unsupported (2010-06-09) | ?
5560 | USB | 0x04a5/0x2311 | Unsupported |  | unsupported (2010-06-09) | ?
7400UT | USB | 0x04a5/0x2202 | Unsupported |  | unsupported (2010-06-09) | ?
ScanWit 2720s | SCSI |  | Good |  | SnapScan (1.4) | sane-snapscan

### Manufacturer: BlackWidow

Link(s): http://www.blackwidow.co.uk/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
BW4800SP | SCSI |  | Complete | rebadged Artec AT3 | artec (unmaintained) | sane-artec

### Manufacturer: Boeder

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Sm@rtScan Office | Parport USB | 0x05cb/0x1483 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
Sm@rtScan Slim Edition | USB | 0x05d8/0x4002 | Good | Similar to Artec Ultima 2000 | gt68xx (1.0-84) | sane-gt68xx

### Manufacturer: BrightScan

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
BrighScan OpticPro | Parport (SPP, EPP) |  | Complete | Reported as P12 | plustek_pp (0.43) | sane-plustek_pp

### Manufacturer: Brother

Link(s): http://www.brother.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
MFC 2500 | USB | 0x04f9/0x000a | Unsupported | Not supported. See link for details. | unsupported (2010-06-09) | ?
MFC 4600 | Parport |  | Unsupported | The parport 200x400dpi grayscale version of this scanner is unsupported. Dmitri Katchalov did some investigations on this scanner. If you want to write a backend, contact him (see link). | unsupported (2010-06-09) | ?
MFC 7300c | Parport USB | 0x04f9/0x0106 | Unsupported |  | unsupported (2010-06-09) | ?
MFC 9600 | USB | 0x04f9/0x0101 | Unsupported |  | unsupported (2010-06-09) | ?

### Manufacturer: C-Channel

Link(s): http://www.c-channel.ch/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
MoneyPen II | USB |  | Unsupported | Probably unsupported. | unsupported (2010-06-09) | ?
MyPen Light | USB | 0x0a93/0x0005 | Unsupported | See bug #306792 for details. | unsupported (2010-06-09) | ?
MyPen Pro | USB |  | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Canon

Link(s): http://www.canon.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Canon Image Formula 101 | USB | 0x1083/0x162e | Unsupported | GL846 based, work in progress | genesys (1.0-63) | sane-genesys
CanoScan 300 | SCSI |  | Good | 1 pass; flatbed scanner | canon (1.12) | sane-canon
CanoScan 600 | SCSI |  | Good | 1 pass; flatbed scanner | canon (1.12) | sane-canon
CanoScan 620S | SCSI |  | Good | 1 pass; flatbed scanner | canon (1.12) | sane-canon
CanoScan 700F | USB | 0x04a9/0x1907 | Good | GL847 based, resolution from 75 to 4800 dpi | genesys (1.0-63) | sane-genesys
CanoScan 1200S | SCSI |  | Good | 1 pass; flatbed scanner | canon (1.12) | sane-canon
CanoScan 2700F | SCSI |  | Good | 1 pass; film scanner | canon (1.12) | sane-canon
CanoScan 2710S | SCSI |  | Good | 1 pass; 36bit film scanner | canon (1.12) | sane-canon
CanoScan 3000 | USB | 0x04a9/0x2215 | Unsupported | GL660+GL646 based. | unsupported (2010-06-09) | ?
CanoScan 3000ex | USB | 0x04a9/0x2215 | Unsupported | GL660+GL646 based. | unsupported (2010-06-09) | ?
CanoScan 3000F | USB | 0x04a9/0x2215 | Unsupported | GL660+GL646 based, to be added to genesys backend | unsupported (2010-06-09) | ?
CanoScan 4200F | USB | 0x04a9/0x221b | Unsupported | Probably unsupported. See link. | unsupported (2010-06-09) | ?
CanoScan 4400F | USB | 0x04a9/0x2228 | Unsupported | GL843 based, to be added to genesys backend | unsupported (2010-06-09) | ?
CanoScan 4400f | USB | 0x04a9/0x2228 | Unsupported | GL843 based, to be added to the genesys backend | genesys (1.0-63) | sane-genesys
CanoScan 5000F | USB | 0x04a9/0x2212 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
CanoScan 5200F | USB | 0x04a9/0x2217 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
CanoScan 5600F | USB | 0x04a9/0x1906 | Unsupported | GL847 based, to be added to the genesys backend | genesys (1.0-63) | sane-genesys
CanoScan 8000F | USB | 0x04a9/0x220f | Unsupported | Not supported. See link for more information. With transparency adapter. | unsupported (2010-06-09) | ?
CanoScan 8400F | USB | 0x04a9/0x221e | Unsupported | GL841 based, to be added to genesys backend | unsupported (2010-06-09) | ?
CanoScan 8600F | USB | 0x04a9/0x2229 | Unsupported | GL841 based, to be added to genesys backend | unsupported (2010-06-09) | ?
CanoScan 8800F | USB | 0x04a9/0x1901 | Complete | Flatbed scan. TPU for negatives and slides. All resolutions supported (up to 4800DPI). | pixma (0.17.4) | sane-pixma
CanoScan 9000F | USB | 0x04a9/0x1908 | Complete | Full flatbed support up to 4800DPI (Note: flatbed does not have 9600DPI capability). Full TPU support (negatives, slides and infrared) up to 9600DPI. | pixma (0.17.4) | sane-pixma
CanoScan 9000F Mark II | USB | 0x04a9/0x190d | Complete | Full flatbed support up to 4800DPI (Note: flatbed does not have 9600DPI capability). Full TPU support (negatives, slides and infrared) up to 9600DPI. | pixma (0.17.4) | sane-pixma
CanoScan 9900F | USB | 0x04a9/0x2210 | Unsupported | Probably unsupported, similar to 8000F. 3200x6400 dpi USB2. With transparency adapter. | unsupported (2010-06-09) | ?
CanoScan 9950F | USB | 0x04a9/0x2219 | Unsupported | Probably unsupported. | unsupported (2010-06-09) | ?
CanoScan D646U | USB | 0x04a9/0x220b | Unsupported | Probably not supported. See link for more information and test program. | unsupported (2010-06-09) | ?
CanoScan D646U ex | USB | 0x04a9/0x220b | Unsupported | Probably not supported. See D646. | unsupported (2010-06-09) | ?
CanoScan D660U | USB | 0x04a9/0x2208 | Good | TPA scans not perfect | plustek (0.52) | sane-plustek
CanoScan D1230U | USB | 0x04a9/0x2209 | Unsupported | Probably not supported. | unsupported (2010-06-09) | ?
CanoScan D1250U2 | USB | 0x04a9/0x220c | Unsupported | Not supported. However, someone started working on this scanner and some information is available (see link). | unsupported (2010-06-09) | ?
CanoScan D2400UF | USB | 0x04a9/0x220a | Unsupported | Not supported. See link. | unsupported (2010-06-09) | ?
CanoScan FB310P | Parport (ECP) |  | Unsupported | Rebadged Avision, different command set | canon_pp (0.33) | sane-canon_pp
CanoScan FB320P | Parport (ECP) |  | Basic | Newly added support | canon_pp (0.33) | sane-canon_pp
CanoScan FB320U | USB | 0x04a9/0x2201 | Unsupported | Probably not supported. No details known. | unsupported (2010-06-09) | ?
CanoScan FB330P | Parport (ECP) |  | Good |  | canon_pp (0.33) | sane-canon_pp
CanoScan FB610P | Parport (ECP) |  | Unsupported | Rebadged Avision, different command set | canon_pp (0.33) | sane-canon_pp
CanoScan FB620P | Parport (ECP) |  | Basic | Newly added support | canon_pp (0.33) | sane-canon_pp
CanoScan FB620U | USB | 0x04a9/0x2202 | Unsupported | Probably not supported. Some information is available. | unsupported (2010-06-09) | ?
CanoScan FB630P | Parport (ECP) |  | Good |  | canon_pp (0.33) | sane-canon_pp
CanoScan fb630u | USB | 0x04a9/0x2204 | Good | OK | canon630u (0.1) | sane-canon630u
CanoScan fb636u | USB | 0x04a9/0x2204 | Good | OK | canon630u (0.1) | sane-canon630u
CanoScan FB1210U | USB | 0x04a9/0x2205 | Unsupported | Not supported. However, a stand-alone program for FreeBSD is available. | unsupported (2010-06-09) | ?
CanoScan LiDE 35 | USB | 0x04a9/0x2213 | Good | Same ids as LiDE 50. | genesys (1.0-63) | sane-genesys
CanoScan LiDE 40 | USB | 0x04a9/0x2213 | Good | Same ids as LiDE 50. | genesys (1.0-63) | sane-genesys
CanoScan LiDE 50 | USB | 0x04a9/0x2213 | Good |  | genesys (1.0-63) | sane-genesys
CanoScan LiDE 60 | USB | 0x04a9/0x221c | Good |  | genesys (1.0-63) | sane-genesys
CanoScan LiDE 70 | USB | 0x04a9/0x2225 | Unsupported | Philips chip. Backend started, see link | unsupported (2010-06-09) | ?
CanoScan LiDE 80 | USB | 0x04a9/0x2214 | Unsupported | GL841 based, to be added to genesys backend | unsupported (2010-06-09) | ?
CanoScan LiDE 90 | USB | 0x04a9/0x1900 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
CanoScan LiDE 100 | USB | 0x04a9/0x1904 | Complete | GL847 based, resolution from 75 to 2400 dpi | genesys (1.0-63) | sane-genesys
CanoScan LiDE 110 | USB | 0x04a9/0x1909 | Complete | GL124 based, resolution from 75 to 2400 dpi | genesys (1.0-63) | sane-genesys
CanoScan LiDE 200 | USB | 0x04a9/0x1905 | Complete | GL847 based, resolution from 75 to 4800 dpi | genesys (1.0-63) | sane-genesys
CanoScan LiDE 210 | USB | 0x04a9/0x190a | Complete | GL124 based, resolution from 75 to 2400 dpi | genesys (1.0-63) | sane-genesys
CanoScan LiDE 500F | USB | 0x04a9/0x221f | Unsupported | GL841 based, to be added to genesys backend | unsupported (2010-06-09) | ?
CanoScan LiDE 600 | USB | 0x04a9/0x2224 | Unsupported | Philips chip. Backend started, see link | unsupported (2010-06-09) | ?
CanoScan LiDE 600F | USB | 0x04a9/0x2224 | Unsupported | Philips chip. Backend started, see link | unsupported (2010-06-09) | ?
CanoScan LiDE25 | USB | 0x04a9/0x2220 | Good |  | plustek (0.52) | sane-plustek
CanoScan N340P | Parport (ECP) |  | Good |  | canon_pp (0.33) | sane-canon_pp
CanoScan N640P | Parport (ECP) |  | Good |  | canon_pp (0.33) | sane-canon_pp
CanoScan N640P ex | Parport (ECP) |  | Good | Just an N640P in a different box? | canon_pp (0.33) | sane-canon_pp
CanoScan N650U/N656U | USB | 0x04a9/0x2206 | Complete |  | plustek (0.52) | sane-plustek
CanoScan N670U/N676U/LiDE20 | USB | 0x04a9/0x220d | Complete |  | plustek (0.52) | sane-plustek
CanoScan N1220U | USB | 0x04a9/0x2207 | Complete |  | plustek (0.52) | sane-plustek
CanoScan N1240U/LiDE30 | USB | 0x04a9/0x220e | Complete |  | plustek (0.52) | sane-plustek
CR-25 | USB | 0x1083/0x161a | Untested | Please test! | canon_dr (41) | sane-canon_dr
CR-50 | USB |  | Untested | Please test! | canon_dr (41) | sane-canon_dr
CR-55 | USB | 0x1083/0x160c | Untested | Please test! | canon_dr (41) | sane-canon_dr
CR-80 | USB |  | Untested | Please test! | canon_dr (41) | sane-canon_dr
CR-135i | USB SCSI | 0x1083/0x1639 | Untested | Please test! | canon_dr (41) | sane-canon_dr
CR-180 | USB SCSI | 0x04a9/0x1602 | Untested | Please test! | canon_dr (41) | sane-canon_dr
CR-180II | USB SCSI | 0x04a9/0x1602 | Untested | Same as CR-180? Please test! | canon_dr (41) | sane-canon_dr
CR-190i | USB SCSI | 0x1083/0x162b | Untested | Please test! | canon_dr (41) | sane-canon_dr
DR-1210C | USB | 0x1083/0x160f | Untested | Later version? Please test! | canon_dr (41) | sane-canon_dr
DR-1210C | USB | 0x04a9/0x2222 | Untested | Older version? Please test! | canon_dr (41) | sane-canon_dr
DR-2010C | USB | 0x1083/0x161b | Complete | Hardware provides: Gray/Color, Simplex/Duplex, Full-width, 300/600dpi horizontal. Driver provides: Binary, Despeckle, Deskew, Cropping, Calibration, other resolutions. | canon_dr (41) | sane-canon_dr
DR-2010M | USB |  | Untested | Mac version of DR-2010C? Please test! | canon_dr (41) | sane-canon_dr
DR-2020U | USB |  | Unsupported | GL84x? | unsupported (2010-06-09) | ?
DR-2050C | USB | 0x04a9/0x160a | Complete | Hardware provides: Gray/Color, Simplex/Duplex, Full-width. Driver provides: Binary, Despeckle, Deskew, Cropping, Calibration. | canon_dr (41) | sane-canon_dr
DR-2050SP | USB | 0x04a9/0x160a | Untested | Same as DR-2050C? Please test! | canon_dr (41) | sane-canon_dr
DR-2080C | USB SCSI | 0x04a9/0x1601 | Complete | Hardware provides: Gray/Color, Simplex/Duplex, Full-width. Driver provides: Binary, Despeckle, Deskew, Cropping, Calibration | canon_dr (41) | sane-canon_dr
DR-2510C | USB | 0x1083/0x1617 | Complete | Hardware provides: Gray/Color, Simplex/Duplex, Full-width, 300/600dpi horizontal. Driver provides: Binary, Despeckle, Deskew, Cropping, Calibration, other resolutions | canon_dr (41) | sane-canon_dr
DR-2510M | USB |  | Untested | Mac version of DR-2510C? Please test! | canon_dr (41) | sane-canon_dr
DR-2580C | USB SCSI | 0x04a9/0x1608 | Complete | Hardware provides: Gray/Color, Simplex/Duplex, Full-width. Driver provides: Binary, Despeckle, Deskew, Cropping, Calibration | canon_dr (41) | sane-canon_dr
DR-3010C | USB | 0x1083/0x161d | Good | Minimal testing, settings copied from DR-2510C | canon_dr (41) | sane-canon_dr
DR-3020C | SCSI |  | Untested | Please test! | canon_dr (41) | sane-canon_dr
DR-3060 | SCSI |  | Untested | Please test! | canon_dr (41) | sane-canon_dr
DR-3080C | SCSI |  | Untested | Almost works, need to investigate traces from windows driver | canon_dr (41) | sane-canon_dr
DR-3080CII | USB SCSI | 0x04a9/0x1609 | Untested | Almost works, need to investigate traces from windows driver | canon_dr (41) | sane-canon_dr
DR-4010C | USB | 0x1083/0x1614 | Good | Binary/HT/Gray/Color, Simplex/Duplex working. Multistream unsupported. | canon_dr (41) | sane-canon_dr
DR-4580U | USB |  | Untested | Please test! | canon_dr (41) | sane-canon_dr
DR-5010C | USB | 0x04a9/0x1606 | Untested | Please test! | canon_dr (41) | sane-canon_dr
DR-5020 | SCSI |  | Good | LineArt, Duplex working, cannot read buttons or screen? | canon_dr (41) | sane-canon_dr
DR-5060F | SCSI |  | Basic | Grayscale works, LineArt might | canon_dr (41) | sane-canon_dr
DR-5080C | SCSI |  | Untested | Please test! | canon_dr (41) | sane-canon_dr
DR-6010C | USB SCSI | 0x1083/0x1626 | Untested | Please test! | canon_dr (41) | sane-canon_dr
DR-6030C | USB SCSI | 0x1083/0x1638 | Untested | Please test! | canon_dr (41) | sane-canon_dr
DR-6050C | USB SCSI | 0x1083/0x1624 | Good | Simplex, duplex, all resolutions, binary/ht/gray working. Can't wake from stand-by mode | canon_dr (41) | sane-canon_dr
DR-6080 | USB SCSI | 0x04a9/0x1607 | Good | Simplex, duplex, all resolutions, binary/ht/gray, async mode, dropout-color, multifeed/staple detection, deskew, buttons and JPEG working. Imprinter, barcode, custom gamma and multistream unsupported | canon_dr (41) | sane-canon_dr
DR-7080C | USB SCSI | 0x04a9/0x1604 | Untested | Please test! | canon_dr (41) | sane-canon_dr
DR-7090C | USB SCSI | 0x1083/0x1620 | Good | ADF and flatbed work | canon_dr (41) | sane-canon_dr
DR-7550C | USB SCSI | 0x1083/0x1623 | Untested | Assumed compatible with DR-6050C | canon_dr (41) | sane-canon_dr
DR-7580 | USB SCSI | 0x04a9/0x160b | Good | Simplex, duplex, all resolutions, binary/ht/gray, async mode, dropout-color, multifeed/staple detection, deskew, buttons and JPEG working. Imprinter, barcode, custom gamma and multistream unsupported | canon_dr (41) | sane-canon_dr
DR-9050C | USB SCSI | 0x1083/0x1622 | Good | Simplex, duplex, all resolutions, binary/ht/gray working. Can't wake from stand-by mode | canon_dr (41) | sane-canon_dr
DR-9080C | USB SCSI | 0x04a9/0x1603 | Good | Simplex, duplex, all resolutions, binary/ht/gray/color, async mode, dropout-color, multifeed/staple detection, deskew, buttons and JPEG working. Imprinter, barcode, custom gamma and multistream unsupported | canon_dr (41) | sane-canon_dr
DR-C125 | USB |  | Untested | Similar protocol to other canon_dr machines, but unsupported image format. | canon_dr (41) | sane-canon_dr
DR-C130 | USB |  | Untested |  | canon_dr (41) | sane-canon_dr
DR-G1100 | USB |  | Untested |  | canon_dr (41) | sane-canon_dr
DR-G1130 | USB |  | Untested |  | canon_dr (41) | sane-canon_dr
DR-M140 | USB |  | Untested |  | canon_dr (41) | sane-canon_dr
DR-M160 | USB |  | Untested |  | canon_dr (41) | sane-canon_dr
DR-X10C | USB SCSI | 0x1083/0x1618 | Untested | Please test! | canon_dr (41) | sane-canon_dr
DR3020 | SCSI |  | Untested | Please test! | canon_dr (41) | sane-canon_dr
DR4080U | USB |  | Untested | Please test! | canon_dr (41) | sane-canon_dr
FS4000 | USB SCSI | 0x04a9/0x3042 | Unsupported | Not supported. See link for more details. | unsupported (2010-06-09) | ?
i-SENSYS MF3010 | USB Ethernet | 0x04a9/0x2759 | Complete | All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
I-SENSYS MF4320d | USB | 0x04a9/0x26ee | Complete | All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
I-SENSYS MF4330d | USB | 0x04a9/0x26ee | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
i-SENSYS MF4550d | USB | 0x04a9/0x2736 | Good | Flatbed and ADF scan. All resolutions supported (up to 600DPI). | pixma (0.17.4) | sane-pixma
i-SENSYS MF5880dn | USB | 0x04a9/0x26f9 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
i-SENSYS MF6680dn | USB | 0x04a9/0x26fa | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
imageCLASS D420 | USB | 0x04a9/0x26ef | Complete | All resolutions supported (up to 600DPI). Flatbed, ADF simplex and Duplex supported. | pixma (0.17.4) | sane-pixma
imageCLASS D480 | USB | 0x04a9/0x26ed | Complete | All resolutions supported (up to 600DPI). Flatbed, ADF simplex and Duplex supported. | pixma (0.17.4) | sane-pixma
imageCLASS MF3110 | USB | 0x04a9/0x2660 | Complete | All resolutions supported (up to 600DPI). | pixma (0.17.4) | sane-pixma
imageCLASS MF3240 | USB | 0x04a9/0x2684 | Complete | All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF4010 | USB | 0x04a9/0x26b4 | Complete | All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF4018 | USB | 0x04a9/0x26b4 | Complete | All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF4120 | USB | 0x04a9/0x26a3 | Complete | All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF4122 | USB | 0x04a9/0x26a3 | Complete | All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF4140 | USB | 0x04a9/0x26a3 | Complete | All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF4150 | USB | 0x04a9/0x26a3 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF4270 | USB | 0x04a9/0x26b5 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF4350d | USB | 0x04a9/0x26ee | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF4370dn | USB | 0x04a9/0x26ec | Good | Flatbed and ADF scan. All resolutions supported (up to 600DPI). Network not supported | pixma (0.17.4) | sane-pixma
imageCLASS MF4380dn | USB | 0x04a9/0x26ec | Good | Flatbed and ADF scan. All resolutions supported (up to 600DPI). Network not supported | pixma (0.17.4) | sane-pixma
imageCLASS MF4410 | USB | 0x04a9/0x2737 | Complete | All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF4430 | USB | 0x04a9/0x2737 | Good | Flatbed and ADF scan. All resolutions supported (up to 600DPI). ADF empty buggy. | pixma (0.17.4) | sane-pixma
imageCLASS MF4570dw | USB | 0x04a9/0x275a | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
imageCLASS MF4660 | USB | 0x04a9/0x26b0 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF4690 | USB | 0x04a9/0x26b0 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF4770n | USB Ethernet | 0x04a9/0x2774 | Good | Flatbed scan. All resolutions supported (up to 600DPI). ADF buggy. | pixma (0.17.4) | sane-pixma
imageCLASS MF5630 | USB | 0x04a9/0x264e | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
imageCLASS MF5730 | USB | 0x04a9/0x265d | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
imageCLASS MF5750 | USB | 0x04a9/0x265e | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
imageCLASS MF5770 | USB | 0x04a9/0x265f | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI). | pixma (0.17.4) | sane-pixma
imageCLASS MF6500 series | USB | 0x04a9/0x2686 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF6550 | USB | 0x04a9/0x2686 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageCLASS MF8030 | USB | 0x04a9/0x2707 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
imageCLASS MF8170c | USB | 0x04a9/0x2659 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
imageRUNNER 1020/1024/1025 | USB | 0x04a9/0x26e6 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
imageRUNNER 1133 | USB | 0x04a9/0x2742 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
ImageRunner iR1018 | USB | 0x04a9/0x269d | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
ImageRunner iR1022 | USB | 0x04a9/0x269d | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
ImageRunner iR1023 | USB | 0x04a9/0x269d | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
IS 12 | USB |  | Unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers. | unsupported (2010-06-09) | ?
IS 22 | Parport |  | Unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers. | unsupported (2010-06-09) | ?
IS 32 | USB | 0x04a9/0x105d | Unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers. | unsupported (2010-06-09) | ?
IS 52 | USB |  | Unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers. | unsupported (2010-06-09) | ?
IX-4015 | SCSI |  | Good | 1 pass; flatbed scanner | canon (1.12) | sane-canon
laserBase MF5650 | USB | 0x04a9/0x264f | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
P-150 | USB |  | Untested |  | canon_dr (41) | sane-canon_dr
P-150M | USB |  | Untested |  | canon_dr (41) | sane-canon_dr
P-208 | USB | 0x1083/0x164c | Basic | All modes and resolutions working, but calibration is poor. | canon_dr (41) | sane-canon_dr
P-215 | USB | 0x1083/0x1646 | Basic | All modes and resolutions working, but calibration is poor. Card reader slot not working. | canon_dr (41) | sane-canon_dr
PIXMA E500 | USB | 0x04a9/0x1758 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA E510 | USB | 0x04a9/0x1761 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA E600 | USB | 0x04a9/0x175a | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA E610 | USB | 0x04a9/0x1767 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG2100 Series | USB | 0x04a9/0x1751 | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MG2200 Series | USB | 0x04a9/0x1760 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG2400 Series | USB | 0x04a9/0x176c | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG2500 Series | USB | 0x04a9/0x176d | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG3100 Series | USB WLAN | 0x04a9/0x1752 | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MG3200 Series | USB | 0x04a9/0x1762 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG3500 Series | USB | 0x04a9/0x176e | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG4100 Series | USB | 0x04a9/0x1753 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG4200 Series | USB | 0x04a9/0x1763 | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MG5100 Series | USB | 0x04a9/0x1748 | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MG5200 Series | USB | 0x04a9/0x1749 | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MG5300 Series | USB | 0x04a9/0x1754 | Complete | All resolutions supported (up to 2400DPI). | pixma (0.17.4) | sane-pixma
PIXMA MG5400 Series | USB | 0x04a9/0x1764 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG5500 Series | USB | 0x04a9/0x1771 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG6100 Series | USB | 0x04a9/0x174a | Complete | All resolutions supported (up to 2400 DPI) | pixma (0.17.4) | sane-pixma
PIXMA MG6200 Series | USB | 0x04a9/0x1755 | Complete | All resolutions supported (up to 4800 DPI) | pixma (0.17.4) | sane-pixma
PIXMA MG6300 Series | USB Ethernet | 0x04a9/0x1765 | Complete | All resolutions supported (up to 2400DPI). | pixma (0.17.4) | sane-pixma
PIXMA MG6400 Series | USB | 0x04a9/0x1770 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG6500 Series | USB | 0x04a9/0x176f | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG7100 Series | USB | 0x04a9/0x1772 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG8100 Series | USB | 0x04a9/0x174b | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MG8200 Series | USB Ethernet | 0x04a9/0x1756 | Complete | All resolutions supported (up to 4800DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP110 | USB | 0x04a9/0x1700 | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
PIXMA MP130 | USB | 0x04a9/0x1701 | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
PIXMA MP140 | USB | 0x04a9/0x172b | Complete | All resolutions supported (up to 600 DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP150 | USB | 0x04a9/0x1709 | Good |  | pixma (0.17.4) | sane-pixma
PIXMA MP160 | USB | 0x04a9/0x1714 | Basic |  | pixma (0.17.4) | sane-pixma
PIXMA MP170 | USB | 0x04a9/0x170a | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP180 | USB | 0x04a9/0x1715 | Basic |  | pixma (0.17.4) | sane-pixma
PIXMA MP190 | USB | 0x04a9/0x1734 | Complete | All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP210 | USB | 0x04a9/0x1721 | Complete | All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP220 | USB | 0x04a9/0x1722 | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP230 | USB | 0x04a9/0x175f | Complete | All resolutions supported (up to 600DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP240 | USB | 0x04a9/0x1732 | Complete | All resolutions supported (up to 1200DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP250 | USB | 0x04a9/0x173a | Complete | All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP260 | USB | 0x04a9/0x1733 | Complete | All resolutions supported (up to 1200DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP270 | USB | 0x04a9/0x173b | Complete | All resolutions supported (up to 1200DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP280 | USB | 0x04a9/0x1746 | Good | All resolutions supported (up to 600DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP360 | USB | 0x04a9/0x263c | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP370 | USB | 0x04a9/0x263d | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP375R | USB | 0x04a9/0x263f | Untested | Same protocol as Pixma MP360/370/390? Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MP390 | USB | 0x04a9/0x263e | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP450 | USB | 0x04a9/0x170b | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP460 | USB | 0x04a9/0x1716 | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP470 | USB | 0x04a9/0x1723 | Complete | All resolutions supported (up to 2400DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP480 | USB | 0x04a9/0x1731 | Complete | All resolutions supported (up to 2400DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP490 | USB | 0x04a9/0x173c | Complete | All resolutions supported (up to 1200DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP493 | USB | 0x04a9/0x1757 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MP495 | USB | 0x04a9/0x1747 | Untested | Same protocol as Pixma MP280? Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MP500 | USB | 0x04a9/0x170c | Good |  | pixma (0.17.4) | sane-pixma
PIXMA MP510 | USB | 0x04a9/0x1717 | Complete | All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP520 | USB | 0x04a9/0x1724 | Complete | All resolutions supported (up to 2400DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP530 | USB | 0x04a9/0x1712 | Good |  | pixma (0.17.4) | sane-pixma
PIXMA MP540 | USB | 0x04a9/0x1730 | Complete | All resolutions supported (up to 2400DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP550 | USB | 0x04a9/0x173d | Complete | All resolutions supported (up to 2400DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP560 | USB | 0x04a9/0x173e | Complete | All resolutions supported (up to 2400DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP600 | USB | 0x04a9/0x1718 | Complete | All resolutions supported (up to 2400DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP600R | USB Ethernet | 0x04a9/0x1719 | Complete | All resolutions supported (up to 2400DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP610 | USB | 0x04a9/0x1725 | Complete | All resolutions supported (up to 4800DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP620 | USB Ethernet | 0x04a9/0x172f | Complete | All resolutions supported (up to 2400DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP630 | USB | 0x04a9/0x172e | Complete | All resolutions supported (up to 4800DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP640 | USB Ethernet | 0x04a9/0x173f | Complete | All resolutions supported (up to 4800DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP700 | USB | 0x04a9/0x2630 | Complete | All resolutions supported (flatbed color up to 1200DPI, grayscale up to 600DPI). | pixma (0.17.4) | sane-pixma
PIXMA MP710 | USB | 0x04a9/0x264d | Complete | All resolutions supported (up to 1200DPI) | pixma (0.17.4) | sane-pixma
PIXMA MP730 | USB | 0x04a9/0x262f | Good | Flatbed color up to 1200DPI, grayscale up to 600DPI. ADF scan to be confirmed. | pixma (0.17.4) | sane-pixma
PIXMA MP740 | USB | 0x04a9/0x264c | Untested | Same protocol as Pixma MP710? Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MP750 | USB | 0x04a9/0x1706 | Minimal | No grayscale. Canceling scan in ADF mode doesn't eject the paper! | pixma (0.17.4) | sane-pixma
PIXMA MP760 | USB | 0x04a9/0x1708 | Minimal | No grayscale. The scanner sometimes hangs! | pixma (0.17.4) | sane-pixma
PIXMA MP770 | USB | 0x04a9/0x1708 | Minimal | No grayscale. The scanner sometimes hangs! | pixma (0.17.4) | sane-pixma
PIXMA MP780 | USB | 0x04a9/0x1707 | Minimal | No grayscale. The scanner sometimes hangs! | pixma (0.17.4) | sane-pixma
PIXMA MP790 | USB | 0x04a9/0x1707 | Minimal | No grayscale. The scanner sometimes hangs! | pixma (0.17.4) | sane-pixma
PIXMA MP800 | USB | 0x04a9/0x170d | Complete | All resolutions supported up to 2400DPI. Full TPU support up to 2400DPI. | pixma (0.17.4) | sane-pixma
PIXMA MP800R | USB | 0x04a9/0x170e | Complete | All resolutions supported up to 2400DPI. Full TPU support up to 2400DPI. | pixma (0.17.4) | sane-pixma
PIXMA MP810 | USB | 0x04a9/0x171a | Complete | All resolutions supported up to 4800DPI. Full TPU support (negative and slides) up to 4800DPI. | pixma (0.17.4) | sane-pixma
PIXMA MP830 | USB | 0x04a9/0x1713 | Complete | All resolutions supported up to 2400DPI. Flatbed, ADF simplex and Duplex supported. | pixma (0.17.4) | sane-pixma
PIXMA MP960 | USB | 0x04a9/0x171b | Complete | All resolutions supported up to 4800DPI. Full TPU support (negative and slides) up to 4800DPI. | pixma (0.17.4) | sane-pixma
PIXMA MP970 | USB Ethernet | 0x04a9/0x1726 | Complete | All resolutions supported (up to 4800DPI). Full TPU support (negative and slides) at 24 or 48 bits. | pixma (0.17.4) | sane-pixma
PIXMA MP980 | USB Ethernet | 0x04a9/0x172d | Complete | Working fine at all resolutions. | pixma (0.17.4) | sane-pixma
PIXMA MP990 | USB Ethernet | 0x04a9/0x1740 | Complete | Working fine at all resolutions. | pixma (0.17.4) | sane-pixma
PIXMA MX300 | USB | 0x04a9/0x1727 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI) | pixma (0.17.4) | sane-pixma
PIXMA MX310 | USB | 0x04a9/0x1728 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI) | pixma (0.17.4) | sane-pixma
PIXMA MX320 | USB | 0x04a9/0x1736 | Untested | Same protocol as Pixma Generation 3? Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MX330 | USB | 0x04a9/0x1737 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI) | pixma (0.17.4) | sane-pixma
PIXMA MX340 | USB | 0x04a9/0x1741 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI) | pixma (0.17.4) | sane-pixma
PIXMA MX350 | USB Ethernet | 0x04a9/0x1742 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI) | pixma (0.17.4) | sane-pixma
PIXMA MX360 | USB | 0x04a9/0x174d | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI). ADF empty buggy. | pixma (0.17.4) | sane-pixma
PIXMA MX370 Series | USB | 0x04a9/0x1759 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI). | pixma (0.17.4) | sane-pixma
PIXMA MX390 Series | USB | 0x04a9/0x1766 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MX410 | USB Ethernet | 0x04a9/0x174e | Untested | Same protocol as Pixma MX420? Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MX420 | USB Ethernet | 0x04a9/0x174f | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI). ADF empty buggy. | pixma (0.17.4) | sane-pixma
PIXMA MX430 Series | USB Ethernet | 0x04a9/0x175b | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MX450 Series | USB | 0x04a9/0x1768 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MX510 Series | USB Ethernet | 0x04a9/0x175c | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MX520 Series | USB | 0x04a9/0x1769 | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MX700 | USB Ethernet | 0x04a9/0x1729 | Complete | Flatbed and ADF scan. All resolutions supported (up to 2400DPI) | pixma (0.17.4) | sane-pixma
PIXMA MX710 Series | USB Ethernet | 0x04a9/0x175d | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MX720 Series | USB | 0x04a9/0x176a | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MX850 | USB Ethernet | 0x04a9/0x172c | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported. | pixma (0.17.4) | sane-pixma
PIXMA MX860 | USB Ethernet | 0x04a9/0x1735 | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported. | pixma (0.17.4) | sane-pixma
PIXMA MX870 | USB Ethernet | 0x04a9/0x1743 | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported, ADF empty buggy. | pixma (0.17.4) | sane-pixma
PIXMA MX880 Series | USB Ethernet | 0x04a9/0x1750 | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported, ADF empty buggy. | pixma (0.17.4) | sane-pixma
PIXMA MX882 | USB Ethernet | 0x04a9/0x1750 | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported, ADF empty buggy. | pixma (0.17.4) | sane-pixma
PIXMA MX885 | USB Ethernet | 0x04a9/0x1750 | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported, ADF empty buggy. | pixma (0.17.4) | sane-pixma
PIXMA MX890 Series | USB Ethernet | 0x04a9/0x175e | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported, ADF empty buggy. | pixma (0.17.4) | sane-pixma
PIXMA MX920 Series | USB | 0x04a9/0x176b | Untested | Testers needed! | pixma (0.17.4) | sane-pixma
PIXMA MX7600 | USB Ethernet | 0x04a9/0x171c | Complete | Flatbed and ADF scan. All resolutions supported (up to 4800DPI) | pixma (0.17.4) | sane-pixma

### Manufacturer: Chinon

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
DS-3000 | Parport Serial Port |  | Unsupported | Unsupported at the moment, but a backend is in preparation. See link. | unsupported (2010-06-09) | ?

### Manufacturer: Compaq

Link(s): http://www.compaq.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
S4-100 | USB | 0x049f/0x001a | Complete | Identical to UMAX 3400 | plustek (0.52) | sane-plustek
S200 | USB | 0x049f/0x0021 | Unsupported | Not supported. 2400x1200 dpi. One bulk-in, one bulk-out and one interrupt endpoint. Type-number: U0001-HB21, another type nr on the inside: 75100512-00 | unsupported (2010-06-09) | ?

### Manufacturer: Compeye

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Simplex 1236C | Parport USB | 0x05cb/0x1483 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Corex

Link(s): http://www.cardscan.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
600c | USB | 0x08f0/0x0002 | Basic | 4 inch wide 8bit Gray or 24bit Color simplex card/receipt scanner | cardscan (2) | sane-cardscan
800c | USB | 0x08f0/0x0005 | Good | 4 inch wide 8bit Gray or 24bit Color simplex card/receipt scanner | cardscan (2) | sane-cardscan
Cardscan 500 | USB | 0x08f0/0x0001 | Unsupported | Probably not supported. Businesscard reader. | unsupported (2010-06-09) | ?
Cardscan 700 C | USB | 0x08f0/0x0004 | Unsupported | Probably not supported. | unsupported (2010-06-09) | ?

### Manufacturer: Cybercom

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
9352 | Parport (EPP) |  | Good | CIS scanner | mustek_pp (13) | sane-mustek_pp

### Manufacturer: DCT

Link(s): http://www.docucap.com/
Comment: Successor of Syscan in the USA

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
DocketPort 487 | USB | 0x1dcc/0x4810 | Basic | All resolution and mode supported, calibration is available, front- and backside side-by-side, with backside mirrored horizontally. | genesys (1.0-63) | sane-genesys

### Manufacturer: Dell

Link(s): http://www.dell.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
922 | USB | 0x413c/0x5109 | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
1600n | Ethernet USB | 0x413c/0x5250 | Basic | Supports colour and monochrome scans over ethernet (USB not supported) | dell1600n_net | ?
A920 | USB | 0x413c/0x5105 | Good | Relabelled X11xx model | lexmark (1.0-0) | sane-lexmark
A940 | USB | 0x413c/0x5106 | Unsupported | Probably rebadged Lexmark X5150. May work with sane-lexmark? See bug #312130 | unsupported (2010-06-09) | ?
A960 | USB | 0x413c/0x5107 | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
Dell 1235cn | USB | 0x413c/0x5310 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
Dell MFP Laser Printer 1815dn | USB | 0x413c/0x5124 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp

### Manufacturer: Devcom

Link(s): http://www.blackwidow.co.uk/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
9630S | SCSI |  | Untested |  | pie (1.0) | sane-pie
9636PRO | SCSI |  | Good |  | pie (1.0) | sane-pie
9636S | SCSI |  | Untested |  | pie (1.0) | sane-pie

### Manufacturer: Dextra

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
DF-600P | SCSI |  | Good | sub model VM3510 | teco1 (1.0-10) | sane-teco1
DF-1200T+ | SCSI |  | Untested | sub model VM3530+ | teco1 (1.0-10) | sane-teco1
DF-4830T | SCSI |  | Untested | sub model VM4542 | teco1 (1.0-10) | sane-teco1
DF-9624 | SCSI |  | Untested | sub model VM6530+ | teco1 (1.0-10) | sane-teco1

### Manufacturer: Dexxa

Link(s): http://www.dexxa.com

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
4800 | Parport |  | Basic | Requires the program 'as6edriver' to run. | as6e (0.5) | sane-as6e

### Manufacturer: E-Lux

Comment: E-Lux and Enhans seem to have been purchased by dysan, now known as MEMOREX

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
j-6121 | Parport |  | Unsupported | Probably unsupported. Sold 1998. Same as E-Lux j-6121. | unsupported (2010-06-09) | ?

### Manufacturer: EDGE

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
KTX-9600US | SCSI |  | Untested | no feedback | umax (1.0-41) | sane-umax

### Manufacturer: EDT (Electronic Document Technology)

Link(s): http://www.bizcardreader.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
BizCardReader 900C | USB | 0x0a53/0x5001 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Enhans

Comment: E-Lux and Enhans seem to have been purchased by dysan, now known as MEMOREX

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
j-6121 | Parport |  | Unsupported | Probably unsupported. Sold 1998. Same as E-Lux j-6121. | unsupported (2010-06-09) | ?
M-3630 A | Parport |  | Unsupported | Probably unsupported. | unsupported (2010-06-09) | ?

### Manufacturer: Epson

Link(s): http://www.epson.com/, http://www.epson.com

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Actionscanner II | parallel SCSI |  | Good | overseas version of the GT-5000 | epson2 (1.0.124) | sane-epson2
Actionscanner II | SCSI Parport |  | Good | US version of GT-5000 | epson (unmaintained) | sane-epson
AcuLaser CX11 | USB | 0x04b8/0x0815 | Good | overseas version of the LP-A500 | epson2 (1.0.124) | sane-epson2
AcuLaser CX11 | USB | 0x04b8/0x0815 | Good |  | epson (unmaintained) | sane-epson
AcuLaser CX11NF | USB Network | 0x04b8/0x0815 | Good | network interface supported AcuLaser CX11 with network interface and fax | epson2 (1.0.124) | sane-epson2
AcuLaser CX11NF | USB | 0x04b8/0x0815 | Good |  | epson (unmaintained) | sane-epson
AcuLaser CX21 | USB | 0x04b8/0x0835 | Good | network interface probably supported | epson2 (1.0.124) | sane-epson2
Artisan 700 | USB Network | 0x04b8/0x0846 | Good | network interface supported all-in-one overseas version of the EP-801A | epson2 (1.0.124) | sane-epson2
Artisan 710 Series | USB | 0x04b8/0x0852 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Artisan 800 | USB | 0x04b8/0x0844 | Good | network interface probably supported all-in-one overseas version of the EP-901A | epson2 (1.0.124) | sane-epson2
Artisan 810 Series | USB | 0x04b8/0x0853 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
CC-500L | USB | 0x04b8/0x010d | Unsupported | all-in-one | epson2 (1.0.124) | sane-epson2
CC-550L | USB | 0x04b8/0x011a | Unsupported | all-in-one | epson2 (1.0.124) | sane-epson2
CC-570L | USB | 0x04b8/0x0802 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
CC-600PX | USB | 0x04b8/0x0801 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
CC-700 | USB | 0x04b8/0x0108 | Unsupported | all-in-one | epson2 (1.0.124) | sane-epson2
CX-3200 | USB | 0x04b8/0x0802 | Good |  | epson (unmaintained) | sane-epson
CX-3600 | USB | 0x04b8/0x080e | Good |  | epson (unmaintained) | sane-epson
CX-3650 | USB | 0x04b8/0x080e | Good |  | epson (unmaintained) | sane-epson
CX-3700 | USB | 0x04b8/0x0818 | Good |  | epson (unmaintained) | sane-epson
CX-3800 | USB | 0x04b8/0x0818 | Good |  | epson (unmaintained) | sane-epson
CX-4200 | USB | 0x04b8/0x0820 | Good |  | epson (unmaintained) | sane-epson
CX-4600 | USB | 0x04b8/0x080d | Good |  | epson (unmaintained) | sane-epson
CX-4800 | USB | 0x04b8/0x0819 | Good |  | epson (unmaintained) | sane-epson
CX-5000 | USB | 0x04b8/0x082b | Good |  | epson (unmaintained) | sane-epson
CX-5200 | USB | 0x04b8/0x0801 | Good |  | epson (unmaintained) | sane-epson
CX-5400 | USB | 0x04b8/0x0808 | Good |  | epson (unmaintained) | sane-epson
CX-5400 | USB | 0x04b8/0x0801 | Good |  | epson (unmaintained) | sane-epson
CX-6300 | USB | 0x04b8/0x0805 | Good |  | epson (unmaintained) | sane-epson
CX-6400 | USB | 0x04b8/0x0805 | Good |  | epson (unmaintained) | sane-epson
CX-6500 | USB | 0x04b8/0x0813 | Good |  | epson (unmaintained) | sane-epson
CX-6600 | USB | 0x04b8/0x0813 | Good |  | epson (unmaintained) | sane-epson
DX-3800 | USB | 0x04b8/0x0818 | Good |  | epson (unmaintained) | sane-epson
DX-3850 | USB | 0x04b8/0x0818 | Good |  | epson (unmaintained) | sane-epson
DX-4050 | USB | 0x04b8/0x082f | Good |  | epson (unmaintained) | sane-epson
DX-5000 | USB | 0x04b8/0x082b | Good |  | epson (unmaintained) | sane-epson
DX-5050 | USB | 0x04b8/0x082b | Good |  | epson (unmaintained) | sane-epson
DX-6000 | USB | 0x04b8/0x082e | Good |  | epson (unmaintained) | sane-epson
DX-7400 | USB | 0x04b8/0x0838 | Good |  | epson (unmaintained) | sane-epson
EP-702A | USB | 0x04b8/0x0850 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
EP-801A | USB Network | 0x04b8/0x0846 | Good | network interface supported all-in-one | epson2 (1.0.124) | sane-epson2
EP-802A | USB | 0x04b8/0x0852 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
EP-901A | USB | 0x04b8/0x0844 | Good | network interface probably supported all-in-one | epson2 (1.0.124) | sane-epson2
EP-901F | USB | 0x04b8/0x0844 | Good | network interface probably supported all-in-one | epson2 (1.0.124) | sane-epson2
EP-902A | USB | 0x04b8/0x0853 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
ES-300C | SCSI parallel |  | Good | overseas version of the GT-6000 | epson2 (1.0.124) | sane-epson2
ES-300C | SCSI Parport |  | Good | US version of GT-6000 | epson (unmaintained) | sane-epson
ES-300GS | SCSI |  | Good |  | epson2 (1.0.124) | sane-epson2
ES-300GS | SCSI |  | Good |  | epson (unmaintained) | sane-epson
ES-600C | parallel |  | Good | overseas version of the GT-5400 | epson2 (1.0.124) | sane-epson2
ES-600C | Parport |  | Good | US version of GT-6500 | epson (unmaintained) | sane-epson
ES-800C | SCSI |  | Good | overseas version of the GT-8000 | epson2 (1.0.124) | sane-epson2
ES-1000C | ? |  | Unsupported | overseas version of the GT-8500 | epson2 (1.0.124) | sane-epson2
ES-1200C | parallel |  | Good | overseas version of the GT-9000 | epson2 (1.0.124) | sane-epson2
ES-1200C | Parport |  | Good | US version of GT-9000 | epson (unmaintained) | sane-epson
ES-2000 | SCSI USB | 0x04b8/0x0107 | Complete | IEEE1394 untested | epson2 (1.0.124) | sane-epson2
ES-2200 | SCSI USB | 0x04b8/0x010e | Complete | IEEE1394 untested | epson2 (1.0.124) | sane-epson2
ES-6000 | SCSI |  | Good |  | epson2 (1.0.124) | sane-epson2
ES-6000H | SCSI |  | Good | IEEE1394 untested | epson2 (1.0.124) | sane-epson2
ES-6000HS | SCSI |  | Good | IEEE1394 untested | epson2 (1.0.124) | sane-epson2
ES-7000H | SCSI USB | 0x04b8/0x0126 | Good | network interface unsupported IEEE1394 untested | epson2 (1.0.124) | sane-epson2
ES-8000 | SCSI |  | Untested |  | epson2 (1.0.124) | sane-epson2
ES-8500 | SCSI USB | 0x04b8/0x0109 | Good | IEEE1394 untested | epson2 (1.0.124) | sane-epson2
ES-8500 | SCSI |  | Good |  | epson (unmaintained) | sane-epson
ES-9000H | SCSI |  | Good | IEEE1394 untested | epson2 (1.0.124) | sane-epson2
ES-10000G | USB | 0x04b8/0x0129 | Good | network interface unsupported IEEE1394 untested | epson2 (1.0.124) | sane-epson2
ES-D400 | USB | 0x04b8/0x0136 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
ES-H300 | USB | 0x04b8/0x012b | Good | network interface probably supported | epson2 (1.0.124) | sane-epson2
ES-H7200 | USB Ethernet | 0x04b8/0x0138 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Expression 636 | SCSI |  | Complete | overseas version of the GT-9500 | epson2 (1.0.124) | sane-epson2
Expression 636 | SCSI |  | Complete | US version of GT-9500 | epson (unmaintained) | sane-epson
Expression 800 | SCSI |  | Complete | overseas version of the GT-9600 | epson2 (1.0.124) | sane-epson2
Expression 800 | SCSI |  | Complete |  | epson (unmaintained) | sane-epson
Expression 836XL | SCSI |  | Untested | overseas version of the ES-8000 | epson2 (1.0.124) | sane-epson2
Expression 1600 | SCSI USB | 0x04b8/0x0107 | Complete | IEEE1394 untested overseas version of the ES-2000 | epson2 (1.0.124) | sane-epson2
Expression 1600 | SCSI USB IEEE-1394 | 0x04b8/0x0107 | Complete |  | epson (unmaintained) | sane-epson
Expression 1640XL | SCSI USB | 0x04b8/0x0109 | Good | IEEE1394 untested overseas version of the ES-8500 | epson2 (1.0.124) | sane-epson2
Expression 1680 | SCSI USB | 0x04b8/0x010e | Complete | IEEE1394 untested overseas version of the ES-2200 | epson2 (1.0.124) | sane-epson2
Expression 1680 | SCSI USB IEEE-1394 | 0x04b8/0x010e | Complete |  | epson (unmaintained) | sane-epson
Expression 1680 Pro | SCSI USB |  | Untested | IEEE1394 option | epson2 (1.0.124) | sane-epson2
Expression 1680XL Pro | SCSI USB |  | Untested |  | epson2 (1.0.124) | sane-epson2
Expression 10000XL | USB | 0x04b8/0x0129 | Good | network interface probably supported IEEE1394 untested overseas version of the ES-10000G | epson2 (1.0.124) | sane-epson2
Expression 10000XL Graphic Arts | USB IEEE1394 |  | Untested | network interface probably supported | epson2 (1.0.124) | sane-epson2
Expression 10000XL Photo | USB IEEE1394 |  | Untested | network interface probably supported | epson2 (1.0.124) | sane-epson2
F-3200 | USB IEEE1394 | 0x04b8/0x080a | Unsupported | Film scanner | epson2 (1.0.124) | sane-epson2
F-3200 Photo | USB IEEE1394 |  | Unsupported |  | epson2 (1.0.124) | sane-epson2
FilmScan 200 | SCSI |  | Minimal | will be supported | epson2 (1.0.124) | sane-epson2
GT-1500 | USB | 0x04b8/0x0133 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-2200 | USB | 0x04b8/0x0102 | Unsupported | Probably unsupported. No details known. | unsupported (2010-06-09) | ?
GT-2200 | USB | 0x04b8/0x0102 | Unsupported |  | epson2 (1.0.124) | sane-epson2
GT-2500 | USB | 0x04b8/0x012b | Good | network interface probably supported overseas version of the ES-H300 | epson2 (1.0.124) | sane-epson2
GT-4000 | ? |  | Untested |  | epson2 (1.0.124) | sane-epson2
GT-5000 | parallel SCSI |  | Good |  | epson2 (1.0.124) | sane-epson2
GT-5000 | SCSI Parport |  | Good |  | epson (unmaintained) | sane-epson
GT-5400 | parallel |  | Good |  | epson2 (1.0.124) | sane-epson2
GT-5500 | SCSI |  | Good |  | epson2 (1.0.124) | sane-epson2
GT-5500 | SCSI |  | Good |  | epson (unmaintained) | sane-epson
GT-6000 | SCSI Parport |  | Good |  | epson2 (1.0.124) | sane-epson2
GT-6000 | SCSI Parport |  | Good |  | epson (unmaintained) | sane-epson
GT-6500 | parallel |  | Good | overseas version of the GT-5400 | epson2 (1.0.124) | sane-epson2
GT-6500 | Parport |  | Good |  | epson (unmaintained) | sane-epson
GT-6600U | USB | 0x04b8/0x0103 | Complete |  | epson2 (1.0.124) | sane-epson2
GT-6700U | USB | 0x04b8/0x010c | Complete |  | epson2 (1.0.124) | sane-epson2
GT-7000 | SCSI |  | Good |  | epson (unmaintained) | sane-epson
GT-7000S | SCSI |  | Complete |  | epson2 (1.0.124) | sane-epson2
GT-7000U | USB | 0x04b8/0x0101 | Complete |  | epson2 (1.0.124) | sane-epson2
GT-7200U | USB | 0x04b8/0x010f | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-7300U | USB | 0x04b8/0x011d | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-7400U | USB | 0x04b8/0x0120 | Unsupported | supported by the snapscan backend | epson2 (1.0.124) | sane-epson2
GT-7600S | SCSI |  | Complete | SCSI version of the GT-7600U | epson2 (1.0.124) | sane-epson2
GT-7600U | USB | 0x04b8/0x0104 | Complete | USB version of the GT-7600S | epson2 (1.0.124) | sane-epson2
GT-7600UF | USB | 0x04b8/0x0104 | Complete | GT-7600U with TPU option bundled | epson2 (1.0.124) | sane-epson2
GT-7700U | USB | 0x04b8/0x010b | Complete |  | epson2 (1.0.124) | sane-epson2
GT-8000 | SCSI |  | Good |  | epson2 (1.0.124) | sane-epson2
GT-8000 | SCSI |  | Good |  | epson (unmaintained) | sane-epson
GT-8200U | USB | 0x04b8/0x0110 | Complete |  | epson2 (1.0.124) | sane-epson2
GT-8200UF | USB | 0x04b8/0x0110 | Good |  | epson2 (1.0.124) | sane-epson2
GT-8300UF | USB | 0x04b8/0x011e | Complete |  | epson2 (1.0.124) | sane-epson2
GT-8400UF | USB | 0x04b8/0x011f | Unsupported |  | epson2 (1.0.124) | sane-epson2
GT-8500 | ? |  | Untested |  | epson2 (1.0.124) | sane-epson2
GT-8700 | SCSI USB | 0x04b8/0x010a | Complete |  | epson2 (1.0.124) | sane-epson2
GT-8700F | SCSI USB | 0x04b8/0x010a | Good | GT-8700U with TPU option bundled | epson2 (1.0.124) | sane-epson2
GT-9000 | parallel |  | Good |  | epson2 (1.0.124) | sane-epson2
GT-9300UF | USB | 0x04b8/0x011b | Complete |  | epson2 (1.0.124) | sane-epson2
GT-9400UF | USB | 0x04b8/0x0116 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-9500 | SCSI |  | Complete |  | epson2 (1.0.124) | sane-epson2
GT-9600 | SCSI |  | Complete |  | epson2 (1.0.124) | sane-epson2
GT-9700F | USB | 0x04b8/0x0112 | Complete | IEEE1394 untested | epson2 (1.0.124) | sane-epson2
GT-9800F | USB | 0x04b8/0x011c | Complete | IEEE1394 untested | epson2 (1.0.124) | sane-epson2
GT-10000 | SCSI |  | Good | overseas version of the ES-6000 | epson2 (1.0.124) | sane-epson2
GT-10000+ | SCSI |  | Good | IEEE1394 untested overseas version of the ES-6000H | epson2 (1.0.124) | sane-epson2
GT-12000 | SCSI |  | Untested | overseas version of the ES-8000 | epson2 (1.0.124) | sane-epson2
GT-15000 | SCSI USB | 0x04b8/0x0126 | Good | IEEE1394 untested overseas version of the ES-7000H | epson2 (1.0.124) | sane-epson2
GT-20000 | USB Ethernet | 0x04b8/0x0138 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-30000 | SCSI |  | Good | IEEE1394 untested overseas version of the ES-9000H | epson2 (1.0.124) | sane-epson2
GT-D1000 | USB | 0x04b8/0x0133 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-F500 | USB | 0x04b8/0x0121 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-F520 | USB | 0x04b8/0x0122 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-F550 | USB | 0x04b8/0x0121 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-F570 | USB | 0x04b8/0x0122 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-F600 | USB | 0x04b8/0x0118 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-F650 | USB | 0x04b8/0x012d | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-F670 | USB | 0x04b8/0x012e | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-F700 | USB | 0x04b8/0x012f | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-F720 | USB | 0x04b8/0x0131 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-S50 | USB | 0x04b8/0x0137 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-S80 | USB | 0x04b8/0x0136 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-S600 | USB | 0x04b8/0x012d | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-S620 | USB | 0x04b8/0x0131 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-X700 | USB | 0x04b8/0x0128 | Complete | IEEE1394 untested | epson2 (1.0.124) | sane-epson2
GT-X750 | USB | 0x04b8/0x0119 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-X770 | USB | 0x04b8/0x0130 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-X800 | USB | 0x04b8/0x012a | Complete | film area guide mode not supported IEEE1394 untested | epson2 (1.0.124) | sane-epson2
GT-X820 | USB | 0x04b8/0x013a | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
GT-X900 | USB | 0x04b8/0x012c | Good | IEEE1394 untested | epson2 (1.0.124) | sane-epson2
GT-X970 | USB | 0x04b8/0x0135 | Good | IEEE1394 untested | epson2 (1.0.124) | sane-epson2
LP-7900CS | ? |  | Untested | business all-in-one; scanner is a ES-7000H | epson2 (1.0.124) | sane-epson2
LP-9000CCH | ? |  | Untested | business all-in-one; scanner is a ES-9000H | epson2 (1.0.124) | sane-epson2
LP-9000CCS | ? |  | Untested | business all-in-one; scanner is a ES-7000H | epson2 (1.0.124) | sane-epson2
LP-9000CFH | ? |  | Untested | business all-in-one; scanner is a ES-9000H | epson2 (1.0.124) | sane-epson2
LP-9500CCS | ? |  | Untested | business all-in-one; scanner is a ES-7000H | epson2 (1.0.124) | sane-epson2
LP-9500CFH | ? |  | Untested | business all-in-one; scanner is a ES-9000H | epson2 (1.0.124) | sane-epson2
LP-9500CH2 | ? |  | Untested | business all-in-one; scanner is a ES-9000H | epson2 (1.0.124) | sane-epson2
LP-9800CCH | ? |  | Untested | business all-in-one; scanner is a ES-9000H | epson2 (1.0.124) | sane-epson2
LP-9800CCS | ? |  | Untested | business all-in-one; scanner is a ES-7000H | epson2 (1.0.124) | sane-epson2
LP-9800CFH | ? |  | Untested | business all-in-one; scanner is a ES-9000H | epson2 (1.0.124) | sane-epson2
LP-A500 | USB Network | 0x04b8/0x0815 | Good | network interface supported business all-in-one | epson2 (1.0.124) | sane-epson2
LP-M5000 | USB | 0x04b8/0x0843 | Good | network interface probably supported business all-in-one | epson2 (1.0.124) | sane-epson2
LP-M5500 | USB | 0x04b8/0x0817 | Good | network interface probably supported business all-in-one | epson2 (1.0.124) | sane-epson2
LP-M5500F | USB | 0x04b8/0x0817 | Good | network interface probably supported business all-in-one LP-M5500 with the fax option bundled | epson2 (1.0.124) | sane-epson2
LP-M5600 | USB | 0x04b8/0x0833 | Good | network interface probably supported business all-in-one | epson2 (1.0.124) | sane-epson2
LP-M6000 | USB | 0x04b8/0x0834 | Good | network interface probably supported business all-in-one | epson2 (1.0.124) | sane-epson2
ME 200 | USB | 0x04b8/0x0830 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
ME 300 | USB | 0x04b8/0x0841 | Good | all-in-one overseas version of the PX-401A | epson2 (1.0.124) | sane-epson2
ME OFFICE 510 | USB | 0x04b8/0x084f | Good | all-in-one | epson2 (1.0.124) | sane-epson2
ME Office 600F | USB | 0x04b8/0x0848 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
ME OFFICE 650FN Series | USB | 0x04b8/0x0854 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
ME Office 700FW | USB | 0x04b8/0x0847 | Good | network interface probably supported all-in-one overseas version of the PX-601F | epson2 (1.0.124) | sane-epson2
Perfection 600 | SCSI |  | Good | OK, SCSI-ID=EPSON Perfection600 | umax (1.0-41) | sane-umax
Perfection 610 | USB | 0x04b8/0x0103 | Complete | overseas version of the GT-6600U | epson2 (1.0.124) | sane-epson2
Perfection 610 | USB | 0x04b8/0x0103 | Complete |  | epson (unmaintained) | sane-epson
Perfection 636 | SCSI |  | Complete |  | epson (unmaintained) | sane-epson
Perfection 636S | SCSI |  | Complete | overseas version of the GT-7000S | epson2 (1.0.124) | sane-epson2
Perfection 636S | SCSI |  | Complete | US version of GT-7000 | epson (unmaintained) | sane-epson
Perfection 636U | USB | 0x04b8/0x0101 | Complete | overseas version of the GT-7000U | epson2 (1.0.124) | sane-epson2
Perfection 636U | USB | 0x04b8/0x0101 | Complete |  | epson (unmaintained) | sane-epson
Perfection 640 | USB | 0x04b8/0x010c | Complete |  | epson (unmaintained) | sane-epson
Perfection 640U | USB | 0x04b8/0x010c | Complete | overseas version of the GT-6700U | epson2 (1.0.124) | sane-epson2
Perfection 660 | USB | 0x04b8/0x0114 | Good |  | SnapScan (1.4) | sane-snapscan
Perfection 1200Photo | USB | 0x04b8/0x0104 | Complete | with TPU | epson (unmaintained) | sane-epson
Perfection 1200S | SCSI |  | Complete | overseas version of the GT-7600S | epson2 (1.0.124) | sane-epson2
Perfection 1200S | SCSI |  | Complete |  | epson (unmaintained) | sane-epson
Perfection 1200U | USB | 0x04b8/0x0104 | Complete | overseas version of the GT-7600U | epson2 (1.0.124) | sane-epson2
Perfection 1200U | USB | 0x04b8/0x0104 | Complete |  | epson (unmaintained) | sane-epson
Perfection 1200U PHOTO | USB | 0x04b8/0x0104 | Complete | Perfection 1200U with TPU option bundled overseas version of the GT-7600UF | epson2 (1.0.124) | sane-epson2
Perfection 1240 | SCSI USB | 0x04b8/0x010b | Complete |  | epson (unmaintained) | sane-epson
Perfection 1240U | USB | 0x04b8/0x010b | Complete | overseas version of the GT-7700U | epson2 (1.0.124) | sane-epson2
Perfection 1250 | USB | 0x04b8/0x010f | Complete |  | plustek (0.52) | sane-plustek
Perfection 1250 PHOTO | USB | 0x04b8/0x010f | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection 1250Photo | USB | 0x04b8/0x010f | Good | TPA scans not perfect | plustek (0.52) | sane-plustek
Perfection 1260 | USB | 0x04b8/0x011d | Complete |  | plustek (0.52) | sane-plustek
Perfection 1260 PHOTO | USB | 0x04b8/0x011d | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection 1260Photo | USB | 0x04b8/0x011d | Good | TPA scans not perfect | plustek (0.52) | sane-plustek
Perfection 1270 | USB | 0x04b8/0x0120 | Good |  | SnapScan (1.4) | sane-snapscan
Perfection 1600 | SCSI |  | Unsupported |  | epson2 (1.0.124) | sane-epson2
Perfection 1640 | SCSI USB | 0x04b8/0x010a | Complete |  | epson (unmaintained) | sane-epson
Perfection 1640SU | SCSI USB | 0x04b8/0x010a | Complete | overseas version of the GT-8700 | epson2 (1.0.124) | sane-epson2
Perfection 1640SU PHOTO | SCSI USB | 0x04b8/0x010a | Good | overseas version of the GT-8700F | epson2 (1.0.124) | sane-epson2
Perfection 1650 | USB | 0x04b8/0x0110 | Complete | overseas version of the GT-8200U | epson2 (1.0.124) | sane-epson2
Perfection 1650 | USB | 0x04b8/0x0110 | Complete |  | epson (unmaintained) | sane-epson
Perfection 1650 PHOTO | USB | 0x04b8/0x0110 | Good | overseas version of the GT-8200UF | epson2 (1.0.124) | sane-epson2
Perfection 1660 | USB | 0x04b8/0x011e | Complete |  | epson (unmaintained) | sane-epson
Perfection 1660 PHOTO | USB | 0x04b8/0x011e | Complete | overseas version of the GT-8300UF | epson2 (1.0.124) | sane-epson2
Perfection 1670 | USB | 0x04b8/0x011f | Good |  | SnapScan (1.4) | sane-snapscan
Perfection 1670 PHOTO | USB | 0x04b8/0x011f | Unsupported | supported by the snapscan backend overseas version of the GT-8400UF | epson2 (1.0.124) | sane-epson2
Perfection 2400 | USB | 0x04b8/0x011b | Complete |  | epson (unmaintained) | sane-epson
Perfection 2400 PHOTO | USB | 0x04b8/0x011b | Complete | overseas version of the GT-9300UF | epson2 (1.0.124) | sane-epson2
Perfection 2450 | USB IEEE-1394 | 0x04b8/0x0112 | Complete |  | epson (unmaintained) | sane-epson
Perfection 2450 PHOTO | USB IEEE-1394 | 0x04b8/0x0112 | Complete | overseas version of the GT-9700F | epson2 (1.0.124) | sane-epson2
Perfection 2480 | USB | 0x04b8/0x0121 | Good |  | SnapScan (1.4) | sane-snapscan
Perfection 2480 PHOTO | USB | 0x04b8/0x0121 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection 2580 | USB | 0x04b8/0x0121 | Basic | Film scanning unit unsupported | SnapScan (1.4) | sane-snapscan
Perfection 2580 PHOTO | USB | 0x04b8/0x0121 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection 3170 PHOTO | USB | 0x04b8/0x0116 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection 3200 | USB IEEE-1394 | 0x04b8/0x011c | Complete | US version of the GT-9800 | epson (unmaintained) | sane-epson
Perfection 3200 PHOTO | USB IEEE-1394 | 0x04b8/0x011c | Complete | overseas version of the GT-9800F | epson2 (1.0.124) | sane-epson2
Perfection 3490 | USB | 0x04b8/0x0122 | Good |  | SnapScan (1.4) | sane-snapscan
Perfection 3490 PHOTO | USB | 0x04b8/0x0122 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection 3590 | USB | 0x04b8/0x0122 | Basic | Film scanning unit unsupported | SnapScan (1.4) | sane-snapscan
Perfection 3590 PHOTO | USB | 0x04b8/0x0122 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection 4180 PHOTO | USB | 0x04b8/0x0118 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection 4490 PHOTO | USB | 0x04b8/0x0119 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection 4870 | USB | 0x04b8/0x0128 | Complete | US version of the GT-X700 | epson (unmaintained) | sane-epson
Perfection 4870 PHOTO | USB | 0x04b8/0x0128 | Complete | IEEE1394 untested overseas version of the GT-X700 | epson2 (1.0.124) | sane-epson2
Perfection 4990 | USB | 0x04b8/0x012a | Complete | US version of the GT-X800 | epson (unmaintained) | sane-epson
Perfection 4990 PHOTO | USB | 0x04b8/0x012a | Good | film area guide mode not supported IEEE1394 untested overseas version of the GT-X800 | epson2 (1.0.124) | sane-epson2
Perfection 4990 Pro | USB IEEE1394 |  | Untested | seems to be a 4990 PHOTO with additional software | epson2 (1.0.124) | sane-epson2
Perfection V10 | USB | 0x04b8/0x012d | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection V30 | USB | 0x04b8/0x0131 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection V100 Photo | USB | 0x04b8/0x012d | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection V200 Photo | USB | 0x04b8/0x012e | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection V300 Photo | USB | 0x04b8/0x0131 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection V350 Photo | USB | 0x04b8/0x012f | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection V500 Photo | USB | 0x04b8/0x0130 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection V600 Photo | USB | 0x04b8/0x013a | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Perfection V700 Photo | USB | 0x04b8/0x012c | Good | IEEE1394 untested overseas version of the GT-X900 | epson2 (1.0.124) | sane-epson2
Perfection V750 Photo | USB | 0x04b8/0x012c | Good | IEEE1394 untested overseas version of the GT-X900 | epson2 (1.0.124) | sane-epson2
PM-A700 | USB | 0x04b8/0x0814 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-A750 | USB | 0x04b8/0x081a | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-A820 | USB | 0x04b8/0x0827 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-A840 | USB | 0x04b8/0x083c | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-A840S | USB | 0x04b8/0x083c | Good | network interface probably supported all-in-one | epson2 (1.0.124) | sane-epson2
PM-A850 | USB | 0x04b8/0x0806 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-A870 | USB | 0x04b8/0x0811 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-A890 | USB | 0x04b8/0x081c | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-A900 | USB | 0x04b8/0x0810 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-A920 | USB | 0x04b8/0x082a | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-A940 | USB | 0x04b8/0x0837 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-A950 | USB | 0x04b8/0x081d | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-A970 | USB | 0x04b8/0x0828 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-T960 | USB | 0x04b8/0x0836 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PM-T990 | USB | 0x04b8/0x0829 | Good | all-in-one PM-A970 with network interface | epson2 (1.0.124) | sane-epson2
PX-401A | USB | 0x04b8/0x0841 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PX-402A | USB | 0x04b8/0x084d | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PX-501A | USB | 0x04b8/0x084a | Good | network interface probably supported all-in-one | epson2 (1.0.124) | sane-epson2
PX-502A | USB | 0x04b8/0x0856 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PX-601F | USB | 0x04b8/0x0847 | Good | network interface probably supported | epson2 (1.0.124) | sane-epson2
PX-A550 | USB | 0x04b8/0x080e | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PX-A620 | USB | 0x04b8/0x082f | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PX-A640 | USB | 0x04b8/0x0838 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PX-A650 | USB | 0x04b8/0x0819 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PX-A720 | USB | 0x04b8/0x082e | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PX-A740 | USB | 0x04b8/0x0839 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
PX-FA700 | USB | 0x04b8/0x083a | Good | all-in-one | epson2 (1.0.124) | sane-epson2
RX-425 | USB | 0x04b8/0x080f | Good |  | epson (unmaintained) | sane-epson
RX-500 | USB | 0x04b8/0x0807 | Good |  | epson (unmaintained) | sane-epson
RX-600 | USB | 0x04b8/0x0806 | Good |  | epson (unmaintained) | sane-epson
RX-620 | USB | 0x04b8/0x0811 | Good |  | epson (unmaintained) | sane-epson
RX-700 | USB | 0x04b8/0x0810 | Good |  | epson (unmaintained) | sane-epson
Stylus CX-1500 | USB | 0x04b8/0x080c | Good |  | SnapScan (1.4) | sane-snapscan
Stylus CX-5800 | USB |  | Unsupported | Probably unsupported at the moment. Not compatible to snapscan backend. It's not known if it may work with epson or epkowa backend. | unsupported (2010-06-09) | ?
Stylus CX1500 | USB | 0x04b8/0x080c | Unsupported | supported by the snapscan backend all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX2800 | USB | 0x04b8/0x0830 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX2900 | USB | 0x04b8/0x0830 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX3100 | USB | 0x04b8/0x0802 | Good | all-in-one overseas version of the CC-570L | epson2 (1.0.124) | sane-epson2
Stylus CX3200 | USB | 0x04b8/0x0802 | Good | all-in-one overseas version of the CC-570L | epson2 (1.0.124) | sane-epson2
Stylus CX3500 | USB | 0x04b8/0x080e | Good | all-in-one overseas version of the PX-A550 | epson2 (1.0.124) | sane-epson2
Stylus CX3600 | USB | 0x04b8/0x080e | Good | all-in-one overseas version of the PX-A550 | epson2 (1.0.124) | sane-epson2
Stylus CX3650 | USB | 0x04b8/0x080e | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX3700 | USB | 0x04b8/0x0818 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX3800 | USB | 0x04b8/0x0818 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX3810 | USB |  | Untested | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX3900 | USB | 0x04b8/0x082f | Good | all-in-one overseas version of the PX-A620 | epson2 (1.0.124) | sane-epson2
Stylus CX4100 | USB | 0x04b8/0x0820 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX4200 | USB | 0x04b8/0x0820 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX4300 | USB | 0x04b8/0x083f | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus CX4400 | USB | 0x04b8/0x083f | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus CX4500 | USB | 0x04b8/0x080d | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX4600 | USB | 0x04b8/0x080d | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX4700 | USB | 0x04b8/0x0819 | Good | all-in-one overseas version of the PX-A650 | epson2 (1.0.124) | sane-epson2
Stylus CX4800 | USB | 0x04b8/0x0819 | Good | all-in-one overseas version of the PX-A650 | epson2 (1.0.124) | sane-epson2
Stylus CX4900 | USB | 0x04b8/0x082b | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX5000 | USB | 0x04b8/0x082b | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX5100 | USB | 0x04b8/0x0801 | Good | all-in-one overseas version of the CC-600PX | epson2 (1.0.124) | sane-epson2
Stylus CX5200 | USB | 0x04b8/0x0801 | Good | all-in-one overseas version of the CC-600PX | epson2 (1.0.124) | sane-epson2
Stylus CX5300 | USB | 0x04b8/0x0808 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX5400 | USB | 0x04b8/0x0808 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX5500 | USB | 0x04b8/0x083f | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus CX5600 | USB | 0x04b8/0x083f | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus CX5700F | USB | 0x04b8/0x0821 | Unsupported | may work with the snapscan backend all-in-one with FAX | epson2 (1.0.124) | sane-epson2
Stylus CX5800F | USB | 0x04b8/0x0821 | Unsupported | may work with the snapscan backend all-in-one with FAX | epson2 (1.0.124) | sane-epson2
Stylus CX5900 | USB | 0x04b8/0x082e | Good | all-in-one overseas version of the PX-A720 | epson2 (1.0.124) | sane-epson2
Stylus CX6000 | USB | 0x04b8/0x082e | Good | all-in-one overseas version of the PX-A720 | epson2 (1.0.124) | sane-epson2
Stylus CX6300 | USB | 0x04b8/0x0805 | Good | all-in-one mistakenly thinks its a PX-A650 | epson2 (1.0.124) | sane-epson2
Stylus CX6400 | USB | 0x04b8/0x0805 | Good | all-in-one mistakenly thinks its a PX-A650 | epson2 (1.0.124) | sane-epson2
Stylus CX6500 | USB | 0x04b8/0x0813 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX6600 | USB | 0x04b8/0x0813 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX6900F | USB | 0x04b8/0x0831 | Unsupported | may work with the snapscan backend all-in-one with FAX | epson2 (1.0.124) | sane-epson2
Stylus CX7000F | USB | 0x04b8/0x0831 | Unsupported | may work with the snapscan backend all-in-one with FAX | epson2 (1.0.124) | sane-epson2
Stylus CX7300 | USB | 0x04b8/0x0838 | Good | all-in-one overseas version of the PX-A640 | epson2 (1.0.124) | sane-epson2
Stylus CX7400 | USB | 0x04b8/0x0838 | Good | all-in-one overseas version of the PX-A640 | epson2 (1.0.124) | sane-epson2
Stylus CX7700 | USB | 0x04b8/0x081f | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX7800 | USB | 0x04b8/0x081f | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus CX8300 | USB | 0x04b8/0x0839 | Good | all-in-one overseas version of the PX-A740 | epson2 (1.0.124) | sane-epson2
Stylus CX8400 | USB | 0x04b8/0x0839 | Good | all-in-one overseas version of the PX-A740 | epson2 (1.0.124) | sane-epson2
Stylus CX9300F | USB | 0x04b8/0x083a | Good | all-in-one overseas version of the PX-FA700 | epson2 (1.0.124) | sane-epson2
Stylus CX9400Fax | USB | 0x04b8/0x083a | Good | all-in-one overseas version of the PX-FA700 | epson2 (1.0.124) | sane-epson2
Stylus DX3800 | USB | 0x04b8/0x0818 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus DX3850 | USB |  | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus DX4000 | USB | 0x04b8/0x082f | Good | all-in-one overseas version of the PX-A620 | epson2 (1.0.124) | sane-epson2
Stylus DX4200 | USB | 0x04b8/0x0820 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus DX4400 | USB | 0x04b8/0x083f | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus DX4450 | USB | 0x04b8/0x083f | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
Stylus DX4800 | USB | 0x04b8/0x0819 | Good | all-in-one overseas version of the PX-A650 | epson2 (1.0.124) | sane-epson2
Stylus DX4850 | USB | 0x04b8/0x0819 | Good | all-in-one DX4800 + card reader | epson2 (1.0.124) | sane-epson2
Stylus DX5000 | USB | 0x04b8/0x082b | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus DX6000 | USB | 0x04b8/0x082e | Good | all-in-one overseas version of the PX-A720 | epson2 (1.0.124) | sane-epson2
Stylus DX7000F | USB | 0x04b8/0x0831 | Unsupported | may work with the snapscan backend all-in-one with FAX | epson2 (1.0.124) | sane-epson2
Stylus DX7400 | USB | 0x04b8/0x0838 | Good | all-in-one overseas version of the PX-A640 | epson2 (1.0.124) | sane-epson2
Stylus DX8400 | USB | 0x04b8/0x0839 | Good | all-in-one overseas version of the PX-A740 | epson2 (1.0.124) | sane-epson2
Stylus DX9400F | USB | 0x04b8/0x083a | Good | all-in-one overseas version of the PX-FA700 | epson2 (1.0.124) | sane-epson2
Stylus NX100 | USB | 0x04b8/0x0841 | Good | all-in-one overseas version of the PX-401A | epson2 (1.0.124) | sane-epson2
Stylus NX110 Series | USB | 0x04b8/0x084d | Good | all-in-one overseas version of the PX-402A | epson2 (1.0.124) | sane-epson2
Stylus NX200 | USB | 0x04b8/0x0849 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus NX210 Series | USB | 0x04b8/0x084f | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus NX300 | USB | 0x04b8/0x0848 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus NX400 | USB | 0x04b8/0x084a | Good | network interface probably supported all-in-one overseas version of the PX-501A | epson2 (1.0.124) | sane-epson2
Stylus NX410 Series | USB | 0x04b8/0x0851 | Good | network interface probably supported all-in-one | epson2 (1.0.124) | sane-epson2
Stylus NX510 Series | USB | 0x04b8/0x0856 | Good | all-in-one overseas version of the PX-502A | epson2 (1.0.124) | sane-epson2
Stylus Office BX300F | USB | 0x04b8/0x0848 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus Office BX310FN Series | USB | 0x04b8/0x0854 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus Office BX600FW | USB | 0x04b8/0x0847 | Good | network interface probably supported all-in-one overseas version of the PX-601F | epson2 (1.0.124) | sane-epson2
Stylus Office BX610FW Series | USB | 0x04b8/0x0855 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus Office TX300F | USB | 0x04b8/0x0848 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus Office TX510FN Series | USB | 0x04b8/0x0854 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus Office TX600FW | USB | 0x04b8/0x0847 | Good | network interface probably supported all-in-one overseas version of the PX-601F | epson2 (1.0.124) | sane-epson2
Stylus Office TX610FW Series | USB | 0x04b8/0x0855 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus Photo PX650 Series | USB | 0x04b8/0x0850 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus Photo PX700W | USB Network | 0x04b8/0x0846 | Good | network interface supported all-in-one overseas version of the EP-801A | epson2 (1.0.124) | sane-epson2
Stylus Photo PX710W Series | USB | 0x04b8/0x0852 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus Photo PX800FW | USB | 0x04b8/0x0844 | Good | network interface probably supported all-in-one overseas version of the EP-901A | epson2 (1.0.124) | sane-epson2
Stylus Photo PX810FW Series | USB | 0x04b8/0x0853 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus Photo RX420 | USB | 0x04b8/0x080f | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus Photo RX425 | USB | 0x04b8/0x080f | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus Photo RX430 | USB | 0x04b8/0x080f | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus Photo RX500 | USB | 0x04b8/0x0807 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus Photo RX510 | USB | 0x04b8/0x0807 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus Photo RX520 | USB | 0x04b8/0x081a | Good | all-in-one overseas version of the PM-A750 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX530 | USB | 0x04b8/0x081a | Good | all-in-one overseas version of the PM-A750 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX560 | USB | 0x04b8/0x0827 | Good | all-in-one overseas version of the PM-A820 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX580 | USB | 0x04b8/0x0827 | Good | all-in-one overseas version of the PM-A820 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX585 | USB | 0x04b8/0x083c | Good | all-in-one overseas version of the PM-A840 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX590 | USB | 0x04b8/0x0827 | Good | all-in-one overseas version of the PM-A820 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX595 | USB | 0x04b8/0x083c | Good | all-in-one overseas version of the PM-A840 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX600 | USB | 0x04b8/0x0806 | Good | all-in-one overseas version of the PM-A850 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX610 | USB | 0x04b8/0x083c | Good | all-in-one overseas version of the PM-A840 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX620 | USB | 0x04b8/0x0811 | Good | all-in-one overseas version of the PM-A870 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX630 | USB | 0x04b8/0x0811 | Good | all-in-one overseas version of the PM-A870 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX640 | USB | 0x04b8/0x081c | Good | all-in-one overseas version of the PM-A890 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX650 | USB | 0x04b8/0x081c | Good | all-in-one overseas version of the PM-A890 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX680 | USB | 0x04b8/0x0837 | Good | all-in-one overseas version of the PM-A940 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX685 | USB | 0x04b8/0x0837 | Good | all-in-one overseas version of the PM-A940 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX690 | USB | 0x04b8/0x0837 | Good | all-in-one overseas version of the PM-A940 | epson2 (1.0.124) | sane-epson2
Stylus Photo RX700 | USB | 0x04b8/0x0810 | Good | all-in-one overseas version of the PM-A900 | epson2 (1.0.124) | sane-epson2
Stylus Photo TX650 Series | USB | 0x04b8/0x0850 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus Photo TX700W | USB | 0x04b8/0x0846 | Good | network interface probably supported all-in-one overseas version of the EP-801A | epson2 (1.0.124) | sane-epson2
Stylus Photo TX710W Series | USB | 0x04b8/0x0852 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus Photo TX800FW | USB | 0x04b8/0x0844 | Good | network interface probably supported all-in-one overseas version of the EP-901A | epson2 (1.0.124) | sane-epson2
Stylus Scan 2000 | USB | 0x04b8/0x0105 | Untested | apparently mostly the same as the Stylus Scan 2500 | epson2 (1.0.124) | sane-epson2
Stylus Scan 2500 | USB | 0x04b8/0x0106 | Untested | scanner is apparently a GT-7000 | epson2 (1.0.124) | sane-epson2
Stylus SX100 | USB | 0x04b8/0x0841 | Good | all-in-one overseas version of the PX-401A | epson2 (1.0.124) | sane-epson2
Stylus SX110 Series | USB | 0x04b8/0x084d | Good | all-in-one overseas version of the PX-402A | epson2 (1.0.124) | sane-epson2
Stylus SX125 | USB | 0x04b8/0x085c | Untested | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus SX200 | USB | 0x04b8/0x0849 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus SX205 | USB | 0x04b8/0x0849 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus SX210 Series | USB | 0x04b8/0x084f | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus SX400 | USB | 0x04b8/0x084a | Good | network interface probably supported all-in-one overseas version of the PX-501A | epson2 (1.0.124) | sane-epson2
Stylus SX405 | USB | 0x04b8/0x084a | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus SX410 Series | USB | 0x04b8/0x0851 | Good | network interface probably supported all-in-one | epson2 (1.0.124) | sane-epson2
Stylus SX510W Series | USB | 0x04b8/0x0856 | Good | all-in-one overseas version of the PX-502A | epson2 (1.0.124) | sane-epson2
Stylus SX600FW | USB | 0x04b8/0x0847 | Good | network interface probably supported all-in-one overseas version of the PX-601F | epson2 (1.0.124) | sane-epson2
Stylus SX610FW Series | USB | 0x04b8/0x0855 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2
Stylus TX100 | USB | 0x04b8/0x0841 | Good | all-in-one overseas version of the PX-401A | epson2 (1.0.124) | sane-epson2
Stylus TX110 Series | USB | 0x04b8/0x084d | Good | all-in-one overseas version of the PX-402A | epson2 (1.0.124) | sane-epson2
Stylus TX200 | USB | 0x04b8/0x0849 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus TX203 | USB | 0x04b8/0x0849 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus TX209 | USB | 0x04b8/0x0849 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus TX210 Series | USB | 0x04b8/0x084f | Good | all-in-one | epson2 (1.0.124) | sane-epson2
Stylus TX400 | USB | 0x04b8/0x084a | Good | network interface probably supported all-in-one overseas version of the PX-501A | epson2 (1.0.124) | sane-epson2
Stylus TX410 Series | USB | 0x04b8/0x0851 | Good | network interface probably supported all-in-one | epson2 (1.0.124) | sane-epson2
Stylus TX550W Series | USB | 0x04b8/0x0856 | Good | all-in-one overseas version of the PX-502A | epson2 (1.0.124) | sane-epson2
StylusScan 2000 | USB | 0x04b8/0x0105 | Unsupported | Probably unsupported. No details known. | unsupported (2010-06-09) | ?
V700 | USB IEEE-1394 | 0x04b8/0x012c | Good |  | epson (unmaintained) | sane-epson
V750 | USB IEEE-1394 | 0x04b8/0x012c | Good |  | epson (unmaintained) | sane-epson
WorkForce 310 Series | USB | 0x04b8/0x0854 | Good | all-in-one | epson2 (1.0.124) | sane-epson2
WorkForce 500 | USB | 0x04b8/0x084c | Good | all-in-one | epson2 (1.0.124) | sane-epson2
WorkForce 600 | USB | 0x04b8/0x0847 | Good | network interface probably supported all-in-one overseas version of the PX-601F | epson2 (1.0.124) | sane-epson2
WorkForce 610 Series | USB | 0x04b8/0x0855 | Unsupported | supported by the epkowa backend plus non-free interpreter | epson2 (1.0.124) | sane-epson2

### Manufacturer: Escom

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Image Scanner 256 | SCSI |  | Good | OK, SCSI-ID=UMAX UG 80 | umax (1.0-41) | sane-umax

### Manufacturer: Escort

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Galleria 600 | SCSI |  | Untested | untested, SCSI-ID=ESCORT Galleria 600S | umax (1.0-41) | sane-umax

### Manufacturer: Fujitsu

Link(s): http://www.fujitsu.com, http://www.fujitsu.com/, http://www.fcpa.fujitsu.com/products/scanners/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
1200CUS | USB | 0x05d8/0x4002 | Basic | Works, but is slow. Probably a Mustek BearPaw 2400 CU clone. | gt68xx (1.0-84) | sane-gt68xx
fi-60F | USB | 0x04c5/0x10c7 | Basic | A6-size flatbed, 300/600 dpi, color/gray/binary | epjitsu (20) | sane-epjitsu
fi-4010CU | USB | 0x04c5/0x1029 | Untested |  | avision (Build: 296) | sane-avision
fi-4110EOX/2/3 | USB | 0x04c5/0x1040 | Unsupported | Uses ma1509 chip, but very different from other scanners supported by the ma1509 backend | ma1509 (1.0-3) | sane-ma1509
fi-4120C | SCSI USB | 0x04c5/0x1041 | Complete | small, recent, discontinued, usb 1.1 | fujitsu (117) | sane-fujitsu
fi-4120C2 | SCSI USB | 0x04c5/0x10ae | Complete | small, recent, discontinued, usb 2.0 | fujitsu (117) | sane-fujitsu
fi-4220C | SCSI USB | 0x04c5/0x1042 | Complete | small, recent, discontinued, usb 1.1 | fujitsu (117) | sane-fujitsu
fi-4220C2 | SCSI USB | 0x04c5/0x10af | Complete | small, recent, discontinued, usb 2.0 | fujitsu (117) | sane-fujitsu
fi-4340C | SCSI USB | 0x04c5/0x10cf | Complete | medium, current | fujitsu (117) | sane-fujitsu
fi-4530C | SCSI USB | 0x04c5/0x1078 | Complete | medium, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-4640S | SCSI |  | Complete | medium, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-4750C | SCSI |  | Complete | medium, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-4750L | SCSI |  | Complete | big, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-4860C | SCSI |  | Complete | big, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-4860C2 | SCSI |  | Complete | big, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-4990C | SCSI |  | Complete | big, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-5000N | Ethernet |  | Untested | Not a scanner, rather a scanner to ethernet interface | fujitsu (117) | sane-fujitsu
fi-5015C | USB | 0x04c5/0x10ef | Good |  | avision (Build: 296) | sane-avision
fi-5110C | USB | 0x04c5/0x1097 | Complete | small, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-5110EOX/2 | USB | 0x04c5/0x1096 | Complete | small, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-5110EOX3 | USB | 0x04c5/0x10e6 | Complete | small, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-5110EOXM | USB | 0x04c5/0x10f2 | Complete | small, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-5120C | SCSI USB | 0x04c5/0x10e0 | Complete | small, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-5220C | SCSI USB | 0x04c5/0x10e1 | Complete | small, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-5530C | SCSI USB | 0x04c5/0x10e2 | Complete | medium, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-5530C2 | SCSI USB | 0x04c5/0x114a | Complete | medium, current | fujitsu (117) | sane-fujitsu
fi-5650C | SCSI USB | 0x04c5/0x10ad | Complete | big, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-5750C | SCSI USB | 0x04c5/0x1095 | Complete | big, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-5900C | SCSI USB | 0x04c5/0x10e7 | Good | big, recent, discontinued. Independent ultrasonic control and multistream unsupported | fujitsu (117) | sane-fujitsu
fi-5950 | SCSI USB | 0x04c5/0x1213 | Untested | big, current. Faster version of fi-5900? | fujitsu (117) | sane-fujitsu
fi-6000NS | Ethernet |  | Untested | small, recent, discontinued, integrated touchscreen and keyboard | fujitsu (117) | sane-fujitsu
fi-6110 | USB | 0x04c5/0x11fc | Complete | small, current | fujitsu (117) | sane-fujitsu
fi-6130 | USB | 0x04c5/0x114f | Complete | small, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-6130Z | USB | 0x04c5/0x11f3 | Complete | small, current | fujitsu (117) | sane-fujitsu
fi-6140 | SCSI USB | 0x04c5/0x114d | Complete | medium, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-6140Z | SCSI USB | 0x04c5/0x11f1 | Complete | medium, current | fujitsu (117) | sane-fujitsu
fi-6230 | USB | 0x04c5/0x1150 | Complete | small, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-6230Z | USB | 0x04c5/0x11f4 | Complete | small, current | fujitsu (117) | sane-fujitsu
fi-6240 | SCSI USB | 0x04c5/0x114e | Complete | medium, recent, discontinued | fujitsu (117) | sane-fujitsu
fi-6240Z | SCSI USB | 0x04c5/0x11f2 | Complete | medium, current | fujitsu (117) | sane-fujitsu
fi-6670 | SCSI USB | 0x04c5/0x1176 | Good | big, current, won't wakeup via software | fujitsu (117) | sane-fujitsu
fi-6670A | SCSI USB | 0x04c5/0x1177 | Good | big, current, VRS CGA board unsupported, won't wakeup via software | fujitsu (117) | sane-fujitsu
fi-6750S | USB | 0x04c5/0x1178 | Untested | Simplex, USB only version of fi-6770, won't wakeup via software, discontinued | fujitsu (117) | sane-fujitsu
fi-6770 | SCSI USB | 0x04c5/0x1174 | Good | big, current, won't wakeup via software | fujitsu (117) | sane-fujitsu
fi-6770A | SCSI USB | 0x04c5/0x1175 | Good | big, current, VRS CGA board unsupported, won't wakeup via software | fujitsu (117) | sane-fujitsu
fi-6800 | SCSI USB | 0x04c5/0x119d | Untested | big, current. Independent ultrasonic control and multistream unsupported | fujitsu (117) | sane-fujitsu
fi-6800-CGA | SCSI USB | 0x04c5/0x119e | Untested | big, current. VRS CGA board unsupported, Independent ultrasonic control and multistream unsupported | fujitsu (117) | sane-fujitsu
M3091DC | SCSI |  | Complete | small, old, discontinued | fujitsu (117) | sane-fujitsu
M3092DC | SCSI |  | Complete | small, old, discontinued | fujitsu (117) | sane-fujitsu
M3093DE | RS232C/Video |  | Unsupported | medium, old, discontinued | fujitsu (117) | sane-fujitsu
M3093DG | SCSI |  | Complete | medium, old, discontinued | fujitsu (117) | sane-fujitsu
M3093E | RS232C/Video |  | Unsupported | medium, old, discontinued | fujitsu (117) | sane-fujitsu
M3093EX | RS232C/Video |  | Unsupported | medium, old, discontinued | fujitsu (117) | sane-fujitsu
M3093GX | SCSI |  | Complete | medium, old, discontinued | fujitsu (117) | sane-fujitsu
M3096EX | RS232C/Video |  | Unsupported | medium, old, discontinued | fujitsu (117) | sane-fujitsu
M3096GX | SCSI |  | Complete | medium, old, discontinued | fujitsu (117) | sane-fujitsu
M3097DE | RS232C/Video |  | Unsupported | medium, old, discontinued | fujitsu (117) | sane-fujitsu
M3097DG | SCSI |  | Complete | medium, old, discontinued | fujitsu (117) | sane-fujitsu
M3097E+ | RS232C/Video |  | Unsupported | medium, old, discontinued | fujitsu (117) | sane-fujitsu
M3097G+ | SCSI |  | Complete | medium, old, discontinued | fujitsu (117) | sane-fujitsu
M3099A | RS232C/Video |  | Unsupported | big, old, discontinued | fujitsu (117) | sane-fujitsu
M3099EH | RS232C/Video |  | Unsupported | big, old, discontinued | fujitsu (117) | sane-fujitsu
M3099EX | RS232C/Video |  | Unsupported | big, old, discontinued | fujitsu (117) | sane-fujitsu
M3099G | SCSI |  | Complete | big, old, discontinued | fujitsu (117) | sane-fujitsu
M3099GH | SCSI |  | Complete | big, old, discontinued | fujitsu (117) | sane-fujitsu
M3099GX | SCSI |  | Complete | big, old, discontinued | fujitsu (117) | sane-fujitsu
M4097D | SCSI |  | Complete | big, old, discontinued | fujitsu (117) | sane-fujitsu
M4099D | SCSI |  | Complete | big, old, discontinued | fujitsu (117) | sane-fujitsu
ScanPartner | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
ScanPartner 10 | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
ScanPartner 10C | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
ScanPartner 15C | SCSI |  | Good |  | sp15c (unmaintained) | sane-sp15c
ScanPartner 300C | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
ScanPartner 600C | SCSI |  | Good |  | sp15c (unmaintained) | sane-sp15c
ScanPartner 620C | SCSI |  | Good |  | avision (Build: 296) | sane-avision
ScanPartner Jr | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
ScanSnap fi-6010N | Ethernet |  | Untested | small, current, integrated touchscreen and keyboard | fujitsu (117) | sane-fujitsu
ScanSnap iX500 | USB WiFi | 0x04c5/0x132b | Good | small, current, WiFi not supported. Hardware only scans in color. Backend generates binary and grayscale modes. | fujitsu (117) | sane-fujitsu
ScanSnap N1800 | Ethernet |  | Untested | small, current, integrated touchscreen and keyboard | fujitsu (117) | sane-fujitsu
ScanSnap S300 | USB | 0x04c5/0x1156 | Good | Duplex, 150/225/300/600 dpi, color/gray/binary, AC/USB power, buttons/sensors all supported. Scanner always scans in _triplex_ color, fast USB required. | epjitsu (20) | sane-epjitsu
ScanSnap S300M | USB | 0x04c5/0x117f | Good | Same as S300, with different usb id | epjitsu (20) | sane-epjitsu
ScanSnap S500 | USB | 0x04c5/0x10fe | Complete | small, recent, discontinued | fujitsu (117) | sane-fujitsu
ScanSnap S500M | USB | 0x04c5/0x1135 | Complete | small, recent, discontinued | fujitsu (117) | sane-fujitsu
ScanSnap S510 | USB | 0x04c5/0x1155 | Complete | small, recent, discontinued | fujitsu (117) | sane-fujitsu
ScanSnap S510M | USB | 0x04c5/0x116f | Complete | small, recent, discontinued | fujitsu (117) | sane-fujitsu
ScanSnap S1100 | USB | 0x04c5/0x1200 | Unsupported | Beta version of backend source available, which works well, but breaks support for other epjitsu scanners. See http://ubuntuforums.org/showthread.php?t=1678335 | epjitsu (20) | sane-epjitsu
ScanSnap S1300 | USB | 0x04c5/0x11ed | Good | Same as S300, with different usb id | epjitsu (20) | sane-epjitsu
ScanSnap S1500 | USB | 0x04c5/0x11a2 | Complete | small, discontinued | fujitsu (117) | sane-fujitsu
ScanSnap S1500M | USB | 0x04c5/0x11a2 | Complete | small, discontinued, same as S1500 | fujitsu (117) | sane-fujitsu
ScanStation | SCSI |  | Untested |  | avision (Build: 296) | sane-avision

### Manufacturer: Gallery

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
4800 | Parport (EPP) |  | Good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp

### Manufacturer: Genius

Link(s): http://www.genius-kye.com/, http://www.geniusmouse.co.uk/, http://www.geniusnet.com.tw/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
ColorPage CS | SCSI |  | Unsupported | Probably unsupported, see link for details. | unsupported (2010-06-09) | ?
ColorPage HR6 V1 | USB | 0x0458/0x2004 | Basic |  | u12 (0.02) | sane-u12
Colorpage HR6 V2 | USB | 0x0458/0x2008 | Complete |  | plustek (0.52) | sane-plustek
Colorpage HR6 V2 | USB | 0x0458/0x2007 | Complete |  | plustek (0.52) | sane-plustek
Colorpage HR6A | USB | 0x0458/0x2009 | Untested |  | plustek (0.52) | sane-plustek
Colorpage HR6X | USB | 0x0458/0x2016 | Untested |  | plustek (0.52) | sane-plustek
Colorpage HR6X EPP | Parport (SPP, EPP) |  | Good | Negative scanning does not work correctly | plustek_pp (0.43) | sane-plustek_pp
ColorPage HR6X Slim | USB | 0x0458/0x2019 | Unsupported | GL646 based, to be added to genesys backend | unsupported (2010-06-09) | ?
Colorpage HR7 | USB | 0x0458/0x2013 | Complete |  | plustek (0.52) | sane-plustek
Colorpage HR7LE | USB | 0x0458/0x2015 | Untested |  | plustek (0.52) | sane-plustek
ColorPage HR7X | USB | 0x0458/0x2018 | Unsupported | GL646 based, to be added to genesys backend | unsupported (2010-06-09) | ?
ColorPage HR7XE | USB | 0x06dc/0x0012 | Unsupported | Unsuported. See link for details. | unsupported (2010-06-09) | ?
ColorPage HR8 | USB | 0x0458/0x201c | Unsupported | GL841 based, to be added to genesys backend | unsupported (2010-06-09) | ?
Colorpage SF600 | USB | 0x0458/0x2021 | Basic |  | gt68xx (1.0-84) | sane-gt68xx
ColorPage Slim 1200 | USB | 0x0458/0x201e | Untested | Untested but should work. | gt68xx (1.0-84) | sane-gt68xx
Colorpage Vivid 1200 X | USB | 0x0458/0x201d | Good |  | gt68xx (1.0-84) | sane-gt68xx
Colorpage Vivid 1200 XE | USB | 0x0458/0x201f | Good |  | gt68xx (1.0-84) | sane-gt68xx
ColorPage Vivid III USB | USB | 0x07b3/0x0001 | Untested | Note: Device has Plustek vendor and product ID (0x07b3/0x0001) | u12 (0.02) | sane-u12
Colorpage Vivid III V2 | Parport (SPP, EPP) |  | Complete | Reported as PT12 | plustek_pp (0.43) | sane-plustek_pp
Colorpage Vivid Pro II Film | Parport (SPP, EPP) |  | Complete | Reported as OP9636T/12000T | plustek_pp (0.43) | sane-plustek_pp
Colorpage Vivid3 V2 | USB | 0x0458/0x2011 | Good | Same as Colorpage Vivid3x | gt68xx (1.0-84) | sane-gt68xx
Colorpage Vivid3x | USB | 0x0458/0x2011 | Good |  | gt68xx (1.0-84) | sane-gt68xx
Colorpage Vivid3xe | USB | 0x0458/0x2017 | Good |  | gt68xx (1.0-84) | sane-gt68xx
Colorpage Vivid4 | USB | 0x0458/0x2014 | Good |  | gt68xx (1.0-84) | sane-gt68xx
Colorpage Vivid4x | USB | 0x0458/0x201b | Good |  | gt68xx (1.0-84) | sane-gt68xx
Colorpage Vivid4xe | USB | 0x0458/0x201a | Good |  | gt68xx (1.0-84) | sane-gt68xx
ColorPage-EP | Parport |  | Good |  | microtek2 (unmaintained) | sane-microtek2
ColorPage-HR5 (Pro) | SCSI |  | Good | OK, SCSI-ID=KYE ColorPage-HR5 | umax (1.0-41) | sane-umax
ColorPage-Life Pro | Parport (EPP/ECP) |  | Good | works (relabelled 1220P and 2000P) | umax_pp (1) | sane-umax_pp
ColorPage-Slim 1200 USB2 | USB | 0x0458/0x2020 | Unsupported | GL841 based, to be added to genesys backend. | unsupported (2010-06-09) | ?
Colorpage-SP2 | SCSI |  | Good | Same as Microtek Scanmaker E3 | microtek (0.13.1) | sane-microtek
FS-1130 Colorpage Scanner | SCSI |  | Good |  | leo (1.0-10) | sane-leo

### Manufacturer: Googlegear

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
2000 | USB | 0x05d8/0x4002 | Good | Same as Artec Ultima 2000. | gt68xx (1.0-84) | sane-gt68xx

### Manufacturer: Guillemot

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Maxi Scan A4 Parallel 36 bit | Parport |  | Unsupported | Probably unsupported. Identical to the Benq Prisa 620P. | unsupported (2010-06-09) | ?
SCAN@HOME 48 USB | USB | 0x080d/0x0102 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Guillemot / Hercules

Link(s): http://www.guillemot.com

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Maxi A4 36 bit | USB | 0x04a5/0x2060 | Good | Rebadged Benq 620U, needs Benq firmware file u96v???.bin | SnapScan (1.4) | sane-snapscan
Maxi Scan A4 Deluxe (SCSI) | SCSI |  | Good | Rebadged SnapScan 310s. | SnapScan (1.4) | sane-snapscan
Maxi Scan A4 USB 640U | USB | 0x04a5/0x2060 | Good | Rebadged Benq 640U. | SnapScan (1.4) | sane-snapscan
Scan@home Touch 1248 (USB) | USB | 0x04a5/0x20de | Good | Rebadged Benq 3300. | SnapScan (1.4) | sane-snapscan

### Manufacturer: Hercules

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
SCAN@HOME 48 USB | USB | 0x080d/0x0102 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Hewlett-Packard

Link(s): http://www.hp.com, http://www.hp.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
LaserJet M1005 MFP | USB | 0x03f0/0x3b17 | Good | grayscale/color (24 bit), 75/100/150/200/300/600/1200 DPI | hpljm1005 (0) | sane-hpljm1005
LaserJet M1120 MFP | USB | 0x03f0/0x5617 | Good | grayscale/color (24 bit), 75/100/150/200/300/600/1200 DPI | hpljm1005 (0) | sane-hpljm1005
LaserJet M1120n MFP | USB | 0x03f0/0x5717 | Good | grayscale/color (24 bit), 75/100/150/200/300/600/1200 DPI | hpljm1005 (0) | sane-hpljm1005
Photo Scanner 1000 | USB | 0x03f0/0x1001 | Unsupported | Not supported by SANE. However, it's detected as mass storage device so just mounting it is reported to work. See link for device data. | unsupported (2010-06-09) | ?
Photosmart 1200 Photo | USB |  | Unsupported | Probably not supported by SANE. No details known. 10x15 cm. Maybe similar to Photo Scanner 1000? | unsupported (2010-06-09) | ?
Photosmart C3180 | USB | 0x03f0/0x5611 | Unsupported | Not supported yet by SANE. See link for details. | unsupported (2010-06-09) | ?
Photosmart C5100 series | USB | 0x03f0/0x5811 | Unsupported | Not supported yet by SANE. See link for details. | unsupported (2010-06-09) | ?
PhotoSmart PhotoScanner | SCSI |  | Complete |  | hp (1.06) | sane-hp
Photosmart S20 (C5101A) | USB | 0x03f0/0x0102 | Unsupported | Not supported yet by SANE. See link for details. | unsupported (2010-06-09) | ?
Photosmart S20xi (C7150A) | USB | 0x03f0/0x0102 | Unsupported | Not supported yet by SANE. See link for details. | unsupported (2010-06-09) | ?
ScanJet 3c | SCSI |  | Complete |  | hp (1.06) | sane-hp
ScanJet 3p | SCSI |  | Complete |  | hp (1.06) | sane-hp
ScanJet 4c | SCSI |  | Complete |  | hp (1.06) | sane-hp
ScanJet 4p | SCSI |  | Complete |  | hp (1.06) | sane-hp
ScanJet 5p | SCSI |  | Complete |  | hp (1.06) | sane-hp
ScanJet 5s | Parport (EPP) |  | Minimal | Requires libieee1284 library. Only gray mode. | hpsj5s (0.03) | sane-hpsj5s
ScanJet 2100C | USB | 0x03f0/0x0505 | Complete |  | plustek (0.52) | sane-plustek
ScanJet 2200C | USB | 0x03f0/0x0605 | Complete |  | plustek (0.52) | sane-plustek
ScanJet 2300C | USB | 0x03f0/0x0901 | Complete | 600x1200 dpi max | genesys (1.0-63) | sane-genesys
ScanJet 2400C | USB | 0x03f0/0x0a01 | Complete | 1200x1200 dpi max | genesys (1.0-63) | sane-genesys
Scanjet 3200C | Parport (EPP/ECP) |  | Good | works (relabelled 1220P and 2000P) | umax_pp (1) | sane-umax_pp
ScanJet 3300c | USB | 0x03f0/0x0205 | Complete |  | niash (0.3) | sane-niash
ScanJet 3400c | USB | 0x03f0/0x0405 | Complete | If you use Linux 2.6, version 2.6.8 or newer is necessary. | niash (0.3) | sane-niash
ScanJet 3500C | USB | 0x03f0/0x2205 | Good |  | hp3500 (1.1) | sane-hp3500
ScanJet 3530C | USB | 0x03f0/0x2005 | Good |  | hp3500 (1.1) | sane-hp3500
ScanJet 3570C | USB | 0x03f0/0x2005 | Good |  | hp3500 (1.1) | sane-hp3500
ScanJet 3670C | USB | 0x03f0/0x1405 | Complete | 1200x1200 dpi max, complete transparency adaptor support | genesys (1.0-63) | sane-genesys
ScanJet 3690C | USB | 0x03f0/0x1405 | Complete | 1200x1200 dpi max, same as HP 3670C | genesys (1.0-63) | sane-genesys
ScanJet 3770 | USB | 0x03f0/0x2505 | Unsupported | While an external binary-only backend exists, it works only on Linux i386. Therefore the scanner is unsupported on other platforms. | unsupported (2010-06-09) | ?
ScanJet 3800 | USB | 0x03f0/0x2605 | Basic | Works with resolutions equal and less than 600dpi | hp3900 (0.12) | sane-hp3900
ScanJet 3970c | USB | 0x03f0/0x2305 | Good |  | hp3900 (0.12) | sane-hp3900
ScanJet 4070 Photosmart | USB | 0x03f0/0x2405 | Good |  | hp3900 (0.12) | sane-hp3900
ScanJet 4100C | USB | 0x03f0/0x0101 | Complete |  | hp (1.06) | sane-hp
ScanJet 4200C | USB | 0x03f0/0x0105 | Basic | 8bpp color, 75/150/300/600 dpi only | hp4200 (1.0-2) | sane-hp4200
ScanJet 4200Cse | USB | 0x03f0/0x0105 | Basic | 8bpp color, 75/150/300/600 dpi only | hp4200 (1.0-2) | sane-hp4200
ScanJet 4200Cxi | USB | 0x03f0/0x0105 | Basic | 8bpp color, 75/150/300/600 dpi only | hp4200 (1.0-2) | sane-hp4200
ScanJet 4300c | USB | 0x03f0/0x0305 | Complete | If you use Linux 2.6, version 2.6.8 or newer is necessary. | niash (0.3) | sane-niash
ScanJet 4300c/Silitek | USB | 0x047b/0x1002 | Complete | If you use Linux 2.6, version 2.6.8 or newer is necessary. | niash (0.3) | sane-niash
ScanJet 4370 | USB | 0x03f0/0x4105 | Basic | Works with resolutions lower than 1200dpi | hp3900 (0.12) | sane-hp3900
scanjet 4400c | USB | 0x03f0/0x0705 | Good | exists with 2 different sensors of which only one works | rts8891 (1.0-0) | sane-rts8891
scanjet 4470c | USB | 0x03f0/0x0805 | Good | re-branded Astra 4400 | rts8891 (1.0-0) | sane-rts8891
ScanJet 4500C | USB | 0x03f0/0x1205 | Complete | Lineart/grayscale/color (24 bit), 100/200/300/600/1200/2400 DPI, flatbed/ADF/ADF duplex/TMA slides/TMA negatives | hp5590 (1.0.5) | sane-hp5590
ScanJet 4570C | USB | 0x03f0/0x1305 | Complete | Lineart/grayscale/color (24 bit), 100/200/300/600/1200/2400 DPI, flatbed/TMA slides/TMA negatives | hp5590 (1.0.5) | sane-hp5590
ScanJet 4600 | USB | 0x03f0/0x3005 | Unsupported | Not supported. See link for details, or http://www.chmil.org/hp4600linux/ for code | unsupported (2010-06-09) | ?
ScanJet 4670 | USB | 0x03f0/0x3005 | Unsupported | Not supported. See ScanJet 4600 entry. | unsupported (2010-06-09) | ?
ScanJet 4850C | USB | 0x03f0/0x1b05 | Untested | resolution from 100 to 2400 supported, UTA not supported yet | genesys (1.0-63) | sane-genesys
ScanJet 4890C | USB | 0x03f0/0x1b05 | Unsupported | GL843, maybe can be added to genesys backend | unsupported (2010-06-09) | ?
ScanJet 5100C | Parport |  | Complete | Requires ppscsi driver and epst module | hp (1.06) | sane-hp
ScanJet 5200C | Parport USB | 0x03f0/0x0401 | Complete | Parallel interface requires ppscsi driver and epst module | hp (1.06) | sane-hp
ScanJet 5300C | USB | 0x03f0/0x0701 | Complete | 1 pass, 2400 dpi - some FW revisions have x-axis image scaling problems over 1200 dpi | avision (Build: 296) | sane-avision
ScanJet 5370C | USB | 0x03f0/0x0701 | Good | 1 pass, 2400 dpi - some FW revisions have x-axis image scaling problems over 1200 dpi | avision (Build: 296) | sane-avision
ScanJet 5400c | USB | 0x03f0/0x1005 | Basic |  | hp5400 (1.0-2) | sane-hp5400
ScanJet 5470c | USB | 0x03f0/0x1105 | Basic |  | hp5400 (1.0-2) | sane-hp5400
ScanJet 5490c | USB |  | Basic |  | hp5400 (1.0-2) | sane-hp5400
ScanJet 5500C | USB | 0x03f0/0x1305 | Untested | Lineart/grayscale/color (24 bit), 100/200/300/600/1200/2400 DPI, flatbed/TMA slides/TMA negatives | hp5590 (1.0.5) | sane-hp5590
ScanJet 5530C Photosmart | USB | 0x03f0/0x1605 | Unsupported | Maybe GL841_HP, but not confirmed, maybe can be added to genesys backend | unsupported (2010-06-09) | ?
ScanJet 5550C | USB | 0x03f0/0x1205 | Complete | Lineart/grayscale/color (24 bit), 100/200/300/600/1200/2400 DPI, flatbed/ADF/ADF duplex/TMA slides/TMA negatives | hp5590 (1.0.5) | sane-hp5590
ScanJet 5590 | USB | 0x03f0/0x1705 | Complete | Lineart/grayscale/color (24 bit), 100/200/300/600/1200/2400 DPI, flatbed/ADF/ADF duplex/TMA slides/TMA negatives | hp5590 (1.0.5) | sane-hp5590
ScanJet 6100C | SCSI |  | Complete |  | hp (1.06) | sane-hp
ScanJet 6200C | SCSI USB | 0x03f0/0x0201 | Complete |  | hp (1.06) | sane-hp
ScanJet 6250C | SCSI USB | 0x03f0/0x0201 | Complete |  | hp (1.06) | sane-hp
ScanJet 6300C | SCSI USB | 0x03f0/0x0601 | Complete |  | hp (1.06) | sane-hp
ScanJet 6350C | SCSI USB | 0x03f0/0x0601 | Complete |  | hp (1.06) | sane-hp
ScanJet 6390C | SCSI USB | 0x03f0/0x0601 | Complete |  | hp (1.06) | sane-hp
ScanJet 7400c | USB | 0x03f0/0x0801 | Good | 1 pass, 2400 dpi - dual USB/SCSI interface | avision (Build: 296) | sane-avision
ScanJet 7450c | USB | 0x03f0/0x0801 | Good | 1 pass, 2400 dpi - dual USB/SCSI interface | avision (Build: 296) | sane-avision
ScanJet 7490c | USB | 0x03f0/0x0801 | Good | 1 pass, 1200 dpi - dual USB/SCSI interface | avision (Build: 296) | sane-avision
ScanJet 7650 | USB | 0x03f0/0x1805 | Complete | Lineart/grayscale/color (24 bit), 100/200/300/600/1200/2400 DPI, flatbed/ADF/ADF duplex/TMA slides/TMA negatives | hp5590 (1.0.5) | sane-hp5590
ScanJet 8200 | USB | 0x03f0/0x0b01 | Good | 1 pass, 4800 (?) dpi - USB 2.0 | avision (Build: 296) | sane-avision
ScanJet 8250 | USB | 0x03f0/0x0b01 | Good | 1 pass, 4800 (?) dpi - USB 2.0 | avision (Build: 296) | sane-avision
ScanJet 8270 | USB | 0x03f0/0x3905 | Good | 1 pass, 4800 (?) dpi - USB 2.0 | avision (Build: 296) | sane-avision
ScanJet 8290 | USB | 0x03f0/0x0b01 | Good | 1 pass, 4800 (?) dpi - USB 2.0 and SCSI - only SCSI tested so far | avision (Build: 296) | sane-avision
ScanJet 8300 | USB | 0x03f0/0x3805 | Good | 1 pass, 4800 (?) dpi - USB 2.0 | avision (Build: 296) | sane-avision
ScanJet 8350 | USB | 0x03f0/0x3805 | Good | 1 pass, 4800 (?) dpi - USB 2.0 | avision (Build: 296) | sane-avision
ScanJet 8390 | USB | 0x03f0/0x3805 | Good | 1 pass, 4800 (?) dpi - USB 2.0 | avision (Build: 296) | sane-avision
ScanJet G2410 | USB | 0x03f0/0x0a01 | Basic | clone of the HP 2400C | genesys (1.0-63) | sane-genesys
ScanJet G2710 | USB | 0x03f0/0x2805 | Basic | Similar to hp scanjet 3800 | hp3900 (0.12) | sane-hp3900
ScanJet G3010 | USB | 0x03f0/0x4205 | Basic | Similar to hp scanjet 4370 | hp3900 (0.12) | sane-hp3900
ScanJet G3110 | USB | 0x03f0/0x4305 | Basic | Similar to hp scanjet 4370 | hp3900 (0.12) | sane-hp3900
ScanJet G4000 | USB | 0x03f0/0x4505 | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
ScanJet G4010 | USB | 0x03f0/0x4505 | Good | resolution from 100 to 2400 supported, UTA not supported yet | genesys (1.0-63) | sane-genesys
ScanJet G4050 | USB | 0x03f0/0x4605 | Good | resolution from 100 to 2400 supported, UTA not supported yet | genesys (1.0-63) | sane-genesys
ScanJet IIc | SCSI |  | Complete |  | hp (1.06) | sane-hp
ScanJet IIcx | SCSI |  | Complete |  | hp (1.06) | sane-hp
ScanJet IIp | SCSI |  | Complete |  | hp (1.06) | sane-hp
ScanJet N6310 | USB | 0x03f0/0x4705 | Untested | Not supported yet | genesys (1.0-63) | sane-genesys
ScanJet Plus | Propietary |  | Complete | Driver for HP parallel interface card required | hp (1.06) | sane-hp

### Manufacturer: IBM

Link(s): http://www.ibm.com/, http://www.ibm.com

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
2456 | SCSI |  | Basic | Was reported to work long time ago. Reports are welcome. | ibm (1.0-4) | sane-ibm
ADF Color Scanner | Proprietary |  | Unsupported | Unsupported. Uses proprietary ISA card. Maybe the same as the Plustek Spectra ADF? | unsupported (2010-06-09) | ?

### Manufacturer: IOMagic

Link(s): http://www.iomagic.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
MobileScan USB | USB Parport | 0x05cb/0x1483 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Iris

Link(s): http://irislink.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
IriScan | USB | 0x0a53/0x1000 | Unsupported | Unsupported. LM9832/3. See link for details. | unsupported (2010-06-09) | ?
IRISCard Pro (IBCR II) | USB | 0x0a38/0x0301 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
IRISPen Translator Executive | USB | 0x0f43/0x015a | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: iVina

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
1200U | USB | 0x0638/0x0268 | Untested |  | avision (Build: 296) | sane-avision

### Manufacturer: Kodak

Link(s): http://www.kodak.com, http://www.kodak.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Color Scanner 3590C | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Color Scanner 4500 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
ESP 5 | USB | 0x040a/0x4032 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 7 | USB | 0x040a/0x403e | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 9 | USB | 0x040a/0x403f | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 2150 | USB | 0x040a/0x4059 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 2170 | USB | 0x040a/0x4066 | Basic | Tested with network | kodakaio (2.4.6) | sane-kodakaio
ESP 3200 | USB | 0x040a/0x4043 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 3300 | USB | 0x040a/0x4031 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 4100 | USB | 0x040a/0x4053 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 5000 | USB | 0x040a/0x4028 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 5100 | USB | 0x040a/0x4025 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 5200 | USB Ethernet | 0x040a/0x4041 | Basic | USB good, Network good | kodakaio (2.4.6) | sane-kodakaio
ESP 5300 | USB | 0x040a/0x4026 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 5500 | USB | 0x040a/0x4027 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 6100 | USB | 0x040a/0x4054 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 7200 | USB | 0x040a/0x4056 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP 9200 | USB | 0x040a/0x4065 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP C110 | USB | 0x040a/0x4057 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP C115 | USB | 0x040a/0x4058 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP C310 | USB | 0x040a/0x405d | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
ESP C315 | USB | 0x040a/0x405e | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
Hero 3.1 | USB | 0x040a/0x406d | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
Hero 4.1 | USB | 0x040a/0x4069 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
Hero 5.1 | USB | 0x040a/0x4064 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
Hero 7.1 | USB | 0x040a/0x4063 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
Hero 9.1 | USB Ethernet | 0x040a/0x4067 | Basic | USB good, Network good | kodakaio (2.4.6) | sane-kodakaio
Hero Office 6.1 | USB | 0x040a/0x4062 | Untested | Please test! | kodakaio (2.4.6) | sane-kodakaio
i30 | USB | 0x040a/0x6001 | Untested |  | avision (Build: 296) | sane-avision
i40 | USB | 0x040a/0x6002 | Basic |  | avision (Build: 296) | sane-avision
i50 | USB | 0x040a/0x6003 | Untested |  | avision (Build: 296) | sane-avision
i55 | USB | 0x040a/0x6003 | Untested |  | avision (Build: 296) | sane-avision
i60 | USB | 0x040a/0x6004 | Untested |  | avision (Build: 296) | sane-avision
i65 | USB | 0x040a/0x6004 | Untested |  | avision (Build: 296) | sane-avision
i80 | USB | 0x040a/0x6005 | Good |  | avision (Build: 296) | sane-avision
i150 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i160 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i250 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i260 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i280 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i610 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i620 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i640 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i660 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i730 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i750 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i780 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i810 Scanner | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
i820 Scanner | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
i830 Scanner | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
i840 Scanner | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
i1840 Scanner | IEEE-1394 |  | Untested | Please test! | kodak (7) | sane-kodak
i1860 Scanner | IEEE-1394 |  | Basic | Uncompressed B&W, Gray and Color, some automatic features supported | kodak (7) | sane-kodak
s1740 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Scanner 900 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Scanner 923 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Scanner 1500 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Scanner 2500 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Scanner 3500 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Scanner 3510 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Scanner 3520 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Scanner 5500 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Scanner 7500 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Scanner 7520 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Scanner 9500 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Scanner 9520 | SCSI |  | Untested | Please test! | kodak (7) | sane-kodak
Snapshot Photo Scanner 1 | Parport |  | Unsupported | Unsupported. FCC ID HWF96PHS | unsupported (2010-06-09) | ?

### Manufacturer: Komodo

Link(s): http://www.komodo.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
S1200 | SCSI |  | Untested | rebadged Sceptre S1200 | sceptre (1.0-10) | sane-sceptre

### Manufacturer: KONICA MINOLTA

Link(s): http://www.konicaminolta.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
BizHub 162/132 | USB Network |  | Unsupported | Uses a similar protocol as the magicolor 1690MF, according to Ilia Sotnikov. | magicolor (1.0.0) | sane-magicolor
DiMage 1611 | USB Network |  | Unsupported | Uses a similar protocol as the magicolor 1690MF, according to Ilia Sotnikov. | magicolor (1.0.0) | sane-magicolor
DiMAGE Scan Elite 5400 | USB IEEE-1394 | 0x0686/0x400e | Unsupported | Probably unsupported. May work with vuescan. See link for details. | unsupported (2010-06-09) | ?
DiMAGE Scan Elite 5400 2 | USB | 0x132b/0x0012 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
DiMAGE Scan Multi Pro | IEEE-1394 |  | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
Dual Scan III | USB | 0x0686/0x400d | Unsupported | Unsupported. May work with vuescan. See link for details. | unsupported (2010-06-09) | ?
Dual Scan IV | USB | 0x132b/0x000a | Unsupported | Unsupported. Works with vuescan. See link for details. | unsupported (2010-06-09) | ?
magicolor 1690MF | USB Network | 0x132b/0x2089 | Good | Multi-function color laser printer with fax, scanner and network interface | magicolor (1.0.0) | sane-magicolor
magicolor 2480MF | USB Network |  | Unsupported | Uses a different scanning protocol than the magicolor 1690MF | unsupported (2010-06-09) | ?

### Manufacturer: Kyocera

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
FS-1016MFP | USB | 0x0482/0x0335 | Untested | 1 pass, ??? dpi, A4 | avision (Build: 296) | sane-avision

### Manufacturer: LEO

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
LEOScan S3 | SCSI |  | Good | FCC ID LUZFS1130 | leo (1.0-10) | sane-leo

### Manufacturer: Lexmark

Link(s): http://www.lexmark.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
P6250 | USB | 0x043d/0x0097 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
Photo 3150 | USB | 0x043d/0x007d | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
X12xx | USB | 0x043d/0x007d | Good | USB1.1 is OK, USB2.0 needs testing | lexmark (1.0-0) | sane-lexmark
X70 | USB | 0x043d/0x002d | Good | Works, some resolutions fail at 16 bit | gt68xx (1.0-84) | sane-gt68xx
X73 | USB | 0x043d/0x002d | Good | Works, some resolutions fail at 16 bit, same as X70 | gt68xx (1.0-84) | sane-gt68xx
X74 | USB | 0x043d/0x0060 | Good | Supports 75, 150, 300, 600 dpi | lexmark (1.0-0) | sane-lexmark
X75 | USB | 0x043d/0x0060 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
X75 PrinTrio | USB | 0x043d/0x0060 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
X83 | USB | 0x043d/0x003d | Unsupported | Unsupported. GL640. | unsupported (2010-06-09) | ?
X1110 | USB | 0x043d/0x007c | Untested |  | lexmark (1.0-0) | sane-lexmark
X1130 | USB | 0x043d/0x007c | Good | Supports 75, 150, 300, 600 dpi | lexmark (1.0-0) | sane-lexmark
X1140 | USB | 0x043d/0x007c | Untested |  | lexmark (1.0-0) | sane-lexmark
X1150 | USB | 0x043d/0x007c | Good | Supports 75, 150, 300, 600 dpi | lexmark (1.0-0) | sane-lexmark
X1170 | USB | 0x043d/0x007c | Good | Supports 75, 150, 300, 600 dpi | lexmark (1.0-0) | sane-lexmark
X1180 | USB | 0x043d/0x007c | Good |  | lexmark (1.0-0) | sane-lexmark
X1185 | USB | 0x043d/0x007c | Good | Tested with xscanimage. Supports 75, 150, 300, 600, 1200(600x1200) dpi resolutions. Does grayscale or colour scans in the following sizes: wallet, 3x5, 4x6, 5x7, 8x10, letter. | lexmark (1.0-0) | sane-lexmark
X1195 | USB | 0x043d/0x007c | Untested |  | lexmark (1.0-0) | sane-lexmark
X2330 | USB | 0x043d/0x00bb | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
X3450 | USB | 0x043d/0x00f6 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
X5130 | USB | 0x043d/0x0065 | Unsupported | Unsupported. | unsupported (2010-06-09) | ?
X5150 | USB | 0x043d/0x0065 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
X5250 | USB | 0x043d/0x0093 | Unsupported | Unsupported. | unsupported (2010-06-09) | ?
X6170 | USB | 0x043d/0x0072 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
X7170 | USB | 0x043d/0x0098 | Unsupported | Unsupported. See bug #310889 for details. | unsupported (2010-06-09) | ?
X7350 | USB | 0x043d/0x00b8 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
X8350 | USB | 0x043d/0x00b9 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Linotype Hell

Link(s): http://www.heidelberg.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Jade | SCSI |  | Good | OK, SCSI-ID=LinoHell JADE | umax (1.0-41) | sane-umax
Jade | SCSI |  | Good | OK, SCSI-ID=LinoHell Office | umax (1.0-41) | sane-umax
Jade2 | SCSI |  | Good | OK, SCSI-ID=LinoHell Office2 | umax (1.0-41) | sane-umax
Linoscan 1400 | SCSI |  | Good | OK, SCSI-ID=HDM LS4H1S | umax (1.0-41) | sane-umax
Opal | SCSI |  | Untested | support disabled until tested - please contact author | umax (1.0-41) | sane-umax
Opal Ultra | SCSI |  | Untested | support disabled until tested - please contact author | umax (1.0-41) | sane-umax
Opal2 | SCSI |  | Good | OK; SCSI-ID=LinoHell OPAL2 | umax (1.0-41) | sane-umax
Saphir | SCSI |  | Untested | support disabled until tested - please contact author | umax (1.0-41) | sane-umax
Saphir HiRes | SCSI |  | Untested | support disabled until tested - please contact author | umax (1.0-41) | sane-umax
Saphir Ultra | SCSI |  | Untested | support disabled until tested - please contact author | umax (1.0-41) | sane-umax
Saphir Ultra II | SCSI |  | Good | OK, SCSI-ID=Linotype SAPHIR4 | umax (1.0-41) | sane-umax
Saphir2 | SCSI |  | Good | OK, SCSI-ID=LinoHell SAPHIR2 | umax (1.0-41) | sane-umax
Saphir3 | SCSI |  | Good | OK, SCSI-ID=LinoHell SAPHIR3 | umax (1.0-41) | sane-umax

### Manufacturer: Logitech

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
PageScan Color | Parport |  | Unsupported | Most probably unsupported. | unsupported (2010-06-09) | ?
PageScan USB | USB | 0x046d/0x040f | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Medion/Lifetec/Tevion/Cytron

Link(s): http://www.medion.com, http://www.medion.com/, http://www.medion.de/
Comment: Sold by Aldi and Tchibo.

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
LT 9452 | USB | 0x05d8/0x4002 | Good | Similar to Mustek ScanExpress 1200 UB Plus | gt68xx (1.0-84) | sane-gt68xx
MD 4394 | USB | 0x05d8/0x4002 | Good | Product id 0x4002. If you have 0x4003, use artec_eplus48u backend. | gt68xx (1.0-84) | sane-gt68xx
MD 6190 | USB | 0x0461/0x037b | Unsupported | Probably unsupported. There seem to exist two different scanners with that name. See link for details. | unsupported (2010-06-09) | ?
MD 6190 | USB | 0x0461/0x0392 | Unsupported | Probably unsupported. There seem to exist two different scanners with that name. See link for details. | unsupported (2010-06-09) | ?
MD 9458 | USB | 0x05d8/0x4002 | Good | Similar to Artec Ultima 2000 (e+?) | gt68xx (1.0-84) | sane-gt68xx
MD 9806 | Parport (EPP) |  | Good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp
MD 9848 | Parport (EPP) |  | Good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp
MD 40420 | USB | 0x05da/0x3008 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
MD 41260 | USB | 0x0461/0x037b | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
MD 41985 | USB | 0x0461/0x037b | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
MD 42666 | USB | 0x05da/0x3008 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
MD 85264 | USB | 0x08ff/0x2580 | Unsupported | Fingerprint sensor. See link for details. | unsupported (2010-06-09) | ?
MD 90009 | USB | 0x05da/0x30e5 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
MD 90070 | USB | 0x05da/0x3022 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
MD 90090 | USB | 0x05da/0x3022 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
MD/LT 935x | Parport (EPP) |  | Good | 600x1200 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
MD/LT 985x | Parport (EPP) |  | Good | 600x1200 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
MD/LT 9375 | USB | 0x05d8/0x4002 | Untested | Untested, but is reported to have the same ids as the Artec Ultima 2000. Please test. | gt68xx (1.0-84) | sane-gt68xx
MD/LT 9385 | USB | 0x05d8/0x4002 | Good | Similar to Artec Ultima 2000 | gt68xx (1.0-84) | sane-gt68xx
MD/LT 9890 | Parport (EPP) |  | Good | 600x1200 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
MD4394 | USB | 0x05d8/0x4003 | Good | Only scanners with product id 0x4003 will work; try the gt68xx backend, if your scanner has product id 0x4002 | artec_eplus48u (unmaintained) | sane-artec_eplus48u
MD5345 | USB | 0x0461/0x0377 | Good | Has a Primax USB ID | genesys (1.0-63) | sane-genesys
MD6228 | USB | 0x0461/0x0377 | Good | Has a Primax USB ID. Same as MD5345 | genesys (1.0-63) | sane-genesys
MD6471 | USB | 0x0461/0x0377 | Complete | Has a Primax USB ID. Same as MD5345 | genesys (1.0-63) | sane-genesys
MD9693 | USB | 0x05d8/0x4003 | Good |  | artec_eplus48u (unmaintained) | sane-artec_eplus48u
MD9705 | USB | 0x05d8/0x4003 | Good |  | artec_eplus48u (unmaintained) | sane-artec_eplus48u

### Manufacturer: Memorex

Link(s): http://www.artecusa.com/, http://www.memorex.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
6136u | USB | 0x0461/0x0346 | Unsupported | Probably unsupported. | unsupported (2010-06-09) | ?
6142u | USB | 0x0461/0x0347 | Unsupported | Probably unsupported. Same as Visioneer Onetouch 4400. See link for details. | unsupported (2010-06-09) | ?
MaxxScan 6122 | USB Parport | 0x05cb/0x1483 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
MEM 48U | USB | 0x05d8/0x4005 | Good |  | artec_eplus48u (unmaintained) | sane-artec_eplus48u
SCF 9612P | Parport |  | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Micromaxx

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
MM-9851 | Parport (EPP) |  | Good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp

### Manufacturer: Microstar

Link(s): http://www.microstar.de/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
MR 9791 | USB | 0x05d8/0x4003 | Good |  | artec_eplus48u (unmaintained) | sane-artec_eplus48u

### Manufacturer: Microtek

Link(s): http://www.microtek.com/
Comment: Microtek makes a wide variety of devices.

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
ArtixScan 2020 | SCSI |  | Unsupported | Unsupported. Same as Agfa DuoScan T2000XL? | unsupported (2010-06-09) | ?
Artixscan 2500f | SCSI IEEE-1384 |  | Unsupported | Unsupported. Same as Agfa DuoScan T2500? | unsupported (2010-06-09) | ?
ArtixScan 4000tf | USB |  | Unsupported | Unsupported. Uses ALI M5611B. | unsupported (2010-06-09) | ?
ArtixScanDI 2020 | USB | 0x05da/0x202e | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
Color PageWiz | SCSI (Parport) |  | Basic | sheet-fed (preliminary, see mapage) | microtek (0.13.1) | sane-microtek
FilmScan 35 | USB | 0x05e3/0x0120 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
Phantom 330CX | Parport |  | Complete |  | microtek2 (unmaintained) | sane-microtek2
Phantom 636 | SCSI |  | Complete |  | microtek2 (unmaintained) | sane-microtek2
Phantom 636CX | Parport |  | Complete |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker 5 | SCSI |  | Unsupported | Probably unsupported. See link for more details. | unsupported (2010-06-09) | ?
Scanmaker 35 | SCSI |  | Good | slide-scanner | microtek (0.13.1) | sane-microtek
Scanmaker 35t+ | SCSI |  | Good | slide-scanner | microtek (0.13.1) | sane-microtek
Scanmaker 45t | SCSI |  | Good | slide-scanner | microtek (0.13.1) | sane-microtek
ScanMaker 330 | SCSI |  | Basic |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker 336 CX | SCSI |  | Unsupported | Probably unsupported. Seems to be similar to the Microtek 330 CX and is detected by the microtek2 backend. Scanning doesn't seem to work however. | unsupported (2010-06-09) | ?
Scanmaker 600G(S) | SCSI |  | Basic | gray only (see manpage) | microtek (0.13.1) | sane-microtek
Scanmaker 600Z(S) | SCSI |  | Untested |  | microtek (0.13.1) | sane-microtek
ScanMaker 630 | SCSI |  | Basic |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker 636 | SCSI |  | Complete |  | microtek2 (unmaintained) | sane-microtek2
Scanmaker 1850S | SCSI |  | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
ScanMaker 3600 | USB | 0x05da/0x40ff | Basic | works | sm3600 (0.1) | sane-sm3600
ScanMaker 3600 | USB | 0x05da/0x40ca | Basic | works | sm3600 (0.1) | sane-sm3600
ScanMaker 3600 | USB | 0x05da/0x40b3 | Basic | works | sm3600 (0.1) | sane-sm3600
ScanMaker 3630 | USB | 0x0461/0x0347 | Unsupported | Unsupported. Doesn't seem to be compatible to 3600 series, see link. | unsupported (2010-06-09) | ?
ScanMaker 3700 | USB | 0x05da/0x40cb | Basic | works | sm3600 (0.1) | sane-sm3600
ScanMaker 3700 | USB | 0x05da/0x40b8 | Basic | works | sm3600 (0.1) | sane-sm3600
ScanMaker 3750 | USB | 0x05da/0x40dd | Basic | works (told) | sm3600 (0.1) | sane-sm3600
ScanMaker 3800 | USB | 0x05da/0x30ce | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
ScanMaker 3830 | USB | 0x05da/0x30ce | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
ScanMaker 3840 | USB | 0x05da/0x30d4 | Good | 8 and 16 bit, color and grayscale | sm3840 (1.1) | sane-sm3840
ScanMaker 3860 | USB | 0x05da/0x3023 | Unsupported | Unsupported. See link for more details. Appears to be similar to ScanMaker 3880. | unsupported (2010-06-09) | ?
ScanMaker 3880 | USB | 0x05da/0x3021 | Unsupported | Unsupported. SQ113 chip. See link for more details. | unsupported (2010-06-09) | ?
ScanMaker 4600 | USB | 0x05da/0x40c7 | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
ScanMaker 4700 | USB | 0x05da/0x20b4 | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
ScanMaker 4800 | USB | 0x05da/0x30cf | Good | Same hardware as SM3840, different color box | sm3840 (1.1) | sane-sm3840
ScanMaker 4850 | USB | 0x05da/0x30d9 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
ScanMaker 4850 II | USB | 0x05da/0x3008 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
ScanMaker 4900 | USB | 0x05da/0x30b9 | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
ScanMaker 5600 | USB | 0x05da/0x20a7 | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
ScanMaker 5700 | USB | 0x05da/0x20bd | Unsupported | Unsupported. Uses ALI M5615 like the ScanMaker 4700. | unsupported (2010-06-09) | ?
ScanMaker 5800 | USB | 0x05da/0x30d8 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
ScanMaker 5800 | USB | 0x05da/0x3008 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
ScanMaker 5900 | USB | 0x05da/0x30d8 | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
ScanMaker 5950 | USB | 0x05da/0x30d8 | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
ScanMaker 6000 | USB | 0x05da/0x30e5 | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
ScanMaker 6100 | USB | 0x05da/0x30e5 | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
ScanMaker 6400XL | SCSI |  | Complete |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker 6700 | USB IEEE-1394 | 0x05da/0x20c9 | Unsupported | Unsupported. See link. | unsupported (2010-06-09) | ?
ScanMaker 8700 | USB IEEE-1394 | 0x05da/0x20b1 | Unsupported | Unsupported. See link for details. USB vendor and product ids to be checked. | unsupported (2010-06-09) | ?
ScanMaker 9600XL | USB IEEE-1394 | 0x05da/0x20de | Unsupported | Probably unsupported. SCSI seems to work with microtek2 backend. | unsupported (2010-06-09) | ?
ScanMaker 9600XL | SCSI |  | Good | only flatbed mode ? | microtek2 (unmaintained) | sane-microtek2
ScanMaker 9800XL | USB SCSI | 0x05da/0x20de | Unsupported | Partly unsupported. IEEE-1394 works with microtek2 backend. See link. | unsupported (2010-06-09) | ?
ScanMaker 9800XL | IEEE-1394 |  | Minimal | IEEE-1394 seems to work. See link. More reports welcome. | microtek2 (unmaintained) | sane-microtek2
Scanmaker E2 | SCSI |  | Good | 3-pass | microtek (0.13.1) | sane-microtek
Scanmaker E3 | SCSI |  | Good |  | microtek (0.13.1) | sane-microtek
ScanMaker E3plus | SCSI |  | Complete |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker E3plus | Parport |  | Complete |  | microtek2 (unmaintained) | sane-microtek2
Scanmaker E6 | SCSI |  | Good |  | microtek (0.13.1) | sane-microtek
ScanMaker i320 | USB | 0x05da/0x30e6 | Unsupported | Unsupported. See link. | unsupported (2010-06-09) | ?
Scanmaker II | SCSI |  | Good | 3-pass | microtek (0.13.1) | sane-microtek
Scanmaker IIG | SCSI |  | Good | gray only | microtek (0.13.1) | sane-microtek
Scanmaker IIHR | SCSI |  | Good | 3-pass | microtek (0.13.1) | sane-microtek
Scanmaker III | SCSI |  | Good |  | microtek (0.13.1) | sane-microtek
Scanmaker IISP | SCSI |  | Good |  | microtek (0.13.1) | sane-microtek
ScanMaker S400 | USB | 0x05da/0x300b | Unsupported | Unsupported. See link. | unsupported (2010-06-09) | ?
ScanMaker s400 | USB | 0x05da/0x201c | Unsupported | Unsupported. See link. | unsupported (2010-06-09) | ?
ScanMaker V6UPL | USB | 0x05da/0x00b6 | Basic | Sometimes scan speed goes to fast and results look badly smudged. | microtek2 (unmaintained) | sane-microtek2
ScanMaker V6USL | USB | 0x05da/0x80a3 | Complete |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker V6USL | USB | 0x05da/0x00a3 | Complete |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker V6USL | SCSI |  | Complete |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker V300 | Parport |  | Good |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker V300 | SCSI |  | Good |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker V310 | Parport |  | Basic |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker V310 | SCSI |  | Basic |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker V600 | Parport |  | Basic |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker V600 | SCSI |  | Basic |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker X6 | SCSI |  | Complete |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker X6EL | SCSI |  | Basic |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker X6USB | USB | 0x05da/0x0099 | Good |  | microtek2 (unmaintained) | sane-microtek2
ScanMaker X12USL | SCSI |  | Good | only Flatbed mode ? | microtek2 (unmaintained) | sane-microtek2
ScanPort 3000 | USB | 0x04a7/0x0224 | Unsupported | Unsupported. Vendor/Product ids: 0x04a7/0x0224. Realtek RTS8801B?. See link for details. | unsupported (2010-06-09) | ?
SlimScan C3 | Parport |  | Complete |  | microtek2 (unmaintained) | sane-microtek2
SlimScan C6 | USB | 0x05da/0x009a | Complete |  | microtek2 (unmaintained) | sane-microtek2

### Manufacturer: Minolta

Link(s): http://www.minolta.com

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Dimage Scan Dual I | SCSI |  | Basic |  | avision (Build: 296) | sane-avision
Dimage Scan Dual II | USB | 0x0638/0x026a | Good | 1 pass, film-scanner | avision (Build: 296) | sane-avision
Dimage Scan Dual III | USB | 0x0686/0x400d | Good | 1 pass, film-scanner | avision (Build: 296) | sane-avision
Dimage Scan Elite 5400 | USB | 0x0686/0x400e | Good | 1 pass, film-scanner | avision (Build: 296) | sane-avision
Elite II | USB | 0x0686/0x4004 | Untested | 1 pass, film-scanner | avision (Build: 296) | sane-avision
Scan Multi Pro | SCSI |  | Untested |  | avision (Build: 296) | sane-avision

### Manufacturer: Minolta-QMS

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
SC-110 | USB | 0x0638/0x0a15 | Untested |  | avision (Build: 296) | sane-avision
SC-215 | USB | 0x0638/0x0a16 | Good |  | avision (Build: 296) | sane-avision

### Manufacturer: Mitsubishi

Link(s): http://www.mitsubishi.com

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Diamondview 648UT | USB | 0x04a5/0x2022 | Good | Rebadged Benq 320u. | SnapScan (1.4) | sane-snapscan
Diamondview 650U | USB | 0x04a5/0x20b0 | Good | Rebadged Benq 4300. | SnapScan (1.4) | sane-snapscan
MCA-ADFC | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
S600C | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
S1200C | SCSI |  | Untested |  | avision (Build: 296) | sane-avision
SS600 | SCSI |  | Good |  | avision (Build: 296) | sane-avision

### Manufacturer: Mustek

Link(s): http://www.mustek.com/, http://www.mustek.com.tw/, http://www.mustek.de/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
96 CP | Parport (EPP) |  | Good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
600 III EP Plus | Parport (EPP) |  | Good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp
1200 III EP | Parport |  | Unsupported | Probably not supported. quarlewm at jmu dot edu offers to temporarily loan such a scanner to anyone who is interested in writing a driver. | unsupported (2010-06-09) | ?
2400 M | USB |  | Unsupported | Probably unsupported. No details known. | unsupported (2010-06-09) | ?
BearPaw 1200 | USB | 0x0400/0x1001 | Complete | both product versions are supported, see backends' man-page | plustek (0.52) | sane-plustek
BearPaw 1200 | USB | 0x0400/0x1000 | Complete | both product versions are supported, see backends' man-page | plustek (0.52) | sane-plustek
BearPaw 1200 CS | USB | 0x055f/0x021e | Good |  | gt68xx (1.0-84) | sane-gt68xx
BearPaw 1200 CU | USB | 0x05d8/0x4002 | Good |  | gt68xx (1.0-84) | sane-gt68xx
BearPaw 1200 CU Plus | USB | 0x055f/0x021c | Good |  | gt68xx (1.0-84) | sane-gt68xx
BearPaw 1200 CU Plus | USB | 0x055f/0x021b | Good |  | gt68xx (1.0-84) | sane-gt68xx
BearPaw 1200 F | USB | 0x055f/0x0010 | Good | Works upto 600 dpi. No support for TA and ADF yet. | ma1509 (1.0-3) | sane-ma1509
BearPaw 1200 TA | USB | 0x055f/0x021e | Good | Transparency adapter supported | gt68xx (1.0-84) | sane-gt68xx
BearPaw 1248 CU | USB | 0x055f/0x021c | Good | Seems to use the same ids as BearPaw 1200 CU Plus. | gt68xx (1.0-84) | sane-gt68xx
BearPaw 2400 | USB | 0x0400/0x1001 | Complete |  | plustek (0.52) | sane-plustek
BearPaw 2400 CS | USB | 0x055f/0x0218 | Untested | Probably works, reports are welcome | gt68xx (1.0-84) | sane-gt68xx
BearPaw 2400 CS Plus | USB | 0x055f/0x0219 | Good | Works, problems with 12/16 bit modes? | gt68xx (1.0-84) | sane-gt68xx
BearPaw 2400 CU | USB | 0x05d8/0x4002 | Basic | Works, but is slow | gt68xx (1.0-84) | sane-gt68xx
BearPaw 2400 CU Plus | USB | 0x055f/0x021d | Good |  | gt68xx (1.0-84) | sane-gt68xx
BearPaw 2400 TA | USB | 0x055f/0x0218 | Good | Transparency adapter supported | gt68xx (1.0-84) | sane-gt68xx
BearPaw 2400 TA Plus | USB | 0x055f/0x0219 | Good | Transparency adapter supported | gt68xx (1.0-84) | sane-gt68xx
BearPaw 2400 TA Pro | USB | 0x055f/0x0400 | Unsupported | Not supported. May be supported by mustek_usb2 backend later. See link for some information. | unsupported (2010-06-09) | ?
BearPaw 2448 CS Plus | USB | 0x055f/0x021a | Basic | Slow. Same as 2448 TA Plus, but without TA. | gt68xx (1.0-84) | sane-gt68xx
BearPaw 2448 CU Pro | USB | 0x055f/0x0408 | Unsupported | Not supported. May be supported by mustek_usb2 backend later. See link for some information. | unsupported (2010-06-09) | ?
BearPaw 2448 TA Plus | USB | 0x055f/0x021a | Basic | Slow. Transparency adapter supported. Slow. Brightness depends on resolution? | gt68xx (1.0-84) | sane-gt68xx
BearPaw 2448TA Pro | USB | 0x055f/0x0409 | Good |  | mustek_usb2 (1.0-10) | sane-mustek_usb2
BearPaw 4800 TA Pro | USB | 0x055f/0x1000 | Unsupported | Not supported. See link for some information. | unsupported (2010-06-09) | ?
BearPaw 4800 TA Pro II | USB | 0x055f/0x040a | Unsupported | Not supported. May be supported by mustek_usb2 backend later. See link for some information. | unsupported (2010-06-09) | ?
BearPaw 6400 TA Pro | USB | 0x055f/0x040b | Unsupported | Not supported. May be supported by mustek_usb2 backend later. See link for some information. | unsupported (2010-06-09) | ?
Paragon 600 II CD | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
Paragon 600 II ED | Parport |  | Untested | Completely untested. If it's the same as the 600 II EP, it may work. Please contact me if you own such a device. | mustek (1.0-138) | sane-mustek
Paragon 600 II EP | Parport |  | Minimal | Works, however only low resolutions and quality in color mode is bad. | mustek (1.0-138) | sane-mustek
Paragon 600 II N | Proprietary |  | Basic | Resolutions above 300 dpi may cause trouble. | mustek (1.0-138) | sane-mustek
Paragon 800 II EP | Parport |  | Unsupported | Not supported. Maybe similar to 600 II EP (SCSI_over-parport)? In this case it could be supported by the mustek SCSI backend. | unsupported (2010-06-09) | ?
Paragon 800 II SP | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
Paragon 1200 A3 Pro | SCSI |  | Complete | ADF and TA untested. Please contact me if you own such equipment. | mustek (1.0-138) | sane-mustek
Paragon 1200 III SP | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
Paragon 1200 LS | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
Paragon 1200 SP Pro | SCSI |  | Good |  | mustek (1.0-138) | sane-mustek
Paragon MFC-600S | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
Paragon MFC-800S | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
Paragon MFS-1200SP | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
Paragon MFS-6000CX | SCSI |  | Good | 3-pass | mustek (1.0-138) | sane-mustek
Paragon MFS-6000SP | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
Paragon MFS-8000SP | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
Paragon MFS-12000CX | SCSI |  | Good | 3-pass | mustek (1.0-138) | sane-mustek
Paragon MFS-12000SP | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
Plug-n-Scan 2400 M | USB | 0x055f/0x0219 | Good | Works but is slow in high resolutions. Same as BearPaw 2400 CS Plus. | gt68xx (1.0-84) | sane-gt68xx
Plug-n-Scan 2400 MT | USB | 0x055f/0x0219 | Good | Works but is slow in high resolutions. Same as BearPaw 2400 TA Plus. | gt68xx (1.0-84) | sane-gt68xx
ScanExpress 600 CP | Parport (EPP) |  | Good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
ScanExpress 600 CU | USB | 0x055f/0x0002 | Complete |  | mustek_usb (1.0-18) | sane-mustek_usb
ScanExpress 600 SEP | Parport (EPP) |  | Good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp
ScanExpress 600 USB | USB | 0x055f/0x0873 | Unsupported | Unsupported. Programming information is available. | unsupported (2010-06-09) | ?
ScanExpress 1200 CP | Parport (EPP) |  | Good | 600x1200 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
ScanExpress 1200 CP+ | Parport (EPP) |  | Good | 600x1200 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
ScanExpress 1200 CU | USB | 0x055f/0x0001 | Complete |  | mustek_usb (1.0-18) | sane-mustek_usb
ScanExpress 1200 CU Plus | USB | 0x055f/0x0008 | Complete |  | mustek_usb (1.0-18) | sane-mustek_usb
ScanExpress 1200 FS | SCSI |  | Untested | One report that it crashes the computer. SCSI driver issue? Please contact me if you own such a device. | mustek (1.0-138) | sane-mustek
ScanExpress 1200 UB | USB | 0x055f/0x0006 | Complete | For the UB Plus, see gt68xx backend | mustek_usb (1.0-18) | sane-mustek_usb
ScanExpress 1200 UB Plus | USB | 0x05d8/0x4002 | Good |  | gt68xx (1.0-84) | sane-gt68xx
ScanExpress 1200 USB | USB | 0x055f/0x0003 | Unsupported | Unsupported. Programming information is available. | unsupported (2010-06-09) | ?
ScanExpress 1200 USB Plus | USB | 0x055f/0x0007 | Unsupported | Unsupported. | unsupported (2010-06-09) | ?
ScanExpress 1248 UB | USB | 0x055f/0x021f | Complete |  | gt68xx (1.0-84) | sane-gt68xx
ScanExpress 2400 USB | USB | 0x05d8/0x4002 | Minimal | Should be detected but may need some more work in the code. Testers welcome. Please contact me if you own this scanner. | gt68xx (1.0-84) | sane-gt68xx
ScanExpress 6000 P | Parport (EPP) |  | Good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp
ScanExpress 6000SP | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
ScanExpress 12000 P | Parport |  | Unsupported | Not supported. Asic 1505/05. | unsupported (2010-06-09) | ?
ScanExpress 12000SP | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
ScanExpress 12000SP Plus | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
ScanExpress A3 EP | Parport |  | Unsupported | Not supported. Maybe it will be supported by the mustek_pp backend in future. | unsupported (2010-06-09) | ?
ScanExpress A3 SP | SCSI |  | Basic | Please test! | mustek (1.0-138) | sane-mustek
ScanExpress A3 USB | USB | 0x055f/0x0210 | Basic | Still some vertical stripes. | gt68xx (1.0-84) | sane-gt68xx
ScanExpress CardSmart | USB |  | Unsupported | Probably unsupported. USB business card scanner. Maybe works as USB storage device? | unsupported (2010-06-09) | ?
ScanMagic 600 CP | Parport (EPP) |  | Good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
ScanMagic 600 II SP | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
ScanMagic 1200 UB Plus | USB | 0x05d8/0x4002 | Good | Same as ScanExpress 1200 UB Plus | gt68xx (1.0-84) | sane-gt68xx
ScanMagic 4800 P | Parport (EPP) |  | Good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp
ScanMagic 4830S | SCSI |  | Untested | sub model VM3575 | teco2 (1.0-9) | sane-teco2
ScanMagic 9636P | Parport |  | Unsupported | Probably not supported. Same as Mustek 12000 P?. ASIC 1505. | unsupported (2010-06-09) | ?
ScanMagic 9636S | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
ScanMagic 9636S Plus | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek
TwainScan II SP | SCSI |  | Complete |  | mustek (1.0-138) | sane-mustek

### Manufacturer: NeatReceipts

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Mobile Scanner | USB | 0x07b3/0x0462 | Basic | Similar to Plustek OpticSlim M12. | gt68xx (1.0-84) | sane-gt68xx
Scanalizer Professional 2.5 | USB | 0x07b3/0x0412 | Untested | Similar to Plustek OpticSlim M12. Please tell us if this scanner works. | gt68xx (1.0-84) | sane-gt68xx

### Manufacturer: NEC

Link(s): http://www.nevt.co.jp/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
PC-IN500/4C | SCSI |  | Good | PC-IN500/4C was sold only in JAPAN | nec (0.12) | sane-nec
Petiscan | USB | 0x0475/0x0100 | Unsupported | Most probably unsupported. See link for details. Vendor ID is Relisys/Teco. Not known if it is similar to other Relisys/Teco USB scanners. | unsupported (2010-06-09) | ?

### Manufacturer: Network

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Easy Plus 30 Bit | Parport (EPP) |  | Good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp

### Manufacturer: Nikon

Link(s): http://www.nikon.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
AX-110 / Scantouch 110 | SCSI |  | Untested | may work, please test and give feedback | umax (1.0-41) | sane-umax
AX-210 | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Coolscan III | SCSI |  | Complete | Rebadged LS 30? | coolscan3 (1.0.0) | sane-coolscan3
Coolscan V ED | USB | 0x04b0/0x4001 | Minimal | Rebadged LS 50? | coolscan3 (1.0.0) | sane-coolscan3
Coolscan V ED | USB | 0x04b0/0x4001 | Minimal |  | coolscan2 (0.1.8) | sane-coolscan2
Coolspan IV | USB | 0x04b0/0x4000 | Complete | Rebadged LS 40? | coolscan3 (1.0.0) | sane-coolscan3
LS 30 | SCSI |  | Complete |  | coolscan3 (1.0.0) | sane-coolscan3
LS 30 | SCSI |  | Complete | working -- model available to developer | coolscan2 (0.1.8) | sane-coolscan2
LS 40 ED | USB | 0x04b0/0x4000 | Complete |  | coolscan3 (1.0.0) | sane-coolscan3
LS 40 ED | USB | 0x04b0/0x4000 | Complete |  | coolscan2 (0.1.8) | sane-coolscan2
LS 50 ED | USB | 0x04b0/0x4001 | Minimal |  | coolscan3 (1.0.0) | sane-coolscan3
LS 50 ED | USB | 0x04b0/0x4001 | Minimal |  | coolscan2 (0.1.8) | sane-coolscan2
LS 2000 | SCSI |  | Good |  | coolscan3 (1.0.0) | sane-coolscan3
LS 2000 | SCSI |  | Good |  | coolscan2 (0.1.8) | sane-coolscan2
LS 4000 ED | IEEE-1394 |  | Good | needs linux kernel 2.4.19 or later | coolscan3 (1.0.0) | sane-coolscan3
LS 4000 ED | IEEE-1394 |  | Good | needs linux kernel 2.4.19 or later | coolscan2 (0.1.8) | sane-coolscan2
LS 8000 ED | IEEE-1394 |  | Good | needs linux kernel 2.4.19 or later | coolscan3 (1.0.0) | sane-coolscan3
LS 8000 ED | IEEE-1394 |  | Good | needs linux kernel 2.4.19 or later | coolscan2 (0.1.8) | sane-coolscan2
LS-20 | SCSI |  | Basic | The LS-20 has been replaced by the LS-30 | coolscan (0.4.3) | sane-coolscan
LS-30 | SCSI |  | Basic | alpha: only 24/30 bit RGB + 32/40 bit RGBI | coolscan (0.4.3) | sane-coolscan
LS-1000 | SCSI |  | Basic | Doesn't support gamma correction | coolscan (0.4.3) | sane-coolscan
LS-2000 | SCSI |  | Basic | alpha: only 24/36 bit + RGB 32/48 bit RGBI | coolscan (0.4.3) | sane-coolscan
LS-9000 ED | IEEE-1394 |  | Unsupported | Probably not supported. See link for details. Possibly similar to LS-8000 ED. | unsupported (2010-06-09) | ?
Super Coolscan LS-5000 ED | USB | 0x04b0/0x4002 | Untested | May work, similar to LS 50 ED, but untested. Please tell us if it works. | coolscan3 (1.0.0) | sane-coolscan3
Super Coolscan LS-5000 ED | USB | 0x04b0/0x4002 | Untested | May work, similar to LS 50 ED, but untested. Please tell us if it works. | coolscan2 (0.1.8) | sane-coolscan2

### Manufacturer: Nortek

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
MyScan 1200 | USB | 0x07b3/0x040b | Untested | Untested. Please test. Similar to Plustek OpticPro S12? | gt68xx (1.0-84) | sane-gt68xx

### Manufacturer: OKI

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
S700 Scancopier | USB | 0x0638/0x0a16 | Good | 1 pass, 600 dpi, A4 | avision (Build: 296) | sane-avision

### Manufacturer: Olivetti

Link(s): http://www.olivetti.com

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Job-Jet M400 | USB | 0x0b3c/0xa880 | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Olympus

Link(s): http://www.olympus.com

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
ES-10P | Parport |  | Unsupported |  | unsupported (2010-06-09) | ?
ES-10S | SCSI |  | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Optoelectronics

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Barcode scanner | USB | 0x065a/0x0001 | Unsupported | Probably not supported. | unsupported (2010-06-09) | ?

### Manufacturer: Optrox

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
PhotoMaker 3C | Parport |  | Unsupported |  | unsupported (2010-06-09) | ?
PhotoMaker 3E | Parport |  | Unsupported |  | unsupported (2010-06-09) | ?
PhotoMaker 3F | Proprietary |  | Unsupported | Special ISA card | unsupported (2010-06-09) | ?
PhotoMaker 3S | Parport |  | Unsupported |  | unsupported (2010-06-09) | ?
PhotoMaker 6E | Parport |  | Unsupported |  | unsupported (2010-06-09) | ?
PhotoMaker 6F | Proprietary |  | Unsupported | Special ISA card | unsupported (2010-06-09) | ?

### Manufacturer: Packard Bell

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Diamond 1200 | USB | 0x05d8/0x4002 | Good | Similar to Mustek BearPaw 1200 (Plus) | gt68xx (1.0-84) | sane-gt68xx
Diamond 1200 Plus | USB | 0x055f/0x021b | Good | Similar to Mustek BearPaw 1200 Plus | gt68xx (1.0-84) | sane-gt68xx
Diamond 1200 Plus | USB | 0x055f/0x021c | Good | Similar to Mustek BearPaw 1200 Plus | gt68xx (1.0-84) | sane-gt68xx
Diamond 2450 | USB | 0x055f/0x0219 | Good |  | gt68xx (1.0-84) | sane-gt68xx

### Manufacturer: Panasonic

Link(s): http://www.panasonic.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
KV-S1020C | USB | 0x04da/0x1007 | Good |  | kvs1025 (unmaintained) | sane-kvs1025
KV-S1025C | USB | 0x04da/0x1006 | Good |  | kvs1025 (unmaintained) | sane-kvs1025
KV-S1045C | USB | 0x04da/0x1010 | Good |  | kvs1025 (unmaintained) | sane-kvs1025
KV-S2025C | SCSI |  | Minimal | no color, no high resolution, no automatic cropping | matsushita (1.0-7) | sane-matsushita
KV-S2026C | USB SCSI | 0x04da/0x1000 | Untested |  | kvs20xx (unmaintained) | sane-kvs20xx
KV-S2028C | USB | 0x04da/0x100a | Untested |  | kvs20xx (unmaintained) | sane-kvs20xx
KV-S2045C | SCSI |  | Minimal | no color, no high resolution, no automatic cropping | matsushita (1.0-7) | sane-matsushita
KV-S2046C | USB SCSI | 0x04da/0x1001 | Untested |  | kvs20xx (unmaintained) | sane-kvs20xx
KV-S2048C | USB | 0x04da/0x1009 | Untested |  | kvs20xx (unmaintained) | sane-kvs20xx
KV-S2055L | SCSI |  | Unsupported | might be supported by matsushita backend. | unsupported (2010-06-09) | ?
KV-S2055W | USB SCSI |  | Unsupported | might be supported by matsushita backend. | unsupported (2010-06-09) | ?
KV-S2065L | SCSI |  | Minimal | no color, no high resolution, no automatic cropping | matsushita (1.0-7) | sane-matsushita
KV-S2065W | SCSI |  | Unsupported | might be supported by matsushita backend. | unsupported (2010-06-09) | ?
KV-S3065CL | USB SCSI |  | Unsupported | might be supported by matsushita backend. | unsupported (2010-06-09) | ?
KV-S3065CW | USB SCSI |  | Unsupported | might be supported by matsushita backend. | unsupported (2010-06-09) | ?
KV-S3085 | USB SCSI |  | Unsupported | might be supported by matsushita backend. | unsupported (2010-06-09) | ?
KV-S3105C | USB SCSI |  | Unsupported | might be supported by matsushita backend. See http://code.google.com/p/kvss905c/ for a standalone scanning tool. | unsupported (2010-06-09) | ?
KV-S4065C | USB | 0x04da/0x100d | Untested |  | kvs40xx (unmaintained) | sane-kvs40xx
KV-S4085C | USB | 0x04da/0x100c | Untested |  | kvs40xx (unmaintained) | sane-kvs40xx
KV-S6040W | SCSI |  | Unsupported | might be supported by matsushita backend. | unsupported (2010-06-09) | ?
KV-S6045W | SCSI |  | Unsupported | might be supported by matsushita backend. | unsupported (2010-06-09) | ?
KV-S6050W | SCSI |  | Unsupported | might be supported by matsushita backend. | unsupported (2010-06-09) | ?
KV-S6055W | SCSI |  | Unsupported | might be supported by matsushita backend. | unsupported (2010-06-09) | ?
KV-S7065C | USB SCSI |  | Unsupported | might be supported by matsushita backend. | unsupported (2010-06-09) | ?
KV-S7075C | USB | 0x04da/0x100e | Untested |  | kvs40xx (unmaintained) | sane-kvs40xx
KV-SS25 | SCSI |  | Complete |  | matsushita (1.0-7) | sane-matsushita
KV-SS25D | SCSI |  | Complete |  | matsushita (1.0-7) | sane-matsushita
KV-SS50 | SCSI |  | Untested |  | matsushita (1.0-7) | sane-matsushita
KV-SS50EX | SCSI |  | Untested |  | matsushita (1.0-7) | sane-matsushita
KV-SS55 | SCSI |  | Untested |  | matsushita (1.0-7) | sane-matsushita
KV-SS55EX | SCSI |  | Minimal | no color, no high resolution, no automatic cropping | matsushita (1.0-7) | sane-matsushita
KV-SS080 | USB | 0x04da/0x100f | Complete | All resolution and mode supported, calibration is available. Support sponsored by cncsolutions (http://www.cncsolutions.com.br) | genesys (1.0-63) | sane-genesys
KV-SS850 | SCSI |  | Untested |  | matsushita (1.0-7) | sane-matsushita
KV-SS855 | SCSI |  | Untested |  | matsushita (1.0-7) | sane-matsushita
KV-SS905C | SCSI |  | Unsupported | might be supported by matsushita backend. See http://code.google.com/p/kvss905c/ for a standalone scanning tool. | unsupported (2010-06-09) | ?

### Manufacturer: Pentax

Link(s): http://www.pentaxtech.com/, http://mobilesolutions.brother-usa.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
DSmobile 600 | USB | 0x04f9/0x2038 | Good | All resolution and mode supported, calibration is available | genesys (1.0-63) | sane-genesys
DSmobile 600 | USB | 0x0a17/0x3210 | Good | All resolution and mode supported, calibration is available | genesys (1.0-63) | sane-genesys
DSmobile USB | USB | 0x0a82/0x2000 | Unsupported | Probably not supported. Some information is available. | unsupported (2010-06-09) | ?

### Manufacturer: PIE

Link(s): http://www.scanace.com/
Comment: Pacific Image Electronics

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
PF3650 Pro3 Film Scanner | USB IEEE-1394 | 0x05e3/0x0143 | Unsupported | Not supported. See link for details. | unsupported (2010-06-09) | ?
Powerslide 3600 | USB IEEE-1394 | 0x05e3/0x0142 | Unsupported | Probably unsupported. Film scanner that can scan directly from the magazine. | unsupported (2010-06-09) | ?
Primefilm 1800u | USB | 0x05e3/0x0120 | Unsupported | Not supported. See link for details. | unsupported (2010-06-09) | ?
Primefilm 2700 | USB |  | Unsupported |  | unsupported (2010-06-09) | ?
Primefilm 3600PRO | USB IEEE-1394 |  | Unsupported | Probably not supported. | unsupported (2010-06-09) | ?
ScanAce 630S | SCSI |  | Untested |  | pie (1.0) | sane-pie
ScanAce 636S | SCSI |  | Untested |  | pie (1.0) | sane-pie
ScanAce 1230S | SCSI |  | Good |  | pie (1.0) | sane-pie
ScanAce 1236S | SCSI |  | Good |  | pie (1.0) | sane-pie
ScanAce II | SCSI |  | Untested |  | pie (1.0) | sane-pie
ScanAce II Plus | SCSI |  | Untested |  | pie (1.0) | sane-pie
ScanAce III | SCSI |  | Good |  | pie (1.0) | sane-pie
ScanAce III Plus | SCSI |  | Untested |  | pie (1.0) | sane-pie
ScanAce Plus | SCSI |  | Untested |  | pie (1.0) | sane-pie
ScanAce ScanMedia | SCSI |  | Untested |  | pie (1.0) | sane-pie
ScanAce ScanMedia II | SCSI |  | Untested |  | pie (1.0) | sane-pie
ScanAce V | SCSI |  | Untested |  | pie (1.0) | sane-pie

### Manufacturer: PIOTECH

Link(s): http://www.image-land.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Splendeur 3024 | SCSI |  | Good | sub model VM3552 | teco3 (1.0-1) | sane-teco3

### Manufacturer: PLANon

Link(s): http://www.planon.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
DocuPen (DPEN-BW) | USB |  | Unsupported | Probably not supported. No details known. | unsupported (2010-06-09) | ?
DocuPen R700 | USB | 0x10c4/0xea60 | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
DocuPen RC800 | USB |  | Unsupported | Probably not supported. No details known. | unsupported (2010-06-09) | ?

### Manufacturer: Plustek

Link(s): http://www.plustek.com/, http://www.plustek.de/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Iriscan Express 2 | USB | 0x07b3/0x045f | Complete | Works up to 1200 dpi. Calibration with external calibration sheet supported | gt68xx (1.0-84) | sane-gt68xx
OptiCard 600+ | USB |  | Unsupported | Business card reader. No further information available. | unsupported (2010-06-09) | ?
OpticBook 3600 | USB | 0x07b3/0x0900 | Basic | Has a Primax USB ID | genesys (1.0-63) | sane-genesys
OpticFilm 7200 | USB | 0x07b3/0x0807 | Unsupported | GL842 based, maybe to be added to genesys backend | unsupported (2010-06-09) | ?
OpticFilm 7200i | USB | 0x07b3/0x0c04 | Unsupported | GL843 based, maybe to be added to genesys backend | unsupported (2010-06-09) | ?
OpticPro 600P/6000P | Parport (SPP, EPP) |  | Complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 1212U | USB | 0x07b3/0x0001 | Basic |  | u12 (0.02) | sane-u12
OpticPro 1236P | Parport (SPP, EPP) |  | Complete | reported as OpticPro 12000P/96000P | plustek_pp (0.43) | sane-plustek_pp
OpticPro 1248U | USB | 0x07b3/0x0401 | Good |  | gt68xx (1.0-84) | sane-gt68xx
OpticPro 1248U | USB | 0x07b3/0x0400 | Good |  | gt68xx (1.0-84) | sane-gt68xx
OpticPro 2400SP | SCSI |  | Untested | sub model VM3552 | teco3 (1.0-1) | sane-teco3
OpticPro 4800P | Parport (SPP, EPP) |  | Complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 4830P | Parport (SPP, EPP) |  | Complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 4831P | Parport (SPP, EPP) |  | Complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 9600P | Parport (SPP, EPP) |  | Complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 9630P | Parport (SPP, EPP) |  | Complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 9630PL | Parport (SPP, EPP) |  | Complete | use driver-switch mov=1 | plustek_pp (0.43) | sane-plustek_pp
OpticPro 9636P | Parport (SPP, EPP) |  | Complete | use driver-switch mov=4 | plustek_pp (0.43) | sane-plustek_pp
OpticPro 9636P+/Turbo | Parport (SPP, EPP) |  | Complete | use driver-switch mov=3 | plustek_pp (0.43) | sane-plustek_pp
OpticPro 9636T | Parport (SPP, EPP) |  | Complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 12000P/96000P | Parport (SPP, EPP) |  | Complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 12000T | Parport (SPP, EPP) |  | Complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 19200S | SCSI |  | Complete | rebadged Artec AM12S | artec (unmaintained) | sane-artec
OpticPro A3U | USB |  | Unsupported | Uses Plustek ASIC P99002 | unsupported (2010-06-09) | ?
OpticPro AI3 | Parport (SPP, EPP) |  | Basic | use driver-switch mov=5, poor picture quality | plustek_pp (0.43) | sane-plustek_pp
OpticPro P8 | Parport |  | Untested |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro P12 | Parport (SPP, EPP) |  | Complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro PT12 | Parport (SPP, EPP) |  | Complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro S6 | USB |  | Unsupported | Uses RealTek chipset (RTL8801D) | unsupported (2010-06-09) | ?
OpticPro S12 | USB | 0x07b3/0x0600 | Unsupported | Product id 0x0600 is unsupported but may be supported by the genesys backend in future. Product id 0x040b is supported by the gt68xx backend. | unsupported (2010-06-09) | ?
OpticPro S12 | USB | 0x07b3/0x040b | Good | Product ID 0x040b only. | gt68xx (1.0-84) | sane-gt68xx
OpticPro S24 | USB | 0x07b3/0x0601 | Unsupported | Product id 0x0601 is unsupported but may be supported by the genesys backend in future /GL646). Product id 0x040e is supported by the gt68xx backend. | unsupported (2010-06-09) | ?
OpticPro S24 | USB | 0x07b3/0x040e | Good | Product ID 0x040e only. Is reported to work. | gt68xx (1.0-84) | sane-gt68xx
OpticPro S28 | USB | 0x07b3/0x0801 | Unsupported | GL841 based, to be added to genesys backend | unsupported (2010-06-09) | ?
OpticPro ST12 | USB | 0x07b3/0x0600 | Unsupported | Product id 0x0600 is unsupported but may be supported by the genesys backend in future. Product id 0x040b is supported by the gt68xx backend. | unsupported (2010-06-09) | ?
OpticPro ST12 | USB | 0x07b3/0x040b | Untested | Product ID 0x040b only. Needs testing. Transparency adapter completely untested. Please contact me if you own such a scanner. | gt68xx (1.0-84) | sane-gt68xx
OpticPro ST16 | USB | 0x07b3/0x0600 | Unsupported | GL646 based, to be added to genesys backend | unsupported (2010-06-09) | ?
OpticPro ST24 | USB | 0x07b3/0x0601 | Unsupported | GL646 based, to be added to genesys backend | unsupported (2010-06-09) | ?
OpticPro ST28 | USB | 0x07b3/0x0802 | Unsupported | GL841 based, to be added to genesys backend | unsupported (2010-06-09) | ?
OpticPro ST28 | USB | 0x07b3/0x0801 | Unsupported | GL841 based, to be added to genesys backend | unsupported (2010-06-09) | ?
OpticPro ST48 | USB | 0x07b3/0x0800 | Unsupported | GL841 based, to be added to genesys backend | unsupported (2010-06-09) | ?
OpticPro ST64 | USB | 0x07b3/0x0c00 | Unsupported | GL843 based, maybe to be added to genesys backend | unsupported (2010-06-09) | ?
OpticPro ST64+ | USB | 0x07b3/0x0c03 | Unsupported | GL843 based. See link for more details. | unsupported (2010-06-09) | ?
OpticPro U12 | USB | 0x07b3/0x0001 | Basic | Note: Only devices with product ID 0x0001 are supported! | u12 (0.02) | sane-u12
OpticPro U12 | USB | 0x07b3/0x0010 | Complete | NOTE: Devices with product ID 0x0001 are not supported! | plustek (0.52) | sane-plustek
OpticPro U16B | USB | 0x07b3/0x0402 | Good |  | gt68xx (1.0-84) | sane-gt68xx
OpticPro U16B+ | USB | 0x07b3/0x0403 | Good |  | gt68xx (1.0-84) | sane-gt68xx
OpticPro U24 | USB | 0x07b3/0x0015 | Complete |  | plustek (0.52) | sane-plustek
OpticPro U24 | USB | 0x07b3/0x0011 | Complete |  | plustek (0.52) | sane-plustek
OpticPro UA18 | USB |  | Unsupported | Probably LM983x based. | unsupported (2010-06-09) | ?
OpticPro UT12 | USB | 0x07b3/0x0001 | Basic | Note: Only devices with product ID 0x0001 are supported! | u12 (0.02) | sane-u12
OpticPro UT12 | USB | 0x07b3/0x0017 | Complete | Note: Devices with product ID 0x0001 are not supported! | plustek (0.52) | sane-plustek
OpticPro UT12 | USB | 0x07b3/0x0013 | Complete |  | plustek (0.52) | sane-plustek
OpticPro UT16 | USB | 0x07b3/0x0017 | Complete |  | plustek (0.52) | sane-plustek
OpticPro UT16B | USB | 0x07b3/0x0403 | Untested | Probably works. Transparency adapter not supported yet. Please contact me if you own such a device. | gt68xx (1.0-84) | sane-gt68xx
OpticPro UT24 | USB | 0x07b3/0x0017 | Complete |  | plustek (0.52) | sane-plustek
OpticSlim 500 | USB | 0x07b3/0x0458 | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
OpticSlim 1200 | USB | 0x07b3/0x0413 | Good |  | gt68xx (1.0-84) | sane-gt68xx
OpticSlim 2400 | USB | 0x07b3/0x0422 | Good | Works up to 1200 dpi. | gt68xx (1.0-84) | sane-gt68xx
OpticSlim 2400 plus | USB | 0x07b3/0x0454 | Good | Same as OpticSlim 2400. | gt68xx (1.0-84) | sane-gt68xx
OpticSlim 2420 | USB | 0x07b3/0x0806 | Unsupported | GL841 based, to be added to genesys backend | unsupported (2010-06-09) | ?
OpticSlim 2420+ | USB | 0x07b3/0x0914 | Unsupported | GL841 based, to be added to genesys backend | unsupported (2010-06-09) | ?
OpticSlim M12 | USB | 0x07b3/0x0412 | Complete | Works up to 1200 dpi. Calibration with external calibration sheet supported | gt68xx (1.0-84) | sane-gt68xx
OpticWorks 2000 | Parport |  | Unsupported | Multifunction device. No further information available. | unsupported (2010-06-09) | ?
PL 806 | USB | 0x07b3/0x0c0c | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
ScanCopy 115 | USB | 0x07b3/0x081c | Unsupported | GL841 based, to be added to genesys backend | unsupported (2010-06-09) | ?
SmartOffice PL 812 | USB | 0x07b3/0x0c0d | Unsupported | Unsupported. See link for more details. | unsupported (2010-06-09) | ?
Spectra ADF | Proprietary |  | Unsupported | Unsupported. Uses proprietary ISA card that also provides power and is labelled GPS-1 PAGE-A from Taiwan. Other labels on the scanner include ADF Color Scanner and SF600AS. Maybe the same as the IBM ADF Color Scanner? | unsupported (2010-06-09) | ?
Umax AstraScan 4750 | USB | 0x07b3/0x0802 | Unsupported | GL841 based, to be added to genesys backend, rebadged Plustek ST28 | unsupported (2010-06-09) | ?
Unknown Plustek Device | USB | 0x07b3/0x0016 | Unsupported | Probably unsupported. Scanner name not known yet. | unsupported (2010-06-09) | ?
Unknown Plustek Device | USB | 0x07b3/0x0014 | Unsupported | Probably unsupported. Scanner name not known yet. | unsupported (2010-06-09) | ?
Unknown Plustek Device | USB | 0x07b3/0x0012 | Unsupported | Probably unsupported. Scanner name not known yet. | unsupported (2010-06-09) | ?
Unknown Plustek Device | USB | 0x07b3/0x000f | Unsupported | Probably unsupported. Scanner name not known yet. | unsupported (2010-06-09) | ?
Unknown Plustek Device | USB | 0x07b3/0x0007 | Unsupported | Probably unsupported. Scanner name not known yet. | unsupported (2010-06-09) | ?
Unknown Plustek Device | USB | 0x07b3/0x0005 | Unsupported | Probably unsupported. Scanner name not known yet. | unsupported (2010-06-09) | ?

### Manufacturer: Portable Peripheral Co., Ltd.

Link(s): http://www.pandp.com.tw/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Q-Scan USB001 (A4 portable scanner) | USB | 0x0a53/0x1000 | Complete |  | plustek (0.52) | sane-plustek
Q-Scan USB201 (A6 portable scanner) | USB | 0x0a53/0x2000 | Good |  | plustek (0.52) | sane-plustek

### Manufacturer: Primax

Link(s): http://www.primax.nl/, http://www.primax.com.tw

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Colorado 600U | USB | 0x0461/0x0341 | Unsupported | Not supported. Some information is available. | unsupported (2010-06-09) | ?
Colorado 1200p | Parport |  | Unsupported | Unsupported by SANE. But is reported to partly work with pxscan. See link. | unsupported (2010-06-09) | ?
Colorado 1200u | USB | 0x0461/0x0361 | Unsupported | Probably unsupported. No details known. | unsupported (2010-06-09) | ?
Colorado 4800 | Parport (SPP, EPP) |  | Untested | same as OpticPro 4800P | plustek_pp (0.43) | sane-plustek_pp
Colorado Direct 600 | Parport |  | Unsupported | Not supported. However, a stand-alone program is available. | unsupported (2010-06-09) | ?
Colorado Direct 9600 | Parport |  | Unsupported | Not supported. However, a stand-alone program is available. | unsupported (2010-06-09) | ?
Colorado USB 9600 | USB | 0x0461/0x0340 | Unsupported | Not supported. See link for details. | unsupported (2010-06-09) | ?
Compact 4800 Direct | Parport (SPP, EPP) |  | Complete | use driver-switch mov=2 | plustek_pp (0.43) | sane-plustek_pp
Compact 4800 Direct-30 | Parport (SPP, EPP) |  | Complete | same as OpticPro 4830P, use driver-switch mov=7 | plustek_pp (0.43) | sane-plustek_pp
Compact 4800 SCSI | SCSI |  | Complete | Mustek 600 II CD compatible | mustek (1.0-138) | sane-mustek
Compact 9600 Direct-30 | Parport (SPP, EPP) |  | Complete | same as OpticPro 9630P | plustek_pp (0.43) | sane-plustek_pp
G2-300 | USB | 0x0461/0x0300 | Unsupported | Probably unsupported. No details known. | unsupported (2010-06-09) | ?
G2-300 #2 | USB | 0x0461/0x0302 | Unsupported | Probably unsupported. No details known. | unsupported (2010-06-09) | ?
G2-600 | USB | 0x0461/0x0380 | Unsupported | Probably unsupported. No details known. | unsupported (2010-06-09) | ?
G2-600 #2 | USB | 0x0461/0x0382 | Unsupported | Probably unsupported. No details known. | unsupported (2010-06-09) | ?
G2E-300 | USB | 0x0461/0x0301 | Unsupported | Probably unsupported. No details known. | unsupported (2010-06-09) | ?
G2E-300 #2 | USB | 0x0461/0x0303 | Unsupported | Probably unsupported. No details known. | unsupported (2010-06-09) | ?
G2E-600 | USB | 0x0461/0x0383 | Unsupported | Probably unsupported. No details known. | unsupported (2010-06-09) | ?
Jewel 4800 | SCSI |  | Good | sub model VM356A | teco2 (1.0-9) | sane-teco2
OneTouch 5300 | Parport |  | Unsupported | Not supported. | unsupported (2010-06-09) | ?
Onetouch 8920 | USB | 0x0461/0x0371 | Unsupported | Not supported. Look similar to Visioneer Onetouch 8920 (same USB product id). | unsupported (2010-06-09) | ?
PagePartner | Parport (EPP/ECP) |  | Basic | Sheetfed scanner, work in gray and color, but uncalibrated scans | p5 (1) | sane-p5
Primascan Colorado 2600u | USB | 0x0461/0x0347 | Unsupported | Unsupported. Same as Visioneer Onetouch 4400. See link for details. | unsupported (2010-06-09) | ?
Profi 9600 | SCSI |  | Basic | sub model VM6575 | teco2 (1.0-9) | sane-teco2
Profi 19200 | SCSI |  | Good | sub model VM6586 | teco2 (1.0-9) | sane-teco2
ReadyScan 636i | USB | 0x0461/0x0381 | Unsupported | Probably unsupported. No details known. | unsupported (2010-06-09) | ?
Slim-Line 1200 | USB |  | Unsupported | Maybe GL646. Maybe similar to Medion MD 6228? | unsupported (2010-06-09) | ?

### Manufacturer: Prolink

Link(s): http://www.fida.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Winscan Pro 2000 | USB Parport |  | Unsupported | Not supported. No further information available. | unsupported (2010-06-09) | ?
Winscan Pro 2448U | USB | 0x06dc/0x0014 | Unsupported | Not supported. Some information is available. RealTek RTS8801. | unsupported (2010-06-09) | ?

### Manufacturer: Quato

Link(s): http://www.quato.de/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
X-Finity | SCSI |  | Unsupported | Probably not supported. No details yet. Originally manufactured by PFU? | unsupported (2010-06-09) | ?
X-Finity Ultra | USB IEEE-1394 |  | Unsupported | Probably not supported. No details yet. | unsupported (2010-06-09) | ?

### Manufacturer: Reflecta

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
DigitDia 3600 | USB IEEE-1394 | 0x05e3/0x0142 | Unsupported | Film scanner that can scan directly from the magazine. | unsupported (2010-06-09) | ?
iScan 1800 | USB | 0x05e3/0x0120 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
ProScan 4000 | USB IEEE-1394 | 0x05e3/0x0143 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Relisys

Link(s): http://www.relisys.com/, http://www.tecoimage.com.tw/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
APOLLO Express 3 | SCSI |  | Basic | sub model VM356A | teco2 (1.0-9) | sane-teco2
APOLLO Express 6 | SCSI |  | Good | sub model VM6565 | teco2 (1.0-9) | sane-teco2
AVEC 2400 | SCSI |  | Complete | sub model VM3520 | teco1 (1.0-10) | sane-teco1
AVEC 2412 | SCSI |  | Complete | sub model VM3520+ | teco1 (1.0-10) | sane-teco1
AVEC 4800 | SCSI |  | Untested | sub model VM4530 | teco1 (1.0-10) | sane-teco1
AVEC 4816 | SCSI |  | Untested | sub model VM4530+ | teco1 (1.0-10) | sane-teco1
AVEC II E3 | Parport |  | Unsupported | Parport version of AVEC II S3?. See bug #304992 for details | unsupported (2010-06-09) | ?
AVEC II S3 | SCSI |  | Good | sub model VM3564 | teco2 (1.0-9) | sane-teco2
AVEC Super 3 | SCSI |  | Untested | sub model VM3575 | teco2 (1.0-9) | sane-teco2
Eclipse 1200U | USB | 0x0475/0x0103 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
Episode | USB | 0x0475/0x0103 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?
Infinity Scorpio | SCSI |  | Good | sub model VM3552 | teco3 (1.0-1) | sane-teco3
RELI 2400 | SCSI |  | Untested | sub model VM3530 | teco1 (1.0-10) | sane-teco1
RELI 2412 | SCSI |  | Complete | sub model VM3530+ | teco1 (1.0-10) | sane-teco1
RELI 4816 | SCSI |  | Complete | sub model VM4540 | teco1 (1.0-10) | sane-teco1
RELI 4830 | SCSI |  | Good | sub model VM4542 | teco1 (1.0-10) | sane-teco1
RELI 9600 | SCSI |  | Untested | sub model VM6530 | teco1 (1.0-10) | sane-teco1
RELI 9612 | SCSI |  | Untested | sub model VM6530* | teco1 (1.0-10) | sane-teco1
RELI 9624 | SCSI |  | Untested | sub model VM6530+ | teco1 (1.0-10) | sane-teco1
RELI 9630 | SCSI |  | Untested | sub model VM6540 | teco1 (1.0-10) | sane-teco1
RELI DS6 | SCSI |  | Untested | sub model VM3420 | teco1 (1.0-10) | sane-teco1
RELI DS15 | SCSI |  | Untested | sub model VM3440 | teco1 (1.0-10) | sane-teco1
SCORPIO Pro | SCSI |  | Good | sub model VM6575 | teco2 (1.0-9) | sane-teco2
SCORPIO Pro-S | SCSI |  | Untested | sub model VM6586 | teco2 (1.0-9) | sane-teco2
SCORPIO Super 3 | SCSI |  | Good | sub model VM3575 | teco2 (1.0-9) | sane-teco2
Scorpio Ultra 3 | USB | 0x0475/0x0210 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: RevScan

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
19200i | USB | 0x07b3/0x0400 | Good | Similar to Plustek OpticPro 1248U | gt68xx (1.0-84) | sane-gt68xx
RevScan Orange R48Ti | USB | 0x07b3/0x0001 | Basic | Rebadged Plustek OpticPro UT12 | u12 (0.02) | sane-u12

### Manufacturer: Ricoh

Link(s): http://www.ricoh.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
IS-410 | SCSI |  | Untested | Untested, please report! | ibm (1.0-4) | sane-ibm
IS-410 | SCSI |  | Untested | Untested, please report! | hs2p (1.00) | sane-hs2p
IS-420 | SCSI |  | Basic | Works at least in flatbed mode. | ibm (1.0-4) | sane-ibm
IS-430 | SCSI |  | Untested | Untested, please report! | ibm (1.0-4) | sane-ibm
IS-430 | SCSI |  | Untested | Untested, please report! | hs2p (1.00) | sane-hs2p
IS450 | SCSI |  | Complete | All major scanning-related features are supported (except for IPU). Certain non-scanning features, such as those related to scanner maintenance, are not supported. Such features would be better implemented in a separate stand-alone tool. For instance, if you replace the ADF Unit, you must recalibrate the scanner optics using a Ricoh Test Sheet and reset the E^2PROM registers. Reports are welcome. | hs2p (1.00) | sane-hs2p
Ricoh IS50 | SCSI |  | Basic |  | ricoh (unmaintained) | sane-ricoh
Ricoh IS60 | SCSI |  | Basic |  | ricoh (unmaintained) | sane-ricoh

### Manufacturer: Samsung

Link(s): http://www.samsung.com

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
C460 | USB | 0x04e8/0x3468 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-2160 | USB | 0x04e8/0x3425 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-3160 | USB | 0x04e8/0x341c | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-3170fn (CLX-3170 Series) | USB | 0x04e8/0x342a | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-3175FW | USB | 0x04e8/0x342a | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-3185 | USB | 0x04e8/0x343d | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-3300 Series | USB | 0x04e8/0x3456 | Basic |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-4190 | USB | 0x04e8/0x345a | Minimal |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-6200 | USB | 0x04e8/0x3427 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-6220 | USB | 0x04e8/0x343a | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-6240 | USB | 0x04e8/0x3428 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-6250 | USB | 0x04e8/0x343b | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-6260 | USB | 0x04e8/0x3455 | Minimal |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-8380 | USB | 0x04e8/0x3421 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-8385 | USB | 0x04e8/0x3439 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-8385X | USB | 0x04e8/0x3444 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
CLX-8540 | USB | 0x04e8/0x343f | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
M267x 287x Series | USB | 0x04e8/0x3461 | Unsupported |  | xerox_mfp (1.0-13) | sane-xerox_mfp
M337x 387x 407x Series | USB | 0x04e8/0x3460 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
MFP-65x | USB | 0x04e8/0x3435 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
MFP-560 | USB | 0x04e8/0x340e | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
MFP-750 | USB | 0x04e8/0x340f | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4x16 | USB | 0x04e8/0x3409 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4x20 | USB | 0x04e8/0x3412 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4x21 | USB | 0x04e8/0x3419 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4x26 | USB | 0x04e8/0x3432 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-5x30 | USB | 0x04e8/0x341a | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-6x20 | USB | 0x04e8/0x340d | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-6x22 | USB | 0x04e8/0x341d | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-6x45 | USB | 0x04e8/0x3420 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-6x55 | USB | 0x04e8/0x3429 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-6x55X | USB | 0x04e8/0x3443 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-470x | USB | 0x04e8/0x3457 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-681x | USB | 0x04e8/0x3466 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-3205W (SCX-3200 Series) | USB Ethernet | 0x04e8/0x3441 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-3400 | USB | 0x04e8/0x344f | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-3405W | Ethernet |  | Basic |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4100 | USB | 0x04e8/0x3413 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4200 | USB | 0x04e8/0x341b | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4300 | USB | 0x04e8/0x342e | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4500 | USB | 0x04e8/0x3426 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4500W | USB Ethernet | 0x04e8/0x342b | Basic |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4600 | USB | 0x04e8/0x3433 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4623 | USB | 0x04e8/0x3434 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4623FW | USB | 0x04e8/0x3440 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4650 4x21S Series | USB | 0x04e8/0x345b | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4725FN | USB | 0x04e8/0x341f | Unsupported | Not supported. See link for details. | unsupported (2010-06-09) | ?
SCX-4729FD | USB | 0x04e8/0x3453 | Basic |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4824 (SCX-4x24 Series) | USB | 0x04e8/0x342c | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4825FN (SCX-4x25 Series) | USB | 0x04e8/0x343c | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4828FN (SCX-4x28 Series) | USB | 0x04e8/0x342d | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4833FD | USB | 0x04e8/0x344b | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-4835FD | Ethernet | 0x04e8/0x344b | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-5635 | USB | 0x04e8/0x3430 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-5835_5935 | USB | 0x04e8/0x342f | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-5835_5935X | USB | 0x04e8/0x3446 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-6545 | USB | 0x04e8/0x3437 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX-6545X | USB | 0x04e8/0x3442 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX4725 | USB | 0x04e8/0x341f | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SCX4725-FN | USB | 0x04e8/0x341f | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
SF-760 | USB | 0x04e8/0x3450 | Untested |  | xerox_mfp (1.0-13) | sane-xerox_mfp

### Manufacturer: Scanport

Link(s): http://www.scanport.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
SQ300 | Parport? |  | Basic |  | microtek2 (unmaintained) | sane-microtek2
SQ2030 | Parport |  | Basic |  | microtek2 (unmaintained) | sane-microtek2
SQ4836 | SCSI |  | Basic |  | microtek2 (unmaintained) | sane-microtek2

### Manufacturer: Scanshell

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
800N | USB | 0x0a82/0x6605 | Unsupported | Not supported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: Sceptre

Link(s): http://www.sceptre.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Vividscan S1200 | SCSI |  | Basic |  | sceptre (1.0-10) | sane-sceptre

### Manufacturer: Sharp

Link(s): http://sharp-world.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
JX-250 | SCSI |  | Good |  | sharp (0.32) | sane-sharp
JX-320 | SCSI |  | Good |  | sharp (0.32) | sane-sharp
JX-325 | SCSI |  | Untested |  | sharp (0.32) | sane-sharp
JX-330 | SCSI |  | Good |  | sharp (0.32) | sane-sharp
JX-350 | SCSI |  | Good |  | sharp (0.32) | sane-sharp
JX-610 | SCSI |  | Good |  | sharp (0.32) | sane-sharp

### Manufacturer: Sicos

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
DMS 2000 | proprietary |  | Unsupported | Not supported until now. Work on a backend has started, contact the author for details (see link) | unsupported (2010-06-09) | ?

### Manufacturer: Siemens

Link(s): http://www.siemens.com/, http://www.siemens.de/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
9036 Flatbed scanner | SCSI |  | Basic |  | s9036 (unmaintained) | sane-s9036
Cherry FingerTIP ID Board - Sensor | USB | 0x0681/0x0010 | Unsupported | Not supported. | unsupported (2010-06-09) | ?
ID Mouse Professional | USB | 0x0681/0x0005 | Unsupported | Not supported. | unsupported (2010-06-09) | ?
S9036 | SCSI |  | Untested | gray only | agfafocus (unmaintained) | sane-agfafocus
ST400 | SCSI |  | Basic | 6 bit gray | st400 (1.6) | sane-st400
ST800 | SCSI |  | Basic | 6 bit gray | st400 (1.6) | sane-st400

### Manufacturer: SmartDisk

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
SmartScan 3600 | USB IEEE-1394 |  | Unsupported | Probably not supported. Same as PIE Primefilm 2600 PRO. | unsupported (2010-06-09) | ?

### Manufacturer: Spot Technology

Comment: Spot seems have gone out of business.

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Maxiscan A4 | proprietary |  | Unsupported | Not supported until now. Work on a backend has started, see link for more information. | unsupported (2010-06-09) | ?
ScanTak 2c | proprietary |  | Unsupported | Not supported. Work on a backend has started, see link for more information. | unsupported (2010-06-09) | ?
ScanTak 3c | proprietary |  | Unsupported | Not supported. Work on a backend has started, see link for more information. | unsupported (2010-06-09) | ?

### Manufacturer: Syscan

Link(s): http://www.syscaninc.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
DocketPort 465 | USB | 0x0a82/0x4802 | Untested | All resolution and mode should be supported, but uncorrected scans | genesys (1.0-63) | sane-genesys
DocketPort 485 | USB | 0x0a82/0x4810 | Basic | All resolution and mode supported, front- and backside side-by-side, with backside mirrored horizontally. | genesys (1.0-63) | sane-genesys
DocketPort 665 | USB | 0x0a82/0x4803 | Basic | All resolution and mode supported, calibration is available | genesys (1.0-63) | sane-genesys
DocketPort 685/ Ambir DS685 | USB | 0x0a82/0x480c | Good | All resolution and mode supported, calibration is available, front- and backside side-by-side, with backside mirrored horizontally. | genesys (1.0-63) | sane-genesys
TravelScan 460/464 | USB | 0x0a82/0x4600 | Complete |  | plustek (0.52) | sane-plustek
TravelScan 662 | USB | 0x0a82/0x6620 | Complete |  | plustek (0.52) | sane-plustek
TravelScan FS-531 | USB | 0x0a82/0x0530 | Unsupported | Not supported. May work with the Plustek backend in future. See link for details. | unsupported (2010-06-09) | ?
TravelScan Pro | USB | 0x0a82/0x2000 | Unsupported | Probably not supported. Some information is available. | unsupported (2010-06-09) | ?

### Manufacturer: Tamarack

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Artiscan 2400FS | USB | 0x05e3/0x0100 | Unsupported | Unsupported. See link for more information. | unsupported (2010-06-09) | ?
Artiscan 6000C | SCSI |  | Good | 3 pass, 300 DPI | tamarack (unmaintained) | sane-tamarack
Artiscan 8000C | SCSI |  | Good | 3 pass, 400 DPI | tamarack (unmaintained) | sane-tamarack
Artiscan 9600 | Parport |  | Unsupported | Unsupported at the moment. See link for a project for that scanner taht may support it in future. | unsupported (2010-06-09) | ?
Artiscan 9600 pro 36 | Parport |  | Unsupported | Unsupported at the moment. See link for a project for that scanner. | unsupported (2010-06-09) | ?
Artiscan 12000C | SCSI |  | Good | 3 pass, 600 DPI | tamarack (unmaintained) | sane-tamarack

### Manufacturer: Targa

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Funline TS6 EP | Parport (EPP) |  | Good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
Funline TS12 EP | Parport (EPP) |  | Good | 600x1200 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp

### Manufacturer: TCE

Link(s): http://www.tce.com.br/
Comment: Brasilian vendor.

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
MK600U | USB | 0x0461/0x0346 | Unsupported | Not supported. Some information is available. | unsupported (2010-06-09) | ?
S450 | Parport |  | Unsupported | Not supported by SANE but is reported to work with pxscan (see link). | unsupported (2010-06-09) | ?

### Manufacturer: Teco

Link(s): http://www.tecoimage.com.tw/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
VM6509F | USB | 0x080d/0x0102 | Unsupported | Probably unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: TemPlate

Link(s): http://www.template.com/, http://www.template.de/
Comment: TemPlate scanners are sometimes labeled "TMP "

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Templ Z | SCSI | 0x1234/0x4321 | Untested | With Z-Axis scrolling | template (0.42, NEW!) | sane-template
Templ ZQ | USB | 0x1234/0x4323 | Minimal |  | template (0.42, NEW!) | sane-template
Templ ZS | USB | 0x1234/0x4322 | Unsupported | No support yet, but we have docs. | template (0.42, NEW!) | sane-template
Templ ZY | SCSI |  | Basic |  | template (0.42, NEW!) | sane-template
Templ ZZ | SCSI |  | Good |  | template (0.42, NEW!) | sane-template

### Manufacturer: Tiny

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
FU661E | USB | 0x0461/0x0347 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: TriGem

Link(s): http://www.nikon.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
PowerScanII | SCSI |  | Good | OK | umax (1.0-41) | sane-umax

### Manufacturer: Trust

Link(s): http://www.trust-site.com, http://www.trust-site.com/home/, http://www.trust.com
Comment: Carefully check the model names. Trust uses similar names for completely different hardware.

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
240H Easy Webscan Gold | USB | 0x05d8/0x4007 | Basic | Works up to 600 dpi | artec_eplus48u (unmaintained) | sane-artec_eplus48u
240TH Easy Webscan Gold | USB | 0x055f/0x0218 | Good | Same as Mustek Bearpaw 2400 TA plus. | gt68xx (1.0-84) | sane-gt68xx
CombiScan 19200 | Parport USB | 0x05cb/0x1483 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
Compact Scan USB 19200 | USB | 0x055f/0x0006 | Complete | Mustek 1200 UB compatible | mustek_usb (1.0-18) | sane-mustek_usb
Compact Scan USB 19200 | USB | 0x05d8/0x4002 | Good | Works, if you have vendor id 0x055f and product id 0x0006, use the mustek_usb backend instead, similar to Mustek ScanExpress 1200 UB (Plus) | gt68xx (1.0-84) | sane-gt68xx
Direct WebScan 19200 | USB | 0x055f/0x021c | Good | Same as Mustek BearPaw 1200 CU Plus (0x021c). | gt68xx (1.0-84) | sane-gt68xx
Easy Connect 9600+ | Parport (EPP) |  | Good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
Easy Connect 19200+ | Parport (EPP) |  | Good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
Easy Scan 9600 Plus | Parport |  | Basic | Requires the program 'as6edriver' to run. | as6e (0.5) | sane-as6e
Easy Webscan 19200 | USB | 0x05d8/0x4006 | Good |  | artec_eplus48u (unmaintained) | sane-artec_eplus48u
EasyScan 19200 | Parport |  | Unsupported |  | unsupported (2010-06-09) | ?
Flat Scan USB 19200 | USB | 0x05d8/0x4002 | Good | Similar to Artec Ultima 2000 | gt68xx (1.0-84) | sane-gt68xx
Imagery 1200 | SCSI |  | Good | 3-pass, Mustek Paragon MFS-6000CX compatible | mustek (1.0-138) | sane-mustek
Imagery 1200 SP | SCSI |  | Complete | Mustek Paragon MFS-6000SP compatible | mustek (1.0-138) | sane-mustek
Imagery 2400 SP | SCSI |  | Good | sub model VM3552 | teco3 (1.0-1) | sane-teco3
Imagery 4800 SP | SCSI |  | Complete | Mustek Paragon 600 II CD compatible | mustek (1.0-138) | sane-mustek
Imagery 4800 SP+ | SCSI |  | Good | sub model VM3552 | teco3 (1.0-1) | sane-teco3
Imagery 9600 SP | SCSI |  | Untested | sub model VM3552 | teco3 (1.0-1) | sane-teco3
Office Scan USB 19200 | USB | 0x047b/0x1000 | Complete |  | niash (0.3) | sane-niash
SCSI Connect 19200 | SCSI |  | Complete | Mustek ScanExpress 12000SP compatible | mustek (1.0-138) | sane-mustek
SCSI excellence series 19200 | SCSI |  | Complete | Mustek ScanExpress 12000SP compatible | mustek (1.0-138) | sane-mustek
SCSI Scan 19200 -Excellence Series- | SCSI |  | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?

### Manufacturer: UMAX

Link(s): http://www.umax.com/, http://www.umax.com.tw/, http://www.umax.de/en, http://www.umax-europe.com, http://www.umaxjapan.co.jp, http://www.umax.com.cn, http://www.umax.com

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Astra 600P | Parport (SPP/ECP) |  | Unsupported | untested, but should be close to 610P | umax_pp (1) | sane-umax_pp
Astra 600S | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Astra 610P | Parport (SPP/ECP) |  | Good |  | umax_pp (1) | sane-umax_pp
Astra 610S | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Astra 1200S | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Astra 1220P | Parport (EPP/ECP) |  | Good |  | umax_pp (1) | sane-umax_pp
Astra 1220S | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Astra 1220U | USB | 0x1606/0x0010 | Good |  | umax1220u (unmaintained) | sane-umax1220u
Astra 1600P | Parport (EPP/ECP) |  | Good |  | umax_pp (1) | sane-umax_pp
Astra 1600U | USB | 0x1606/0x0030 | Good |  | umax1220u (unmaintained) | sane-umax1220u
Astra 2000P | Parport (EPP/ECP) |  | Good |  | umax_pp (1) | sane-umax_pp
Astra 2000U | USB | 0x1606/0x0030 | Good |  | umax1220u (unmaintained) | sane-umax1220u
Astra 2100S | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Astra 2100U | USB | 0x1606/0x0130 | Good |  | umax1220u (unmaintained) | sane-umax1220u
Astra 2200 (SU) | USB | 0x1606/0x0230 | Good | OK, needs USB control messages | umax (1.0-41) | sane-umax
Astra 2200 (SU) | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Astra 2400S | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Astra 2500 | USB | 0x0461/0x0374 | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
Astra 2850 | USB | 0x07b3/0x0601 | Unsupported | Probably not supported. Same IDs as Plustek OpticPro ST24. See link for details. | unsupported (2010-06-09) | ?
Astra 3000 | USB | 0x0461/0x038a | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
Astra 3600 | USB | 0x0461/0x038a | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
Astra 4000 | USB | 0x1606/0x1030 | Unsupported | Not supported. See link for details. | unsupported (2010-06-09) | ?
Astra 4100 | USB | 0x0461/0x038c | Unsupported | Not supported, to be added to genesys backend. | unsupported (2010-06-09) | ?
Astra 4400 | USB | 0x1606/0x0070 | Good | Supports 75, 150, 300, 600 and 1200 dpi | rts8891 (1.0-0) | sane-rts8891
Astra 4450 | USB | 0x1606/0x0070 | Untested |  | rts8891 (1.0-0) | sane-rts8891
Astra 4500 | USB | 0x0638/0x0a10 | Unsupported | GL646 based, to be added to genesys backend. Avision iVina FB1600 clone | unsupported (2010-06-09) | ?
Astra 4600 | USB |  | Unsupported | Probably not supported, no details known. | unsupported (2010-06-09) | ?
Astra 4700 | USB | 0x0638/0x0a20 | Unsupported | GL646/GL660 based. Avision iVina FB1800 clone. | unsupported (2010-06-09) | ?
Astra 4900 | USB | 0x06dc/0x0020 | Minimal | developing yet | hp3900 (0.12) | sane-hp3900
Astra 6400 | IEEE-1394 |  | Unsupported | will probably work one day | umax (1.0-41) | sane-umax
Astra 6450 | IEEE-1394 |  | Unsupported | will probably work one day | umax (1.0-41) | sane-umax
Astra 6700 | USB |  | Unsupported | Not supported. No chipset information available. Same as Avision iVina FB2400. | unsupported (2010-06-09) | ?
Astra MX3 | USB |  | Good | OK, needs USB control messages | umax (1.0-41) | sane-umax
Astra MX3 | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
AstraSlim | USB | 0x080d/0x0104 | Unsupported | Probably not supported currently. See link for more details. | unsupported (2010-06-09) | ?
AstraSlim 1200 | USB | 0x080d/0x0110 | Unsupported | See link for more details. | unsupported (2010-06-09) | ?
AstraSlim 1200 SE | USB | 0x05d8/0x4010 | Good |  | artec_eplus48u (unmaintained) | sane-artec_eplus48u
AstraSlim 6000 | USB | 0x080d/0x0104 | Unsupported | Probably not supported currently. See link for more details. | unsupported (2010-06-09) | ?
AstraSlim SE | USB | 0x05d8/0x4009 | Good |  | artec_eplus48u (unmaintained) | sane-artec_eplus48u
Gemini D-16 | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Mirage D-16L | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Mirage II | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Mirage IIse | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Nete3470' | Parport |  | Unsupported | Probably not supported. No details known.. | unsupported (2010-06-09) | ?
PL-II | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
PowerLook | SCSI |  | Good | OK, SCSI-ID=PS-2400X | umax (1.0-41) | sane-umax
Powerlook 180 | USB |  | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
PowerLook 270 | SCSI |  | Unsupported | incompatible | umax (1.0-41) | sane-umax
PowerLook 270plus | SCSI |  | Unsupported | incompatible | umax (1.0-41) | sane-umax
Powerlook 1000 USB | USB |  | Unsupported | Probably not supported. No further information available. | unsupported (2010-06-09) | ?
PowerLook 1100 | IEEE-1394 |  | Unsupported | will probably work one day | umax (1.0-41) | sane-umax
PowerLook 2000 | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
PowerLook 2100XL | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
PowerLook 3000 | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
PowerLook III | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
PSD | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Supervista S-12 | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
UC 630 | SCSI |  | Good | Version 2.8 OK, others only lineart OK | umax (1.0-41) | sane-umax
UC 840 | SCSI |  | Good | Version 1.6 OK, others only lineart OK | umax (1.0-41) | sane-umax
UC 1200S | SCSI |  | Untested | may work, please test and give feedback | umax (1.0-41) | sane-umax
UC 1200SE | SCSI |  | Good | Version 3.0 OK, others unknown | umax (1.0-41) | sane-umax
UC 1260 | SCSI |  | Good | Version 1.6 OK, others unknown | umax (1.0-41) | sane-umax
UG 80 | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
UG 630 | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
UMAX 3400 | USB | 0x1606/0x0060 | Complete | there are some UMAX 3400 outside the U.S. which are not supported, as they use another chipset than the LM983x | plustek (0.52) | sane-plustek
UMAX 3400 | USB | 0x1606/0x0050 | Complete | there are some UMAX 3400 outside the U.S. which are not supported, as they use another chipset than the LM983x | plustek (0.52) | sane-plustek
UMAX 3450 | USB | 0x1606/0x0060 | Complete |  | plustek (0.52) | sane-plustek
UMAX 5400 | USB | 0x1606/0x0160 | Complete |  | plustek (0.52) | sane-plustek
UMAX Astranet ia101 | USB | 0x1606/0x0060 | Complete | seems to be a renamed UMAX 3400 | plustek (0.52) | sane-plustek
UMAX S-6E | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
UMAX S-6EG | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
UMAX S-12 | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
UMAX S-12G | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
UMAX VT600 | SCSI |  | Untested | may work, please test and give feedback | umax (1.0-41) | sane-umax
Vista S6 | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Vista S6E | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Vista-S8 | SCSI |  | Good | OK | umax (1.0-41) | sane-umax
Vista-T630 | SCSI |  | Good | OK for some firmwareversions, on others only lineart OK | umax (1.0-41) | sane-umax

### Manufacturer: Vantas

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
3000 | USB | 0x04a7/0x0224 | Unsupported | Not supported. See link for more details. | unsupported (2010-06-09) | ?

### Manufacturer: Visioneer

Link(s): http://www.visioneer.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
4800 One Touch | USB | 0x04a7/0x03a0 | Unsupported | Unsupported. See link for details. Different id compared to One Touch 4800? | unsupported (2010-06-09) | ?
6200 | USB | 0x0461/0x0345 | Unsupported | Not supported. Is reported to use the E5 chipset. Uses a Primax ID. Looks similar to Primascan Colorado 2600u. | unsupported (2010-06-09) | ?
6200 EPP/USB | USB | 0x04a7/0x0311 | Unsupported | Not supported. Id is from Primax? Yet another scanner with the same name? | unsupported (2010-06-09) | ?
9320 | USB | 0x04a7/0x0420 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
9420 | USB | 0x0461/0x03a8 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
9450 | USB | 0x04a7/0x0421 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
9450 USB | USB | 0x04a7/0x0421 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
9450-G | USB | 0x04a7/0x047a | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
9550 | USB | 0x04a7/0x0422 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
9650 | USB | 0x04a7/0x0390 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
9650-G | USB | 0x04a7/0x047b | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
9750 | USB | 0x04a7/0x0423 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
9750-G | USB | 0x04a7/0x0493 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
DocuImage 620S | SCSI |  | Unsupported | Not supported. See link for more details. | unsupported (2010-06-09) | ?
DocuMate 510 | USB | 0x04a7/0x047c | Unsupported | Not supported. See link for more details. Yet another USB id. | unsupported (2010-06-09) | ?
DocuMate 510 | USB | 0x04a7/0x0446 | Unsupported | Not supported. See link for more details. | unsupported (2010-06-09) | ?
One Touch 4800 | USB | 0x04a7/0x0224 | Unsupported | Unsupported. See link for details. Different id compared to 4800 One Touch? | unsupported (2010-06-09) | ?
Onetouch 4400 | USB | 0x0461/0x0347 | Unsupported | Not supported. E5 chipset? See link for more details. | unsupported (2010-06-09) | ?
OneTouch 4800 USB | USB | 0x04a7/0x0224 | Unsupported | Unsupported. Seems to use Realtek RTS8801B. Same as Microtek Scanport 3000. See link for details. | unsupported (2010-06-09) | ?
OneTouch 5300 | USB | 0x04a7/0x0221 | Unsupported | Not supported. Yet another scanner with this name? | unsupported (2010-06-09) | ?
OneTouch 5300 USB | USB | 0x04a7/0x0226 | Unsupported | Not supported. Chipset is RTS8801B(?). See link for output of /proc/bus/usb/devices. | unsupported (2010-06-09) | ?
OneTouch 5800 USB | USB | 0x04a7/0x0226 | Unsupported | Unsupported. 48 bit scanner, doesn't work with viceo backend. RTS8801C. | unsupported (2010-06-09) | ?
OneTouch 6600 | USB | 0x04a7/0x022a | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
Onetouch 7100 | USB | 0x04a7/0x0229 | Unsupported | GL646 based, to be added to genesys backend | unsupported (2010-06-09) | ?
OneTouch 7300 | USB | 0x04a7/0x0444 | Good | Works upto 1200 dpi and 12 bits/color. | gt68xx (1.0-84) | sane-gt68xx
Onetouch 7700 | USB | 0x04a7/0x0380 | Unsupported | LM9832/3 based, to be added to plustek backend | unsupported (2010-06-09) | ?
OneTouch 8100 | USB | 0x04a7/0x0321 | Unsupported | Unsupported. See link for details. | unsupported (2010-06-09) | ?
Onetouch 8700 | USB | 0x04a7/0x0371 | Unsupported | Not supported. See link for details. | unsupported (2010-06-09) | ?
Onetouch 8900 | USB | 0x04a7/0x0371 | Unsupported | Not supported. Same as 8920 but without TA? | unsupported (2010-06-09) | ?
Onetouch 8920 | USB | 0x04a7/0x0371 | Unsupported | Not supported. Same as 8700 and 8900 but includes a TA. Uses a Primax ID. Chipset is RTS8801C. See link for output of /proc/bus/usb/devices. | unsupported (2010-06-09) | ?
Onetouch 9000 | USB | 0x04a7/0x022c | Unsupported | Not supported. See link for details. | unsupported (2010-06-09) | ?
Onetouch 9020 | USB | 0x04a7/0x022c | Unsupported | Not supported. See link for details. | unsupported (2010-06-09) | ?
Onetouch 9320 | USB | 0x04a7/0x0362 | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
Onetouch Pro 8800 | USB | 0x04a7/0x0410 | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
Onetouch Pro 8820 | USB | 0x04a7/0x0410 | Unsupported | Probably not supported. See link for details. | unsupported (2010-06-09) | ?
PaperPort 3100b | Parport |  | Unsupported | Most probably not supported. See link for details. | unsupported (2010-06-09) | ?
PaperPort 6100 | Parport |  | Unsupported | Most probably not supported. More details would be appreciated. | unsupported (2010-06-09) | ?
PaperPort OneTouch | Parport |  | Unsupported | Most probably not supported. See link for details. | unsupported (2010-06-09) | ?
Patriot 430 | USB | 0x04a7/0x0497 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
Patriot 470 | USB | 0x04a7/0x048f | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
Patriot 680 | USB | 0x04a7/0x0498 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
Patriot 780 | USB | 0x04a7/0x0499 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
Roadwarrior | USB | 0x04a7/0x0494 | Basic | All resolution and mode supported, calibration is available | genesys (1.0-63) | sane-genesys
Strobe Pro USB | USB | 0x04a7/0x0102 | Unsupported | Not supported. See link for details. | unsupported (2010-06-09) | ?
Strobe XP 100 | USB | 0x04a7/0x0427 | Basic |  | plustek (0.52) | sane-plustek
Strobe XP 100,r3 | USB | 0x04a7/0x049b | Good | All resolution and mode supported, calibration is available | genesys (1.0-63) | sane-genesys
Strobe XP 200 | USB | 0x04a7/0x0426 | Good | All resolution and mode supported, calibration is available | genesys (1.0-63) | sane-genesys
Strobe XP 300 | USB | 0x04a7/0x0474 | Good | All resolution and mode supported, calibration is available, front- and backside side-by-side, with backside mirrored horizontally. | genesys (1.0-63) | sane-genesys
Strobe XP 450 | USB | 0x04a7/0x0424 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
Strobe XP 450-G | USB | 0x04a7/0x0491 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
Strobe XP 470 | USB | 0x04a7/0x0479 | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
Strobe XP 470-G | USB | 0x04a7/0x048f | Complete | sheetfed scanner | avision (Build: 296) | sane-avision
Visioneer OneTouch 7100 | USB | 0x04a7/0x0229 | Complete | Same as MD5345 | genesys (1.0-63) | sane-genesys
WorkCentre 470cx | Parport |  | Unsupported | Not supported. See link for more details. | unsupported (2010-06-09) | ?
WorkCentre M15i | USB | 0x0924/0xffef | Unsupported | Not supported. See link for more details. | unsupported (2010-06-09) | ?
WorkCentre PE16 | USB Parport | 0x0924/0x4220 | Unsupported | Not supported. See link for more details. | unsupported (2010-06-09) | ?
WorkCentre PE120i | USB | 0x0924/0x4237 | Unsupported | Not supported. See link for more details. | unsupported (2010-06-09) | ?
WorkCentre Pro 412 | USB Parport | 0x043d/0x4303 | Unsupported | Not supported. See link for more details. | unsupported (2010-06-09) | ?
WorkCentre XK35c | USB Parport | 0x043d/0x0020 | Unsupported | Not supported. See link for more details. | unsupported (2010-06-09) | ?
WorkCentre XK50cx | USB | 0x04e8/0x3903 | Unsupported | Not supported. See link for more details. | unsupported (2010-06-09) | ?

### Manufacturer: Viviscan

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Compact II | Parport (EPP) |  | Good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp

### Manufacturer: Vobis

Link(s): http://www.vobis.de/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
HighScan | SCSI |  | Complete | only E3plus based models | microtek2 (unmaintained) | sane-microtek2
Highscreen Realscan | SCSI |  | Good |  | microtek (0.13.1) | sane-microtek
Highscreen Scanboostar Premium | SCSI |  | Good | OK, SCSI-ID=LinoHell Office2 | umax (1.0-41) | sane-umax

### Manufacturer: Vuego

Comment: Company was renamed to Benq.

### Manufacturer: Xerox

Link(s): http://www.xerox.com/, http://www.office.xerox.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
2400 Onetouch | USB | 0x0461/0x038b | Complete | GL646 based, resolution from 75 to 2400 dpi | genesys (1.0-63) | sane-genesys
DocuMate150 | USB | 0x04a7/0x049c | Good |  | avision (Build: 296) | sane-avision
DocuMate152 | USB | 0x04a7/0x0477 | Good |  | avision (Build: 296) | sane-avision
DocuMate162 | USB | 0x04a7/0x049d | Good |  | avision (Build: 296) | sane-avision
DocuMate232 | USB | 0x04a7/0x0476 | Good |  | avision (Build: 296) | sane-avision
DocuMate250 | USB | 0x04a7/0x0448 | Good |  | avision (Build: 296) | sane-avision
DocuMate250-G | USB | 0x04a7/0x0490 | Good |  | avision (Build: 296) | sane-avision
DocuMate252 | USB | 0x04a7/0x0449 | Good |  | avision (Build: 296) | sane-avision
DocuMate252-G | USB | 0x04a7/0x048c | Good |  | avision (Build: 296) | sane-avision
DocuMate262 | USB | 0x04a7/0x044c | Good |  | avision (Build: 296) | sane-avision
DocuMate262-G | USB | 0x04a7/0x048d | Good |  | avision (Build: 296) | sane-avision
DocuMate262i | USB | 0x04a7/0x04a7 | Good |  | avision (Build: 296) | sane-avision
DocuMate272 | USB | 0x04a7/0x0475 | Untested |  | avision (Build: 296) | sane-avision
DocuMate272-G | USB | 0x04a7/0x048e | Untested |  | avision (Build: 296) | sane-avision
DocuMate510 | USB | 0x04a7/0x0446 | Untested |  | avision (Build: 296) | sane-avision
DocuMate510-G | USB | 0x04a7/0x047c | Untested |  | avision (Build: 296) | sane-avision
DocuMate512 | USB | 0x04a7/0x0495 | Untested |  | avision (Build: 296) | sane-avision
DocuMate520 | USB | 0x04a7/0x0447 | Untested |  | avision (Build: 296) | sane-avision
DocuMate520-G | USB | 0x04a7/0x0492 | Untested |  | avision (Build: 296) | sane-avision
DocuMate632 | USB | 0x04a7/0x0498 | Untested |  | avision (Build: 296) | sane-avision
DocuMate752 | USB | 0x04a7/0x049a | Untested |  | avision (Build: 296) | sane-avision
DocuMate752 | USB | 0x04a7/0x0478 | Untested |  | avision (Build: 296) | sane-avision
Phaser 3200MFP | USB | 0x0924/0x3da4 | Complete |  | xerox_mfp (1.0-13) | sane-xerox_mfp
Phaser 6110MFP | USB | 0x0924/0x3d5d | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
Travel Scanner 100 | USB | 0x04a7/0x04ac | Good | All resolution and mode supported, calibration is available | genesys (1.0-63) | sane-genesys
WorkCentre 3119 Series | USB | 0x0924/0x4265 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
WorkCentre 3210 | USB | 0x0924/0x4293 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
WorkCentre 3220 | USB | 0x0924/0x4294 | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp
WorkCentre 4118 Series | USB | 0x0924/0x420c | Good |  | xerox_mfp (1.0-13) | sane-xerox_mfp

### Manufacturer: Yakumo

Link(s): http://www.yakumo.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Scan50 | USB | 0x05d8/0x4011 | Good |  | artec_eplus48u (unmaintained) | sane-artec_eplus48u

## Still Cameras

Manufacturers: Kodak, Polaroid

### Manufacturer: Kodak

Link(s): http://www.kodak.com/global/en/service/digCam/dc25/dc25.shtml, http://www.kodak.com/global/en/service/digCam/dc210/dc210.shtml, http://www.kodak.com/global/en/service/products/ekn006568.jhtml

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
DC20 | Serial port |  | Basic | DC-20 untested by author but reported to work | dc25 (1.2) | sane-dc25
DC25 | Serial port |  | Complete |  | dc25 (1.2) | sane-dc25
DC210 | Serial port |  | Basic |  | dc210 (0.0) | sane-dc210
DC240 | Serial port |  | Good | Use gphoto2 backend to get USB support | dc240 (0.0) | sane-dc240

### Manufacturer: Polaroid

Link(s): http://www.polaroid.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
DMC | SCSI |  | Good |  | dmc (unmaintained) | sane-dmc

## Video Cameras

Manufacturers: Aiptek, Biolux, Connectix, Creative, Digital Dream, Grandtek Scopecam, Konica

### Manufacturer: Aiptek

Link(s): http://www.aiptek.com.tw

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Aiptek Pencam | USB | 0x0553/0x0202 | Minimal | image is OK for CIF and QCIF, VGA and QVGA untested, streaming video is a problem | stv680 (1.0-1) | sane-stv680

### Manufacturer: Biolux

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
654 (micrOcular) | USB | 0x0923/0x010f | Unsupported | Not supported yet. See link for more details. | unsupported (2010-06-09) | ?

### Manufacturer: Connectix

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
Color QuickCam | Parport |  | Good | Requires root privileges. | qcam (unmaintained) | sane-qcam
Greyscale QuickCam | Parport |  | Minimal | Requires root privileges. Partly working. | qcam (unmaintained) | sane-qcam

### Manufacturer: Creative

Link(s): http://www.creative.com/

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
WebCam Go Mini | USB | 0x041e/0x4007 | Untested |  | stv680 (1.0-1) | sane-stv680

### Manufacturer: Digital Dream

Link(s): http://www.digitaldreamco.com/en/index.shtml

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
l' espion XS | USB | 0x1183/0x0001 | Untested |  | stv680 (1.0-1) | sane-stv680

### Manufacturer: Grandtek Scopecam

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
8x30 Binocular & Digital Camera | USB | 0x0797/0x801c | Unsupported | Not Supported yet. See link for more details. | unsupported (2010-06-09) | ?

### Manufacturer: Konica

Link(s): http://www.konicaminolta.com

Model | Interface | USB id | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | --- | ---
e-mini | USB | 0x04c8/0x0722 | Untested |  | stv680 (1.0-1) | sane-stv680

## APIs

Backends: gphoto2, pint, pnm, template, test, v4l

### Backend: gphoto2 (0.0)

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-gphoto2
Description: Multiple cameras supported by the gphoto2 libraries
Comment: The long-term plan is to support all the cameras supported by the gphoto2 libraries (currently over 140 models). However, at this stage, only a handful of cameras are definitely known to work with SANE. Other cameras will probably work if the native file format is EXIF or JPEG. Testers welcome!

### Backend: pint (unmaintained)

Manual page: sane-pint
Description: Scanners with the machine-independent PINT interface
Comment: Haven't been tested for a long time. Handle with care.

### Backend: pnm (1.0.8)

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-pnm
Description: Reads PNM files
Comment: Used for debugging frontends. Obsolete, use test backend instead.

### Backend: template (0.42, NEW!)

Link(s): http://www.luser.com/temp/, http://www.luser.com/b/
Manual page: sane-template
Comment: This backend supports only the USB and SCSI models
Description: Interface to FrObYz API
Comment: Only FrObYz version 2.0 is supported!

### Backend: test (1.0-28)

Link(s): http://www.meier-geinitz.de/sane/test-backend/
Manual page: sane-test
Description: Frontend-tester
Comment: Backend for testing frontends. Also serves as example for SANE backend options.

### Backend: v4l (1.0-3)

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-v4l
Description: Interface to Video For Linux API
Comment: Supports video cameras and other devices accessed by the v4l kernel API, e.g. bttv devices. Quite a lot of known bugs.

## Meta Backends

Backends: dll, net

### Backend: dll (1.0.13)

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-dll
Description: Dynamic loading of shared-library backends.

### Backend: net (1.0.14)

Link(s): http://www.penguin-breeder.org/?page=sane-net
Manual page: sane-net
Description: Network access to saned servers
Comment: Can be used to access any scanner supported by SANE over the net. Supports IPv4 and IPv6.

### Legend:

> Model:
>   Name of the the device.
> Interface:
>   How the device is connected to the computer.
> USB id:
>   The USB vendor and product ids as printed by sane-find-scanner -q (only applicable for USB devices).
> Status:
>   Indicates how many of the features the device provides are supported by SANE.
>   - unsupported means the device is not supported at least by this backend. It may be supported by other backends, however.
>   - untested means the device may be supported but couldn't be tested. Be very careful and report success/failure.
>   - minimal means that the device is detected and scans at least in one mode. But the quality is bad or important features won't work.
>   - basic means it works at least in the most important modes but quality is not perfect.
>   - good means the device is usable for day-to-day work. Some rather exotic features may be missing.
>   - complete means the backends supports everything the device can do.
> Comment:
>   More information about the backend or model, e.g. the level of support and possible problems.
> Backend:
>   Name of the backend, in parentheses if available: Version of backend/driver; newer versions may be available from their home sites.
>   NEW! means brand-new to the current release of SANE.
>   UNMAINTAINED means that nobody maintains that backend. Expect no new features or newly supported devices. You are welcome to take over maintainership.
> Manual Page:
>   A link to the man-page online, if it exists.
> Manufacturer:
>   Manufacturer, vendor or brand name of the device.
> Description:
>   The scope of application of the backend.

SANE homepage
This page was last updated on Tue Jan 13 19:27:30 2015 by sane-desc 3.5 from sane-backends 1.0.24